<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<text>B-Spec V2.0.1</text>
<text>M. McPartlan, 2019</text>
<text>Loyola Marymount University</text>
<wire x1="97.79" y1="133.35" x2="97.79" y2="47.5608625" width="0.1524" layer="20"/>
<wire x1="97.79" y1="47.5608625" x2="89.5991375" y2="39.37" width="0.1524" layer="20" curve="-90"/>
<wire x1="89.5991375" y1="39.37" x2="3.81" y2="39.37" width="0.1524" layer="20"/>
<wire x1="3.81" y1="39.37" x2="-2.54" y2="45.72" width="0.1524" layer="20" curve="-90"/>
<wire x1="-2.54" y1="45.72" x2="-2.54" y2="131.5091375" width="0.1524" layer="20"/>
<wire x1="-2.54" y1="131.5091375" x2="5.6508625" y2="139.7" width="0.1524" layer="20" curve="-90"/>
<wire x1="5.6508625" y1="139.7" x2="91.44" y2="139.7" width="0.1524" layer="20"/>
<wire x1="91.44" y1="139.7" x2="97.79" y2="133.35" width="0.1524" layer="20" curve="-90"/>
<text>RESET</text>
<text>MEAS</text>
<text>LNAV</text>
<text>RNAV</text>
<text>MODE</text>
<text>TRANS</text>
<text>ABS</text>
<text>LNAV</text>
<text>BUT</text>
<text>D0</text>
<text>LS0</text>
<text>ABS</text>
<text>D1</text>
<text>LS1</text>
<text>EN0</text>
<text>EN3</text>
<text>EN1</text>
<text>MEAS</text>
<text>S7</text>
<text>S4</text>
<text>D9</text>
<text>S5</text>
<text>S3</text>
<text>EN2</text>
<text>RES_MCU</text>
<text>D5</text>
<text>D8</text>
<text>S6</text>
<text>S2</text>
<text>D6</text>
<text>D7</text>
<text>S0</text>
<text>S1</text>
<text>RESET_BUTTON</text>
<text>RNAV</text>
<text>MODE</text>
<text>D4</text>
<text>TRANS</text>
<text>D2</text>
<text>D3</text>
<text>SN74HC595</text>
<text>SN74HC595</text>
<text>SN74HC595</text>
<text>SN74HC595</text>
<text>SENSE</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>S7</text>
<text>S6</text>
<text>S5</text>
<text>S4</text>
<text>S3</text>
<text>S2</text>
<text>S1</text>
<text>S0</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_5MM">
<description>&lt;B&gt;LED 5mm PTH&lt;/B&gt;&lt;p&gt;
5 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-IR-THRU&lt;/li&gt;</description>
</package>
<package name="7-SEGMENT-4DIGIT-20MM">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="0805-THM">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_BARGRAPH_10">
<description>&lt;h3&gt;10 Segment LED Bar Graph&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.74mm&lt;/li&gt;
&lt;li&gt;Area:10mm x 25.5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://www.sparkfun.com/datasheets/Components/LED/YSLB-102510B5-10.pdf"&gt;YSLB-102510B5&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="7-SEGMENT-4DIGIT-20MM">
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STANDOFF-ELECTRICAL">
<description>&lt;h3&gt;Standoff (#4 Screw) - w/ Electrical Connection&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw.&lt;/p&gt;
&lt;p&gt;The drill is surrounded by a copper ring, which can be connected to any net.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-B-PTH">
<description>&lt;h3&gt;USB Type B Female PTH Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4 main, 2 shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/USB-B%20Connector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12">
<description>&lt;h3&gt;Plated Through Hole -12 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07">
<description>&lt;h3&gt;Plated Through Hole -7 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="BeagleBone_Blue_R3">
<description>Generated from &lt;b&gt;BeagleBone_Blue.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SOT323">
</package>
</packages>
</library>
<library name="74ttl-din">
<description>&lt;b&gt;TTL Devices with DIN Symbols&lt;/b&gt;&lt;p&gt;
CadSoft and the author do not warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by Holger Bettenbühl, hol.bet.@rhein-main.net&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ABSO" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="E1,8-4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="E1,8-4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="SparkFun-LED" package="LED_BARGRAPH_10" value="BLUE">
<attribute name="PROD_ID" value="DIO-10613"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="SparkFun-LED" package="LED_BARGRAPH_10" value="GREEN">
<attribute name="PROD_ID" value="DIO-10612"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="SparkFun-LED" package="LED_BARGRAPH_10" value="RED">
<attribute name="PROD_ID" value="DIO-10615"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="SparkFun-LED" package="LED_BARGRAPH_10" value="YELLOW">
<attribute name="PROD_ID" value="DIO-10614"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED_BARGRAPH_10" value="BLUE">
<attribute name="PROD_ID" value="DIO-10613"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-LED" package="LED_BARGRAPH_10" value="GREEN">
<attribute name="PROD_ID" value="DIO-10612"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="SparkFun-LED" package="LED_BARGRAPH_10" value="RED">
<attribute name="PROD_ID" value="DIO-10615"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="SparkFun-LED" package="LED_BARGRAPH_10" value="YELLOW">
<attribute name="PROD_ID" value="DIO-10614"/>
<attribute name="VALUE"/>
</element>
<element name="H2" library="SparkFun-Hardware" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL">
<attribute name="VALUE"/>
</element>
<element name="H3" library="SparkFun-Hardware" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL">
<attribute name="VALUE"/>
</element>
<element name="H4" library="SparkFun-Hardware" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="atmel" package="DIL08" value="TINY13V-10PU">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10PU"/>
<attribute name="OC_FARNELL" value="9171576"/>
<attribute name="OC_NEWARK" value="96K6523"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="linear" package="TO220V" value="7805TV">
<attribute name="POPULARITY" value="57"/>
</element>
<element name="LED11" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED12" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED13" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED14" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED15" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED16" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED17" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LEFTNAV" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="MEAS" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="MODE" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="Q1" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="BeagleBone_Blue_R3" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="0805-THM" value="8k">
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="0805-THM" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R12" library="adafruit" package="0805-THM" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R13" library="adafruit" package="0805-THM" value="3k">
<attribute name="VALUE"/>
</element>
<element name="R14" library="adafruit" package="0805-THM" value="5k">
<attribute name="VALUE"/>
</element>
<element name="R15" library="adafruit" package="0805-THM" value="5k">
<attribute name="VALUE"/>
</element>
<element name="R20" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R21" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R22" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R23" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R24" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R25" library="adafruit" package="0805-THM" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R26" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R27" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R28" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R29" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R30" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R31" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R32" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0805-THM" value="150">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0805-THM" value="150">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="RIGHTNAV" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="TRANS" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V1" library="74ttl-din" package="DIL16" value="74595N">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="V2" library="74ttl-din" package="DIL16" value="74595N">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="V3" library="74ttl-din" package="DIL16" value="74595N">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="V4" library="74ttl-din" package="DIL16" value="74595N">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="USB-B-PTH" value="USB_B_PTH">
<attribute name="PROD_ID" value="CONN-08278"/>
<attribute name="SF_ID" value="PRT-00139"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R16" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R17" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="R18" library="adafruit" package="0805-THM" value="60">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="DISP1" library="SparkFun-LED" package="7-SEGMENT-4DIGIT-20MM" value="ATA8041AG">
<attribute name="PROD_ID" value="COMP-11447"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="R11" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="C2" pad="+"/>
<contactref element="R15" pad="1"/>
<contactref element="V4" pad="10"/>
<contactref element="V3" pad="10"/>
<contactref element="V2" pad="10"/>
<contactref element="V1" pad="10"/>
<contactref element="J2" pad="2"/>
<contactref element="V4" pad="16"/>
<contactref element="V3" pad="16"/>
<contactref element="V1" pad="16"/>
<contactref element="V2" pad="16"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="RESET_MC">
<contactref element="R11" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="IC4" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="H4" pad="P1"/>
<contactref element="H3" pad="P1"/>
<contactref element="H2" pad="P1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="LED17" pad="K"/>
<contactref element="LED16" pad="K"/>
<contactref element="LED14" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED12" pad="K"/>
<contactref element="LED11" pad="K"/>
<contactref element="LED13" pad="K"/>
<contactref element="LED15" pad="K"/>
<contactref element="V3" pad="13"/>
<contactref element="V4" pad="13"/>
<contactref element="V2" pad="13"/>
<contactref element="V1" pad="13"/>
<contactref element="J1" pad="GND"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="SHLD2"/>
<contactref element="J1" pad="SHLD1"/>
<contactref element="V4" pad="8"/>
<contactref element="V3" pad="8"/>
<contactref element="V1" pad="8"/>
<contactref element="V2" pad="8"/>
<contactref element="TRANS" pad="K"/>
<contactref element="ABSO" pad="K"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="IC4" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="J1" pad="VBUS"/>
</signal>
<signal name="DATA0">
<contactref element="D6" pad="1"/>
<contactref element="D12" pad="1"/>
<contactref element="D7" pad="10"/>
<contactref element="D9" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="D10" pad="1"/>
<contactref element="D11" pad="10"/>
<contactref element="D13" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="DISP1" pad="3"/>
</signal>
<signal name="DATA1">
<contactref element="D12" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D7" pad="9"/>
<contactref element="D9" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="D11" pad="9"/>
<contactref element="D13" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="DISP1" pad="5"/>
</signal>
<signal name="DATA3">
<contactref element="D12" pad="4"/>
<contactref element="D6" pad="4"/>
<contactref element="D7" pad="7"/>
<contactref element="D9" pad="4"/>
<contactref element="D8" pad="4"/>
<contactref element="D10" pad="4"/>
<contactref element="D11" pad="7"/>
<contactref element="D13" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="DISP1" pad="1"/>
</signal>
<signal name="DATA4">
<contactref element="D6" pad="5"/>
<contactref element="D12" pad="5"/>
<contactref element="D7" pad="6"/>
<contactref element="D9" pad="5"/>
<contactref element="D8" pad="5"/>
<contactref element="D10" pad="5"/>
<contactref element="D11" pad="6"/>
<contactref element="D13" pad="5"/>
<contactref element="R6" pad="2"/>
<contactref element="DISP1" pad="2"/>
</signal>
<signal name="DATA5">
<contactref element="D12" pad="6"/>
<contactref element="D6" pad="6"/>
<contactref element="D7" pad="5"/>
<contactref element="D9" pad="6"/>
<contactref element="D8" pad="6"/>
<contactref element="D10" pad="6"/>
<contactref element="D11" pad="5"/>
<contactref element="D13" pad="6"/>
<contactref element="R7" pad="2"/>
<contactref element="DISP1" pad="4"/>
</signal>
<signal name="DATA7">
<contactref element="D12" pad="8"/>
<contactref element="D6" pad="8"/>
<contactref element="D7" pad="3"/>
<contactref element="D9" pad="8"/>
<contactref element="D8" pad="8"/>
<contactref element="D10" pad="8"/>
<contactref element="D11" pad="3"/>
<contactref element="D13" pad="8"/>
<contactref element="R16" pad="2"/>
<contactref element="DISP1" pad="11"/>
</signal>
<signal name="N$10">
<contactref element="V2" pad="9"/>
<contactref element="V1" pad="14"/>
</signal>
<signal name="BUTTON">
<contactref element="RESET" pad="3"/>
<contactref element="MODE" pad="3"/>
<contactref element="MEAS" pad="3"/>
<contactref element="R15" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="LEFTNAV" pad="3"/>
<contactref element="RIGHTNAV" pad="3"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="RESET" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="MEAS">
<contactref element="R13" pad="2"/>
<contactref element="MEAS" pad="1"/>
</signal>
<signal name="MODE">
<contactref element="R14" pad="2"/>
<contactref element="MODE" pad="1"/>
</signal>
<signal name="SERIAL">
<contactref element="IC1" pad="5"/>
<contactref element="V4" pad="14"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="CLOCK">
<contactref element="IC1" pad="6"/>
<contactref element="V3" pad="11"/>
<contactref element="V4" pad="11"/>
<contactref element="V2" pad="11"/>
<contactref element="V1" pad="11"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="SENSE">
<contactref element="IC1" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="LATCH">
<contactref element="IC1" pad="7"/>
<contactref element="V4" pad="12"/>
<contactref element="V3" pad="12"/>
<contactref element="V2" pad="12"/>
<contactref element="V1" pad="12"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="V1" pad="9"/>
<contactref element="V3" pad="14"/>
</signal>
<signal name="DATA8">
<contactref element="D6" pad="9"/>
<contactref element="D12" pad="9"/>
<contactref element="D7" pad="2"/>
<contactref element="D9" pad="9"/>
<contactref element="D8" pad="9"/>
<contactref element="D10" pad="9"/>
<contactref element="D11" pad="2"/>
<contactref element="D13" pad="9"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="DATA9">
<contactref element="D12" pad="10"/>
<contactref element="D6" pad="10"/>
<contactref element="D7" pad="1"/>
<contactref element="D9" pad="10"/>
<contactref element="D8" pad="10"/>
<contactref element="D10" pad="10"/>
<contactref element="D11" pad="1"/>
<contactref element="D13" pad="10"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="DATA6">
<contactref element="D6" pad="7"/>
<contactref element="D12" pad="7"/>
<contactref element="D7" pad="4"/>
<contactref element="D9" pad="7"/>
<contactref element="D8" pad="7"/>
<contactref element="D10" pad="7"/>
<contactref element="D11" pad="4"/>
<contactref element="D13" pad="7"/>
<contactref element="R9" pad="2"/>
<contactref element="DISP1" pad="7"/>
</signal>
<signal name="DATA2">
<contactref element="D6" pad="3"/>
<contactref element="D12" pad="3"/>
<contactref element="D7" pad="8"/>
<contactref element="D9" pad="3"/>
<contactref element="D8" pad="3"/>
<contactref element="D10" pad="3"/>
<contactref element="D11" pad="8"/>
<contactref element="D13" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="DISP1" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="D7" pad="20"/>
<contactref element="D7" pad="11"/>
<contactref element="D7" pad="12"/>
<contactref element="D7" pad="13"/>
<contactref element="D7" pad="14"/>
<contactref element="D7" pad="15"/>
<contactref element="D7" pad="16"/>
<contactref element="D7" pad="17"/>
<contactref element="D7" pad="18"/>
<contactref element="D7" pad="19"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="D9" pad="20"/>
<contactref element="D9" pad="19"/>
<contactref element="D9" pad="18"/>
<contactref element="D9" pad="17"/>
<contactref element="D9" pad="16"/>
<contactref element="D9" pad="15"/>
<contactref element="D9" pad="14"/>
<contactref element="D9" pad="13"/>
<contactref element="D9" pad="12"/>
<contactref element="D9" pad="11"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="D8" pad="20"/>
<contactref element="D8" pad="19"/>
<contactref element="D8" pad="18"/>
<contactref element="D8" pad="17"/>
<contactref element="D8" pad="16"/>
<contactref element="D8" pad="15"/>
<contactref element="D8" pad="14"/>
<contactref element="D8" pad="13"/>
<contactref element="D8" pad="12"/>
<contactref element="D8" pad="11"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$36">
<contactref element="D10" pad="20"/>
<contactref element="D10" pad="19"/>
<contactref element="D10" pad="18"/>
<contactref element="D10" pad="17"/>
<contactref element="D10" pad="16"/>
<contactref element="D10" pad="15"/>
<contactref element="D10" pad="14"/>
<contactref element="D10" pad="13"/>
<contactref element="D10" pad="12"/>
<contactref element="D10" pad="11"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="N$38">
<contactref element="D11" pad="20"/>
<contactref element="D11" pad="19"/>
<contactref element="D11" pad="18"/>
<contactref element="D11" pad="17"/>
<contactref element="D11" pad="16"/>
<contactref element="D11" pad="15"/>
<contactref element="D11" pad="14"/>
<contactref element="D11" pad="13"/>
<contactref element="D11" pad="12"/>
<contactref element="D11" pad="11"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$39">
<contactref element="D13" pad="20"/>
<contactref element="D13" pad="19"/>
<contactref element="D13" pad="18"/>
<contactref element="D13" pad="17"/>
<contactref element="D13" pad="16"/>
<contactref element="D13" pad="15"/>
<contactref element="D13" pad="14"/>
<contactref element="D13" pad="13"/>
<contactref element="D13" pad="12"/>
<contactref element="D13" pad="11"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="N$40">
<contactref element="D12" pad="20"/>
<contactref element="D12" pad="19"/>
<contactref element="D12" pad="18"/>
<contactref element="D12" pad="17"/>
<contactref element="D12" pad="16"/>
<contactref element="D12" pad="15"/>
<contactref element="D12" pad="14"/>
<contactref element="D12" pad="13"/>
<contactref element="D12" pad="12"/>
<contactref element="D12" pad="11"/>
<contactref element="Q8" pad="3"/>
</signal>
<signal name="G_ENABLE0">
<contactref element="Q1" pad="1"/>
<contactref element="V1" pad="2"/>
</signal>
<signal name="G_ENABLE1">
<contactref element="Q3" pad="1"/>
<contactref element="V1" pad="3"/>
</signal>
<signal name="G_ENABLE2">
<contactref element="Q4" pad="1"/>
<contactref element="V1" pad="4"/>
</signal>
<signal name="G_ENABLE3">
<contactref element="Q2" pad="1"/>
<contactref element="V1" pad="5"/>
</signal>
<signal name="N$35">
<contactref element="Q1" pad="3"/>
<contactref element="D6" pad="11"/>
<contactref element="D6" pad="20"/>
<contactref element="D6" pad="19"/>
<contactref element="D6" pad="18"/>
<contactref element="D6" pad="17"/>
<contactref element="D6" pad="16"/>
<contactref element="D6" pad="15"/>
<contactref element="D6" pad="14"/>
<contactref element="D6" pad="13"/>
<contactref element="D6" pad="12"/>
</signal>
<signal name="G_ENABLE4">
<contactref element="V1" pad="6"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="G_ENABLE5">
<contactref element="V1" pad="7"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="G_ENABLE6">
<contactref element="V3" pad="15"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="G_ENABLE7">
<contactref element="Q8" pad="1"/>
<contactref element="V3" pad="1"/>
</signal>
<signal name="D_ENABLE0">
<contactref element="R20" pad="2"/>
<contactref element="DISP1" pad="6"/>
</signal>
<signal name="D_ENABLE1">
<contactref element="R21" pad="2"/>
<contactref element="DISP1" pad="8"/>
</signal>
<signal name="D_ENABLE2">
<contactref element="R22" pad="2"/>
<contactref element="DISP1" pad="9"/>
</signal>
<signal name="D_ENABLE3">
<contactref element="R23" pad="2"/>
<contactref element="DISP1" pad="12"/>
</signal>
<signal name="SD_ENABLE0">
<contactref element="R20" pad="1"/>
<contactref element="V3" pad="2"/>
</signal>
<signal name="SD_ENABLE1">
<contactref element="R21" pad="1"/>
<contactref element="V3" pad="3"/>
</signal>
<signal name="SD_ENABLE2">
<contactref element="R22" pad="1"/>
<contactref element="V3" pad="4"/>
</signal>
<signal name="SD_ENABLE3">
<contactref element="V3" pad="5"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="LNAV">
<contactref element="R10" pad="2"/>
<contactref element="LEFTNAV" pad="1"/>
</signal>
<signal name="RNAV">
<contactref element="R25" pad="2"/>
<contactref element="RIGHTNAV" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="V4" pad="9"/>
<contactref element="V2" pad="14"/>
</signal>
<signal name="LSOURCE0">
<contactref element="R24" pad="2"/>
<contactref element="LED17" pad="A"/>
</signal>
<signal name="LSOURCE1">
<contactref element="R26" pad="2"/>
<contactref element="LED16" pad="A"/>
</signal>
<signal name="LSOURCE2">
<contactref element="LED15" pad="A"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="LSOURCE3">
<contactref element="R30" pad="2"/>
<contactref element="LED14" pad="A"/>
</signal>
<signal name="LSOURCE4">
<contactref element="LED13" pad="A"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="LSOURCE5">
<contactref element="R32" pad="2"/>
<contactref element="LED12" pad="A"/>
</signal>
<signal name="LSOURCE6">
<contactref element="LED11" pad="A"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="LSOURCE7">
<contactref element="R28" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="SOURCE0">
<contactref element="V4" pad="15"/>
<contactref element="R24" pad="1"/>
<contactref element="J2" pad="12"/>
</signal>
<signal name="SOURCE1">
<contactref element="V4" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="SOURCE2">
<contactref element="V4" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="SOURCE3">
<contactref element="V4" pad="3"/>
<contactref element="R30" pad="1"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="SOURCE4">
<contactref element="V4" pad="4"/>
<contactref element="R31" pad="1"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="SOURCE5">
<contactref element="V4" pad="5"/>
<contactref element="R32" pad="1"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="SOURCE6">
<contactref element="V4" pad="6"/>
<contactref element="R27" pad="1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="SOURCE7">
<contactref element="V4" pad="7"/>
<contactref element="R28" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="SDATA0">
<contactref element="V2" pad="15"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="SDATA1">
<contactref element="R1" pad="1"/>
<contactref element="V2" pad="1"/>
</signal>
<signal name="SDATA2">
<contactref element="V2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SDATA3">
<contactref element="R3" pad="1"/>
<contactref element="V2" pad="3"/>
</signal>
<signal name="SDATA4">
<contactref element="V2" pad="4"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="SDATA5">
<contactref element="R7" pad="1"/>
<contactref element="V2" pad="5"/>
</signal>
<signal name="SDATA6">
<contactref element="V2" pad="6"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SDATA7">
<contactref element="R16" pad="1"/>
<contactref element="V2" pad="7"/>
</signal>
<signal name="SDATA8">
<contactref element="V1" pad="15"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="SDATA9">
<contactref element="R18" pad="1"/>
<contactref element="V1" pad="1"/>
</signal>
<signal name="TRANS">
<contactref element="TRANS" pad="A"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="STRANS">
<contactref element="V3" pad="6"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="SABS">
<contactref element="R4" pad="1"/>
<contactref element="V3" pad="7"/>
</signal>
<signal name="ABS">
<contactref element="R4" pad="2"/>
<contactref element="ABSO" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
