(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.2)
    (drawings 69)
    (tracks 618)
    (zones 0)
    (modules 55)
    (nets 64)
  )
  (page User 148.006 105.004)
  (title_block
    (title "STM32WLE5 Breakout")
    (date "6 August 2020")
    (rev 0.9)
    (company "John Adriaan")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.185)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (user_trace_width 0.64)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.08)
    (pcb_text_size 0.5 0.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.2 0.2)
    (mod_text_width 0.01)
    (pad_size 0.59 0.64)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 42.85 59.4)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../Gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 VDDA)
  (net 4 BOOT0)
  (net 5 JTRST)
  (net 6 NRST)
  (net 7 OSC32-)
  (net 8 OSC32+)
  (net 9 /A0)
  (net 10 /A1)
  (net 11 /A2)
  (net 12 /A3)
  (net 13 /A4)
  (net 14 /A5)
  (net 15 /A6)
  (net 16 /A7)
  (net 17 /A8)
  (net 18 /A9)
  (net 19 /A10)
  (net 20 /A11)
  (net 21 /A12)
  (net 22 /B2)
  (net 23 /B5)
  (net 24 /B6)
  (net 25 /B7)
  (net 26 /B8)
  (net 27 /B12)
  (net 28 /C13)
  (net 29 /TMS)
  (net 30 /TCK)
  (net 31 /TDO)
  (net 32 /TDI)
  (net 33 /~RESET~)
  (net 34 /JTMS)
  (net 35 /JTCK)
  (net 36 /JTDO)
  (net 37 /JTDI)
  (net 38 /VFB)
  (net 39 /YVCC)
  (net 40 /TCXO)
  (net 41 /VLX)
  (net 42 /OSC-)
  (net 43 /~OSC~)
  (net 44 /OSC)
  (net 45 /PA)
  (net 46 /RF2)
  (net 47 /RX+)
  (net 48 /RX-)
  (net 49 /TX)
  (net 50 /~TX~)
  (net 51 /~RF1~)
  (net 52 /RF1)
  (net 53 /CTRL)
  (net 54 /RF)
  (net 55 /RFC)
  (net 56 /ANT)
  (net 57 /TXH)
  (net 58 /TXL)
  (net 59 /VDDPA)
  (net 60 VBAT)
  (net 61 TxD)
  (net 62 RxD)
  (net 63 AntSw)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.175)
    (diff_pair_gap 0.175)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /B12)
    (add_net /B2)
    (add_net /B5)
    (add_net /B6)
    (add_net /B7)
    (add_net /B8)
    (add_net /C13)
    (add_net /CTRL)
    (add_net /JTCK)
    (add_net /JTDI)
    (add_net /JTDO)
    (add_net /JTMS)
    (add_net /OSC)
    (add_net /OSC-)
    (add_net /TCK)
    (add_net /TCXO)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /TX)
    (add_net /VDDPA)
    (add_net /VFB)
    (add_net /VLX)
    (add_net /YVCC)
    (add_net /~OSC~)
    (add_net /~RESET~)
    (add_net AntSw)
    (add_net BOOT0)
    (add_net JTRST)
    (add_net NRST)
    (add_net OSC32+)
    (add_net OSC32-)
    (add_net RxD)
    (add_net TxD)
    (add_net VBAT)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.2)
    (add_net +3V3)
    (add_net GND)
    (add_net VDDA)
  )
  (net_class RF ""
    (clearance 0.1524)
    (trace_width 0.64)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.64)
    (diff_pair_gap 0.508)
    (add_net /ANT)
    (add_net /PA)
    (add_net /RF)
    (add_net /RF1)
    (add_net /RF2)
    (add_net /RFC)
    (add_net /RX+)
    (add_net /RX-)
    (add_net /TXH)
    (add_net /TXL)
    (add_net /~RF1~)
    (add_net /~TX~)
  )
  (module JohnAdriaan:SJ3_Vias_0.5x0.75mm_Labels (layer F.Cu) (tedit 5F64D4D1)
    (at 38.05 58.4 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 2.4 0.35 90) (layer F.SilkS))
    (fp_text value PA (at -0.05 0 90) (layer F.Fab))
    (fp_text user H (at -1.55 0 90) (layer F.SilkS))
    (fp_text user L|H (at 1.55 -0.5 90) (layer F.SilkS))
    (pad 2 thru_hole rect (at 0 0 270) (size 0.5 0.75) (drill 0.254) (layers *.Cu *.Mask)
      (net 59 /VDDPA))
    (pad 3 thru_hole custom (at 0.8 0 270) (size 0.75 0.75) (drill 0.254) (layers *.Cu *.Mask)
      (net 38 /VFB) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.375 -0.375) (xy 0 -0.375) (xy 0 0.375) (xy -0.375 0.375)) (width 0))
      ))
    (pad 1 thru_hole custom (at -0.8 0 270) (size 0.75 0.75) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0.375 -0.375) (xy 0 -0.375) (xy 0 0.375) (xy 0.375 0.375)) (width 0))
      ))
  )
  (module JohnAdriaan:Header_0.10_1x08 (layer F.Cu) (tedit 5F687D35)
    (at 50.39 73.5 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at 0.8 -2.31 unlocked) (layer F.SilkS))
    (fp_text value FTDI (at 0 17.24 180) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.127 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0.127 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -0.127 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 4 thru_hole oval (at 0.127 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 RxD))
    (pad 5 thru_hole oval (at -0.127 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 TxD))
    (pad 6 thru_hole oval (at 0.127 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at -0.127 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 VBAT))
    (pad 8 thru_hole oval (at 0.127 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:Header_0.05_1x17 (layer F.Cu) (tedit 5F687BC9)
    (at 51.65 70.7 180)
    (descr "Through hole straight pin header, 1x17, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x17 1.27mm single row")
    (fp_text reference J2 (at 0.3 22.5 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x17 (at -0.15 16.31 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 10.16 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.0635 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 VDDA))
    (pad 2 thru_hole oval (at 0.0635 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at -0.0635 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 /B2))
    (pad 4 thru_hole oval (at 0.0635 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 NRST))
    (pad 5 thru_hole oval (at -0.0635 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 JTRST))
    (pad 6 thru_hole oval (at 0.0635 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 /B5))
    (pad 7 thru_hole oval (at -0.0635 7.62 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 /B6))
    (pad 8 thru_hole oval (at 0.0635 8.89 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 /B7))
    (pad 9 thru_hole oval (at -0.0635 10.16 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 /B8))
    (pad 10 thru_hole oval (at 0.0635 11.43 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at -0.0635 12.7 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 BOOT0))
    (pad 12 thru_hole oval (at 0.0635 13.97 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 13 thru_hole oval (at -0.0635 15.24 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 /B12))
    (pad 14 thru_hole oval (at 0.0635 16.51 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 /C13))
    (pad 15 thru_hole oval (at -0.0635 17.78 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 OSC32-))
    (pad 16 thru_hole oval (at 0.0635 19.05 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 OSC32+))
    (pad 17 thru_hole oval (at -0.0635 20.32 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 63 AntSw))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x17_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:Header_0.05_1x17 (layer F.Cu) (tedit 5F687BC9)
    (at 31.35 70.7 180)
    (descr "Through hole straight pin header, 1x17, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x17 1.27mm single row")
    (fp_text reference J1 (at -0.4 22.05 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x17 (at -0.1 16.26 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 10.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.0635 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 /A0))
    (pad 2 thru_hole oval (at 0.0635 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /A1))
    (pad 3 thru_hole oval (at -0.0635 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /A2))
    (pad 4 thru_hole oval (at 0.0635 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 5 thru_hole oval (at -0.0635 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /A4))
    (pad 6 thru_hole oval (at 0.0635 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 7 thru_hole oval (at -0.0635 7.62 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /A6))
    (pad 8 thru_hole oval (at 0.0635 8.89 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /A7))
    (pad 9 thru_hole oval (at -0.0635 10.16 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /A8))
    (pad 10 thru_hole oval (at 0.0635 11.43 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /A9))
    (pad 11 thru_hole oval (at -0.0635 12.7 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /A10))
    (pad 12 thru_hole oval (at 0.0635 13.97 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 /A11))
    (pad 13 thru_hole oval (at -0.0635 15.24 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 /A12))
    (pad 14 thru_hole oval (at 0.0635 16.51 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 15 thru_hole oval (at -0.0635 17.78 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 62 RxD))
    (pad 16 thru_hole oval (at 0.0635 19.05 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /A2))
    (pad 17 thru_hole oval (at -0.0635 20.32 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 61 TxD))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x17_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:SJ3_Open_0.5x0.75mm_Labels (layer F.Cu) (tedit 5F64CA30)
    (at 40.85 54 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -2.2 0.35 unlocked) (layer F.SilkS))
    (fp_text value TX (at 0.05 -0.05) (layer F.Fab))
    (fp_text user L (at -1.45 0.05) (layer F.SilkS) hide)
    (fp_text user 3 (at 1.4 0.05) (layer F.SilkS) hide)
    (fp_text user H (at 1.3 0.05 unlocked) (layer F.SilkS))
    (fp_text user L|H (at -1.35 -0.5 unlocked) (layer F.SilkS))
    (pad 2 smd rect (at 0 0 180) (size 0.5 0.75) (layers F.Cu F.Mask)
      (net 49 /TX))
    (pad 3 smd custom (at 0.675 0 180) (size 0.5 0.25) (layers F.Cu F.Mask)
      (net 57 /TXH) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.125) (end 0.25 0.125) (width 0))
        (gr_circle (center 0 -0.125) (end 0.25 -0.125) (width 0))
        (gr_poly (pts
           (xy -0.25 -0.375) (xy 0 -0.375) (xy 0 0.375) (xy -0.25 0.375)) (width 0))
      ))
    (pad 1 smd custom (at -0.675 0 180) (size 0.5 0.25) (layers F.Cu F.Mask)
      (net 58 /TXL) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.125) (end 0.25 0.125) (width 0))
        (gr_circle (center 0 -0.125) (end 0.25 -0.125) (width 0))
        (gr_poly (pts
           (xy 0.25 -0.375) (xy 0 -0.375) (xy 0 0.375) (xy 0.25 0.375)) (width 0))
      ))
  )
  (module JohnAdriaan:CS10 (layer F.Cu) (tedit 5F641264)
    (at 44.55 67.75 90)
    (descr "Pogo Straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Pogo pin header THT SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J4 (at 0 -5.15 unlocked) (layer F.SilkS))
    (fp_text value CS10 (at 0.014 -0.5904 180) (layer F.Fab))
    (fp_text user %R (at 0.014 0.6542) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.635 -2.54 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 smd custom (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.815 -0.5) (xy 1.815 -0.5) (xy 1.815 0.5) (xy 0.815 0.5)) (width 0))
      ))
    (pad 2 thru_hole oval (at 0.635 -2.54 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 /TMS))
    (pad 2 smd custom (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 29 /TMS) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 3 thru_hole oval (at -0.635 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 smd custom (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 4 thru_hole oval (at 0.635 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 /TCK))
    (pad 4 smd custom (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 30 /TCK) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 5 thru_hole oval (at -0.635 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 smd custom (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 6 thru_hole oval (at 0.635 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 /TDO))
    (pad 6 smd custom (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 31 /TDO) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 7 thru_hole oval (at -0.635 1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 smd custom (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 8 thru_hole oval (at 0.635 1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 /TDI))
    (pad 8 smd custom (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 32 /TDI) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
    (pad 9 thru_hole oval (at -0.635 2.54 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 smd custom (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 1.315 0) (end 1.815 0) (width 0))
      ))
    (pad 10 thru_hole oval (at 0.635 2.54 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 33 /~RESET~))
    (pad 10 smd custom (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RESET~) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center -1.315 0) (end -0.815 0) (width 0))
      ))
  )
  (module JohnAdriaan:u.FL_SMD (layer F.Cu) (tedit 5F102DDD)
    (at 41.5 33 90)
    (fp_text reference J5 (at 0.05 3.05 unlocked) (layer F.SilkS))
    (fp_text value u.FL (at -0.1 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 56 /ANT))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 36.435 66.4 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CE1 (at 1.885 0 unlocked) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:STM32WLE5_UFQFPN48 (layer F.Cu) (tedit 5F645D49)
    (at 42.85 59.4 180)
    (descr "UFQFPN48, 7x7mm package, pitch 0.5mm")
    (tags QFN)
    (attr smd)
    (fp_text reference U1 (at 4.55 -3.55 270) (layer F.SilkS))
    (fp_text value STM32WLE5 (at 0 0.15 270) (layer F.Fab))
    (pad 1 smd oval (at -3.4 -2.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /JTDO))
    (pad 2 smd oval (at -3.4 -2.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 JTRST))
    (pad 3 smd oval (at -3.4 -1.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /B5))
    (pad 4 smd oval (at -3.4 -1.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /B6))
    (pad 5 smd oval (at -3.4 -0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /B7))
    (pad 6 smd oval (at -3.4 -0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /B8))
    (pad 7 smd oval (at -3.4 0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /A0))
    (pad 8 smd oval (at -3.4 0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /A1))
    (pad 9 smd oval (at -3.4 1.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /A2))
    (pad 10 smd oval (at -3.4 1.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /A3))
    (pad 11 smd oval (at -3.4 2.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 12 smd oval (at -3.4 2.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /A4))
    (pad 13 smd oval (at -2.75 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /A5))
    (pad 14 smd oval (at -2.25 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /A6))
    (pad 15 smd oval (at -1.75 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /A7))
    (pad 16 smd oval (at -1.25 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /A8))
    (pad 17 smd oval (at -0.75 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /A9))
    (pad 18 smd oval (at -0.25 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 19 smd oval (at 0.25 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 BOOT0))
    (pad 20 smd oval (at 0.75 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /RX+))
    (pad 21 smd oval (at 1.25 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /RX-))
    (pad 22 smd oval (at 1.75 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 /TXL))
    (pad 23 smd oval (at 2.25 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 /TXH))
    (pad 24 smd oval (at 2.75 3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /PA))
    (pad 25 smd oval (at 3.4 2.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 /VDDPA))
    (pad 26 smd oval (at 3.4 2.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /OSC-))
    (pad 27 smd oval (at 3.4 1.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd oval (at 3.4 1.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 29 smd oval (at 3.4 0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /VFB))
    (pad 30 smd oval (at 3.4 0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /TCXO))
    (pad 31 smd oval (at 3.4 -0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /B2))
    (pad 32 smd oval (at 3.4 -0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /B12))
    (pad 33 smd oval (at 3.4 -1.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /A10))
    (pad 34 smd oval (at 3.4 -1.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /A11))
    (pad 35 smd oval (at 3.4 -2.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /A12))
    (pad 36 smd oval (at 3.4 -2.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /JTMS))
    (pad 37 smd oval (at 2.75 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 VBAT))
    (pad 38 smd oval (at 2.25 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /C13))
    (pad 39 smd oval (at 1.75 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 OSC32-))
    (pad 40 smd oval (at 1.25 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 OSC32+))
    (pad 41 smd oval (at 0.75 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VDDA))
    (pad 42 smd oval (at 0.25 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /JTCK))
    (pad 43 smd oval (at -0.25 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /JTDI))
    (pad 44 smd oval (at -0.75 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 45 smd oval (at -1.25 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /VFB))
    (pad 46 smd oval (at -1.75 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 47 smd oval (at -2.25 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /VLX))
    (pad 48 smd oval (at -2.75 -3.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 49 smd rect (at -1.4 -1.4 180) (size 2.7 2.7) (drill (offset -0.05 -0.05)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.75))
    (pad 49 smd rect (at -1.4 1.4 180) (size 2.7 2.7) (drill (offset -0.05 0.05)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.75))
    (pad 49 smd rect (at 1.4 -1.4 180) (size 2.7 2.7) (drill (offset 0.05 -0.05)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.75))
    (pad 49 smd rect (at 1.4 1.4 180) (size 2.7 2.7) (drill (offset 0.05 0.05)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.75))
    (pad 49 thru_hole circle (at 0 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_paste_margin -0.75))
  )
  (module JohnAdriaan:Mandel_medium (layer B.Cu) (tedit 0)
    (at 41.65 41.85 270)
    (fp_text reference S0 (at 1.7 0.15 90) (layer B.SilkS) hide)
    (fp_text value Logo (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 43.6 62.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CD3 (at 1.942857 0.2 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 37.85 56.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RH1 (at 3.75 -0.45 unlocked) (layer F.SilkS))
    (fp_text value 220R (at -0.1 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /OSC-))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /~OSC~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 42.1 62.3 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CG2 (at -1.942857 0.15 270) (layer B.SilkS))
    (fp_text value 10nF (at 0 0.1 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VDDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 39.95 56.65)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CF3 (at -0.05 -0.95 unlocked) (layer B.SilkS))
    (fp_text value 33pF (at 0 -0.05) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 /VDDPA))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 39.4 57.6)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CF2 (at 0 0.9 unlocked) (layer B.SilkS))
    (fp_text value 33pF (at 0.1 0) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 44.6 62.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CF1 (at 1.9 0.15 90) (layer B.SilkS))
    (fp_text value 33pF (at 0 0 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 45.75 57.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CD2 (at 0 -0.95 unlocked) (layer B.SilkS))
    (fp_text value 100nF (at 0 0.05 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:Crystal_C002RX_D2mm_L6mm_Vertical (layer F.Cu) (tedit 5F2D4138)
    (at 39.8 65 90)
    (descr "Crystal THT C002RX 6mm length 2mm diameter")
    (tags ['C002RX'])
    (fp_text reference Y2 (at 0.35 -1.5 90) (layer F.SilkS))
    (fp_text value 32.768kHz (at 0.4 0 180) (layer F.Fab))
    (fp_text user %R (at 0.35 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 7 OSC32-))
    (pad 2 thru_hole circle (at 0.7 0 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 8 OSC32+))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_DS10_D1.0mm_L4.3mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 46.65 50)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference CH4 (at 1.35 -1.5 unlocked) (layer F.SilkS))
    (fp_text value 18pF (at 1.6 0) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 OSC32+))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 46.65 52.44)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference CH3 (at 1.35 1.46 unlocked) (layer F.SilkS))
    (fp_text value 18pF (at 1.65 0.05) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 OSC32-))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.5 36.8 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference LX6 (at 0 0.95 90) (layer F.SilkS))
    (fp_text value 9n1H (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /RF))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /ANT))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:Panasonic_B (layer F.Cu) (tedit 5F0ED822)
    (at 35.95 69.35 270)
    (fp_text reference CD1 (at 1.35 -3.4 unlocked) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0 1.75 270) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.066)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.75 270) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
  )
  (module JohnAdriaan:VCTCXO_2.0X1.6 (layer F.Cu) (tedit 5F102E5C)
    (at 36.25 58.4 90)
    (fp_text reference Y1 (at 0.05 -1.55 90) (layer F.SilkS))
    (fp_text value 32MHz (at 0.05 -0.35 90) (layer F.Fab))
    (pad 4 smd roundrect (at -0.9 -0.6 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.167)
      (net 39 /YVCC))
    (pad 3 smd roundrect (at 0.9 -0.6 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.167)
      (net 44 /OSC))
    (pad 2 smd roundrect (at 0.9 0.6 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.167)
      (net 1 GND))
    (pad 1 smd rect (at -0.9 0.6 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module JohnAdriaan:PE4259 (layer F.Cu) (tedit 5F102FAC)
    (at 41.5 42.5)
    (fp_text reference U3 (at -1.75 0 90 unlocked) (layer F.SilkS))
    (fp_text value PE4259 (at 0 0.05) (layer F.Fab))
    (pad 6 smd roundrect (at -0.65 -1.05) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 5 smd roundrect (at 0 -1.05) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /RFC))
    (pad 4 smd roundrect (at 0.65 -1.05) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /CTRL))
    (pad 3 smd roundrect (at 0.65 1.05) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /RF2))
    (pad 2 smd roundrect (at 0 1.05) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd rect (at -0.65 1.05) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 /RF1))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 47.09 65.591 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RJ5 (at -1.741 0 90) (layer B.SilkS))
    (fp_text value 50R (at 0 -0.01 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 NRST))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 /~RESET~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 45.82 65.591 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RJ4 (at -1.741 0 90) (layer B.SilkS))
    (fp_text value 50R (at 0 0.02 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 /JTDI))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /TDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 44.55 65.591 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RJ3 (at -1.741 0 90) (layer B.SilkS))
    (fp_text value 50R (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 /JTDO))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 /TDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 43.28 65.591 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RJ2 (at -1.741 0 90) (layer B.SilkS))
    (fp_text value 50R (at 0 -0.02 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 /JTCK))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 /TCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 42.01 65.591 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RJ1 (at -1.741 0 90) (layer B.SilkS))
    (fp_text value 50R (at 0 0.01 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 /JTMS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 /TMS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 44.6 41.9 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RX1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 100R (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /CTRL))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 AntSw))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 40.85 46.25 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference LX5 (at 0 -0.9 90) (layer F.SilkS))
    (fp_text value 4n7H (at 0.05 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /~RF1~))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /RF1))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 40.85 51.25 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference LX4 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 2n5H (at 0 -0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /TX))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /~TX~))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 37.3 54.8 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference LX3 (at 0.15 -2.8 270) (layer F.SilkS))
    (fp_text value 47nH (at 0 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /PA))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /TX))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 43.35 52.75)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference LX1 (at 0 -3.9 unlocked) (layer F.SilkS))
    (fp_text value 15nH (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /RX-))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /RX+))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 49.3 63.2 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference LF1 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 15uH (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /VLX))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /VFB))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 36.35 61.15 180)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FH1 (at 1.8 0 unlocked) (layer F.SilkS))
    (fp_text value 10R@100MHz (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /TCXO))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /YVCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41 35.3 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX14 (at 2.1 0 unlocked) (layer F.SilkS))
    (fp_text value 3p3F (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /ANT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41 38.3 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX13 (at 2.1 0 unlocked) (layer F.SilkS))
    (fp_text value 3p3F (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /RF))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.5 39.85 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX12 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 39pF (at -0.05 -0.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /RF))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /RFC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 43.5 41.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX11 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /CTRL))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 40.35 44.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX10 (at -2.1 0 unlocked) (layer F.SilkS))
    (fp_text value 1p8F (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /RF1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 40.85 48.25 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX9 (at 0 0.9 90) (layer F.SilkS))
    (fp_text value 39pF (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /~RF1~))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /~TX~))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 40.35 49.75 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX8 (at 1.85 0 unlocked) (layer F.SilkS))
    (fp_text value 5p6F (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /~TX~))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 39.85 51.25 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX7 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 3pF (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /~TX~))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 40.35 52.75 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX6 (at 1.85 0 unlocked) (layer F.SilkS))
    (fp_text value 5p6F (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /TX))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 43.35 49.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX5 (at 0 -3.6 unlocked) (layer F.SilkS))
    (fp_text value 1p8F (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /RF2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 42.85 51.25 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX4 (at -3.75 0 90) (layer F.SilkS))
    (fp_text value 1p8F (at 0 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /RX-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 43.85 51.25 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX3 (at -3.75 0 90) (layer F.SilkS))
    (fp_text value 2p4F (at -0.05 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /RF2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /RX+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 36.3 54.8 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX2 (at 0.15 -2.7 270) (layer F.SilkS))
    (fp_text value 47nF (at 0 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /PA))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 38.3 54.8 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CX1 (at 0.15 -2.9 270) (layer F.SilkS))
    (fp_text value 47pF (at -0.1 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /PA))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 35.95 56.4 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CH2 (at 2.5 0.5 unlocked) (layer F.SilkS))
    (fp_text value 10pF (at 0 -0.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /~OSC~))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /OSC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 36.35 60.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CH1 (at -1.9 0.05 unlocked) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /YVCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 49.3 70.7)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CG1 (at 0 -0.95 unlocked) (layer F.SilkS))
    (fp_text value 1uF (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VDDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 47.8 63 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CF5 (at -1.85 0.15 90) (layer F.SilkS))
    (fp_text value 470nF (at 0.05 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /VFB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 49.3 57.95 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference CF4 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value 4u7F (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 29.3 75.6) (end 28.8 75.6) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 53.7 75.6) (end 53.7 76.1) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text Gnd (at 32.61 75.15) (layer F.SilkS))
  (gr_text A2 (at 30.3 51.65) (layer F.SilkS))
  (gr_text A3 (at 30.3 54.19) (layer F.SilkS))
  (gr_text AntSw (at 51.65 49.25) (layer F.SilkS))
  (gr_text "VDD\n A" (at 52.65 70.7) (layer F.SilkS))
  (gr_text 3v3 (at 52.65 69.43) (layer F.SilkS))
  (gr_text B2 (at 52.65 68.16) (layer F.SilkS))
  (gr_text NRst (at 52.65 66.89) (layer F.SilkS))
  (gr_text JRst (at 52.65 65.62) (layer F.SilkS))
  (gr_text B5 (at 52.65 64.35) (layer F.SilkS))
  (gr_text B6 (at 52.65 63.08) (layer F.SilkS))
  (gr_text B7 (at 52.65 61.81) (layer F.SilkS))
  (gr_text B8 (at 52.65 60.54) (layer F.SilkS))
  (gr_text Gnd (at 52.65 59.27) (layer F.SilkS))
  (gr_text Boot (at 52.65 58) (layer F.SilkS))
  (gr_text 3v3 (at 52.65 56.73) (layer F.SilkS))
  (gr_text B12 (at 52.65 55.46) (layer F.SilkS))
  (gr_text Batt (at 35.15 75.15) (layer F.SilkS))
  (gr_text Gnd (at 50.39 75.15) (layer F.SilkS))
  (gr_text 3v3 (at 45.31 75.15) (layer F.SilkS))
  (gr_text ↑RxD↑ (at 42.77 75.15) (layer F.SilkS))
  (gr_text ↓TxD↓ (at 40.23 75.15) (layer F.SilkS))
  (gr_text RxD (at 30.3 52.92) (layer F.SilkS))
  (gr_text TxD (at 30.3 50.38) (layer F.SilkS))
  (gr_text C15 (at 52.65 51.65) (layer F.SilkS))
  (gr_text C14 (at 52.65 52.92) (layer F.SilkS))
  (gr_text C13 (at 52.65 54.19) (layer F.SilkS))
  (gr_text A12 (at 30.3 55.46) (layer F.SilkS))
  (gr_text A11 (at 30.3 56.73) (layer F.SilkS))
  (gr_text A10 (at 30.3 58) (layer F.SilkS))
  (gr_text A9 (at 30.3 59.27) (layer F.SilkS))
  (gr_text A8 (at 30.3 60.54) (layer F.SilkS))
  (gr_text A7 (at 30.3 61.81) (layer F.SilkS))
  (gr_text A6 (at 30.3 63.08) (layer F.SilkS))
  (gr_text A5 (at 30.3 64.35) (layer F.SilkS))
  (gr_text A4 (at 30.3 65.62) (layer F.SilkS))
  (gr_text A3 (at 30.3 66.89) (layer F.SilkS))
  (gr_text A2 (at 30.3 68.16) (layer F.SilkS))
  (gr_text A1 (at 30.3 69.43) (layer F.SilkS))
  (gr_text A0 (at 30.3 70.7) (layer F.SilkS))
  (gr_text https://JohnAdriaan.blog/ (at 45.6 41.85 90) (layer B.SilkS))
  (gr_text "STM32WLE5C\nBreakout" (at 36.7 41.75 90) (layer B.SilkS))
  (gr_line (start 54.2 50.7) (end 44.9 29.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 28.8 50.7) (end 38.1 29.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 29.3 76.1) (end 53.7 76.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 28.8 50.7) (end 28.8 75.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.9 29.4) (end 38.1 29.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.2 75.6) (end 54.2 50.7) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 38.1 29.3) (xy 44.9 29.3) (xy 54.2 50.7) (xy 54.2 76.1) (xy 28.8 76.1)
        (xy 28.8 50.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 38.1 29.3) (xy 44.9 29.3) (xy 54.2 50.7) (xy 54.2 76.1) (xy 28.8 76.1)
        (xy 28.8 50.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 38.1 29.3) (xy 44.9 29.3) (xy 54.2 50.7) (xy 54.2 76.1) (xy 28.8 76.1)
        (xy 28.8 50.7)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 39.05 30.85) (xy 43.95 30.85) (xy 52.7 51.2) (xy 52.7 74.6) (xy 30.3 74.6)
        (xy 30.3 51.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 38.1 29.3) (xy 44.9 29.3) (xy 54.2 50.7) (xy 54.2 76.1) (xy 28.8 76.1)
        (xy 28.8 50.7)
      )
    )
    (polygon
      (pts
        (xy 29.8 75.1) (xy 53.2 75.1) (xy 53.2 51) (xy 44.35 30.4) (xy 38.65 30.4)
        (xy 29.8 51)
      )
    )
  )
)
