(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (42 "Eco1.User" user "User.Eco1")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
      (castellated_pads yes)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 0.15 0.15)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Print/")
    )
  )
  (net 0 "")
  (net 1 "+BATT")
  (net 2 "GND")
  (net 3 "Net-(JP1-A)")
  (net 4 "Net-(D1-K)")
  (net 5 "Net-(D1-A)")
  (net 6 "SCL_PMIC")
  (net 7 "SDA_PMIC")
  (net 8 "Net-(U2-PROG)")
  (net 9 "ALERT")
  (net 10 "Net-(JP1-B)")
  (net 11 "Net-(JP2-B)")
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580" (layer "F.Cu")
    (at 99.4132 109.3446)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO14580")
    (tags "mounting hole 2.2mm no annular m2 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "*" (at 0.4572 0.1016) (layer "F.SilkS"))
    (fp_text value "MountingHole_2.2mm_M2_ISO14580" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 91.3868 82.5532 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at -3.0988 1.6312) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Open" (at 0 2) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(JP1-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "+BATT") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(JP1-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 82.7 86.0274)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0.0743 -1.397) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal" (layer "F.Cu")
    (at 81.5344 101.8472)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "POWER-BAT" (at 0.175 -5.5328) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 5.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.35 2.9) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666673333))
    (pad "MP" smd roundrect (at 3.35 2.9) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666673333))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 91.0566 85.5702 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0.3556 1.1938) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "SDA_PMIC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(JP1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_B4B-PH-SM4-TB_1x04-1MP_P2.00mm_Vertical" (layer "F.Cu")
    (at 93.0914 102.0214 180)
    (descr "JST PH series connector, B4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "I2C_QWIIC" (at 0.4092 4.4116) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 4.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3 0.5 180) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0.5 180) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "SDA_PMIC") (pinfunction "Pin_3") (pintype "passive"))
    (pad "3.3" smd roundrect (at -1 0.5 180) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at 3 0.5 180) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "SCL_PMIC") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at -5.4 -1.75 180) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625))
    (pad "MP" smd roundrect (at 5.4 -1.75 180) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B4B-PH-SM4-TB_1x04-1MP_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580" (layer "F.Cu")
    (at 76.1214 79.779)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO14580")
    (tags "mounting hole 2.2mm no annular m2 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "*" (at -0.1016 0.3048) (layer "F.SilkS"))
    (fp_text value "MountingHole_2.2mm_M2_ISO14580" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 82.8374 82.2682)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at -2.7282 -1.5494) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 9 "ALERT") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(JP2-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 86.9672 82.3717 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 2.1863 0 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(JP2-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 86.7405 86.1036)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -0.4337 -1.6002) (layer "F.SilkS"))
    (fp_text value "2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U2-PROG)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580" (layer "F.Cu")
    (at 99.5148 79.5758)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO14580")
    (tags "mounting hole 2.2mm no annular m2 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "*" (at 0.2032 0.0254) (layer "F.SilkS"))
    (fp_text value "MountingHole_2.2mm_M2_ISO14580" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 88.0848 94.0792 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -2.2352 0.0508) (layer "F.SilkS"))
    (fp_text value "0.01µ" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Castellated_PinHeaders_1x04:Castellated_PinHeader_1x04_P2.54mm" (layer "F.Cu")
    (at 73.81 86.36)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 1.3208 -2.39) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 4.385 9.89) (layer "F.Fab"))
    (pad "" thru_hole circle (at 2 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND"))
    (pad "" thru_hole circle (at 2 2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 9 "ALERT"))
    (pad "" thru_hole circle (at 2 5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 6 "SCL_PMIC"))
    (pad "" thru_hole circle (at 2 7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "SDA_PMIC"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "2" thru_hole rect (at 0 2.54) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 9 "ALERT") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "3" thru_hole rect (at 0 5.08) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 6 "SCL_PMIC") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "4" thru_hole rect (at 0 7.62) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 7 "SDA_PMIC") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 84.5034 94.0792 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 2.1336 -0.0508) (layer "F.SilkS"))
    (fp_text value "4.7µ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm" (layer "F.Cu")
    (at 93.7196 91.3837 90)
    (descr "TDFN, 8 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0168.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "TDFN NoLead")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "MAX17048G+T10")
    (attr smd)
    (fp_text reference "MAX17048G+T10" (at -2.5431 0.2834 180) (layer "F.SilkS"))
    (fp_text value "MAX17048G+T10" (at 0 1.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.2 -0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.2 0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.2 -0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.2 0.3 90) (size 0.32 0.48) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.9875 -0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "CTG") (pintype "unspecified"))
    (pad "2" smd roundrect (at -0.9875 -0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "CELL") (pintype "unspecified"))
    (pad "3" smd roundrect (at -0.9875 0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd roundrect (at -0.9875 0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 0.9875 0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "ALERT") (pinfunction "*ALRT") (pintype "output"))
    (pad "6" smd roundrect (at 0.9875 0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "QSTRT") (pintype "input"))
    (pad "7" smd roundrect (at 0.9875 -0.25 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "SCL_PMIC") (pinfunction "SCL") (pintype "input"))
    (pad "8" smd roundrect (at 0.9875 -0.75 90) (size 0.775 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "SDA_PMIC") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "9" smd rect (at 0 0 90) (size 0.8 1.2) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "EPAD") (pintype "unspecified"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580" (layer "F.Cu")
    (at 75.9436 109.4208)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO14580")
    (tags "mounting hole 2.2mm no annular m2 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "*" (at 0.4572 0.1016) (layer "F.SilkS"))
    (fp_text value "MountingHole_2.2mm_M2_ISO14580" (at 0 2.9) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.28 89.7 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D1" (at -2.2756 0.5104) (layer "F.SilkS"))
    (fp_text value "LED_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.28 93.98 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -2.1614 -0.0484 -180) (layer "F.SilkS"))
    (fp_text value "4.7µ" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Castellated_PinHeaders_1x04:Castellated_PinHeader_1x04_P2.54mm" (layer "F.Cu")
    (at 102.0228 94.384 180)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.4666 10.1854) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 4.385 9.89) (layer "F.Fab"))
    (pad "" thru_hole circle (at 2 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "SDA_PMIC"))
    (pad "" thru_hole circle (at 2 2.54 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 6 "SCL_PMIC"))
    (pad "" thru_hole circle (at 2 5.08 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 1 "+BATT"))
    (pad "" thru_hole circle (at 2 7.62 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "GND"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 7 "SDA_PMIC") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "2" thru_hole rect (at 0 2.54 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 6 "SCL_PMIC") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "3" thru_hole rect (at 0 5.08 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 1 "+BATT") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (pad "4" thru_hole rect (at 0 7.62 180) (size 2 1.7) (drill 1 (offset 1 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.04) (solder_paste_margin_ratio 0.1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 94.3078 86.5862 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 2.0828 0.8382 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "SCL_PMIC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(JP1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 84.9575 89.65)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "PMIC_module.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Open-Drain Status Output, in SOT23-5 package")
    (property "ki_keywords" "battery charger lithium")
    (attr smd)
    (fp_text reference "MCP73832" (at 0.9429 -2.2002) (layer "F.SilkS"))
    (fp_text value "MCP73832-2-OT" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-A)") (pinfunction "STAT") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "V_{SS}") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "V_{BAT}") (pintype "power_out"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "V_{DD}") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U2-PROG)") (pinfunction "PROG") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line locked (start 102.2072 78.1026) (end 102.2072 110.513)
    (layer "Edge.Cuts"))
  (gr_line locked (start 73.6576 110.5892) (end 73.6576 78.1788)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 102.2072 110.6146) (mid 101.835226 111.512626) (end 100.9372 111.8846)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 73.6576 78.1788) (mid 74.029574 77.280774) (end 74.9276 76.9088)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 100.9372 76.8326) (mid 101.835226 77.204574) (end 102.2072 78.1026)
    (layer "Edge.Cuts"))
  (gr_line locked (start 100.9372 111.8846) (end 74.9276 111.8592)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 74.9276 111.8592) (mid 74.029574 111.487226) (end 73.6576 110.5892)
    (layer "Edge.Cuts"))
  (gr_line locked (start 74.9276 76.9088) (end 100.9372 76.8326)
    (layer "Edge.Cuts"))
  (image (at 86.9164 109.6748) (layer "F.SilkS") (scale 0.051184))
  (gr_text "BATT" (at 91.6916 79.950753 90) (layer "F.SilkS"))
  (gr_text "BAT Monitor" (at 91.7424 89.1516) (layer "F.SilkS"))
  (gr_text "SCL" (at 89.6596 107.973) (layer "F.SilkS"))
  (gr_text "SDA" (at 98.8798 95.0444 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 91.5646 107.973) (layer "F.SilkS"))
  (gr_text "PMIC" (at 94.5872 79.1694) (layer "F.SilkS"))
  (gr_text "SDA" (at 77.0358 93.3426 -90) (layer "F.SilkS"))
  (gr_text "SDA" (at 90.2692 79.80561 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 93.1902 79.793514 90) (layer "F.SilkS"))
  (gr_text "BATT" (at 83.4874 79.950753 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 77.0358 90.9804 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 98.8798 87.3482 90) (layer "F.SilkS"))
  (gr_text "ALERT" (at 82.3698 80.192657 90) (layer "F.SilkS"))
  (gr_text "BATT" (at 81.7856 107.973) (layer "F.SilkS"))
  (gr_text "GND" (at 95.8318 107.973) (layer "F.SilkS"))
  (gr_text "3.3V" (at 93.7236 107.973) (layer "F.SilkS"))
  (gr_text "BATT" (at 98.8798 90.0914 90) (layer "F.SilkS"))
  (gr_text "GND" (at 79.8552 107.973) (layer "F.SilkS"))
  (gr_text "GND" (at 77.0358 85.5194 -90) (layer "F.SilkS"))
  (gr_text "ALERT" (at 77.0358 87.949332 270) (layer "F.SilkS"))
  (gr_text "SCL" (at 98.8798 92.479 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 74.77621 76.844297)
        (xy 101.97961 76.768097)
        (xy 102.5628 111.8592)
        (xy 73.43001 111.972497)
        (xy 73.65861 76.945897)
      )
    )
  )
)
