(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 91)
    (zones 0)
    (modules 60)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 8.1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad1)")
  (net 3 Earth)
  (net 4 /RF)
  (net 5 /RF+DC)
  (net 6 /DC+)
  (net 7 /RF2)
  (net 8 /RF+DC2)
  (net 9 /DC+2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class DC ""
    (clearance 0.2)
    (trace_width 3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DC+)
    (add_net /DC+2)
    (add_net Earth)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
  )
  (net_class RF ""
    (clearance 2.5)
    (trace_width 3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RF)
    (add_net /RF+DC)
    (add_net /RF+DC2)
    (add_net /RF2)
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 56D1B4CB)
    (at 190.5 92.5)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Symbol:OSHW-Logo2_14.6x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 179.5 81)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:KiCad-Logo2_5mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 179.5 91.5)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_SilkScreen (at 0 5.08) (layer F.Fab) hide)
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 56D1B4CB)
    (at 99 93)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 94)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 96)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 92)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 82)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 86)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 88)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 84)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 78)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 90)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 80)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 76)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 74)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 66)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 68)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 70)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 62)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 72)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 58)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 56)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 64)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 60)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 54)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 52)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 50)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 48)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 46)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 44)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 42)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 40)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 38)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module alm:hole-1.5mm (layer F.Cu) (tedit 5F7E4C69)
    (at 105 36)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole-1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Symbol:KiCad-Logo2_5mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 87.5 91.5)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_SilkScreen (at 0 5.08) (layer F.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_14.6x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 87.5 81)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module alm:alm (layer F.Cu) (tedit 0)
    (at 168 41.5 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module alm:alm (layer F.Cu) (tedit 0)
    (at 76.5 41.5 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 80.5 67.5 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value 1uF (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /DC+))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 80.5 64.5 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C5 (at 1.25 -2.25 90) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /DC+))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 86.5 67.5 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value " 0.1uF" (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /DC+))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177 64.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C10 (at 2.5 -2.2 90) (layer F.SilkS))
    (fp_text value 1uF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177 67.5 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C11 (at 1.25 -2.55 90) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 2.55 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 183 64.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C12 (at 2.5 -2.2 90) (layer F.SilkS))
    (fp_text value " 0.1uF" (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-2_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 99 53.5 270)
    (descr "TO-220-2, Vertical, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF")
    (tags "TO-220-2 Vertical RM 5.08mm")
    (fp_text reference D1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value D (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-2_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-2_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 191.5 54 270)
    (descr "TO-220-2, Vertical, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF")
    (tags "TO-220-2 Vertical RM 5.08mm")
    (fp_text reference D2 (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text value D (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-2_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Blade_ATO_Littelfuse_Pudenz_2_Pin (layer F.Cu) (tedit 5A1C8E73)
    (at 81.5 53)
    (descr "Fuseholder ATO Blade littelfuse Pudenz 2 Pin")
    (tags "Fuseholder ATO Blade littelfuse Pudenz 2 Pin")
    (fp_text reference F1 (at -4 1 90) (layer F.SilkS))
    (fp_text value 10A (at 5.07 5.22) (layer F.Fab))
    (fp_text user %R (at 4.5 3.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 6 /DC+))
    (pad "" np_thru_hole circle (at 4.6 1.2) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 9.2 0) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuseholder_Blade_ATO_Littelfuse_Pudenz_2_Pin.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SO-239:N (layer F.Cu) (tedit 5F825839)
    (at 31.5 39.5)
    (descr "N-Type Pnl Mount Jk 2-H Solder Cup 50 Ohm horizontal")
    (tags N,connector,horizontal)
    (attr smd)
    (fp_text reference J1 (at 0 -6.25) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -3.25) (layer F.Fab))
    (pad 3 smd custom (at 12.9 0.25) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 2 smd custom (at -12.9 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 1 smd custom (at 0 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 4 /RF) (die_length 8.1) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 98.5 64.5 270)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at 1.27 2 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 1.27 4.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SO-239:N (layer F.Cu) (tedit 5F82582E)
    (at 31.5 92.5)
    (descr "N-Type Pnl Mount Jk 2-H Solder Cup 50 Ohm horizontal")
    (tags N,connector,horizontal)
    (attr smd)
    (fp_text reference J3 (at 0 -2) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -3.25) (layer F.Fab))
    (pad 1 smd custom (at 0 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 5 /RF+DC) (die_length 8.1) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 2 smd custom (at -12.9 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 3 smd custom (at 12.9 0.25) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
  )
  (module SO-239:N (layer F.Cu) (tedit 5F825818)
    (at 124.4 39.5)
    (descr "N-Type Pnl Mount Jk 2-H Solder Cup 50 Ohm horizontal")
    (tags N,connector,horizontal)
    (attr smd)
    (fp_text reference J4 (at 0 -6.25) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -3.25) (layer F.Fab))
    (pad 3 smd custom (at 12.9 0.25) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 2 smd custom (at -12.9 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 1 smd custom (at 0 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 8 /RF+DC2) (die_length 8.1) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 191 64.5 270)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J5 (at 1.27 2 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 1.27 4.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SO-239:N (layer F.Cu) (tedit 5F825823)
    (at 124.4 92.5)
    (descr "N-Type Pnl Mount Jk 2-H Solder Cup 50 Ohm horizontal")
    (tags N,connector,horizontal)
    (attr smd)
    (fp_text reference J6 (at 0.1 -3) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -3.25) (layer F.Fab))
    (pad 1 smd custom (at 0 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 7 /RF2) (die_length 8.1) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 2 smd custom (at -12.9 0) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 3 smd custom (at 12.9 0.25) (size 5 8.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
  )
  (module "SnapEDA Library:INDRD2921W163D3810H2616P" (layer F.Cu) (tedit 5F7CCECD)
    (at 58.105 66)
    (fp_text reference L1 (at 0 0) (layer F.SilkS))
    (fp_text value 1140-101K-RC (at 7.7922 22.07132) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.605 0) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask)
      (net 5 /RF+DC))
    (pad 2 thru_hole circle (at 14.605 0) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 /DC+))
  )
  (module "SnapEDA Library:INDRD2921W163D3810H2616P" (layer F.Cu) (tedit 5F7CCECD)
    (at 153.105 66)
    (fp_text reference L2 (at 0 0) (layer F.SilkS))
    (fp_text value 1140-101K-RC (at 7.7922 22.07132) (layer F.Fab))
    (pad 2 thru_hole circle (at 14.605 0) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (pad 1 thru_hole circle (at -14.605 0) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /RF+DC2))
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 86.5 62.5)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference LA1 (at 0 -2.06) (layer F.SilkS))
    (fp_text value Lamp (at 0 4.06) (layer F.Fab))
    (fp_text user %R (at 0 1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /DC+))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 183 70.5 180)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference LA2 (at 0 -2.06) (layer F.SilkS))
    (fp_text value Lamp (at 0 4.06) (layer F.Fab))
    (fp_text user %R (at 0 1 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /DC+2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D8.0mm_W5.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 124.5 66 90)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 8mm width 5.0mm Capacitor")
    (fp_text reference C1 (at 3.75 0 90) (layer F.SilkS))
    (fp_text value "33 pF" (at 3.75 3.75 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RF2))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RF+DC2))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D8.0mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D8.0mm_W5.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 31.5 66 90)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 8mm width 5.0mm Capacitor")
    (fp_text reference C2 (at 3.75 0 90) (layer F.SilkS))
    (fp_text value "33 pF" (at 3.75 3.75 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RF+DC))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RF))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D8.0mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Bias-T extractor, MAX 60V DC 10A" (at 114 65.5 90) (layer F.SilkS))
  (gr_text "Bias-T Injector, MAX 60V DC 10A" (at 20.5 66 90) (layer F.SilkS))
  (gr_text "CUT ALONG LINE" (at 107 66 90) (layer F.SilkS))
  (gr_text + (at 186.5 64) (layer F.SilkS))
  (gr_text + (at 94 64.5) (layer F.SilkS))
  (gr_text "10A FAST" (at 85.5 50) (layer F.SilkS))
  (gr_text "RF OUT" (at 124.5 78.5 90) (layer F.SilkS))
  (gr_text "RF+DC IN" (at 124.5 50.5 90) (layer F.SilkS))
  (gr_text "RF IN" (at 31.5 50 90) (layer F.SilkS))
  (gr_text "RF+DC OUT" (at 31.5 79.5 90) (layer F.SilkS))
  (dimension 31 (width 0.15) (layer Dwgs.User)
    (gr_text "31.000 mm" (at 15.3 81.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 14 66) (xy 14.586421 66)))
    (feature2 (pts (xy 14 97) (xy 14.586421 97)))
    (crossbar (pts (xy 14 97) (xy 14 66)))
    (arrow1a (pts (xy 14 66) (xy 14.586421 67.126504)))
    (arrow1b (pts (xy 14 66) (xy 13.413579 67.126504)))
    (arrow2a (pts (xy 14 97) (xy 14.586421 95.873496)))
    (arrow2b (pts (xy 14 97) (xy 13.413579 95.873496)))
  )
  (dimension 62 (width 0.15) (layer Dwgs.User)
    (gr_text "62.000 mm" (at 107.7 66 270) (layer Dwgs.User))
    (feature1 (pts (xy 109 97) (xy 108.413579 97)))
    (feature2 (pts (xy 109 35) (xy 108.413579 35)))
    (crossbar (pts (xy 109 35) (xy 109 97)))
    (arrow1a (pts (xy 109 97) (xy 108.413579 95.873496)))
    (arrow1b (pts (xy 109 97) (xy 109.586421 95.873496)))
    (arrow2a (pts (xy 109 35) (xy 108.413579 36.126504)))
    (arrow2b (pts (xy 109 35) (xy 109.586421 36.126504)))
  )
  (gr_line (start 195 35) (end 14 35) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 195 97) (end 195 35) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 14 97) (end 195 97) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 14 35) (end 14 97) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103 97) (xy 13.5 97) (xy 13.5 35) (xy 103 35)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103 97) (xy 13.5 97) (xy 13.5 35) (xy 103 35)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195 97) (xy 107 97) (xy 107 35) (xy 195 35)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195 97) (xy 107 97) (xy 107 35) (xy 195 35)
      )
    )
  )
)
