(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.567)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" power)
		(2 "In2.Cu" power)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0254)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.2021)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.2021)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0254)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 2.000000)
			(dashed_line_gap_ratio 1.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "External +3.3V Source")
	(net 2 "+3.3V")
	(net 3 "GNDD")
	(net 4 "unconnected-(J2-Pin_19-Pad19)")
	(net 5 "unconnected-(J2-Pin_20-Pad20)")
	(net 6 "unconnected-(J3-Pin_1-Pad1)")
	(net 7 "/F2")
	(net 8 "/E1")
	(net 9 "/E2")
	(net 10 "/D1")
	(net 11 "/D2")
	(net 12 "/D3")
	(net 13 "/D-1")
	(net 14 "/D-2")
	(net 15 "unconnected-(J3-Pin_19-Pad19)")
	(net 16 "unconnected-(J3-Pin_20-Pad20)")
	(net 17 "Glasgow +3.3V Source")
	(net 18 "/K1")
	(net 19 "/J1")
	(net 20 "/H1")
	(net 21 "/H2")
	(net 22 "/H3")
	(net 23 "/G1")
	(net 24 "/G3")
	(net 25 "/G2")
	(net 26 "/F3")
	(net 27 "/F1")
	(net 28 "/F4")
	(net 29 "/D-3")
	(net 30 "/E3")
	(net 31 "/D-4")
	(net 32 "/D-5")
	(net 33 "/D-6")
	(net 34 "/C1")
	(net 35 "/C2")
	(net 36 "/C3")
	(net 37 "/B1")
	(net 38 "/C4")
	(net 39 "/B2")
	(net 40 "/D-17")
	(net 41 "/D-18")
	(net 42 "/D-19")
	(net 43 "/D-20")
	(net 44 "/D-21")
	(net 45 "/D-22")
	(net 46 "/D-23")
	(net 47 "/D-24")
	(net 48 "Net-(J5-Pin_1)")
	(net 49 "Net-(J5-Pin_2)")
	(net 50 "/Z12_P")
	(net 51 "/Z12_N")
	(net 52 "/D-7")
	(net 53 "/D-8")
	(net 54 "/D-9")
	(net 55 "/D-10")
	(net 56 "/D-11")
	(net 57 "/D-12")
	(net 58 "/D-13")
	(net 59 "/D-14")
	(net 60 "/D-15")
	(net 61 "/D-16")
	(net 62 "unconnected-(J4-Pin_1-Pad1)")
	(net 63 "unconnected-(J4-Pin_19-Pad19)")
	(net 64 "unconnected-(J4-Pin_20-Pad20)")
	(footprint "OBI Data Interconnect:IDC-Header_Receptacle_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
		(locked yes)
		(layer "F.Cu")
		(at 165.81 52.48)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J2"
			(at 1.27 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 28.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:IDC-Header_Receptacle_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "External +3.3V Source")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/D-17")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/D-18")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/D-19")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/D-20")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/D-21")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/D-22")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/D-23")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/D-24")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(J2-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J2-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KIPRJMOD}/3D Models/SFH11-PBPC-D10-ST-BK.step"
			(offset
				(xyz 1.25 -11.43 -1.65)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 -90)
			)
		)
	)
	(footprint "OBI Data Interconnect:IDC-Header_Receptacle_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
		(locked yes)
		(layer "F.Cu")
		(at 165.81 88.04)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J4"
			(at 1.27 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 28.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:IDC-Header_Receptacle_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 62 "unconnected-(J4-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/D-9")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/D-10")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/D-11")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/D-12")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/D-13")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/D-14")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/D-15")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/D-16")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(J4-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(J4-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KIPRJMOD}/3D Models/SFH11-PBPC-D10-ST-BK.step"
			(offset
				(xyz 1.25 -11.43 -1.65)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 -90)
			)
		)
	)
	(footprint "OBI Data Interconnect:IDC-Header_Receptacle_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
		(locked yes)
		(layer "F.Cu")
		(at 155.65 88.04)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J3"
			(at 1.27 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 28.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:IDC-Header_Receptacle_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 6 "unconnected-(J3-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/D-1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/D-2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/D-3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/D-4")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/D-5")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/D-6")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/D-7")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/D-8")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GNDD")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J3-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J3-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KIPRJMOD}/3D Models/SFH11-PBPC-D10-ST-BK.step"
			(offset
				(xyz 1.25 -11.43 -1.65)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 -90)
			)
		)
	)
	(footprint "OBI Data Interconnect:MountingHole_3.5mm_Pad_Via_CrtYd"
		(locked yes)
		(layer "F.Cu")
		(at 155.65 120.9)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H3"
			(at 6.402 0.004 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "OBI Data Interconnect:MountingHole_3.5mm_Pad_Via_CrtYd"
		(locked yes)
		(layer "F.Cu")
		(at 137.65 48.9)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H1"
			(at 6.114 0.122 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "OBI Data Interconnect:MountingHole_3.5mm_Pad_Via_CrtYd"
		(locked yes)
		(layer "F.Cu")
		(at 155.65 48.9)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H2"
			(at -6.298 0.122 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 147.495 59.81 180)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J5"
			(at -2.765 -0.87 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 5.31 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OBI Data Interconnect:nanographs smaller"
		(layer "F.Cu")
		(at 147.94383 76.93)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "nanographs smaller"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 142.68 57.79)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0.02 -1.31 0)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/Z12_P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 49 "Net-(J5-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OBI Data Interconnect:RES_EXB2HV"
		(layer "B.Cu")
		(at 155.75 64.74 180)
		(tags "EXB-2HV471JV ")
		(property "Reference" "RN1"
			(at -0.67 3.34 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "R_Pack08"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:RES_EXB2HV"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/EXB-2HV471JV/285315"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4699 1.4478 180)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4699 1.4478 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.9144 1.9812 180)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 40 "/D-17")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9144 1.233678 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "/D-18")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9144 0.740156 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "/D-19")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9144 0.246634 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "/D-20")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.9144 -0.246888 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "/D-21")
			(pinfunction "R5.1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -0.9144 -0.74041 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 45 "/D-22")
			(pinfunction "R6.1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -0.9144 -1.233932 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "/D-23")
			(pinfunction "R7.1")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.9144 -1.9812 180)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "/D-24")
			(pinfunction "R8.1")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.9144 -1.9812 180)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "/G1")
			(pinfunction "R8.2")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.9144 -1.233932 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "/F3")
			(pinfunction "R7.2")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.9144 -0.74041 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "/H2")
			(pinfunction "R6.2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 0.9144 -0.246888 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "/G3")
			(pinfunction "R5.2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.9144 0.246634 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "/H1")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.9144 0.740156 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "/H3")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0.9144 1.233678 180)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "/J1")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0.9144 1.9812 180)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "/K1")
			(pinfunction "R1.2")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 142.685 59.26)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0.135 1.45 0)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/Z12_N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 48 "Net-(J5-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OBI Data Interconnect:RES_EXB2HV"
		(layer "B.Cu")
		(at 154.47 77.94 -45)
		(tags "EXB-2HV471JV ")
		(property "Reference" "RN2"
			(at -3.24562 -2.694077 -45)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "R_Pack08"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:RES_EXB2HV"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -0.4699 1.4478 135)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4699 1.4478 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.914399 1.9812 315)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "/B2")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9144 1.233679 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "/C4")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9144 0.740156 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 37 "/B1")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9144 0.246634 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 36 "/C3")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.9144 -0.246888 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "/C2")
			(pinfunction "R5.1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -0.9144 -0.740409 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 34 "/C1")
			(pinfunction "R6.1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -0.9144 -1.233932 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "/D3")
			(pinfunction "R7.1")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.914399 -1.9812 315)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "/D1")
			(pinfunction "R8.1")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.914399 -1.9812 315)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 53 "/D-8")
			(pinfunction "R8.2")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.9144 -1.233932 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "/D-7")
			(pinfunction "R7.2")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.9144 -0.740409 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "/D-6")
			(pinfunction "R6.2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 0.9144 -0.246888 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 32 "/D-5")
			(pinfunction "R5.2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.9144 0.246634 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 31 "/D-4")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.9144 0.740156 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 29 "/D-3")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0.9144 1.233679 315)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "/D-2")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0.914399 1.9812 315)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "/D-1")
			(pinfunction "R1.2")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 160.2 59.28 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0.03 2.05 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 160.21 55.22)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "JP1"
			(at 0.01 -1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "Jumper_2_Open"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "External +3.3V Source")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OBI Data Interconnect:RES_EXB2HV"
		(layer "B.Cu")
		(at 158.6 73.77 135)
		(tags "EXB-2HV471JV ")
		(property "Reference" "RN3"
			(at 3.181981 2.729432 -45)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "R_Pack08"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:RES_EXB2HV"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -0.4699 1.4478 -45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4699 1.4478 -45)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.914399 1.9812 135)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 54 "/D-9")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9144 1.233679 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 55 "/D-10")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9144 0.740156 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 56 "/D-11")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9144 0.246634 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 57 "/D-12")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.9144 -0.246888 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "/D-13")
			(pinfunction "R5.1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -0.9144 -0.740409 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 59 "/D-14")
			(pinfunction "R6.1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -0.9144 -1.233932 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/D-15")
			(pinfunction "R7.1")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.914399 -1.9812 135)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 61 "/D-16")
			(pinfunction "R8.1")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.914399 -1.9812 135)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 11 "/D2")
			(pinfunction "R8.2")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.9144 -1.233932 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "/E1")
			(pinfunction "R7.2")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.9144 -0.740409 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "/F2")
			(pinfunction "R6.2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 0.9144 -0.246888 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "/E2")
			(pinfunction "R5.2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.9144 0.246634 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "/F1")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.9144 0.740156 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "/E3")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0.9144 1.233679 135)
			(size 0.7874 0.3556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "/G2")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0.914399 1.9812 135)
			(size 0.7874 0.8636)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "/F4")
			(pinfunction "R1.2")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 141.97 80.26)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.02 -1.94 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 144.9 58.52 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.27 0.065 0)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 48 "Net-(J5-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 49 "Net-(J5-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OBI Data Interconnect:PinReceptacle_2x22_P1.27mm_Vertical_BackSide_SMD"
		(locked yes)
		(layer "B.Cu")
		(at 136.15 68.66)
		(descr "surface-mounted straight pin header, 2x22, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x22 1.27mm double row")
		(property "Reference" "J1"
			(at -1.97 -16.34 180)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x22_Odd_Even"
			(at 0 13.76 180)
			(layer "B.Fab")
		)
		(property "Footprint" "OBI Data Interconnect:PinReceptacle_2x22_P1.27mm_Vertical_BackSide_SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.875 -14.605)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.875 -14.605)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Glasgow +3.3V Source")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.875 -13.335)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/K1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.875 -13.335)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -1.875 -12.065)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/J1")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.875 -12.065)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -1.875 -10.795)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 1.875 -10.795)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/Z12_P")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -1.875 -9.525)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/H1")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 1.875 -9.525)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/Z12_N")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -1.875 -8.255)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/H2")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 1.875 -8.255)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at -1.875 -6.985)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 1.875 -6.985)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/H3")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at -1.875 -5.715)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/G1")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 1.875 -5.715)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/G3")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at -1.875 -4.445)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/G2")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at 1.875 -4.445)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at -1.875 -3.175)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 1.875 -3.175)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/F3")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at -1.875 -1.905)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/F1")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 1.875 -1.905)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/F4")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at -1.875 -0.635)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/F2")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at 1.875 -0.635)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd roundrect
			(at -1.875 0.635)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" smd roundrect
			(at 1.875 0.635)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/E3")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at -1.875 1.905)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/E1")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd roundrect
			(at 1.875 1.905)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/E2")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd roundrect
			(at -1.875 3.175)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/D1")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd roundrect
			(at 1.875 3.175)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd roundrect
			(at -1.875 4.445)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd roundrect
			(at 1.875 4.445)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/D2")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at -1.875 5.715)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/C1")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd roundrect
			(at 1.875 5.715)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/D3")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" smd roundrect
			(at -1.875 6.985)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/C2")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" smd roundrect
			(at 1.875 6.985)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd roundrect
			(at -1.875 8.255)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" smd roundrect
			(at 1.875 8.255)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/C3")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd roundrect
			(at -1.875 9.525)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/B1")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" smd roundrect
			(at 1.875 9.525)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/C4")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(pad "41" smd roundrect
			(at -1.875 10.795)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/B2")
			(pinfunction "Pin_41")
			(pintype "passive")
		)
		(pad "42" smd roundrect
			(at 1.875 10.795)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_42")
			(pintype "passive")
		)
		(pad "43" smd roundrect
			(at -1.875 12.065)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pinfunction "Pin_43")
			(pintype "passive")
		)
		(pad "44" smd roundrect
			(at 1.875 12.065)
			(size 1.47 0.76)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pinfunction "Pin_44")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 55.452) (xy 135.388 55.706) (xy 135.642 55.706) (xy 135.896 55.452) (xy 135.896 55.198)
					(xy 135.642 54.944) (xy 135.388 54.944) (xy 135.134 55.198)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 56.722) (xy 135.388 56.976) (xy 135.642 56.976) (xy 135.896 56.722) (xy 135.896 56.468)
					(xy 135.642 56.214) (xy 135.388 56.214) (xy 135.134 56.468)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 59.262) (xy 135.388 59.516) (xy 135.642 59.516) (xy 135.896 59.262) (xy 135.896 59.008)
					(xy 135.642 58.754) (xy 135.388 58.754) (xy 135.134 59.008)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 60.532) (xy 135.388 60.786) (xy 135.642 60.786) (xy 135.896 60.532) (xy 135.896 60.278)
					(xy 135.642 60.024) (xy 135.388 60.024) (xy 135.134 60.278)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 63.072) (xy 135.388 63.326) (xy 135.642 63.326) (xy 135.896 63.072) (xy 135.896 62.818)
					(xy 135.642 62.564) (xy 135.388 62.564) (xy 135.134 62.818)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 64.342) (xy 135.388 64.596) (xy 135.642 64.596) (xy 135.896 64.342) (xy 135.896 64.088)
					(xy 135.642 63.834) (xy 135.388 63.834) (xy 135.134 64.088)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 66.882) (xy 135.388 67.136) (xy 135.642 67.136) (xy 135.896 66.882) (xy 135.896 66.628)
					(xy 135.642 66.374) (xy 135.388 66.374) (xy 135.134 66.628)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 68.152) (xy 135.388 68.406) (xy 135.642 68.406) (xy 135.896 68.152) (xy 135.896 67.898)
					(xy 135.642 67.644) (xy 135.388 67.644) (xy 135.134 67.898)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 70.692) (xy 135.388 70.946) (xy 135.642 70.946) (xy 135.896 70.692) (xy 135.896 70.438)
					(xy 135.642 70.184) (xy 135.388 70.184) (xy 135.134 70.438)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 71.962) (xy 135.388 72.216) (xy 135.642 72.216) (xy 135.896 71.962) (xy 135.896 71.708)
					(xy 135.642 71.454) (xy 135.388 71.454) (xy 135.134 71.708)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 74.502) (xy 135.388 74.756) (xy 135.642 74.756) (xy 135.896 74.502) (xy 135.896 74.248)
					(xy 135.642 73.994) (xy 135.388 73.994) (xy 135.134 74.248)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 75.772) (xy 135.388 76.026) (xy 135.642 76.026) (xy 135.896 75.772) (xy 135.896 75.518)
					(xy 135.642 75.264) (xy 135.388 75.264) (xy 135.134 75.518)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 78.312) (xy 135.388 78.566) (xy 135.642 78.566) (xy 135.896 78.312) (xy 135.896 78.058)
					(xy 135.642 77.804) (xy 135.388 77.804) (xy 135.134 78.058)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 135.134 79.582) (xy 135.388 79.836) (xy 135.642 79.836) (xy 135.896 79.582) (xy 135.896 79.328)
					(xy 135.642 79.074) (xy 135.388 79.074) (xy 135.134 79.328)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 54.182) (xy 136.658 54.436) (xy 136.912 54.436) (xy 137.166 54.182) (xy 137.166 53.928)
					(xy 136.912 53.674) (xy 136.658 53.674) (xy 136.404 53.928)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 57.992) (xy 136.658 58.246) (xy 136.912 58.246) (xy 137.166 57.992) (xy 137.166 57.738)
					(xy 136.912 57.484) (xy 136.658 57.484) (xy 136.404 57.738)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 59.262) (xy 136.658 59.516) (xy 136.912 59.516) (xy 137.166 59.262) (xy 137.166 59.008)
					(xy 136.912 58.754) (xy 136.658 58.754) (xy 136.404 59.008)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 61.802) (xy 136.658 62.056) (xy 136.912 62.056) (xy 137.166 61.802) (xy 137.166 61.548)
					(xy 136.912 61.294) (xy 136.658 61.294) (xy 136.404 61.548)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 63.072) (xy 136.658 63.326) (xy 136.912 63.326) (xy 137.166 63.072) (xy 137.166 62.818)
					(xy 136.912 62.564) (xy 136.658 62.564) (xy 136.404 62.818)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 65.612) (xy 136.658 65.866) (xy 136.912 65.866) (xy 137.166 65.612) (xy 137.166 65.358)
					(xy 136.912 65.104) (xy 136.658 65.104) (xy 136.404 65.358)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 66.882) (xy 136.658 67.136) (xy 136.912 67.136) (xy 137.166 66.882) (xy 137.166 66.628)
					(xy 136.912 66.374) (xy 136.658 66.374) (xy 136.404 66.628)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 69.422) (xy 136.658 69.676) (xy 136.912 69.676) (xy 137.166 69.422) (xy 137.166 69.168)
					(xy 136.912 68.914) (xy 136.658 68.914) (xy 136.404 69.168)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 70.692) (xy 136.658 70.946) (xy 136.912 70.946) (xy 137.166 70.692) (xy 137.166 70.438)
					(xy 136.912 70.184) (xy 136.658 70.184) (xy 136.404 70.438)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 73.232) (xy 136.658 73.486) (xy 136.912 73.486) (xy 137.166 73.232) (xy 137.166 72.978)
					(xy 136.912 72.724) (xy 136.658 72.724) (xy 136.404 72.978)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 74.502) (xy 136.658 74.756) (xy 136.912 74.756) (xy 137.166 74.502) (xy 137.166 74.248)
					(xy 136.912 73.994) (xy 136.658 73.994) (xy 136.404 74.248)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 77.042) (xy 136.658 77.296) (xy 136.912 77.296) (xy 137.166 77.042) (xy 137.166 76.788)
					(xy 136.912 76.534) (xy 136.658 76.534) (xy 136.404 76.788)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 78.312) (xy 136.658 78.566) (xy 136.912 78.566) (xy 137.166 78.312) (xy 137.166 78.058)
					(xy 136.912 77.804) (xy 136.658 77.804) (xy 136.404 78.058)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "Dwgs.User")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.404 80.852) (xy 136.658 81.106) (xy 136.912 81.106) (xy 137.166 80.852) (xy 137.166 80.598)
					(xy 136.912 80.344) (xy 136.658 80.344) (xy 136.404 80.598)
				)
			)
		)
		(model "${KIPRJMOD}/3D Models/FLE-122-01-G-DV-A.stp"
			(offset
				(xyz 0 -1.25 0.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 156.25 58.85)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -3.2 0.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "GNDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 145.8 79.84 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -3.28 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.85 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "GNDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 141.94 53.98 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "JP2"
			(at -0.14 1.63 180)
			(layer "B.SilkS")
		)
		(property "Value" "Jumper_2_Open"
			(at 0 -1.43 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Glasgow +3.3V Source")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 162.81 117.81 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -0.02 -1.53 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GNDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 166.85 118.24)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -0.02 1.93 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "OBI Data Interconnect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "GNDD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 168.15 124.9)
		(end 155.65 124.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.81 48.9)
		(mid 132.981573 46.071573)
		(end 135.81 44.9)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 168.15 44.9)
		(mid 170.978427 46.071573)
		(end 172.15 48.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.65 81.616)
		(end 151.65 120.9)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.81 81.616)
		(end 151.65 81.616)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.81 48.896)
		(end 131.81 81.616)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 135.81 44.9)
		(end 168.15 44.9)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.15 120.9)
		(mid 170.978427 123.728427)
		(end 168.15 124.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.15 120.9)
		(end 172.15 48.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 155.65 124.9)
		(mid 152.821573 123.728427)
		(end 151.65 120.9)
		(layer "Edge.Cuts")
	)
	(gr_text "+3.3V\nFrom\nExternal"
		(at 157.93 56.88 0)
		(layer "B.SilkS")
	)
	(gr_text "**DO NOT**\nplace both\nJP1 and JP2"
		(at 150.11 49.98 -0)
		(layer "B.SilkS")
	)
	(gr_text "+3.3V\nFrom\nGlasgow"
		(at 143.77 54.32 0)
		(layer "B.SilkS")
	)
	(gr_text "0\n1\n1\n0\n1\n1\n0\n0"
		(at 134.674 72.695548 345)
		(layer "F.SilkS")
	)
	(gr_text "0\n1\n1\n0\n1\n1\n0\n0"
		(at 136.198 72.695548 345)
		(layer "F.SilkS")
	)
	(gr_text "0\n1\n1\n0\n1\n0\n0\n0"
		(at 132.134 72.187548 345)
		(layer "F.SilkS")
	)
	(gr_text "Isabel Burgos"
		(at 141.986 72.103412 0)
		(layer "F.SilkS")
	)
	(gr_text "LVDS I/O\nBreakout\nfor Glasgow"
		(at 141.732 70.104 0)
		(layer "F.SilkS")
	)
	(gr_text "Adam McCombs"
		(at 141.986 73.627412 0)
		(layer "F.SilkS")
	)
	(gr_text "0\n1\n1\n0\n0\n1\n0\n1"
		(at 133.15 72.695548 345)
		(layer "F.SilkS")
	)
	(gr_text "0\n1\n1\n0\n1\n1\n1\n1"
		(at 137.722 72.695548 345)
		(layer "F.SilkS")
	)
	(gr_text "revA3 2024-07-01"
		(at 141.88 75.14 0)
		(layer "F.SilkS")
	)
	(gr_text "0\n0\n1\n0\n0\n0\n0\n1"
		(at 138.992 72.441548 345)
		(layer "F.SilkS")
	)
	(gr_text "SolderJumper_2_Open"
		(at 160.05 85.7 180)
		(layer "B.Fab")
	)
	(gr_text "Wave soldering keepout"
		(at 143.25 99.5 -90)
		(layer "B.Fab")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 155.65 48.9) (xy 172.15 48.9)
		)
		(height 0)
		(gr_text "16.5000 mm"
			(at 163.9 47.75 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 124.13 44.9) (xy 124.13 87.47)
		)
		(height -5)
		(gr_text "42.5700 mm"
			(at 127.33 66.185 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 155.65 48.9) (xy 155.65 120.9)
		)
		(height -34)
		(gr_text "72.0000 mm"
			(at 187.85 84.9 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 124.13 110.33) (xy 124.13 124.9)
		)
		(height -5)
		(gr_text "14.5700 mm"
			(at 127.33 117.615 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 124.13 87.47) (xy 124.13 110.33)
		)
		(height -5)
		(gr_text "22.8600 mm"
			(at 127.33 98.9 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 151.65 124.9) (xy 151.65 110.9)
		)
		(height -2.42)
		(orientation 1)
		(gr_text "14.0000 mm"
			(at 147.17 117.96 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 137.65 48.9) (xy 155.65 48.9)
		)
		(height -17.58)
		(orientation 0)
		(gr_text "18.0000 mm"
			(at 146.65 29.52 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 137.65 48.9) (xy 136.398 44.831)
		)
		(height 0)
		(orientation 1)
		(gr_text "4.0000 mm"
			(at 136.5 46.8655 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(override_value "4.0000")
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 155.65 120.9) (xy 165.65 118.9)
		)
		(height 14.75)
		(orientation 0)
		(gr_text "10.0000 mm"
			(at 160.72 137.67 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 3)
		(net_name "GNDD")
		(layers "F.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.76 81.62) (xy 131.76 44.9) (xy 172.15 44.9) (xy 172.15 124.9) (xy 151.65 124.9) (xy 151.65 81.62)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GNDD")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.4)
		)
		(polygon
			(pts
				(xy 131.76 81.62) (xy 131.76 44.9) (xy 172.15 44.9) (xy 172.15 124.9) (xy 151.65 124.9) (xy 151.65 81.62)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.3V")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.77 81.69) (xy 131.77 44.97) (xy 172.17 44.97) (xy 172.17 124.97) (xy 151.67 124.97) (xy 151.67 81.69)
			)
		)
	)
)