(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 712)
    (zones 0)
    (modules 17)
    (nets 145)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1)
    (trace_clearance 0.04)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.05)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 77.8 71.3)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /TOP_A70)
  (net 2 /TOP_A69)
  (net 3 /TOP_A68)
  (net 4 /TOP_A67)
  (net 5 /TOP_A66)
  (net 6 /TOP_A65)
  (net 7 /TOP_A64)
  (net 8 /TOP_A63)
  (net 9 /TOP_A62)
  (net 10 /TOP_A61)
  (net 11 /TOP_A60)
  (net 12 /TOP_A59)
  (net 13 /TOP_A58)
  (net 14 /TOP_A57)
  (net 15 /TOP_A56)
  (net 16 /TOP_A55)
  (net 17 /TOP_A54)
  (net 18 /TOP_A53)
  (net 19 /TOP_A52)
  (net 20 /TOP_A51)
  (net 21 /TOP_A50)
  (net 22 /TOP_A49)
  (net 23 /TOP_A48)
  (net 24 /TOP_A47)
  (net 25 /TOP_A46)
  (net 26 /TOP_A45)
  (net 27 /TOP_A44)
  (net 28 /TOP_A43)
  (net 29 /TOP_A42)
  (net 30 /TOP_A41)
  (net 31 /TOP_A40)
  (net 32 /TOP_A39)
  (net 33 /TOP_A38)
  (net 34 /TOP_A37)
  (net 35 /TOP_A36)
  (net 36 /TOP_A35)
  (net 37 /TOP_A34)
  (net 38 /TOP_A33)
  (net 39 /TOP_A32)
  (net 40 /TOP_A31)
  (net 41 /TOP_A30)
  (net 42 /TOP_A29)
  (net 43 /TOP_A28)
  (net 44 /TOP_A27)
  (net 45 /TOP_A26)
  (net 46 /TOP_A25)
  (net 47 /TOP_A24)
  (net 48 /TOP_A23)
  (net 49 /TOP_A22)
  (net 50 /TOP_A21)
  (net 51 /TOP_A20)
  (net 52 /TOP_A19)
  (net 53 /TOP_A18)
  (net 54 /TOP_A17)
  (net 55 /TOP_A16)
  (net 56 /TOP_A15)
  (net 57 /TOP_A14)
  (net 58 /TOP_A13)
  (net 59 /TOP_A12)
  (net 60 /TOP_A11)
  (net 61 /TOP_A10)
  (net 62 /TOP_A9)
  (net 63 /TOP_A8)
  (net 64 /TOP_A7)
  (net 65 /TOP_A6)
  (net 66 /TOP_A5)
  (net 67 /TOP_A4)
  (net 68 /TOP_A3)
  (net 69 /TOP_A2)
  (net 70 /TOP_A1)
  (net 71 /TOP_B70)
  (net 72 /TOP_B69)
  (net 73 /TOP_B68)
  (net 74 /TOP_B67)
  (net 75 /TOP_B66)
  (net 76 /TOP_B65)
  (net 77 /TOP_B64)
  (net 78 /TOP_B63)
  (net 79 /TOP_B62)
  (net 80 /TOP_B61)
  (net 81 /TOP_B60)
  (net 82 /TOP_B59)
  (net 83 /TOP_B58)
  (net 84 /TOP_B57)
  (net 85 /TOP_B56)
  (net 86 /TOP_B55)
  (net 87 /TOP_B54)
  (net 88 /TOP_B53)
  (net 89 /TOP_B52)
  (net 90 /TOP_B51)
  (net 91 /TOP_B50)
  (net 92 /TOP_B49)
  (net 93 /TOP_B48)
  (net 94 /TOP_B47)
  (net 95 /TOP_B46)
  (net 96 /TOP_B45)
  (net 97 /TOP_B44)
  (net 98 /TOP_B43)
  (net 99 /TOP_B42)
  (net 100 /TOP_B41)
  (net 101 /TOP_B40)
  (net 102 /TOP_B39)
  (net 103 /TOP_B38)
  (net 104 /TOP_B37)
  (net 105 /TOP_B36)
  (net 106 /TOP_B35)
  (net 107 /TOP_B34)
  (net 108 /TOP_B33)
  (net 109 /TOP_B32)
  (net 110 /TOP_B31)
  (net 111 /TOP_B30)
  (net 112 /TOP_B29)
  (net 113 /TOP_B28)
  (net 114 /TOP_B27)
  (net 115 /TOP_B26)
  (net 116 /TOP_B25)
  (net 117 /TOP_B24)
  (net 118 /TOP_B23)
  (net 119 /TOP_B22)
  (net 120 /TOP_B21)
  (net 121 /TOP_B20)
  (net 122 /TOP_B19)
  (net 123 /TOP_B18)
  (net 124 /TOP_B17)
  (net 125 /TOP_B16)
  (net 126 /TOP_B15)
  (net 127 /TOP_B14)
  (net 128 /TOP_B13)
  (net 129 /TOP_B12)
  (net 130 /TOP_B11)
  (net 131 /TOP_B10)
  (net 132 /TOP_B9)
  (net 133 /TOP_B8)
  (net 134 /TOP_B7)
  (net 135 /TOP_B6)
  (net 136 /TOP_B5)
  (net 137 /TOP_B4)
  (net 138 /TOP_B3)
  (net 139 /TOP_B2)
  (net 140 /TOP_B1)
  (net 141 /BOT_GRP1)
  (net 142 /BOT_GRP2)
  (net 143 /BOT_GRP3)
  (net 144 /BOT_GRP4)
  (net_class Default "This is the default net class."
    (clearance 0.04)
    (trace_width 0.1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BOT_GRP1)
    (add_net /BOT_GRP2)
    (add_net /BOT_GRP3)
    (add_net /BOT_GRP4)
    (add_net /TOP_A1)
    (add_net /TOP_A10)
    (add_net /TOP_A11)
    (add_net /TOP_A12)
    (add_net /TOP_A13)
    (add_net /TOP_A14)
    (add_net /TOP_A15)
    (add_net /TOP_A16)
    (add_net /TOP_A17)
    (add_net /TOP_A18)
    (add_net /TOP_A19)
    (add_net /TOP_A2)
    (add_net /TOP_A20)
    (add_net /TOP_A21)
    (add_net /TOP_A22)
    (add_net /TOP_A23)
    (add_net /TOP_A24)
    (add_net /TOP_A25)
    (add_net /TOP_A26)
    (add_net /TOP_A27)
    (add_net /TOP_A28)
    (add_net /TOP_A29)
    (add_net /TOP_A3)
    (add_net /TOP_A30)
    (add_net /TOP_A31)
    (add_net /TOP_A32)
    (add_net /TOP_A33)
    (add_net /TOP_A34)
    (add_net /TOP_A35)
    (add_net /TOP_A36)
    (add_net /TOP_A37)
    (add_net /TOP_A38)
    (add_net /TOP_A39)
    (add_net /TOP_A4)
    (add_net /TOP_A40)
    (add_net /TOP_A41)
    (add_net /TOP_A42)
    (add_net /TOP_A43)
    (add_net /TOP_A44)
    (add_net /TOP_A45)
    (add_net /TOP_A46)
    (add_net /TOP_A47)
    (add_net /TOP_A48)
    (add_net /TOP_A49)
    (add_net /TOP_A5)
    (add_net /TOP_A50)
    (add_net /TOP_A51)
    (add_net /TOP_A52)
    (add_net /TOP_A53)
    (add_net /TOP_A54)
    (add_net /TOP_A55)
    (add_net /TOP_A56)
    (add_net /TOP_A57)
    (add_net /TOP_A58)
    (add_net /TOP_A59)
    (add_net /TOP_A6)
    (add_net /TOP_A60)
    (add_net /TOP_A61)
    (add_net /TOP_A62)
    (add_net /TOP_A63)
    (add_net /TOP_A64)
    (add_net /TOP_A65)
    (add_net /TOP_A66)
    (add_net /TOP_A67)
    (add_net /TOP_A68)
    (add_net /TOP_A69)
    (add_net /TOP_A7)
    (add_net /TOP_A70)
    (add_net /TOP_A8)
    (add_net /TOP_A9)
    (add_net /TOP_B1)
    (add_net /TOP_B10)
    (add_net /TOP_B11)
    (add_net /TOP_B12)
    (add_net /TOP_B13)
    (add_net /TOP_B14)
    (add_net /TOP_B15)
    (add_net /TOP_B16)
    (add_net /TOP_B17)
    (add_net /TOP_B18)
    (add_net /TOP_B19)
    (add_net /TOP_B2)
    (add_net /TOP_B20)
    (add_net /TOP_B21)
    (add_net /TOP_B22)
    (add_net /TOP_B23)
    (add_net /TOP_B24)
    (add_net /TOP_B25)
    (add_net /TOP_B26)
    (add_net /TOP_B27)
    (add_net /TOP_B28)
    (add_net /TOP_B29)
    (add_net /TOP_B3)
    (add_net /TOP_B30)
    (add_net /TOP_B31)
    (add_net /TOP_B32)
    (add_net /TOP_B33)
    (add_net /TOP_B34)
    (add_net /TOP_B35)
    (add_net /TOP_B36)
    (add_net /TOP_B37)
    (add_net /TOP_B38)
    (add_net /TOP_B39)
    (add_net /TOP_B4)
    (add_net /TOP_B40)
    (add_net /TOP_B41)
    (add_net /TOP_B42)
    (add_net /TOP_B43)
    (add_net /TOP_B44)
    (add_net /TOP_B45)
    (add_net /TOP_B46)
    (add_net /TOP_B47)
    (add_net /TOP_B48)
    (add_net /TOP_B49)
    (add_net /TOP_B5)
    (add_net /TOP_B50)
    (add_net /TOP_B51)
    (add_net /TOP_B52)
    (add_net /TOP_B53)
    (add_net /TOP_B54)
    (add_net /TOP_B55)
    (add_net /TOP_B56)
    (add_net /TOP_B57)
    (add_net /TOP_B58)
    (add_net /TOP_B59)
    (add_net /TOP_B6)
    (add_net /TOP_B60)
    (add_net /TOP_B61)
    (add_net /TOP_B62)
    (add_net /TOP_B63)
    (add_net /TOP_B64)
    (add_net /TOP_B65)
    (add_net /TOP_B66)
    (add_net /TOP_B67)
    (add_net /TOP_B68)
    (add_net /TOP_B69)
    (add_net /TOP_B7)
    (add_net /TOP_B70)
    (add_net /TOP_B8)
    (add_net /TOP_B9)
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer B.Cu) (tedit 5E45C4FB)
    (at 102.2 72)
    (fp_text reference J8 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 0.5) (layer B.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 144 /BOT_GRP4))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer B.Cu) (tedit 5E45C4FB)
    (at 102.2 92.9)
    (fp_text reference J7 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 0.5) (layer B.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 143 /BOT_GRP3))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer B.Cu) (tedit 5E45C4FB)
    (at 81.3 92.9)
    (fp_text reference J6 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 0.5) (layer B.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 142 /BOT_GRP2))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer B.Cu) (tedit 5E45C4FB)
    (at 81.3 72)
    (fp_text reference J5 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 0.5) (layer B.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers B.Cu B.Mask)
      (net 141 /BOT_GRP1))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer F.Cu) (tedit 5E45C4FB)
    (at 102.2 92.9)
    (fp_text reference J4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 -0.5) (layer F.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 71 /TOP_B70))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 72 /TOP_B69))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 73 /TOP_B68))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 74 /TOP_B67))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 75 /TOP_B66))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 76 /TOP_B65))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 77 /TOP_B64))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 78 /TOP_B63))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 79 /TOP_B62))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 80 /TOP_B61))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 81 /TOP_B60))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 82 /TOP_B59))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 83 /TOP_B58))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 84 /TOP_B57))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 85 /TOP_B56))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 86 /TOP_B55))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 87 /TOP_B54))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 88 /TOP_B53))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 89 /TOP_B52))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 90 /TOP_B51))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 91 /TOP_B50))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 92 /TOP_B49))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 93 /TOP_B48))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 94 /TOP_B47))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 95 /TOP_B46))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 96 /TOP_B45))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 97 /TOP_B44))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 98 /TOP_B43))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 99 /TOP_B42))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 100 /TOP_B41))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 101 /TOP_B40))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 102 /TOP_B39))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 103 /TOP_B38))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 104 /TOP_B37))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 105 /TOP_B36))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 106 /TOP_B35))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 107 /TOP_B34))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 108 /TOP_B33))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 109 /TOP_B32))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 110 /TOP_B31))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 111 /TOP_B30))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 112 /TOP_B29))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 113 /TOP_B28))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 114 /TOP_B27))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 115 /TOP_B26))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 116 /TOP_B25))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 117 /TOP_B24))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 118 /TOP_B23))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 119 /TOP_B22))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 120 /TOP_B21))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 121 /TOP_B20))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 122 /TOP_B19))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 123 /TOP_B18))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 124 /TOP_B17))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 125 /TOP_B16))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 126 /TOP_B15))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 127 /TOP_B14))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 128 /TOP_B13))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 129 /TOP_B12))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 130 /TOP_B11))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 131 /TOP_B10))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 132 /TOP_B9))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 133 /TOP_B8))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 134 /TOP_B7))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 135 /TOP_B6))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 136 /TOP_B5))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 137 /TOP_B4))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 138 /TOP_B3))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 139 /TOP_B2))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 140 /TOP_B1))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer F.Cu) (tedit 5E45C4FB)
    (at 81.3 72)
    (fp_text reference J3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 -0.5) (layer F.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 1 /TOP_A70))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 2 /TOP_A69))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 3 /TOP_A68))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 4 /TOP_A67))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 5 /TOP_A66))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 6 /TOP_A65))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 7 /TOP_A64))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 8 /TOP_A63))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 9 /TOP_A62))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 10 /TOP_A61))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 11 /TOP_A60))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 12 /TOP_A59))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 13 /TOP_A58))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 14 /TOP_A57))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 15 /TOP_A56))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 16 /TOP_A55))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 17 /TOP_A54))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 18 /TOP_A53))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 19 /TOP_A52))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 20 /TOP_A51))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 21 /TOP_A50))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 22 /TOP_A49))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 23 /TOP_A48))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 24 /TOP_A47))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 25 /TOP_A46))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 26 /TOP_A45))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 27 /TOP_A44))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 28 /TOP_A43))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 29 /TOP_A42))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 30 /TOP_A41))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 31 /TOP_A40))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 32 /TOP_A39))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 33 /TOP_A38))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 34 /TOP_A37))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 35 /TOP_A36))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 36 /TOP_A35))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 37 /TOP_A34))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 38 /TOP_A33))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 39 /TOP_A32))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 40 /TOP_A31))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 41 /TOP_A30))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 42 /TOP_A29))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 43 /TOP_A28))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 44 /TOP_A27))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 45 /TOP_A26))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 46 /TOP_A25))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 47 /TOP_A24))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 48 /TOP_A23))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 49 /TOP_A22))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 50 /TOP_A21))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 51 /TOP_A20))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 52 /TOP_A19))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 53 /TOP_A18))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 54 /TOP_A17))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 55 /TOP_A16))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 56 /TOP_A15))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 57 /TOP_A14))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 58 /TOP_A13))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 59 /TOP_A12))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 60 /TOP_A11))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 61 /TOP_A10))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 62 /TOP_A9))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 63 /TOP_A8))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 64 /TOP_A7))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 65 /TOP_A6))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 66 /TOP_A5))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 67 /TOP_A4))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 68 /TOP_A3))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 69 /TOP_A2))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 70 /TOP_A1))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer F.Cu) (tedit 5E45C4FB)
    (at 102.2 72)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 -0.5) (layer F.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 71 /TOP_B70))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 72 /TOP_B69))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 73 /TOP_B68))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 74 /TOP_B67))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 75 /TOP_B66))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 76 /TOP_B65))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 77 /TOP_B64))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 78 /TOP_B63))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 79 /TOP_B62))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 80 /TOP_B61))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 81 /TOP_B60))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 82 /TOP_B59))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 83 /TOP_B58))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 84 /TOP_B57))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 85 /TOP_B56))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 86 /TOP_B55))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 87 /TOP_B54))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 88 /TOP_B53))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 89 /TOP_B52))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 90 /TOP_B51))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 91 /TOP_B50))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 92 /TOP_B49))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 93 /TOP_B48))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 94 /TOP_B47))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 95 /TOP_B46))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 96 /TOP_B45))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 97 /TOP_B44))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 98 /TOP_B43))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 99 /TOP_B42))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 100 /TOP_B41))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 101 /TOP_B40))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 102 /TOP_B39))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 103 /TOP_B38))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 104 /TOP_B37))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 105 /TOP_B36))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 106 /TOP_B35))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 107 /TOP_B34))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 108 /TOP_B33))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 109 /TOP_B32))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 110 /TOP_B31))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 111 /TOP_B30))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 112 /TOP_B29))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 113 /TOP_B28))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 114 /TOP_B27))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 115 /TOP_B26))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 116 /TOP_B25))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 117 /TOP_B24))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 118 /TOP_B23))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 119 /TOP_B22))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 120 /TOP_B21))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 121 /TOP_B20))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 122 /TOP_B19))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 123 /TOP_B18))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 124 /TOP_B17))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 125 /TOP_B16))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 126 /TOP_B15))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 127 /TOP_B14))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 128 /TOP_B13))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 129 /TOP_B12))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 130 /TOP_B11))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 131 /TOP_B10))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 132 /TOP_B9))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 133 /TOP_B8))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 134 /TOP_B7))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 135 /TOP_B6))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 136 /TOP_B5))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 137 /TOP_B4))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 138 /TOP_B3))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 139 /TOP_B2))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 140 /TOP_B1))
  )
  (module unl_silab:ETROC_70pad_100x150um_200um_pitch (layer F.Cu) (tedit 5E45C4FB)
    (at 81.3 92.9)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_02x35_Top_Bottom (at 0 -0.5) (layer F.Fab) hide)
    (pad 70 smd rect (at 13.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 1 /TOP_A70))
    (pad 69 smd rect (at 13.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 2 /TOP_A69))
    (pad 68 smd rect (at 13.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 3 /TOP_A68))
    (pad 67 smd rect (at 13.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 4 /TOP_A67))
    (pad 66 smd rect (at 13 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 5 /TOP_A66))
    (pad 65 smd rect (at 12.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 6 /TOP_A65))
    (pad 64 smd rect (at 12.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 7 /TOP_A64))
    (pad 63 smd rect (at 12.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 8 /TOP_A63))
    (pad 62 smd rect (at 12.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 9 /TOP_A62))
    (pad 61 smd rect (at 12 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 10 /TOP_A61))
    (pad 60 smd rect (at 11.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 11 /TOP_A60))
    (pad 59 smd rect (at 11.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 12 /TOP_A59))
    (pad 58 smd rect (at 11.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 13 /TOP_A58))
    (pad 57 smd rect (at 11.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 14 /TOP_A57))
    (pad 56 smd rect (at 11 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 15 /TOP_A56))
    (pad 55 smd rect (at 10.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 16 /TOP_A55))
    (pad 54 smd rect (at 10.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 17 /TOP_A54))
    (pad 53 smd rect (at 10.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 18 /TOP_A53))
    (pad 52 smd rect (at 10.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 19 /TOP_A52))
    (pad 51 smd rect (at 10 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 20 /TOP_A51))
    (pad 50 smd rect (at 9.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 21 /TOP_A50))
    (pad 49 smd rect (at 9.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 22 /TOP_A49))
    (pad 48 smd rect (at 9.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 23 /TOP_A48))
    (pad 47 smd rect (at 9.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 24 /TOP_A47))
    (pad 46 smd rect (at 9 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 25 /TOP_A46))
    (pad 45 smd rect (at 8.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 26 /TOP_A45))
    (pad 44 smd rect (at 8.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 27 /TOP_A44))
    (pad 43 smd rect (at 8.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 28 /TOP_A43))
    (pad 42 smd rect (at 8.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 29 /TOP_A42))
    (pad 41 smd rect (at 8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 30 /TOP_A41))
    (pad 40 smd rect (at 7.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 31 /TOP_A40))
    (pad 39 smd rect (at 7.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 32 /TOP_A39))
    (pad 38 smd rect (at 7.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 33 /TOP_A38))
    (pad 37 smd rect (at 7.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 34 /TOP_A37))
    (pad 36 smd rect (at 7 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 35 /TOP_A36))
    (pad 35 smd rect (at 6.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 36 /TOP_A35))
    (pad 34 smd rect (at 6.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 37 /TOP_A34))
    (pad 33 smd rect (at 6.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 38 /TOP_A33))
    (pad 32 smd rect (at 6.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 39 /TOP_A32))
    (pad 31 smd rect (at 6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 40 /TOP_A31))
    (pad 30 smd rect (at 5.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 41 /TOP_A30))
    (pad 29 smd rect (at 5.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 42 /TOP_A29))
    (pad 28 smd rect (at 5.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 43 /TOP_A28))
    (pad 27 smd rect (at 5.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 44 /TOP_A27))
    (pad 26 smd rect (at 5 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 45 /TOP_A26))
    (pad 25 smd rect (at 4.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 46 /TOP_A25))
    (pad 24 smd rect (at 4.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 47 /TOP_A24))
    (pad 23 smd rect (at 4.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 48 /TOP_A23))
    (pad 22 smd rect (at 4.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 49 /TOP_A22))
    (pad 21 smd rect (at 4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 50 /TOP_A21))
    (pad 20 smd rect (at 3.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 51 /TOP_A20))
    (pad 19 smd rect (at 3.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 52 /TOP_A19))
    (pad 18 smd rect (at 3.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 53 /TOP_A18))
    (pad 17 smd rect (at 3.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 54 /TOP_A17))
    (pad 16 smd rect (at 3 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 55 /TOP_A16))
    (pad 15 smd rect (at 2.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 56 /TOP_A15))
    (pad 14 smd rect (at 2.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 57 /TOP_A14))
    (pad 13 smd rect (at 2.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 58 /TOP_A13))
    (pad 12 smd rect (at 2.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 59 /TOP_A12))
    (pad 11 smd rect (at 2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 60 /TOP_A11))
    (pad 10 smd rect (at 1.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 61 /TOP_A10))
    (pad 9 smd rect (at 1.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 62 /TOP_A9))
    (pad 8 smd rect (at 1.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 63 /TOP_A8))
    (pad 7 smd rect (at 1.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 64 /TOP_A7))
    (pad 6 smd rect (at 1 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 65 /TOP_A6))
    (pad 5 smd rect (at 0.8 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 66 /TOP_A5))
    (pad 4 smd rect (at 0.6 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 67 /TOP_A4))
    (pad 3 smd rect (at 0.4 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 68 /TOP_A3))
    (pad 2 smd rect (at 0.2 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 69 /TOP_A2))
    (pad 1 smd rect (at 0 0) (size 0.1 0.15) (layers F.Cu F.Mask)
      (net 70 /TOP_A1))
  )
  (module unl_silab:crossed_circle_fiducial (layer B.Cu) (tedit 5DEEB95A)
    (at 119 93.1)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer B.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer B.Cu) (tedit 5DEEB95A)
    (at 118.9 72.6)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer B.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer B.Cu) (tedit 5DEEB95A)
    (at 78.4 72.6)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer B.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer B.Cu) (tedit 5DEEB95A)
    (at 78.3 93.1)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer B.Fab) hide)
  )
  (module unl_silab:NLOGO (layer F.Cu) (tedit 5D65A532)
    (at 99.2 91.3 180)
    (fp_text reference G*** (at 7.112 1.016) (layer F.SilkS) hide)
    (fp_text value LOGO (at 8.128 -2.032) (layer F.SilkS) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 78.3 93.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 119 93.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 118.9 72.6)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (module unl_silab:crossed_circle_fiducial (layer F.Cu) (tedit 5DEEB95A)
    (at 78.4 72.6)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value crossed_circle_fiducial (at 0 0) (layer F.Fab) hide)
  )
  (dimension 22.3 (width 0.15) (layer Dwgs.User)
    (gr_text "22.300 mm" (at 122.2 82.45 90) (layer Dwgs.User))
    (feature1 (pts (xy 119.5 71.3) (xy 121.486421 71.3)))
    (feature2 (pts (xy 119.5 93.6) (xy 121.486421 93.6)))
    (crossbar (pts (xy 120.9 93.6) (xy 120.9 71.3)))
    (arrow1a (pts (xy 120.9 71.3) (xy 121.486421 72.426504)))
    (arrow1b (pts (xy 120.9 71.3) (xy 120.313579 72.426504)))
    (arrow2a (pts (xy 120.9 93.6) (xy 121.486421 92.473496)))
    (arrow2b (pts (xy 120.9 93.6) (xy 120.313579 92.473496)))
  )
  (dimension 41.700005 (width 0.15) (layer Dwgs.User)
    (gr_text "41.700 mm" (at 98.648843 96.001894 -0.02747998807) (layer Dwgs.User))
    (feature1 (pts (xy 77.8 93.58) (xy 77.799185 95.278315)))
    (feature2 (pts (xy 119.5 93.6) (xy 119.499185 95.298315)))
    (crossbar (pts (xy 119.499467 94.711894) (xy 77.799467 94.691894)))
    (arrow1a (pts (xy 77.799467 94.691894) (xy 78.926252 94.106014)))
    (arrow1b (pts (xy 77.799467 94.691894) (xy 78.925689 95.278855)))
    (arrow2a (pts (xy 119.499467 94.711894) (xy 118.373245 94.124933)))
    (arrow2b (pts (xy 119.499467 94.711894) (xy 118.372682 95.297774)))
  )
  (gr_text "ETROC Mech Mockup\nPad Size: 100x150 um\nPitch: 200 um\n" (at 98.6 88.9 90) (layer F.SilkS))
  (gr_line (start 119.5 93.6) (end 119.5 71.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.8 93.58) (end 119.5 93.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.8 71.3) (end 77.8 93.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.8 71.3) (end 119.5 71.3) (layer Edge.Cuts) (width 0.05))
  (zone (net 142) (net_name /BOT_GRP2) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.4 91) (xy 78.5 91) (xy 78.5 83.2) (xy 80.4 83.2)
      )
    )
  )
  (zone (net 143) (net_name /BOT_GRP3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.9 91) (xy 118.8 91) (xy 118.8 83.2) (xy 116.9 83.2)
      )
    )
  )
  (zone (net 141) (net_name /BOT_GRP1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.4 73.9) (xy 78.5 73.9) (xy 78.5 81.7) (xy 80.4 81.7)
      )
    )
  )
  (zone (net 144) (net_name /BOT_GRP4) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.9 73.897922) (xy 118.8 73.897922) (xy 118.8 81.697922) (xy 116.9 81.697922)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.4 91) (xy 78.5 91) (xy 78.5 83.2) (xy 80.4 83.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.8 91) (xy 116.9 91) (xy 116.9 83.2) (xy 118.8 83.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.4 81.7) (xy 78.5 81.7) (xy 78.5 73.9) (xy 80.4 73.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.8 81.7) (xy 116.9 81.7) (xy 116.9 73.9) (xy 118.8 73.9)
      )
    )
  )
)
