(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "/SCL")
  (net 4 "/SDA")
  (net 5 "/RST")
  (net 6 "/PB2")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 148.3 84.7)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "OLEDinitLoading.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "I2CIN" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/SDA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 139.9 84.7)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "OLEDinitLoading.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "I2CIN" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/SDA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCadCustomLibs:PAD_2x3" (layer "B.Cu")
    (tedit 5F784E42)
    (at 145.6 91.8 180)
    (property "Sheetfile" "OLEDinitLoading.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -1.6) (layer "B.SilkS") hide)
    (fp_text value "RST" (at -0.1 1.6) (layer "B.Fab") hide)
    (pad "1" smd rect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 5 "/RST") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "B.Cu")
    (tedit 5F6F9B37)
    (at 144.1 86.2)
    (descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "OLEDinitLoading.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 2.4) (layer "B.SilkS") hide)
    (fp_text value "ATtiny10-TS" (at 0 -2.4) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/PB2") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at 1.1375 0) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/RST") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCadCustomLibs:PAD_2x3" (layer "B.Cu")
    (tedit 5F784E42)
    (at 142.6 91.8 180)
    (property "Sheetfile" "OLEDinitLoading.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -1.6) (layer "B.SilkS") hide)
    (fp_text value "PB2" (at -0.1 1.6) (layer "B.Fab") hide)
    (pad "1" smd rect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 6 "/PB2") (pinfunction "Pin_1") (pintype "passive"))
  )
  (gr_rect (start 138.5 83.3) (end 149.7 93.7) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "PB2" (at 142.6 90) (layer "B.SilkS"))
  (gr_text "RST" (at 145.6 90) (layer "B.SilkS"))
  (gr_text "VCC" (at 144 87.2) (layer "F.SilkS"))
  (gr_text "SCL" (at 144 89.7) (layer "F.SilkS"))
  (gr_text "SDA" (at 144 92.3) (layer "F.SilkS"))
  (gr_text "GND" (at 144 84.7) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149.7 93.7) (xy 149.7 83.3))
    (height 5)
    (gr_text "10,4000 mm" (at 153.55 88.5 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149.7 83.3) (xy 138.5 83.3))
    (height 3.199999)
    (gr_text "11,2000 mm" (at 144.1 78.950001) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
)
