(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 118)
    (zones 0)
    (modules 19)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.254)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C3-Pad2)")
  (net 3 "Net-(C4-Pad2)")
  (net 4 /V3_3)
  (net 5 "Net-(J1-Pad4)")
  (net 6 /V12)
  (net 7 "Net-(J1-Pad1)")
  (net 8 "Net-(U2-Pad9)")
  (net 9 "Net-(U2-Pad7)")
  (net 10 "Net-(U2-Pad5)")
  (net 11 "Net-(U2-Pad4)")
  (net 12 "Net-(U2-Pad3)")
  (net 13 "Net-(U2-Pad1)")
  (net 14 "Net-(U3-Pad8)")
  (net 15 "Net-(U3-Pad9)")
  (net 16 "Net-(U3-Pad7)")
  (net 17 /V5)
  (net 18 "Net-(C3-Pad1)")
  (net 19 "Net-(C4-Pad1)")
  (net 20 "Net-(C5-Pad2)")
  (net 21 "Net-(C6-Pad2)")
  (net 22 "Net-(LS1-Pad2)")
  (net 23 "Net-(R1-Pad1)")
  (net 24 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /V12)
    (add_net /V3_3)
    (add_net /V5)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(LS1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
  )
  (module LK201:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ECAB9C4)
    (at 47.625 -31.115 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 2.54 1.905) (layer F.SilkS))
    (fp_text value 3.3k (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /V12))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(LS1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ECAB9C4)
    (at 18.415 -19.05 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 2.54 90) (layer F.SilkS))
    (fp_text value 1k (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5EC9668E)
    (at 36.195 -27.94 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at -1.905 -1.905 90) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /V3_3))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 "Net-(LS1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.step
      (offset (xyz 0 0 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 39.37 -27.305)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /V5))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 45.085 -21.59)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /V12))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5EC9668E)
    (at 45.72 -27.94 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value L78L05 (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /V12))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 /V5))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.step
      (offset (xyz 0 0 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:AK_Design_9mm (layer F.Cu) (tedit 5EC6EF5E)
    (at 33.655 -33.655)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value AK_Design_9mm (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 2.54 -2.54)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 2.54 -35.56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 48.26 -35.56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module LK201:DIP-16_296_ELL (layer F.Cu) (tedit 5EC68F95)
    (at 29.26 -11.43 270)
    (fp_text reference U3 (at -3.175 0.05) (layer F.SilkS))
    (fp_text value ICL3232CPZ (at 0 0 270) (layer F.Fab))
    (pad 8 thru_hole oval (at 8.89 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U3-Pad8)"))
    (pad 9 thru_hole oval (at 8.89 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U3-Pad9)"))
    (pad 7 thru_hole oval (at 6.35 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U3-Pad7)"))
    (pad 10 thru_hole oval (at 6.35 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.81 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (pad 11 thru_hole oval (at 3.81 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad3)"))
    (pad 5 thru_hole oval (at 1.27 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 12 thru_hole oval (at 1.27 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad4)"))
    (pad 4 thru_hole oval (at -1.27 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 13 thru_hole oval (at -1.27 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at -3.81 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C3-Pad2)"))
    (pad 14 thru_hole oval (at -3.81 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at -6.35 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C6-Pad2)"))
    (pad 15 thru_hole oval (at -6.35 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at -8.89 3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
    (pad 16 thru_hole oval (at -8.89 -3.76 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /V3_3))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.step
      (offset (xyz 8.890000000000001 3.81 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LK201:Trinket_M0 (layer F.Cu) (tedit 5EC69031)
    (at 8.89 -19.05 180)
    (fp_text reference U2 (at 0 6.985 180) (layer F.SilkS))
    (fp_text value "Trinket M0" (at 0 -0.5 180) (layer F.Fab))
    (fp_text user USB (at -3.175 3.81 180) (layer F.SilkS))
    (fp_text user 0 (at -4.445 1.27 180) (layer F.SilkS))
    (fp_text user 1 (at -4.445 -1.27 180) (layer F.SilkS))
    (fp_text user 2 (at -4.445 -3.81 180) (layer F.SilkS))
    (fp_text user 3V (at -3.81 -6.35 180) (layer F.SilkS))
    (fp_text user Rst (at 3.81 -6.35 180) (layer F.SilkS))
    (fp_text user 3 (at 4.445 -3.81 180) (layer F.SilkS))
    (fp_text user 4 (at 4.445 -1.27 180) (layer F.SilkS))
    (fp_text user Gnd (at 3.81 1.27 180) (layer F.SilkS))
    (fp_text user Bat (at 3.81 3.81 180) (layer F.SilkS))
    (pad 10 thru_hole circle (at -6.35 3.81 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 17 /V5))
    (pad 9 thru_hole circle (at -6.35 1.27 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at -6.35 -1.27 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(R1-Pad1)"))
    (pad 7 thru_hole circle (at -6.35 -3.81 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at -6.35 -6.35 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 4 /V3_3))
    (pad 5 thru_hole circle (at 6.35 -6.35 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 4 thru_hole circle (at 6.35 -3.81 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad4)"))
    (pad 3 thru_hole circle (at 6.35 -1.27 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at 6.35 1.27 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.35 3.81 180) (size 1.93 1.93) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad1)"))
    (pad "" np_thru_hole circle (at -5.715 -10.16 180) (size 2.2 2.2) (drill 2.2) (layers *.Mask F.Cu))
    (pad "" np_thru_hole circle (at 5.715 -10.16 180) (size 2.2 2.2) (drill 2.2) (layers *.Mask F.Cu))
    (pad "" np_thru_hole circle (at 6.096 6.223 180) (size 2.2 2.2) (drill 2.2) (layers *.Mask F.Cu))
    (pad "" np_thru_hole circle (at -6.096 6.223 180) (size 2.2 2.2) (drill 2.2) (layers *.Mask F.Cu))
    (model /Users/pkoning/Documents/kicad/Trinket/Trinket.step
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LK201:PS1420_buzzer (layer F.Cu) (tedit 5EC6900F)
    (at 26.035 -30.48 180)
    (fp_text reference LS1 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value PS1420 (at 0 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.5 0 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(LS1-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 6 /V12))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_15x7.5RM7.6.step
      (offset (xyz -3.6 0 0))
      (scale (xyz 0.93 0.93 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:RJ22 (layer F.Cu) (tedit 5EC6901D)
    (at 42.545 -8.89)
    (fp_text reference J1 (at 0 2.54) (layer F.SilkS))
    (fp_text value RJ22 (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at -3.81 0) (size 3.2 3.2) (drill 3.2) (layers *.Mask F.Cu))
    (pad "" np_thru_hole circle (at 3.81 0) (size 3.2 3.2) (drill 3.2) (layers *.Mask F.Cu))
    (pad 4 thru_hole circle (at 1.905 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 0.635 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -0.635 -8.89) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /V12))
    (pad 1 thru_hole rect (at -1.905 -6.35) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad1)"))
    (model /Users/pkoning/Downloads/101744862-3-modular_jack_a-20040/modular_jack_a-20040.step
      (offset (xyz 0 -10.5 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 180))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 40.64 -24.13 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 1.25 -2.56 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /V3_3))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 21.59 -5.08 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 36.83 -21.59 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 1.25 -2.56 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 21.59 -13.97 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 1.27 2.54 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5EC69084)
    (at 21.59 -20.32 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 3.135 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.016 1 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "AK-003 A" (at 12.7 -2.54) (layer B.Cu))
  (gr_text "AK-003 A" (at 6.35 -2.54) (layer F.Cu))
  (gr_text "LK201 emulator by\nPaul Koning\nMay 2020" (at 5.715 -34.925) (layer F.SilkS))
  (gr_line (start 50.8 0) (end 0 0) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 50.8 -38.1) (end 50.8 0) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 0 -38.1) (end 50.8 -38.1) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 0 0) (end 0 -38.1) (layer Edge.Cuts) (width 0.12))
)
