(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 231)
    (zones 0)
    (modules 20)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.1016)
    (pad_size 1.98 1.98)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(ANT1-Pad1)")
  (net 2 GND)
  (net 3 V_BAT)
  (net 4 VDD)
  (net 5 DIO5)
  (net 6 LORA_CS)
  (net 7 DIO3)
  (net 8 SCK_R)
  (net 9 DIO4)
  (net 10 MOSI_R)
  (net 11 DIO0)
  (net 12 MISO_R)
  (net 13 DIO1)
  (net 14 DIO2)
  (net 15 BME_CS)
  (net 16 RESET)
  (net 17 UPDI)
  (net 18 "Net-(Q1-Pad3)")
  (net 19 BAT_EN)
  (net 20 BAT_IN)
  (net 21 SCK)
  (net 22 MOSI)
  (net 23 MISO)
  (net 24 CLK32K)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net BAT_EN)
    (add_net BAT_IN)
    (add_net BME_CS)
    (add_net CLK32K)
    (add_net DIO0)
    (add_net DIO1)
    (add_net DIO2)
    (add_net DIO3)
    (add_net DIO4)
    (add_net DIO5)
    (add_net GND)
    (add_net LORA_CS)
    (add_net MISO)
    (add_net MISO_R)
    (add_net MOSI)
    (add_net MOSI_R)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net RESET)
    (add_net SCK)
    (add_net SCK_R)
    (add_net UPDI)
    (add_net VDD)
    (add_net V_BAT)
  )
  (module lora_node:BatteryHolder_Keystone_1079_2xCR123A (layer B.Cu) (tedit 5E1A8F65)
    (at 3 30.8)
    (descr "BATT HOLDER CR123A 2 CELL PC PIN")
    (tags "CR123A battery cell holder")
    (zone_connect 1)
    (fp_text reference BT1 (at 20.4 -0.8 180) (layer B.SilkS))
    (fp_text value Battery_Cellx2 (at 18.796 -25.908 180) (layer B.Fab))
    (fp_text user + (at 29.843 -16.13 180) (layer B.SilkS))
    (fp_text user - (at 8.253 -16.13 180) (layer B.SilkS))
    (fp_text user + (at 8.253 -2.54 180) (layer B.SilkS))
    (fp_text user - (at 29.843 -2.54 180) (layer B.SilkS))
    (fp_text user %R (at 25.4 -12.192 180) (layer B.Fab))
    (pad B1- thru_hole circle (at 37.82 0) (size 2 2) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 1) (thermal_width 0.5) (thermal_gap 0.25))
    (pad B2+ thru_hole circle (at 37.82 -18.29) (size 2 2) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 V_BAT) (zone_connect 1))
    (pad B2- thru_hole circle (at 0 -18.29) (size 2 2) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 1) (thermal_width 0.5) (thermal_gap 0.25))
    (pad B1+ thru_hole circle (at 0 0) (size 2 2) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 V_BAT) (zone_connect 1))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_MPD_BC2AAPC_2xAA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 3.4 27.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.35 1.2) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 V_BAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 3.4 23 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.35 1.25) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 3.2 25.4 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at 1.45 1.18 90) (layer F.SilkS))
    (fp_text value MCP1811AT-028_TT (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 V_BAT))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lora_node:DSC6083MI2A (layer F.Cu) (tedit 5CF5BC41)
    (at 12.6 30 90)
    (attr smd)
    (fp_text reference U5 (at 2 -0.85 180) (layer F.SilkS))
    (fp_text value DSC6083 (at 0 2.794 90) (layer F.Fab))
    (pad 4 smd rect (at -0.775 -0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 3 smd rect (at 0.775 -0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.775 0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.775 0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 CLK32K))
  )
  (module lora_node:BME280 (layer F.Cu) (tedit 5B2F0E9C)
    (at 28.25 34.45 180)
    (fp_text reference U3 (at 3.25 -1.15) (layer F.SilkS))
    (fp_text value BME280 (at 0 3) (layer F.Fab))
    (pad 8 smd rect (at -1.025 -0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 7 smd rect (at -1.025 -0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.025 0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 5 smd rect (at -1.025 0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 MISO_R))
    (pad 4 smd rect (at 1.025 0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK_R))
    (pad 3 smd rect (at 1.025 0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 MOSI_R))
    (pad 2 smd rect (at 1.025 -0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 15 BME_CS))
    (pad 1 smd rect (at 1.025 -0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module lora_node:RFM95W (layer F.Cu) (tedit 58C0EDBF)
    (at 29.13 14 270)
    (fp_text reference U2 (at -7.47 -10.62) (layer F.SilkS))
    (fp_text value RFM95W-915S2 (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 7 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 7 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad1)"))
    (pad 7 smd rect (at 5 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 5 DIO5))
    (pad 10 smd rect (at 5 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 16 RESET))
    (pad 11 smd rect (at 3 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 DIO3))
    (pad 5 smd rect (at 1 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 LORA_CS))
    (pad 12 smd rect (at 1 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 9 DIO4))
    (pad 4 smd rect (at -1 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK_R))
    (pad 13 smd rect (at -1 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 3 smd rect (at -3 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 10 MOSI_R))
    (pad 14 smd rect (at -3 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 11 DIO0))
    (pad 2 smd rect (at -5 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 12 MISO_R))
    (pad 15 smd rect (at -5 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 13 DIO1))
    (pad 1 smd rect (at -7 8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -7 -8 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 14 DIO2))
  )
  (module lora_node:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5CF5BD77)
    (at 18 28.25)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 1.5 -5.25 180) (layer F.SilkS))
    (fp_text value ATtiny814 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 LORA_CS))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 RESET))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 DIO0))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 DIO5))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 CLK32K))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 BAT_EN))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 BME_CS))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 BAT_IN))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 UPDI))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 MOSI))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 MISO))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 SCK))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 23.5 27 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -4.5 0) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 MISO))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 MISO_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 23.5 28.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -4.5 0) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 MOSI))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 MOSI_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 23.5 25.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -4.5 0) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 SCK))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 SCK_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 20.25 34.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1 -1.25 90) (layer F.SilkS))
    (fp_text value 90.9k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 BAT_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 18.75 34.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.9 -1.15 90) (layer F.SilkS))
    (fp_text value 39.2k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 BAT_IN))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 15.4 34.8)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.8 1.2) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 V_BAT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 BAT_EN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x12_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41B)
    (at 7 35.25 180)
    (descr "Through hole straight socket strip, 2x12, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x12 2.54mm double row")
    (fp_text reference J1 (at 2.25 -0.25 90) (layer F.SilkS))
    (fp_text value Conn_02x12_Odd_Even (at -1.27 30.71) (layer F.Fab))
    (fp_text user %R (at -1.27 13.97 90) (layer F.Fab))
    (pad 24 thru_hole oval (at -2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 MISO_R))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 DIO2))
    (pad 22 thru_hole oval (at -2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 MOSI_R))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 DIO1))
    (pad 20 thru_hole oval (at -2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCK_R))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 DIO0))
    (pad 18 thru_hole oval (at -2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 DIO4))
    (pad 16 thru_hole oval (at -2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 RESET))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 DIO3))
    (pad 14 thru_hole oval (at -2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 LORA_CS))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 DIO5))
    (pad 12 thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 BME_CS))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 V_BAT))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 UPDI))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VDD))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 39.6 15 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.25 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 12.2 33 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.3 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 31 34.45 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 15.2 22.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -0.05 -1.45 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lora_node:0915AT43A0026 (layer F.Cu) (tedit 5CF5BB60)
    (at 47.5 21)
    (attr smd)
    (fp_text reference ANT1 (at 0 -2) (layer F.SilkS))
    (fp_text value 0915AT43A0026 (at 0 7.25) (layer F.Fab))
    (pad "" smd rect (at -2.85 4.5) (size 0.5 2) (layers F.Cu F.Mask))
    (pad "" smd rect (at 0.45 5.75 90) (size 0.5 7.1) (layers F.Cu F.Mask))
    (pad "" smd rect (at 3.75 3.2) (size 0.5 4.6) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 3.5 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3.5 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad1)"))
  )
  (gr_text "LoRaAtmo v0.52" (at 41.75 36) (layer F.SilkS))
  (gr_line (start 0.5 37.2) (end 0.5 4.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52 37.2) (end 0.5 37.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52 4.75) (end 52 37.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.5 4.75) (end 52 4.75) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.24)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 42.5 4.75) (xy 42.5 37.2) (xy 0.5 37.2) (xy 0.5 4.75)
      )
    )
  )
  (zone (net 4) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 42.5 4.75) (xy 42.5 37.2) (xy 0.5 37.2) (xy 0.5 4.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 35.6 12) (xy 38.2 12) (xy 39.4 13.2) (xy 39.4 16.2) (xy 35.6 16.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 11.51 28.71) (xy 13.69 28.71) (xy 13.69 31.8) (xy 11.51 31.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 26.75346 32.95) (xy 31.35346 32.95) (xy 31.35346 35.95) (xy 26.75346 35.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 21.6 23.8) (xy 21.6 32.6) (xy 14.4 32.6) (xy 14.4 23.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 4.755 23.84) (xy 4.755 27) (xy 2.4 27) (xy 2.4 23.84)
      )
    )
  )
)
