(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 1019)
    (zones 0)
    (modules 43)
    (nets 109)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /D4)
  (net 3 /D6)
  (net 4 /D8)
  (net 5 /D13)
  (net 6 /D12)
  (net 7 /D10)
  (net 8 /D9)
  (net 9 /D7)
  (net 10 /A0)
  (net 11 /A3)
  (net 12 /A5)
  (net 13 /SCK)
  (net 14 /MOSI)
  (net 15 /MISO)
  (net 16 /D5)
  (net 17 /RXLED)
  (net 18 /TXLED)
  (net 19 /~RESET)
  (net 20 /D+)
  (net 21 /D-)
  (net 22 "Net-(F1-Pad2)")
  (net 23 +5V)
  (net 24 "Net-(D22-Pad1)")
  (net 25 "Net-(D23-Pad1)")
  (net 26 "Net-(J1-Pad2)")
  (net 27 "Net-(J1-Pad3)")
  (net 28 "Net-(D21-Pad1)")
  (net 29 "Net-(R26-Pad2)")
  (net 30 "Net-(R26-Pad1)")
  (net 31 /D3_SCL)
  (net 32 /D2_SDA)
  (net 33 /D0)
  (net 34 /D1)
  (net 35 /D11)
  (net 36 /A1)
  (net 37 /A2)
  (net 38 /A4)
  (net 39 "Net-(J1-Pad4)")
  (net 40 "Net-(LED1-Pad4)")
  (net 41 "Net-(P1-Pad1)")
  (net 42 "Net-(P2-Pad1)")
  (net 43 "Net-(P3-Pad1)")
  (net 44 "Net-(P4-Pad1)")
  (net 45 "Net-(P5-Pad1)")
  (net 46 "Net-(P6-Pad1)")
  (net 47 "Net-(U1-Pad2)")
  (net 48 /AREF)
  (net 49 "Net-(U3-Pad8)")
  (net 50 "Net-(U3-Pad6)")
  (net 51 "Net-(U3-Pad5)")
  (net 52 "Net-(U3-Pad4)")
  (net 53 "Net-(U2-Pad4)")
  (net 54 "Net-(U2-Pad5)")
  (net 55 "Net-(U2-Pad6)")
  (net 56 "Net-(U2-Pad8)")
  (net 57 /01)
  (net 58 /02)
  (net 59 /03)
  (net 60 /04)
  (net 61 /05)
  (net 62 /06)
  (net 63 /07)
  (net 64 /08)
  (net 65 /09)
  (net 66 /10)
  (net 67 /11)
  (net 68 /12)
  (net 69 /13)
  (net 70 /14)
  (net 71 /15)
  (net 72 /16)
  (net 73 /24)
  (net 74 /23)
  (net 75 /22)
  (net 76 /21)
  (net 77 /20)
  (net 78 /19)
  (net 79 /18)
  (net 80 /17)
  (net 81 "Net-(U4-Pad8)")
  (net 82 "Net-(U4-Pad6)")
  (net 83 "Net-(U4-Pad5)")
  (net 84 "Net-(U4-Pad4)")
  (net 85 "Net-(U5-Pad4)")
  (net 86 "Net-(U5-Pad5)")
  (net 87 "Net-(U5-Pad6)")
  (net 88 "Net-(U5-Pad8)")
  (net 89 /25)
  (net 90 /26)
  (net 91 /27)
  (net 92 /28)
  (net 93 /29)
  (net 94 /30)
  (net 95 /31)
  (net 96 /32)
  (net 97 /40)
  (net 98 /39)
  (net 99 /38)
  (net 100 /37)
  (net 101 /36)
  (net 102 /35)
  (net 103 /34)
  (net 104 /33)
  (net 105 "Net-(U6-Pad8)")
  (net 106 "Net-(U6-Pad6)")
  (net 107 "Net-(U6-Pad5)")
  (net 108 "Net-(U6-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.25)
    (add_net +5V)
    (add_net /01)
    (add_net /02)
    (add_net /03)
    (add_net /04)
    (add_net /05)
    (add_net /06)
    (add_net /07)
    (add_net /08)
    (add_net /09)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /14)
    (add_net /15)
    (add_net /16)
    (add_net /17)
    (add_net /18)
    (add_net /19)
    (add_net /20)
    (add_net /21)
    (add_net /22)
    (add_net /23)
    (add_net /24)
    (add_net /25)
    (add_net /26)
    (add_net /27)
    (add_net /28)
    (add_net /29)
    (add_net /30)
    (add_net /31)
    (add_net /32)
    (add_net /33)
    (add_net /34)
    (add_net /35)
    (add_net /36)
    (add_net /37)
    (add_net /38)
    (add_net /39)
    (add_net /40)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /D+)
    (add_net /D-)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2_SDA)
    (add_net /D3_SCL)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RXLED)
    (add_net /SCK)
    (add_net /TXLED)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad1)")
    (add_net "Net-(D23-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(LED1-Pad4)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U6-Pad8)")
  )
  (module footprints:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 63CC6AF2)
    (at 150.622 124.206)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.Fab))
    (fp_text value I2C (at -0.022 9.294) (layer F.SilkS))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D3_SCL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D2_SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MEC8-113-CARD_2outline locked (layer F.Cu) (tedit 637EA855)
    (at 116.5 97.75 90)
    (fp_text reference CardOutline2 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value SYM_Arrow_Large (at 10.9 -1 90) (layer F.Fab))
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 141.65 78.35 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 4K7 (at -2.5 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /D3_SCL))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm (layer F.Cu) (tedit 63CC3BF1)
    (at 132 113 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U5 (at 0 -3.3 180) (layer F.SilkS))
    (fp_text value MCP23008-xML (at 0 3.3 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 3 smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 4 smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(U5-Pad4)"))
    (pad 5 smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(U5-Pad5)"))
    (pad 6 smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(U5-Pad6)"))
    (pad 7 smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /D9))
    (pad 8 smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(U5-Pad8)"))
    (pad 9 smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /32))
    (pad 10 smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /31))
    (pad 11 smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /30))
    (pad 12 smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /29))
    (pad 13 smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /28))
    (pad 14 smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /27))
    (pad 15 smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /26))
    (pad 16 smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /25))
    (pad 17 smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 18 smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 19 smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /D3_SCL))
    (pad 20 smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /D2_SDA))
    (pad 17 smd rect (at 0 0 180) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SAMTEC_MEC8-113-TOP-BOTTOM (layer F.Cu) (tedit 63786631)
    (at 119 87.75 90)
    (fp_text reference X1 (at -0.5 -5.75 90) (layer F.SilkS))
    (fp_text value MEC8-113 (at 8.21 6.135 90) (layer F.Fab))
    (pad 1 smd rect (at -6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 57 /01))
    (pad 14 smd rect (at -6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 67 /11))
    (pad 2 smd rect (at -5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 58 /02))
    (pad 15 smd rect (at -5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 68 /12))
    (pad 3 smd rect (at -4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 59 /03))
    (pad 16 smd rect (at -4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 69 /13))
    (pad 4 smd rect (at -4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 60 /04))
    (pad 17 smd rect (at -4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 70 /14))
    (pad 5 smd rect (at -3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 61 /05))
    (pad 18 smd rect (at -3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 71 /15))
    (pad 6 smd rect (at -2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 62 /06))
    (pad 19 smd rect (at -2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 72 /16))
    (pad 7 smd rect (at 1.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 63 /07))
    (pad 20 smd rect (at 1.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 80 /17))
    (pad 8 smd rect (at 2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 64 /08))
    (pad 21 smd rect (at 2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 79 /18))
    (pad 9 smd rect (at 3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 65 /09))
    (pad 22 smd rect (at 3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 78 /19))
    (pad 10 smd rect (at 4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 66 /10))
    (pad 23 smd rect (at 4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 77 /20))
    (pad None np_thru_hole circle (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad 11 smd rect (at 4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /A0))
    (pad 24 smd rect (at 4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /D3_SCL))
    (pad 12 smd rect (at 5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 25 smd rect (at 5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 /D2_SDA))
    (pad 13 smd rect (at 6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 26 smd rect (at 6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 110 91 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -2.54 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -2.5 0 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D21-Pad1)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 141.65 79.85 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 4K7 (at -2.5 1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /D2_SDA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 637975D3)
    (at 157.9 80.3)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.31 -2.395) (layer F.SilkS))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 19 /~RESET))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 14 /MOSI))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 13 /SCK))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 23 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 0.508) (layers *.Cu F.Mask)
      (net 15 /MISO))
  )
  (module footprints:INPI33TBTPRPGPB (layer F.Cu) (tedit 0)
    (at 110 108 180)
    (descr IN-PI33TBTPRPGPB-5)
    (tags LED)
    (attr smd)
    (fp_text reference LED1 (at 0.53 0) (layer F.SilkS) hide)
    (fp_text value IN-PI33TBTPRPGPB (at 0.53 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0.53 0) (layer F.Fab))
    (pad 1 smd rect (at 1.59 1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.59 -1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /A2))
    (pad 3 smd rect (at -1.59 -1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 4 smd rect (at -1.59 1.07 270) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(LED1-Pad4)"))
    (model IN-PI33TBTPRPGPB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/IN-PI33TBTPRPGPB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 636FC06B)
    (at 110.5 94 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference F1 (at -3.17 0) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 110 89 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D22 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value TX (at 2 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D22-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SW_TS10-63-26-BE-250-SMT-TR (layer F.Cu) (tedit 63700F95)
    (at 169.4 100.3 90)
    (fp_text reference SW3 (at 0 -0.09 90) (layer F.SilkS))
    (fp_text value RESET (at -5.67 0) (layer F.SilkS))
    (pad 1 smd rect (at -3.25 0 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.25 0 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /~RESET))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 141.65 83 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 2.54 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -2.1 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D22-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /TXLED))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M25standoff (layer F.Cu) (tedit 636FF644)
    (at 168 87.75)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P5 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Standoff (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask)
      (net 45 "Net-(P5-Pad1)"))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/99607A263_Stainless Steel Flared-Collar Knurled-Head Thumb Screw.STEP"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M25standoff (layer F.Cu) (tedit 636FF644)
    (at 168 110)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P6 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value Standoff (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask)
      (net 46 "Net-(P6-Pad1)"))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/M2_5X6MM.step
      (offset (xyz 0 0 6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 110.49 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 41 "Net-(P1-Pad1)"))
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 110 85 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D21 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 1.25 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D21-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636FBDBF)
    (at 110 87 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D23 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value RX (at 2 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D23-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 141.65 81.4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at -0.127 1.27 180) (layer Dwgs.User))
    (fp_text value 1K (at -2.032 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D23-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /RXLED))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 120 100 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 1.905 0 180) (layer Dwgs.User) hide)
    (fp_text value 22 (at -2 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /D+))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 120 98 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 22 (at -2 -0.055 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /D-))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 147.7 79.91 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 3.175 0 180) (layer Dwgs.User))
    (fp_text value 1M (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R26-Pad1)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 116.25 100 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV1 (at 2 -0.75 180) (layer F.SilkS))
    (fp_text value Varistor (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636FC042)
    (at 116.25 98 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV2 (at 2.25 0.75 180) (layer F.SilkS))
    (fp_text value Varistor (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (model ${KIPRJMOD}/3D/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Resonator_SMD_CTSC_1.3mmx3.2mm (layer F.Cu) (tedit 636FC12A)
    (at 147.77 81.815)
    (descr "SMD Resomator/Filter Murata TPSKA, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 7.9x3.8mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at -0.127 -1.27) (layer F.SilkS) hide)
    (fp_text value "16 Mhz" (at -0.07 1.785) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1.2 0) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R26-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.2 0) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R26-Pad2)"))
    (model ${KIPRJMOD}/3D/resontator_CSTNE16M0V530000R0.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 636FBFD2)
    (at 147.7 90.705 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 5.45 6.27 180) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at 0.1 -7.395 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /D7))
    (pad 2 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /D-))
    (pad 4 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /D+))
    (pad 5 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 7 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 8 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /RXLED))
    (pad 9 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 10 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 11 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 12 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /D11))
    (pad 13 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /~RESET))
    (pad 14 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 15 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R26-Pad1)"))
    (pad 17 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R26-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /D3_SCL))
    (pad 19 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /D2_SDA))
    (pad 20 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /D0))
    (pad 21 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /D1))
    (pad 22 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /TXLED))
    (pad 23 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 25 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /D4))
    (pad 26 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /D12))
    (pad 27 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /D6))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /D8))
    (pad 29 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /D9))
    (pad 30 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /D10))
    (pad 31 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /D5))
    (pad 32 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /D13))
    (pad 33 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 34 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 35 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /A0))
    (pad 37 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /A1))
    (pad 38 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /A2))
    (pad 39 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /A3))
    (pad 40 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /A4))
    (pad 41 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /A5))
    (pad 42 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 /AREF))
    (pad 43 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:USB_Micro-B_Molex-105017-0001 locked (layer F.Cu) (tedit 636FBEAD)
    (at 109.22 100.33 270)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J1 (at 4.699 -2.032) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at 0.3 3.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.8 270) (layer Dwgs.User))
    (pad 6 smd rect (at -2.9 0.35 270) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.9 0.35 270) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 0.35 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 0.35 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1 0.35 270) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.3 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(F1-Pad2)"))
    (pad 2 smd rect (at -0.65 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (pad 6 thru_hole circle (at -2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1 0.35 270) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3D/USB_micro_105017-0001.stp
      (offset (xyz 0 0 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:C_0805 (layer F.Cu) (tedit 636FC0BD)
    (at 139.445 95.785 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.75 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model ${KIPRJMOD}/3D/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 167.64 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P2 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value M3 (at 0.1 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 42 "Net-(P2-Pad1)"))
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 110.49 131)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P3 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value M3 (at 0.1 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 43 "Net-(P3-Pad1)"))
  )
  (module footprints:M3mount (layer F.Cu) (tedit 636FC1C2)
    (at 167.64 131)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (fp_text reference P4 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value M3 (at 0.1 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 44 "Net-(P4-Pad1)"))
  )
  (module footprints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 124 118.11)
    (fp_text reference MadeInOregon1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0 0) (layer F.SilkS) hide)
  )
  (module footprints:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 140 121.92 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference MadeWithKiCAD1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0.75 0) (layer B.Fab) hide)
  )
  (module footprints:OSHW-Logo_11.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 157.5 118.5 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference OSHW1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module footprints:SAMTEC_MEC8-113-TOP-BOTTOM (layer F.Cu) (tedit 63786631)
    (at 119 110 90)
    (fp_text reference X2 (at -0.5 -5.75 90) (layer F.SilkS))
    (fp_text value MEC8-113 (at 8.21 6.135 90) (layer F.Fab))
    (pad 26 smd rect (at 6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 25 smd rect (at 5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 32 /D2_SDA))
    (pad 12 smd rect (at 5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /D3_SCL))
    (pad 11 smd rect (at 4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 36 /A1))
    (pad None np_thru_hole circle (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad 23 smd rect (at 4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 97 /40))
    (pad 10 smd rect (at 4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 94 /30))
    (pad 22 smd rect (at 3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 98 /39))
    (pad 9 smd rect (at 3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 93 /29))
    (pad 21 smd rect (at 2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 99 /38))
    (pad 8 smd rect (at 2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 92 /28))
    (pad 20 smd rect (at 1.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 100 /37))
    (pad 7 smd rect (at 1.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 91 /27))
    (pad 19 smd rect (at -2.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 101 /36))
    (pad 6 smd rect (at -2.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 90 /26))
    (pad 18 smd rect (at -3.2 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 102 /35))
    (pad 5 smd rect (at -3.2 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 89 /25))
    (pad 17 smd rect (at -4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 103 /34))
    (pad 4 smd rect (at -4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 73 /24))
    (pad 16 smd rect (at -4.8 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 104 /33))
    (pad 3 smd rect (at -4.8 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 74 /23))
    (pad 15 smd rect (at -5.6 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 96 /32))
    (pad 2 smd rect (at -5.6 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 75 /22))
    (pad 14 smd rect (at -6.4 -4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 95 /31))
    (pad 1 smd rect (at -6.4 4 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 76 /21))
    (model ${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:SW_TS10-63-26-BE-250-SMT-TR (layer F.Cu) (tedit 63700F76)
    (at 156 129 270)
    (fp_text reference SW2 (at 0.075 0 90) (layer F.SilkS))
    (fp_text value D0 (at 5 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.25 0 270) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /D0))
    (pad 2 smd rect (at 3.25 0 270) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MEC8-113-CARD_2outline locked (layer F.Cu) (tedit 637EA855)
    (at 116.459 120 90)
    (fp_text reference CardOutline1 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value SYM_Arrow_Large (at 10.9 -1 90) (layer F.Fab))
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm (layer F.Cu) (tedit 63CC3C2E)
    (at 132 89 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U2 (at 0 -3.3) (layer F.SilkS))
    (fp_text value MCP23008-xML (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U2-Pad4)"))
    (pad 5 smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(U2-Pad5)"))
    (pad 6 smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U2-Pad6)"))
    (pad 7 smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /SCK))
    (pad 8 smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(U2-Pad8)"))
    (pad 9 smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /08))
    (pad 10 smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /07))
    (pad 11 smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /06))
    (pad 12 smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /05))
    (pad 13 smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /04))
    (pad 14 smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /03))
    (pad 15 smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /02))
    (pad 16 smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /01))
    (pad 17 smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 18 smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 19 smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /D3_SCL))
    (pad 20 smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /D2_SDA))
    (pad 17 smd rect (at 0 0 180) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm (layer F.Cu) (tedit 63CC3C39)
    (at 132 81 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U3 (at 0 -3.3) (layer F.SilkS))
    (fp_text value MCP23008-xML (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 4 smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(U3-Pad4)"))
    (pad 5 smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(U3-Pad5)"))
    (pad 6 smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(U3-Pad6)"))
    (pad 7 smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /MOSI))
    (pad 8 smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(U3-Pad8)"))
    (pad 9 smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /16))
    (pad 10 smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /15))
    (pad 11 smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /14))
    (pad 12 smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /13))
    (pad 13 smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /12))
    (pad 14 smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /11))
    (pad 15 smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /10))
    (pad 16 smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /09))
    (pad 17 smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 18 smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 19 smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /D3_SCL))
    (pad 20 smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /D2_SDA))
    (pad 17 smd rect (at 0 0 180) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm (layer F.Cu) (tedit 63CC3C1A)
    (at 132 97.675 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U4 (at 0 -3.3) (layer F.SilkS))
    (fp_text value MCP23008-xML (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad 17 smd rect (at 0 0 180) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 20 smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /D2_SDA))
    (pad 19 smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /D3_SCL))
    (pad 18 smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 17 smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 16 smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 /17))
    (pad 15 smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 /18))
    (pad 14 smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 /19))
    (pad 13 smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /20))
    (pad 12 smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /21))
    (pad 11 smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /22))
    (pad 10 smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /23))
    (pad 9 smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /24))
    (pad 8 smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U4-Pad8)"))
    (pad 7 smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /MISO))
    (pad 6 smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U4-Pad6)"))
    (pad 5 smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(U4-Pad5)"))
    (pad 4 smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(U4-Pad4)"))
    (pad 3 smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 1 smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm (layer F.Cu) (tedit 63CC3C0E)
    (at 132 105 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U6 (at 0 -3.3) (layer F.SilkS))
    (fp_text value MCP23008-xML (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers F.Paste) (roundrect_rratio 0.229358))
    (pad 17 smd rect (at 0 0 180) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 20 smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /D2_SDA))
    (pad 19 smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /D3_SCL))
    (pad 18 smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (pad 17 smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 16 smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /33))
    (pad 15 smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 /34))
    (pad 14 smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /35))
    (pad 13 smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /36))
    (pad 12 smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /37))
    (pad 11 smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /38))
    (pad 10 smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /39))
    (pad 9 smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /40))
    (pad 8 smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(U6-Pad8)"))
    (pad 7 smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /D8))
    (pad 6 smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(U6-Pad6)"))
    (pad 5 smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(U6-Pad5)"))
    (pad 4 smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(U6-Pad4)"))
    (pad 3 smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +5V))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Snake (layer B.Cu) (tedit 0)
    (at 138.5 92.7 180)
    (fp_text reference SnakeBack1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value SYM_Arrow_Large (at 0.75 0) (layer B.SilkS) hide)
  )
  (module footprints:SW_TS10-63-26-BE-250-SMT-TR (layer F.Cu) (tedit 63700F76)
    (at 162 129 270)
    (fp_text reference SW1 (at 0 0 90) (layer F.SilkS))
    (fp_text value D1 (at 5 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.25 0 270) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /D1))
    (pad 2 smd rect (at 3.25 0 270) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text "I2C OLED Display" (at 132.9 128.4) (layer F.SilkS))
  (dimension 64.77 (width 0.15) (layer Dwgs.User)
    (gr_text "64.770 mm" (at 139.065 140.3) (layer Dwgs.User))
    (feature1 (pts (xy 171.45 131.19) (xy 171.45 139.586421)))
    (feature2 (pts (xy 106.68 131.19) (xy 106.68 139.586421)))
    (crossbar (pts (xy 106.68 139) (xy 171.45 139)))
    (arrow1a (pts (xy 171.45 139) (xy 170.323496 139.586421)))
    (arrow1b (pts (xy 171.45 139) (xy 170.323496 138.413579)))
    (arrow2a (pts (xy 106.68 139) (xy 107.806504 139.586421)))
    (arrow2b (pts (xy 106.68 139) (xy 107.806504 138.413579)))
  )
  (dimension 58.8 (width 0.15) (layer Dwgs.User)
    (gr_text "58.800 mm" (at 96.7 105.6 270) (layer Dwgs.User))
    (feature1 (pts (xy 110.49 135) (xy 97.413579 135)))
    (feature2 (pts (xy 110.49 76.2) (xy 97.413579 76.2)))
    (crossbar (pts (xy 98 76.2) (xy 98 135)))
    (arrow1a (pts (xy 98 135) (xy 97.413579 133.873496)))
    (arrow1b (pts (xy 98 135) (xy 98.586421 133.873496)))
    (arrow2a (pts (xy 98 76.2) (xy 97.413579 77.326504)))
    (arrow2b (pts (xy 98 76.2) (xy 98.586421 77.326504)))
  )
  (gr_text "SDA SCL VCC GND" (at 148.9 128 90) (layer F.SilkS))
  (gr_line (start 171.45 123.19) (end 171.45 131.19) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.68 123.19) (end 106.68 131.19) (layer Edge.Cuts) (width 0.15))
  (dimension 2.8 (width 0.15) (layer Dwgs.User)
    (gr_text "2.800 mm" (at 138.3 85 270) (layer Dwgs.User))
    (feature1 (pts (xy 134.6 86.4) (xy 137.586421 86.4)))
    (feature2 (pts (xy 134.6 83.6) (xy 137.586421 83.6)))
    (crossbar (pts (xy 137 83.6) (xy 137 86.4)))
    (arrow1a (pts (xy 137 86.4) (xy 136.413579 85.273496)))
    (arrow1b (pts (xy 137 86.4) (xy 137.586421 85.273496)))
    (arrow2a (pts (xy 137 83.6) (xy 136.413579 84.726504)))
    (arrow2b (pts (xy 137 83.6) (xy 137.586421 84.726504)))
  )
  (gr_text github.com/aspro648/RPB (at 140.5 107.5) (layer B.SilkS))
  (gr_text "Keep It\nSimple\nStupid" (at 164.1 95.9) (layer B.Mask))
  (gr_text "Killroy was\nhere!" (at 132.8 131.4) (layer B.Cu))
  (gr_text M3 (at 163.7 83.95) (layer F.SilkS))
  (gr_text A0 (at 110.2 110.7) (layer F.SilkS))
  (gr_text "Rapid Prototyping\nBoard" (at 146.7 111.1) (layer F.SilkS))
  (gr_text 648.ken@gmail.com (at 140.335 110) (layer B.SilkS))
  (gr_text M2.5 (at 158.115 92.075) (layer F.SilkS))
  (gr_text "Rapid Prototyping Board" (at 139.7 104.14) (layer B.SilkS))
  (gr_text - (at 159.5 86) (layer F.SilkS))
  (gr_text + (at 159.5 80.5) (layer F.SilkS))
  (gr_arc (start 110.49 80.01) (end 110.49 76.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 110.49 131.19) (end 106.68 131.19) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 80.01) (end 171.45 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 80.01) (end 171.45 80.01) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 131.19) (end 167.64 135) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 76.2) (end 110.49 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 135) (end 167.64 135) (layer Edge.Cuts) (width 0.15))
  (gr_text "Rev 1.1\nJam 2023" (at 124.46 123.19) (layer B.SilkS))
  (gr_line (start 106.68 123.19) (end 106.68 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.958 137) (xy 105.8 137.1) (xy 106.1 74.2) (xy 172.2 74.3)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.466 137) (xy 105.664 137) (xy 105.8 74.4) (xy 172.8 74.3)
      )
    )
  )
)
