(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (footprint "sdsLogos:sdsLabs-small-fSilk" (layer "F.Cu")
    (at 140.335 123.825)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -3.81) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0 -2.54) (layer "F.SilkS") hide)
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 133.35 69.215)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND"))
  )
  (footprint "MountingHole:MountingHole_6.5mm_Pad" (layer "F.Cu")
    (at 114.3 90.28)
    (descr "Mounting Hole 6.5mm")
    (tags "mounting hole 6.5mm")
    (property "Sheetfile" "citation1-4input.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at 25.4 -0.11) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 25.4 -12.175) (size 9.525 9.525) (drill 6.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_6.5mm_Pad" (layer "F.Cu")
    (at 114.3 104.83)
    (descr "Mounting Hole 6.5mm")
    (tags "mounting hole 6.5mm")
    (property "Sheetfile" "citation1-4input.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at 25.4 -3.23) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 25.4 -15.295) (size 9.525 9.525) (drill 6.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 133.35 121.92)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -0.635) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND"))
  )
  (footprint "MountingHole:MountingHole_6.5mm_Pad" (layer "F.Cu")
    (at 114.3 75.73)
    (descr "Mounting Hole 6.5mm")
    (tags "mounting hole 6.5mm")
    (property "Sheetfile" "citation1-4input.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at 25.4 3.01) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 25.4 36.665) (size 9.525 9.525) (drill 6.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 146.05 69.215)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 146.685 121.92)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -0.635 -0.635) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND"))
  )
  (footprint "MountingHole:MountingHole_6.5mm_Pad" (layer "F.Cu")
    (at 114.3 119.38)
    (descr "Mounting Hole 6.5mm")
    (tags "mounting hole 6.5mm")
    (property "Sheetfile" "citation1-4input.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at 25.4 -6.35) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 25.4 -18.415) (size 9.525 9.525) (drill 6.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (gr_line (start 127 127) (end 152.4 127)
    (layer "Edge.Cuts"))
  (gr_line (start 152.4 127) (end 152.4 63.5)
    (layer "Edge.Cuts"))
  (gr_circle (center 146.05 121.285) (end 147.6375 121.285)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 133.35 69.215) (end 134.9375 69.215)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 152.4 63.5) (end 127 63.5)
    (layer "Edge.Cuts"))
  (gr_line (start 127 63.5) (end 127 127)
    (layer "Edge.Cuts"))
  (gr_circle (center 133.35 121.285) (end 134.9375 121.285)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 146.05 69.215) (end 147.6375 69.215)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999999))
    (polygon
      (pts
        (xy 127 127)
        (xy 127 118.11)
        (xy 152.4 118.11)
        (xy 152.4 127)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999999))
    (polygon
      (pts
        (xy 127 63.5)
        (xy 152.4 63.5)
        (xy 152.4 72.39)
        (xy 127 72.39)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999999))
    (polygon
      (pts
        (xy 127 72.39)
        (xy 132.08 72.39)
        (xy 132.08 118.11)
        (xy 127 118.11)
      )
    )
  )
)
