(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(J1-In)")
  (net 3 "Net-(U1-OUT)")
  (net 4 "unconnected-(U1-NULL-Pad1)")
  (net 5 "unconnected-(U1-NC-Pad5)")
  (net 6 "unconnected-(U1-NC-Pad8)")
  (net 7 "Net-(U2-+IN)")
  (net 8 "Net-(D1-K)")
  (net 9 "-15V")
  (net 10 "+15V")
  (net 11 "unconnected-(U2-NIC-Pad1)")
  (net 12 "unconnected-(U2-NIC-Pad5)")
  (net 13 "unconnected-(U2-DISABLE-Pad8)")
  (footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (at 128.075 97.5)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Photodiode")
    (property "ki_keywords" "photodiode diode opto")
    (attr smd)
    (fp_text reference "D1" (at 0.075 -2.05) (layer "F.SilkS"))
    (fp_text value "D_Photo" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.225 0) (size 0.55 0.55) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.225 0) (size 0.55 0.55) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm" (layer "F.Cu")
    (at 134.135 97.435 180)
    (descr "LFCSP, 8 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/lfcspcp/cp-8/CP_8_13.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "LFCSP NoLead")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.45) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.2875 -0.75 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "unconnected-(U1-NULL-Pad1)") (pinfunction "NULL") (pintype "no_connect"))
    (pad "2" smd roundrect (at -1.2875 -0.25 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+15V") (pinfunction "V+") (pintype "input"))
    (pad "3" smd roundrect (at -1.2875 0.25 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "+IN") (pintype "input"))
    (pad "4" smd roundrect (at -1.2875 0.75 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "-15V") (pinfunction "V-") (pintype "input"))
    (pad "5" smd roundrect (at 1.2875 0.75 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "unconnected-(U1-NC-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 1.2875 0.25 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U1-OUT)") (pinfunction "OUT") (pintype "output"))
    (pad "7" smd roundrect (at 1.2875 -0.25 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D1-K)") (pinfunction "-IN") (pintype "input"))
    (pad "8" smd roundrect (at 1.2875 -0.75 180) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "unconnected-(U1-NC-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 132.5 87.2 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0.01 -2.49) (layer "F.SilkS"))
    (fp_text value "9.1p" (at -0.02 2.39) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "Net-(U1-OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 8 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 146.6375 102.6)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4) (layers "*.Cu" "*.Mask")
      (net 9 "-15V") (pinfunction "Ext") (pintype "passive+no_connect"))
  )
  (footprint "Connector_Coaxial:BNC_TEConnectivity_1478204_Vertical" (layer "F.Cu")
    (at 154.35 90.025)
    (descr "BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html")
    (tags "BNC female PCB mount 4 pin straight chassis connector ")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J1" (at -0.05 6.425) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 0 6.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.175 -3.175 90) (size 2 2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.175 3.175) (size 2 2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.175 -3.175) (size 2 2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.175 3.175) (size 2 2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_TEConnectivity_1478204_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 138.1 102.7)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4) (layers "*.Cu" "*.Mask")
      (net 10 "+15V") (pinfunction "Ext") (pintype "passive+no_connect"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 136 92.2 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(U1-OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 8 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_CSP:LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm" (layer "F.Cu")
    (at 145.3875 87.45)
    (descr "LFCSP, 8 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/lfcspcp/cp-8/CP_8_13.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "LFCSP NoLead")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.45) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.2875 -0.75) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "unconnected-(U2-NIC-Pad1)") (pinfunction "NIC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -1.2875 -0.25) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J1-In)") (pinfunction "-IN") (pintype "input"))
    (pad "3" smd roundrect (at -1.2875 0.25) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(U2-+IN)") (pinfunction "+IN") (pintype "input"))
    (pad "4" smd roundrect (at -1.2875 0.75) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "-15V") (pinfunction "V-") (pintype "power_out"))
    (pad "5" smd roundrect (at 1.2875 0.75) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "unconnected-(U2-NIC-Pad5)") (pinfunction "NIC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 1.2875 0.25) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J1-In)") (pinfunction "OUT") (pintype "output"))
    (pad "7" smd roundrect (at 1.2875 -0.25) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 1.2875 -0.75) (size 0.575 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "unconnected-(U2-DISABLE-Pad8)") (pinfunction "DISABLE") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_CSP.3dshapes/LFCSP-8-1EP_3x3mm_P0.5mm_EP1.45x1.74mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 142.1 92.4)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -0.01 2.28) (layer "F.SilkS"))
    (fp_text value "1.5n" (at -0.01 -2.32) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 7 "Net-(U2-+IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 155.2 102.6)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Ext") (pintype "passive+no_connect"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 139.4 87.2)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TIA_PhotodiodeWizard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0.01 1.75) (layer "F.SilkS"))
    (fp_text value "210" (at 0.01 -1.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(U1-OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 7 "Net-(U2-+IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 125.4 83.8) (end 161.75 109.9)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "-15V\n" (at 144.5375 107.3) (layer "F.SilkS"))
  (gr_text "+15V\n" (at 136 107.4) (layer "F.SilkS"))
  (gr_text "GND" (at 153.9 107.3) (layer "F.SilkS"))
  (zone (net 10) (net_name "+15V") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.35043 83.8)
        (xy 161.57543 84.025)
        (xy 161.65043 109.825)
        (xy 125.45043 110.025)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.450284 83.8)
        (xy 161.600284 84.375)
        (xy 161.475284 110.3)
        (xy 125.350284 110.25)
        (xy 125.450284 84)
        (xy 156.350284 83.9)
      )
    )
  )
)
