(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "PiExp")
		(date "2024-09-29")
		(rev "1b")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0254)
		(solder_mask_min_width 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "GP2_SDA")
	(net 4 "GP3_SCL")
	(net 5 "+3V3")
	(net 6 "GP13")
	(net 7 "GP14_TXD")
	(net 8 "GP15_RXD")
	(net 9 "unconnected-(JP_I4-Pin_13-Pad13)")
	(net 10 "GP4_1Wire")
	(net 11 "GP19")
	(net 12 "AIN3")
	(net 13 "unconnected-(JP_I4-Pin_16-Pad16)")
	(net 14 "GP9_MISO")
	(net 15 "GP25_NINT")
	(net 16 "GP8_CE0")
	(net 17 "GP1_EESCL")
	(net 18 "GP18")
	(net 19 "GP20")
	(net 20 "GP0_EESDA")
	(net 21 "unconnected-(JP_I4-Pin_18-Pad18)")
	(net 22 "GP17_NRST")
	(net 23 "unconnected-(JP_I4-Pin_26-Pad26)")
	(net 24 "unconnected-(JP_I4-Pin_37-Pad37)")
	(net 25 "GP21")
	(net 26 "GP5")
	(net 27 "GP6")
	(net 28 "GP12")
	(net 29 "GP11_SCLK")
	(net 30 "unconnected-(JP_I4-Pin_15-Pad15)")
	(net 31 "GP10_MOSI")
	(net 32 "unconnected-(JP_I4-Pin_36-Pad36)")
	(net 33 "AIN0")
	(net 34 "/ADDR")
	(net 35 "/RDY")
	(net 36 "AIN2")
	(net 37 "/OPT1")
	(net 38 "/OPT2")
	(net 39 "AIN1")
	(net 40 "Net-(SPENA1-A)")
	(net 41 "Net-(SPSCL1-C)")
	(net 42 "Net-(SPSDA1-C)")
	(net 43 "/VSER+")
	(net 44 "Net-(SPA2-B)")
	(net 45 "Net-(SPA3-B)")
	(net 46 "Net-(JPOPT12-Pin_2)")
	(net 47 "Net-(SPL1-A)")
	(net 48 "Net-(LED1-A)")
	(net 49 "Net-(SPUD5-C)")
	(net 50 "Net-(SPUD6-C)")
	(net 51 "Net-(SPW1-A)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 15.3416 8.382)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RW1"
			(at 2.8702 -0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 51 "Net-(SPW1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(locked yes)
		(layer "F.Cu")
		(at 3.5 3.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H1"
			(at 0 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0.1016 0.7112 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(locked yes)
		(layer "F.Cu")
		(at 61.5 3.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H2"
			(at 0 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0.1016 0.7112 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 37.084 26.67)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "JPWIR1"
			(at -2.7178 -3.937 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "GP4_1Wire")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "AIN0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 53.6174 8.845725 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RPDOP1"
			(at -0.0782 1.3469 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 6 "GP13")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 3.937 18.1102 -90)
		(descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
		(tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
		(property "Reference" "JV5"
			(at 4.953 -1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.27 3.37 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 15.5194 18.4508 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPA3"
			(at 2.1486 0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 12 "AIN3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 45 "Net-(SPA3-B)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 60.2488 12.065 180)
		(descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH vertical")
		(property "Reference" "JPDAT2"
			(at 2.6416 2.9972 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0254 2.4892 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "GP18")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "GP21")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "GP20")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "GP19")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 45.593 26.67)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "JPDAT1"
			(at -2.6416 -3.7084 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "GP5")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "GP6")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 49.4304 12.593275 -90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q_OP2"
			(at 3.1482 0.066 0)
			(layer "F.SilkS")
		)
		(property "Value" "2N7002K"
			(at -0.0508 0.2794 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30896.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "GP12")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/OPT2")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 3.230373 12.0396 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RADUP1"
			(at 0.0254 -1.3208 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 35 "/RDY")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 24.8966 10.2108 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPSER1"
			(at -0.0762 -1.7526 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 1.524 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "+3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 43 "/VSER+")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "+5V")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 11.0998 26.67)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "JPAD23"
			(at -2.5654 -3.7846 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "AIN2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "AIN3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 59.9948 16.9418 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RLED1"
			(at -2.3368 0.0762 180)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at -0.0254 1.27 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 48 "Net-(LED1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 47 "Net-(SPL1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 17.0434 10.6426)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPW1"
			(at 0.0104 1.8034 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 51 "Net-(SPW1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "GP4_1Wire")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 53.6526 12.618675 -90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q_OP1"
			(at 3.2258 0.1524 0)
			(layer "F.SilkS")
		)
		(property "Value" "2N7002K"
			(at -0.0508 0.2794 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30896.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GP13")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/OPT1")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 39.8018 18.8623 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPUD6"
			(at 0 -1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 1.524 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "+3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 50 "Net-(SPUD6-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 43.815 18.6182 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RU6"
			(at 2.3716 -0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 27 "GP6")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 50 "Net-(SPUD6-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 54.102 26.67)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "JPOPT12"
			(at -2.6924 -4.064 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/OPT2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "Net-(JPOPT12-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/OPT1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 31.0342 19.0754 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPUD5"
			(at 0.0208 -1.7018 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 1.524 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "+3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 49 "Net-(SPUD5-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 19.812 26.67)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "JPI2C1"
			(at -2.667 -3.6576 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GP2_SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GP3_SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 4.199873 9.0932 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RADDN1"
			(at -0.1016 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 34 "/ADDR")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 35.3314 18.7612 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RU5"
			(at -2.2352 0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 26 "GP5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 49 "Net-(SPUD5-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(locked yes)
		(layer "F.Cu")
		(at 3.5 26.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H3"
			(at 0 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0.1016 0.7112 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(locked yes)
		(layer "F.Cu")
		(at 61.5 26.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H4"
			(at 0 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0.1016 0.7112 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 49.4558 8.820325 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RPDOP2"
			(at 0.0782 1.3737 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 28 "GP12")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 51.4904 19.1008 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPOPT2"
			(at 0.03 1.9812 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 1.524 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "+5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 46 "Net-(JPOPT12-Pin_2)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "+3V3")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 9.8591 15.5702)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CAD1"
			(at 3.1203 -0.5334 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.2446 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Digi-Key_PN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 17.8816 18.6342 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0.1176 1.4478 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 45 "Net-(SPA3-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 61.34 21.7678)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D_BEM1"
			(at -0.1016 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "MBR230LSFT1G"
			(at 0 0.9652 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MBR230LSFT1-D.PDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MBR230LSFT1GOSCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "MBR230LSFT1G"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.889 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/OPT1")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 41.2002 11.0786 180)
		(descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH vertical")
		(property "Reference" "JPN1"
			(at -2.7164 2.468 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0254 2.4892 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GP25_NINT")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "GP17_NRST")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 9.8298 18.6088 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -0.0668 1.3716 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 44 "Net-(SPA2-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 28.5242 26.67)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "JPSER1"
			(at -2.6924 -3.7592 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/VSER+")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GP15_RXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GP14_TXD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 8.111473 12.446)
		(descr "MSOP, 10 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U1115"
			(at -0.0508 -2.2352 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115"
			(at 0 2.45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -2.1125 -1)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/ADDR")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.1125 -0.5)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/RDY")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -2.1125 0)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.1125 0.5)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "AIN0")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.1125 1)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "AIN1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.1125 1)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "AIN2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.1125 0.5)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "AIN3")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.1125 0)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.1125 -0.5)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GP2_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.1125 -1)
			(size 1.625 0.32)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GP3_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 33.2754 11.0786 180)
		(descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH vertical")
		(property "Reference" "JPN2"
			(at -2.7418 2.468 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0254 2.4892 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "GP8_CE0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "GP11_SCLK")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "GP9_MISO")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "GP10_MOSI")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 12.2174 18.4254 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPA2"
			(at 2.1186 -0.1016 180)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 36 "AIN2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 44 "Net-(SPA2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 56.7944 17.8308 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at 2.1844 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "Blue"
			(at 0 0.9144 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/OPT1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 62.7888 17.5618 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPL1"
			(at -2.032 -0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 47 "Net-(SPL1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "+5V")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical"
		(locked yes)
		(layer "B.Cu")
		(at 8.3566 4.77 -90)
		(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x20 2.54mm double row")
		(property "Reference" "JP_I4"
			(at -1.27 2.1844 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x20_Odd_Even"
			(at -1.2192 -40.0558 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 -24.13 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GP2_SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GP3_SCL")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GP4_1Wire")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at -2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "GP14_TXD")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at -2.54 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GP15_RXD")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "GP17_NRST")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at -2.54 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GP18")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(JP_I4-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole oval
			(at -2.54 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(JP_I4-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole oval
			(at -2.54 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(JP_I4-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole oval
			(at 0 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at -2.54 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(JP_I4-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
		)
		(pad "19" thru_hole oval
			(at 0 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "GP10_MOSI")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at -2.54 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GP9_MISO")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at -2.54 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GP25_NINT")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "GP11_SCLK")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at -2.54 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GP8_CE0")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at -2.54 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(JP_I4-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
		)
		(pad "27" thru_hole oval
			(at 0 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "GP0_EESDA")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at -2.54 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GP1_EESCL")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole oval
			(at 0 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GP5")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole oval
			(at -2.54 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole oval
			(at 0 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "GP6")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole oval
			(at -2.54 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GP12")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole oval
			(at 0 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GP13")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole oval
			(at -2.54 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" thru_hole oval
			(at 0 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GP19")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" thru_hole oval
			(at -2.54 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(JP_I4-Pin_36-Pad36)")
			(pinfunction "Pin_36")
			(pintype "passive+no_connect")
		)
		(pad "37" thru_hole oval
			(at 0 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(JP_I4-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
		)
		(pad "38" thru_hole oval
			(at -2.54 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GP20")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" thru_hole oval
			(at 0 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" thru_hole oval
			(at -2.54 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GP21")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "B.Cu")
		(at 31.3332 17.6417)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "UCS1"
			(at -0.3706 2.3227 0)
			(layer "B.SilkS")
		)
		(property "Value" "24CS256"
			(at 0 -1.56 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "150-24CS256T-I/OTCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "24CS256T-I/OT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(SPSCL1-C)")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(SPSDA1-C)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(SPENA1-A)")
			(pinfunction "WP")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 40.4772 18.3388 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RWRPU1"
			(at 0 1.4478 90)
			(layer "B.SilkS")
		)
		(property "Value" "1K"
			(at -0.0254 -1.27 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 40 "Net-(SPENA1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 21.3708 13.2588 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RESCLPU1"
			(at 0.5936 1.3208 0)
			(layer "B.SilkS")
		)
		(property "Value" "3.9K"
			(at -0.0254 -1.27 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "RMCF0805FT3K90CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "RMCF0805FT3K90"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 20 "GP0_EESDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 25.2222 19.9436 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPSCL1"
			(at 0.097 -2.1844 90)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 -1.524 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 17 "GP1_EESCL")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 41 "Net-(SPSCL1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 4 "GP3_SCL")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 36.718 16.2306 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CE1"
			(at 0 1.397 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.2446 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property " Manufacturer Part#" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "B.Cu")
		(at 14.986 18.542 180)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "GND1"
			(at -0.1524 -2.0066 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0.1016 -0.6604 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at -0.0508 0.381 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 37.0736 19.0246)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPENA1"
			(at -0.269 1.7526 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 -1.3462 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 40 "Net-(SPENA1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 25.2476 12.9494 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SPSDA1"
			(at 0.1062 -2.2098 90)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 -1.524 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 20 "GP0_EESDA")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 42 "Net-(SPSDA1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "GP2_SDA")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 21.352 17.9832 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RESDAPU1"
			(at 0.5494 1.3716 0)
			(layer "B.SilkS")
		)
		(property "Value" "3.9K"
			(at -0.0254 -1.27 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "RMCF0805FT3K90CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "RMCF0805FT3K90"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 17 "GP1_EESCL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "B.Cu")
		(at 8.636 18.542 180)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "A1"
			(at 0 -1.9558 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0.1016 -0.6604 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "PiExp_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at -0.0508 0.381 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 39 "AIN1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(gr_line
		(start 0 26.5)
		(end 0 3.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 65 26.5)
		(mid 63.974874 28.974874)
		(end 61.5 30)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61.5 30)
		(end 3.5 30)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 65 3.5)
		(end 65 26.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 61.5 0)
		(mid 63.974874 1.025126)
		(end 65 3.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 3.5 30)
		(mid 1.025126 28.974874)
		(end 0 26.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 3.5 0)
		(end 61.5 0)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 0 3.5)
		(mid 1.025126 1.025126)
		(end 3.5 0)
		(layer "Edge.Cuts")
	)
	(gr_text "5V"
		(at 10.922 0.508 0)
		(layer "B.SilkS")
	)
	(gr_text "ESCL"
		(at 25.2476 17.272 0)
		(layer "B.SilkS")
	)
	(gr_text "3V"
		(at 8.509 6.6548 0)
		(layer "B.SilkS")
	)
	(gr_text "SDA1"
		(at 25.273 15.7226 0)
		(layer "B.SilkS")
	)
	(gr_text "ESDA"
		(at 25.273 10.2616 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 13.4112 0.5334 0)
		(layer "B.SilkS")
	)
	(gr_text "Copyright S. Cooper 2024.\nCERN OHL v.1.2  (Open Hardware Licence)\nhttp://ohwr.org/cernohl"
		(at 30.734 27.0256 0)
		(layer "B.SilkS")
	)
	(gr_text "SCL1"
		(at 25.2984 22.733 0)
		(layer "B.SilkS")
	)
	(gr_text "PiExp\nVersion 1b\n30 Sept 2024"
		(at 56.3626 13.1064 0)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 8.3566 0.5588 0)
		(layer "B.SilkS")
	)
	(gr_text "3V"
		(at 36.5506 22.7838 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 35.5092 22.3774 90)
		(layer "F.SilkS")
	)
	(gr_text "GP4"
		(at 37.6174 22.4028 90)
		(layer "F.SilkS")
	)
	(gr_text "PiExp\nVersion 1b\n30 Sept 2024"
		(at 23.6728 15.1892 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 56.6928 6.4516 0)
		(layer "F.SilkS")
	)
	(gr_text "A0"
		(at 38.608 22.733 90)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 30.0482 22.7838 90)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 13.5128 6.5024 0)
		(layer "F.SilkS")
	)
	(gr_text "SCLK"
		(at 33.8582 7.5692 90)
		(layer "F.SilkS")
	)
	(gr_text "GP21"
		(at 60.8584 8.1026 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 54.4068 19.2278 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 18.5166 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 9.7282 22.3266 90)
		(layer "F.SilkS")
	)
	(gr_text "GP25"
		(at 40.7162 14.4018 90)
		(layer "F.SilkS")
	)
	(gr_text "GP10"
		(at 31.9024 14.3764 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 41.1226 16.637 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 19.3802 22.7584 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 32.3596 16.8656 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 13.4366 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "NINT"
		(at 40.8686 7.747 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 41.8846 8.2296 90)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 21.4122 22.4536 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 55.753 22.8346 90)
		(layer "F.SilkS")
	)
	(gr_text "1W"
		(at 16.0274 6.477 0)
		(layer "F.SilkS")
	)
	(gr_text "GP20"
		(at 59.8424 8.1026 90)
		(layer "F.SilkS")
	)
	(gr_text "A3"
		(at 12.8016 22.7584 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 23.5966 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 18.3134 22.352 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 28.702 6.3754 0)
		(layer "F.SilkS")
	)
	(gr_text "OPT1"
		(at 54.6862 22.098 90)
		(layer "F.SilkS")
	)
	(gr_text "MOSI"
		(at 31.8262 7.6454 90)
		(layer "F.SilkS")
	)
	(gr_text "GP11"
		(at 33.9598 14.351 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 10.8966 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 1.2446 15.6464 0)
		(layer "F.SilkS")
	)
	(gr_text "GP8"
		(at 35.0012 14.097 90)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 16.0274 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 11.811 22.3774 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 48.9458 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "GP17"
		(at 39.7256 14.4526 90)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 10.7442 22.7838 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 38.5318 16.6878 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 27.8638 10.1346 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 8.3312 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 48.4886 19.177 0)
		(layer "F.SilkS")
	)
	(gr_text "GP9"
		(at 32.9692 14.097 90)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 20.3708 22.4282 90)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 32.9184 7.62 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 43.8912 0.6604 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 10.9474 6.5024 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 42.9006 14.097 90)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 29.0068 22.7838 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 41.7068 13.843 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 42.799 7.874 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 18.4912 6.5024 0)
		(layer "F.SilkS")
	)
	(gr_text "GP19"
		(at 58.7756 8.0518 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 29.8196 16.891 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 45.1612 22.7584 90)
		(layer "F.SilkS")
	)
	(gr_text "NRST"
		(at 39.7256 7.62 90)
		(layer "F.SilkS")
	)
	(gr_text "V+"
		(at 53.6194 22.6568 90)
		(layer "F.SilkS")
	)
	(gr_text "CE0"
		(at 34.8234 7.874 90)
		(layer "F.SilkS")
	)
	(gr_text "GP6"
		(at 47.1678 22.3774 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 31.1912 0.635 0)
		(layer "F.SilkS")
	)
	(gr_text "GP5"
		(at 46.1772 22.4028 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 21.8694 10.3378 0)
		(layer "F.SilkS")
	)
	(gr_text "GP18"
		(at 61.8236 8.1026 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 27.0002 22.4028 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 1.397 23.1648 0)
		(layer "F.SilkS")
	)
	(gr_text "V+"
		(at 28.0162 22.6568 90)
		(layer "F.SilkS")
	)
	(gr_text "OPT2"
		(at 52.5526 22.0726 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 43.9928 22.3774 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 38.9382 6.0706 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 8.382 6.5532 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.635 -0.635) (xy 65.405 -0.635) (xy 65.405 30.48) (xy -0.635 30.48)
			)
		)
	)
)
