(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 52)
    (tracks 323)
    (zones 0)
    (modules 10)
    (nets 81)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad24)")
  (net 2 "Net-(J1-Pad23)")
  (net 3 "Net-(J1-Pad22)")
  (net 4 "Net-(J1-Pad21)")
  (net 5 "Net-(J1-Pad20)")
  (net 6 "Net-(J1-Pad19)")
  (net 7 "Net-(J1-Pad18)")
  (net 8 "Net-(J1-Pad17)")
  (net 9 "Net-(J1-Pad16)")
  (net 10 "Net-(J1-Pad15)")
  (net 11 "Net-(J1-Pad14)")
  (net 12 "Net-(J1-Pad13)")
  (net 13 "Net-(J1-Pad12)")
  (net 14 "Net-(J1-Pad11)")
  (net 15 "Net-(J1-Pad10)")
  (net 16 "Net-(J1-Pad9)")
  (net 17 "Net-(J1-Pad8)")
  (net 18 "Net-(J1-Pad7)")
  (net 19 "Net-(J1-Pad6)")
  (net 20 "Net-(J1-Pad5)")
  (net 21 "Net-(J1-Pad4)")
  (net 22 "Net-(J1-Pad3)")
  (net 23 "Net-(J1-Pad2)")
  (net 24 "Net-(J1-Pad1)")
  (net 25 "Net-(J2-Pad16)")
  (net 26 "Net-(J2-Pad15)")
  (net 27 "Net-(J2-Pad14)")
  (net 28 "Net-(J2-Pad13)")
  (net 29 "Net-(J2-Pad12)")
  (net 30 "Net-(J2-Pad11)")
  (net 31 "Net-(J2-Pad10)")
  (net 32 "Net-(J2-Pad9)")
  (net 33 "Net-(J2-Pad8)")
  (net 34 "Net-(J2-Pad7)")
  (net 35 "Net-(J2-Pad6)")
  (net 36 "Net-(J2-Pad5)")
  (net 37 "Net-(J2-Pad4)")
  (net 38 "Net-(J2-Pad3)")
  (net 39 "Net-(J2-Pad2)")
  (net 40 "Net-(J2-Pad1)")
  (net 41 "Net-(J3-Pad24)")
  (net 42 "Net-(J3-Pad23)")
  (net 43 "Net-(J3-Pad22)")
  (net 44 "Net-(J3-Pad21)")
  (net 45 "Net-(J3-Pad20)")
  (net 46 "Net-(J3-Pad19)")
  (net 47 "Net-(J3-Pad18)")
  (net 48 "Net-(J3-Pad17)")
  (net 49 "Net-(J3-Pad16)")
  (net 50 "Net-(J3-Pad15)")
  (net 51 "Net-(J3-Pad14)")
  (net 52 "Net-(J3-Pad13)")
  (net 53 "Net-(J3-Pad12)")
  (net 54 "Net-(J3-Pad11)")
  (net 55 "Net-(J3-Pad10)")
  (net 56 "Net-(J3-Pad9)")
  (net 57 "Net-(J3-Pad8)")
  (net 58 "Net-(J3-Pad7)")
  (net 59 "Net-(J3-Pad6)")
  (net 60 "Net-(J3-Pad5)")
  (net 61 "Net-(J3-Pad4)")
  (net 62 "Net-(J3-Pad3)")
  (net 63 "Net-(J3-Pad2)")
  (net 64 "Net-(J3-Pad1)")
  (net 65 "Net-(J4-Pad16)")
  (net 66 "Net-(J4-Pad15)")
  (net 67 "Net-(J4-Pad14)")
  (net 68 "Net-(J4-Pad13)")
  (net 69 "Net-(J4-Pad12)")
  (net 70 "Net-(J4-Pad11)")
  (net 71 "Net-(J4-Pad10)")
  (net 72 "Net-(J4-Pad9)")
  (net 73 "Net-(J4-Pad8)")
  (net 74 "Net-(J4-Pad7)")
  (net 75 "Net-(J4-Pad6)")
  (net 76 "Net-(J4-Pad5)")
  (net 77 "Net-(J4-Pad4)")
  (net 78 "Net-(J4-Pad3)")
  (net 79 "Net-(J4-Pad2)")
  (net 80 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad18)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad20)")
    (add_net "Net-(J3-Pad21)")
    (add_net "Net-(J3-Pad22)")
    (add_net "Net-(J3-Pad23)")
    (add_net "Net-(J3-Pad24)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad15)")
    (add_net "Net-(J4-Pad16)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
  )
  (module IGG_64_breakout:wyatt_negative_big (layer B.Cu) (tedit 0)
    (at 151 74 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 166 93)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 11 0) (layer Dwgs.User))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 136 93)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at -9 1) (layer Dwgs.User))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 136 56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at -4 -9) (layer Dwgs.User))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 166 56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 9 -1) (layer Dwgs.User))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 142 57 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x16 (at 1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J4-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J4-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J4-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J4-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J4-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J4-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J4-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J4-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(J4-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:PQFP-80_14x20mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 150.65 74.25)
    (descr "PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at -0.05 -3.05) (layer F.SilkS))
    (fp_text value PQFP-80 (at 0 12.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 80 smd rect (at -6 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(J4-Pad1)"))
    (pad 79 smd rect (at -5.2 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(J4-Pad2)"))
    (pad 78 smd rect (at -4.4 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(J4-Pad3)"))
    (pad 77 smd rect (at -3.6 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(J4-Pad4)"))
    (pad 76 smd rect (at -2.8 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(J4-Pad5)"))
    (pad 75 smd rect (at -2 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(J4-Pad6)"))
    (pad 74 smd rect (at -1.2 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J4-Pad7)"))
    (pad 73 smd rect (at -0.4 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J4-Pad8)"))
    (pad 72 smd rect (at 0.4 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J4-Pad9)"))
    (pad 71 smd rect (at 1.2 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J4-Pad10)"))
    (pad 70 smd rect (at 2 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J4-Pad11)"))
    (pad 69 smd rect (at 2.8 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J4-Pad12)"))
    (pad 68 smd rect (at 3.6 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J4-Pad13)"))
    (pad 67 smd rect (at 4.4 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J4-Pad14)"))
    (pad 66 smd rect (at 5.2 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J4-Pad15)"))
    (pad 65 smd rect (at 6 -11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J4-Pad16)"))
    (pad 64 smd rect (at 8.15 -9.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(J3-Pad1)"))
    (pad 63 smd rect (at 8.15 -8.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J3-Pad2)"))
    (pad 62 smd rect (at 8.15 -7.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J3-Pad3)"))
    (pad 61 smd rect (at 8.15 -6.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J3-Pad4)"))
    (pad 60 smd rect (at 8.15 -6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J3-Pad5)"))
    (pad 59 smd rect (at 8.15 -5.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J3-Pad6)"))
    (pad 58 smd rect (at 8.15 -4.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J3-Pad7)"))
    (pad 57 smd rect (at 8.15 -3.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J3-Pad8)"))
    (pad 56 smd rect (at 8.15 -2.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J3-Pad9)"))
    (pad 55 smd rect (at 8.15 -2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J3-Pad10)"))
    (pad 54 smd rect (at 8.15 -1.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J3-Pad11)"))
    (pad 53 smd rect (at 8.15 -0.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J3-Pad12)"))
    (pad 52 smd rect (at 8.15 0.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J3-Pad13)"))
    (pad 51 smd rect (at 8.15 1.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J3-Pad14)"))
    (pad 50 smd rect (at 8.15 2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J3-Pad15)"))
    (pad 49 smd rect (at 8.15 2.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J3-Pad16)"))
    (pad 48 smd rect (at 8.15 3.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J3-Pad17)"))
    (pad 47 smd rect (at 8.15 4.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J3-Pad18)"))
    (pad 46 smd rect (at 8.15 5.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J3-Pad19)"))
    (pad 45 smd rect (at 8.15 6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J3-Pad20)"))
    (pad 44 smd rect (at 8.15 6.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J3-Pad21)"))
    (pad 43 smd rect (at 8.15 7.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J3-Pad22)"))
    (pad 42 smd rect (at 8.15 8.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J3-Pad23)"))
    (pad 41 smd rect (at 8.15 9.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J3-Pad24)"))
    (pad 40 smd rect (at 6 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J2-Pad1)"))
    (pad 39 smd rect (at 5.2 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J2-Pad2)"))
    (pad 38 smd rect (at 4.4 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad3)"))
    (pad 37 smd rect (at 3.6 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad4)"))
    (pad 36 smd rect (at 2.8 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J2-Pad5)"))
    (pad 35 smd rect (at 2 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad6)"))
    (pad 34 smd rect (at 1.2 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad7)"))
    (pad 33 smd rect (at 0.4 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J2-Pad8)"))
    (pad 32 smd rect (at -0.4 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J2-Pad9)"))
    (pad 31 smd rect (at -1.2 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad10)"))
    (pad 30 smd rect (at -2 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad11)"))
    (pad 29 smd rect (at -2.8 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad12)"))
    (pad 28 smd rect (at -3.6 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-Pad13)"))
    (pad 27 smd rect (at -4.4 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad14)"))
    (pad 26 smd rect (at -5.2 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad15)"))
    (pad 25 smd rect (at -6 11.15 90) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad16)"))
    (pad 24 smd rect (at -8.15 9.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-Pad1)"))
    (pad 23 smd rect (at -8.15 8.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad2)"))
    (pad 22 smd rect (at -8.15 7.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad3)"))
    (pad 21 smd rect (at -8.15 6.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad 20 smd rect (at -8.15 6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (pad 19 smd rect (at -8.15 5.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad6)"))
    (pad 18 smd rect (at -8.15 4.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad7)"))
    (pad 17 smd rect (at -8.15 3.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad8)"))
    (pad 16 smd rect (at -8.15 2.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad9)"))
    (pad 15 smd rect (at -8.15 2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad10)"))
    (pad 14 smd rect (at -8.15 1.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad11)"))
    (pad 13 smd rect (at -8.15 0.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad12)"))
    (pad 12 smd rect (at -8.15 -0.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad13)"))
    (pad 11 smd rect (at -8.15 -1.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 10 smd rect (at -8.15 -2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad15)"))
    (pad 9 smd rect (at -8.15 -2.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad16)"))
    (pad 8 smd rect (at -8.15 -3.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad17)"))
    (pad 7 smd rect (at -8.15 -4.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad18)"))
    (pad 6 smd rect (at -8.15 -5.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad19)"))
    (pad 5 smd rect (at -8.15 -6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad20)"))
    (pad 4 smd rect (at -8.15 -6.8) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad21)"))
    (pad 3 smd rect (at -8.15 -7.6) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad22)"))
    (pad 2 smd rect (at -8.15 -8.4) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad23)"))
    (pad 1 smd rect (at -8.15 -9.2) (size 1.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad24)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 165 61)
    (descr "Through hole straight pin header, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x12 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x24 (at 1.27 30.27) (layer F.Fab))
    (fp_text user %R (at 1.27 13.97 90) (layer F.Fab))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad24)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad22)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad21)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J3-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J3-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J3-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J3-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J3-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J3-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J3-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J3-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J3-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J3-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J3-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J3-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 160 92 270)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x16 (at 1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137 88.7 180)
    (descr "Through hole straight pin header, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x12 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x24 (at 1.27 30.27) (layer F.Fab))
    (fp_text user %R (at 1.27 13.97 90) (layer F.Fab))
    (pad 24 thru_hole oval (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad24)"))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad22)"))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad21)"))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text NC (at 154.9 90) (layer F.SilkS))
  (gr_text NC (at 155.1 96.4) (layer F.SilkS))
  (gr_text VPP (at 159.9 90) (layer F.SilkS))
  (gr_text DIOB (at 162.5 96) (layer F.SilkS))
  (gr_text LE (at 157.4 90) (layer F.SilkS))
  (gr_text CLK (at 157.5 96.4) (layer F.SilkS))
  (gr_text NC (at 144.9 90) (layer F.SilkS))
  (gr_text NC (at 144.7 96.4) (layer F.SilkS))
  (gr_text HVGND (at 152.3 90) (layer F.SilkS))
  (gr_text GND (at 152.3 96.4) (layer F.SilkS))
  (gr_text DIR (at 149.8 90) (layer F.SilkS))
  (gr_text VDD (at 149.9 96.4) (layer F.SilkS))
  (gr_text POL (at 147.3 90) (layer F.SilkS))
  (gr_text BL (at 147.3 96.4) (layer F.SilkS))
  (gr_text DIOA (at 139.5 93) (layer F.SilkS))
  (gr_text VPP (at 139.5 95.8) (layer F.SilkS))
  (gr_text "PQFP-80\n0.8mm" (at 151 74) (layer F.SilkS))
  (gr_text paulsc.how (at 151 60.5) (layer F.SilkS))
  (dimension 46 (width 0.15) (layer Dwgs.User)
    (gr_text "46.000 mm" (at 194.3 74 90) (layer Dwgs.User))
    (feature1 (pts (xy 159 51) (xy 193.586421 51)))
    (feature2 (pts (xy 159 97) (xy 193.586421 97)))
    (crossbar (pts (xy 193 97) (xy 193 51)))
    (arrow1a (pts (xy 193 51) (xy 193.586421 52.126504)))
    (arrow1b (pts (xy 193 51) (xy 192.413579 52.126504)))
    (arrow2a (pts (xy 193 97) (xy 193.586421 95.873496)))
    (arrow2b (pts (xy 193 97) (xy 192.413579 95.873496)))
  )
  (dimension 40 (width 0.15) (layer Dwgs.User)
    (gr_text "40.000 mm" (at 151 113.3) (layer Dwgs.User))
    (feature1 (pts (xy 171 77) (xy 171 112.586421)))
    (feature2 (pts (xy 131 77) (xy 131 112.586421)))
    (crossbar (pts (xy 131 112) (xy 171 112)))
    (arrow1a (pts (xy 171 112) (xy 169.873496 112.586421)))
    (arrow1b (pts (xy 171 112) (xy 169.873496 111.413579)))
    (arrow2a (pts (xy 131 112) (xy 132.126504 112.586421)))
    (arrow2b (pts (xy 131 112) (xy 132.126504 111.413579)))
  )
  (gr_text 79 (at 142 52) (layer F.SilkS))
  (gr_text 80 (at 142 59.5) (layer F.SilkS))
  (gr_text 65 (at 160 52) (layer F.SilkS))
  (gr_text 66 (at 160 59.5) (layer F.SilkS))
  (gr_text 64 (at 162.5 61) (layer F.SilkS))
  (gr_text 63 (at 170 61) (layer F.SilkS))
  (gr_text 42 (at 162.5 89) (layer F.SilkS))
  (gr_text 41 (at 170 89) (layer F.SilkS))
  (gr_text 39 (at 162.5 95) (layer F.SilkS))
  (gr_text 40 (at 162.5 91.5) (layer F.SilkS))
  (gr_text 25 (at 139.5 95) (layer F.SilkS))
  (gr_text 26 (at 139.5 92) (layer F.SilkS))
  (gr_text 24 (at 139.5 89) (layer F.SilkS))
  (gr_text 23 (at 132 89) (layer F.SilkS))
  (gr_text 2 (at 139.5 61) (layer F.SilkS))
  (gr_text 1 (at 132 60.5) (layer F.SilkS))
  (gr_text 24 (at 142.5 84.5) (layer F.SilkS))
  (gr_text 25 (at 143.5 85.5) (layer F.SilkS))
  (gr_text 40 (at 158 85.5) (layer F.SilkS))
  (gr_text 41 (at 159 84.5) (layer F.SilkS))
  (gr_text 64 (at 159 64) (layer F.SilkS))
  (gr_text 65 (at 158 63) (layer F.SilkS))
  (gr_text 80 (at 143.5 63) (layer F.SilkS))
  (gr_text 1 (at 142.5 64) (layer F.SilkS))
  (gr_line (start 139 51) (end 163 51) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131 89) (end 131 59) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139 97) (end 163 97) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171 89) (end 171 59) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 163 89) (end 163 97) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139 89) (end 131 89) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139 59) (end 139 51) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 163 59) (end 171 59) (angle -90) (layer Edge.Cuts) (width 0.05))
)
