(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 46)
    (no_connects 0)
    (area 99.899999 79.899999 118.100001 105.100001)
    (thickness 0.8)
    (drawings 28)
    (tracks 287)
    (zones 0)
    (modules 25)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.2)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.1 2.1)
    (pad_drill 2.1)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x20000_00000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(R4-Pad2)")
  (net 4 /VID_SWITCH)
  (net 5 "Net-(J1-Pad1)")
  (net 6 /VID_SENSE)
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J3-Pad3)")
  (net 9 /SCK)
  (net 10 /MISO)
  (net 11 /MOSI)
  (net 12 /RST)
  (net 13 "Net-(C5-Pad1)")
  (net 14 "Net-(Q1-Pad1)")
  (net 15 +5V)
  (net 16 /K3)
  (net 17 /K1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /K1)
    (add_net /K3)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net /VID_SENSE)
    (add_net /VID_SWITCH)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net VCC)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A5E0A42)
    (at 108 82)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask)
      (clearance 1))
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A5D079D)
    (at 110.67 86.59)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MAX4624/5 (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad3)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D0930)
    (at 107.82 98.02 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 10uf (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D0936)
    (at 107.81 99.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D090F)
    (at 107.86 87.03 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D091A)
    (at 106.3 87.03 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5E00A2)
    (at 112.42 101.47 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /K1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5E009C)
    (at 112.43 99.8 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /K3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5E00A5)
    (at 104.41 89.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /VID_SENSE))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5E004B)
    (at 109.26 90.23 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 5A5E0068)
    (at 107.75 94.06)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0.01 0.01) (layer F.SilkS))
    (fp_text value ATTINY15-1SC (at 0 3.68) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
    (pad 2 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R4-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (pad 4 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 6 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 7 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 8 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:USB_3_PADS (layer F.Cu) (tedit 5A5E0461)
    (at 102.23 81.09 180)
    (fp_text reference J1 (at 0.3 1.6 180) (layer F.SilkS) hide)
    (fp_text value EV100 (at 0.1 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.25 0 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 0 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.25 0 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /VID_SENSE))
  )
  (module KiCadCustomLibs:USB_3_PADS (layer F.Cu) (tedit 5A5E042A)
    (at 116.8 86.9 90)
    (fp_text reference J3 (at 0.3 1.6 90) (layer F.SilkS) hide)
    (fp_text value DVR_VIDEO (at 0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.25 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.25 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad3)"))
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 5A5E0466)
    (at 101.25 85.16 90)
    (fp_text reference J4 (at 0.1 1.8 90) (layer F.SilkS) hide)
    (fp_text value PWR (at 0.3 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 2 smd rect (at 0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 5A5E0441)
    (at 116.8 91 90)
    (fp_text reference J5 (at 0.1 1.8 90) (layer F.SilkS) hide)
    (fp_text value PWR_DVR (at 0.3 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module KiCadCustomLibs:Pads_prog_6pin1.25mm (layer F.Cu) (tedit 5A5E082B)
    (at 101.4 97.06 90)
    (fp_text reference J6 (at 0.5 2 90) (layer F.SilkS) hide)
    (fp_text value PROG (at 0 -2.25 90) (layer F.Fab) hide)
    (pad 6 smd oval (at 3.125 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd oval (at -3.125 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 5 smd oval (at 1.875 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -1.875 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 3 smd oval (at -0.625 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 4 smd oval (at 0.625 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A5E0A4E)
    (at 116.5 103)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask)
      (clearance 1))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5E1569)
    (at 114.3 90.8 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 22uf (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 5AB389E5)
    (at 116.9 98.5 270)
    (fp_text reference J2 (at 0.16 -3.76 270) (layer F.SilkS) hide)
    (fp_text value Buttons (at 0.3 -1.6 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 /K3))
    (pad 2 smd rect (at 0.9 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 /K1))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5AB38A4F)
    (at 115.9 94.8)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value "AO3415 (P)" (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB38BC7)
    (at 111.99 90.22)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB39C57)
    (at 113.2 94.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 5AB3AA99)
    (at 102.5 89.12 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value B5819WS (at 0.1 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB56501)
    (at 106.55 90.23 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB56516)
    (at 112.44 98.15 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 47K (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text V1.0 (at 110.59 103.96) (layer F.SilkS))
  (gr_line (start 114 80) (end 100 80) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 114 83.5) (end 118 83.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 114 80) (end 114 83.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_text 4-5V (at 103.91 85.15 270) (layer F.SilkS))
  (gr_text "nppc\n2018" (at 111.94 103.04) (layer B.SilkS))
  (gr_text EV100 (at 100.77 89.02 270) (layer F.SilkS))
  (gr_text DVR (at 116.4 84.3) (layer F.SilkS))
  (gr_text Vout (at 114.92 85.68) (layer F.SilkS))
  (gr_text Vin (at 115.31 88.09) (layer F.SilkS))
  (gr_text SigG (at 101.3 82.5) (layer F.SilkS))
  (gr_text VidG (at 105.1 81.1) (layer F.SilkS))
  (gr_text - (at 115.5 90.1 90) (layer F.SilkS))
  (gr_text - (at 102.5 84.2 90) (layer F.SilkS))
  (gr_text + (at 115.5 92.51) (layer F.SilkS))
  (gr_text + (at 102.6 86) (layer F.SilkS))
  (gr_text + (at 101.4 92.6) (layer F.SilkS))
  (gr_text SCK (at 103.8 97.8) (layer F.SilkS))
  (gr_text MISO (at 103.8 99) (layer F.SilkS))
  (gr_text MOSI (at 103.8 100.2) (layer F.SilkS))
  (gr_text K3 (at 115.55 97.6) (layer F.SilkS))
  (gr_text K1 (at 115.54 99.4) (layer F.SilkS))
  (gr_line (start 108.5 105) (end 118 105) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.5 101) (end 100 101) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 108.5 101) (end 106.5 101) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 108.5 105) (end 108.5 101) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 118 83.5) (end 118 105) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 101) (end 100 80) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 99 79) (xy 119 79) (xy 119 106) (xy 99 106)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 100 105) (xy 120 105) (xy 120 80) (xy 100 80)
      )
    )
  )
)
