(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 0.9346)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0711)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.762)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0711)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VOUT")
	(net 2 "GND")
	(net 3 "/vchg")
	(net 4 "/vsw")
	(net 5 "/btn_led")
	(net 6 "/vbuf")
	(net 7 "Net-(J1-Pin_5)")
	(net 8 "VIN")
	(net 9 "/vgate")
	(net 10 "/vfb")
	(net 11 "/vinv")
	(net 12 "unconnected-(U1-NC-Pad1)")
	(net 13 "unconnected-(U2-NC-Pad1)")
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 119 106.5 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 10 "/vfb")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 7 "Net-(J1-Pin_5)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 119 83 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.25 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u, 50V"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 8 "VIN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "My_Footprints:AMASS_XT90PW-M_1x02_P10.90mm_Horizontal"
		(layer "F.Cu")
		(at 111.5 97.95 90)
		(descr "Connector XT90 Horizontal PCB Male  500V 30A IP40, https://www.bto.pl/pdf/09025/XT90PW-M.pdf")
		(tags "RC")
		(property "Reference" "J2"
			(at 16.25 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "XT90 SMT Male"
			(at 3.6 4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr through_hole)
		(fp_text user "-"
			(at -3.9 2.5 90)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at 15.3 2.5 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.449999 -8.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 10.9 0 90)
			(size 7.2 7.2)
			(drill 3.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 8 "VIN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 0 90)
			(size 7.2 7.2)
			(drill 3.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -4 -9.4 90)
			(size 1.6 2.7)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 14.9 -9.4 90)
			(size 1.6 2.7)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT90PW-M_1x02_P10.90mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5"
		(layer "F.Cu")
		(at 119 96.7)
		(descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at -3 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "BU4S584G2"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1gu04.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Inverter Gate, SOT-553"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT*553*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "unconnected-(U2-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/vbuf")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/vinv")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "VIN")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 135 97 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -3.4625 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.83 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 3 "/vchg")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 4 "/vsw")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 135 100.5)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 3.525 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u, 50V"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "/vchg")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 123.25 91 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 3.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1Meg"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 8 "VIN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 9 "/vgate")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 135 104)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1Meg"
			(at 0 1.83 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 3 "/vchg")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 119 101.5 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1Meg"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 11 "/vinv")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 270)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 10 "/vfb")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:PowerPAK_SO-8_Single"
		(layer "F.Cu")
		(at 128.5 87.75)
		(descr "PowerPAK SO-8 Single (https://www.vishay.com/docs/71655/powerpak.pdf, https://www.vishay.com/docs/72599/72599.pdf)")
		(tags "PowerPAK SO-8 Single")
		(property "Reference" "Q1"
			(at -2 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Si7141DP"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.vishay.com/docs/65596/si7141dp.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-60A Id, -20V Vds, 1.9 mOhm Ron, PowerPAK-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PowerPAK*SO*Single*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.67 -1.905)
			(size 1.27 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "VIN")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.67 -0.635)
			(size 1.27 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "VIN")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.67 0.635)
			(size 1.27 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "VIN")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.67 1.905)
			(size 1.27 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/vgate")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0.69 0)
			(size 3.81 3.91)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "VOUT")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.795 -1.905)
			(size 1.02 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "VOUT")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.795 -0.635)
			(size 1.02 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "VOUT")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.795 0.635)
			(size 1.02 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "VOUT")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.795 1.905)
			(size 1.02 0.61)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "VOUT")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 135 107.5 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.83 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 1 "VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 5 "/btn_led")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 138 83 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.25 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u, 50V"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD"
		(layer "F.Cu")
		(at 126.5 105)
		(descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x03 2.54mm double row")
		(property "Reference" "J1"
			(at -1 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x03_Odd_Even"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.525 -2.54)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/vbuf")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.525 -2.54)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/vchg")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.525 0)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.525 0)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/btn_led")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.525 2.54)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.525 2.54)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/vsw")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5"
		(layer "F.Cu")
		(at 119 92.7)
		(descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at -3 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "BU4S584G2"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1gu04.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Inverter Gate, SOT-553"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT*553*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "unconnected-(U1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/vfb")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/vbuf")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "VIN")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "My_Footprints:AMASS_XT90PW-F_1x02_P10.90mm_Horizontal"
		(layer "F.Cu")
		(at 144 87.1 -90)
		(descr "Connector XT90 Horizontal PCB Female  500V 30A IP40, https://www.bto.pl/pdf/09025/XT90PW-F.pdf")
		(tags "RC")
		(property "Reference" "J3"
			(at -5.6 1 90)
			(layer "F.SilkS")
		)
		(property "Value" "XT90 SMT Female"
			(at 3.6 4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -4.5 2.5 90)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 14.7 2.5 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.449999 -8.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 7.2 7.2)
			(drill 3.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 1 "VOUT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 10.9 0 270)
			(size 7.2 7.2)
			(drill 3.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -4 -8.9 270)
			(size 1.6 2.7)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 14.9 -8.9 270)
			(size 1.6 2.7)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT90PW-M_1x02_P10.90mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 134 83 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.25 -1.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "1Meg"
			(at 0 1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 1 "VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 129.0625 98 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at -0.9375 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "2N7002BK"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Nexperia 60 V, 300 mA dual N-channel Trench MOSFET"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "RPS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/vsw")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/vgate")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen"
		(layer "B.Cu")
		(at 129 96 180)
		(descr "Open Source Hardware Logo")
		(tags "Logo OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo_5.7x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Symbol:ESD-Logo_6.6x6mm_SilkScreen"
		(layer "B.Cu")
		(at 122 96 180)
		(descr "Electrostatic discharge Logo")
		(tags "Logo ESD")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "ESD-Logo_6.6x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(footprint "Symbol:KiCad-Logo2_6mm_SilkScreen"
		(layer "B.Cu")
		(at 128 103 180)
		(descr "KiCad Logo")
		(tags "Logo KiCad")
		(property "Reference" "REF**"
			(at 0 5.08 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "KiCad-Logo2_6mm_SilkScreen"
			(at 0 -6.35 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(footprint "Symbol:WEEE-Logo_4.2x6mm_SilkScreen"
		(layer "B.Cu")
		(at 135 96 180)
		(descr "Waste Electrical and Electronic Equipment Directive")
		(tags "Logo WEEE")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "WEEE-Logo_4.2x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(gr_rect
		(start 99.5 80)
		(end 156 110)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "GD"
		(at 120.3 105.6 0)
		(layer "F.SilkS")
	)
	(gr_text "LE"
		(at 130.6 105.6 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 120.2 103.1 0)
		(layer "F.SilkS")
	)
	(gr_text "NO"
		(at 120.2 108.1 0)
		(layer "F.SilkS")
	)
	(gr_text "Male XT90"
		(at 103.1 96.44 90)
		(layer "F.SilkS")
	)
	(gr_text "Female XT90"
		(at 152.4 87.7 270)
		(layer "F.SilkS")
	)
	(gr_text "NO"
		(at 130.5 103.1 0)
		(layer "F.SilkS")
	)
	(gr_text "+12~16V\nMax 30A"
		(at 99.9 109.4 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 130.6 108.2 0)
		(layer "F.SilkS")
	)
	(gr_text "LOAD\n"
		(at 147.3 107.7 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 4)
		)
		(polygon
			(pts
				(xy 99.5 80) (xy 99.5 110) (xy 156 110) (xy 156 80)
			)
		)
	)
	(zone
		(net 1)
		(net_name "VOUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 5)
		)
		(polygon
			(pts
				(xy 127.5 83.5) (xy 127.5 92.5) (xy 150 92.5) (xy 150 83.5)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VIN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 5)
		)
		(polygon
			(pts
				(xy 106 83.5) (xy 126.5 83.5) (xy 126.5 91) (xy 117 91) (xy 115.5 93) (xy 106 93)
			)
		)
	)
	(zone
		(net 1)
		(net_name "VOUT")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 5)
		)
		(polygon
			(pts
				(xy 127.5 83.5) (xy 150 83.5) (xy 150 92.5) (xy 127.5 92.5)
			)
		)
	)
	(zone
		(net 8)
		(net_name "VIN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 5)
		)
		(polygon
			(pts
				(xy 106 83.5) (xy 126.5 83.5) (xy 126.5 91) (xy 117 91) (xy 115.5 93) (xy 106 93)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 4)
		)
		(polygon
			(pts
				(xy 99.5 80) (xy 99.5 110) (xy 156 110) (xy 156 80)
			)
		)
	)
	(embedded_fonts no)
)
