(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 149)
    (zones 0)
    (modules 30)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(B1-Pad1)")
  (net 2 "Net-(B1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(B1-Pad5)")
  (net 5 "Net-(B1-Pad6)")
  (net 6 "Net-(B1-Pad7)")
  (net 7 "Net-(B1-Pad8)")
  (net 8 "Net-(B1-Pad9)")
  (net 9 "Net-(B1-Pad10)")
  (net 10 "Net-(B1-Pad11)")
  (net 11 "Net-(B1-Pad12)")
  (net 12 "Net-(B1-Pad13)")
  (net 13 "Net-(B1-Pad14)")
  (net 14 "Net-(B1-Pad15)")
  (net 15 "Net-(B1-Pad16)")
  (net 16 "Net-(B1-Pad17)")
  (net 17 "Net-(B1-Pad18)")
  (net 18 "Net-(B1-Pad19)")
  (net 19 "Net-(B1-Pad20)")
  (net 20 +5V)
  (net 21 "Net-(B1-Pad22)")
  (net 22 "Net-(B1-Pad24)")
  (net 23 +12V)
  (net 24 "Net-(D2-Pad2)")
  (net 25 "Net-(D3-Pad2)")
  (net 26 "Net-(F1-Pad2)")
  (net 27 "Net-(Q1-Pad1)")
  (net 28 "Net-(Q2-Pad1)")
  (net 29 "Net-(C3-Pad1)")
  (net 30 "Net-(J3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B1-Pad10)")
    (add_net "Net-(B1-Pad11)")
    (add_net "Net-(B1-Pad12)")
    (add_net "Net-(B1-Pad13)")
    (add_net "Net-(B1-Pad14)")
    (add_net "Net-(B1-Pad15)")
    (add_net "Net-(B1-Pad16)")
    (add_net "Net-(B1-Pad17)")
    (add_net "Net-(B1-Pad18)")
    (add_net "Net-(B1-Pad19)")
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(B1-Pad20)")
    (add_net "Net-(B1-Pad22)")
    (add_net "Net-(B1-Pad24)")
    (add_net "Net-(B1-Pad5)")
    (add_net "Net-(B1-Pad6)")
    (add_net "Net-(B1-Pad7)")
    (add_net "Net-(B1-Pad8)")
    (add_net "Net-(B1-Pad9)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
  )
  (net_class 12V ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(F1-Pad2)")
  )
  (net_class 5V ""
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(J3-Pad3)")
  )
  (module Connector_BarrelJack:BarrelJack_CUI_PJ-102AH_Horizontal (layer F.Cu) (tedit 5BB98D54)
    (at -1038.86 -121.92 180)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J2 (at 5.75 8.45 270) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -5.5 6.2 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 26 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 0 6 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 4.7 3 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6F1)
    (at -1054.1 -120.65)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10uF (at 3.81 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boards:SPARKFUN_PRO_MICRO (layer F.Cu) (tedit 200000)
    (at -1062.99 -116.84 90)
    (descr "SPARKFUN PRO MICO FOOTPRINT (WITH USB CONNECTOR)")
    (tags "SPARKFUN PRO MICO FOOTPRINT (WITH USB CONNECTOR)")
    (attr virtual)
    (fp_text reference B1 (at 0 16.51 90) (layer F.SilkS))
    (fp_text value SPARKFUN_PRO_MICRO (at 0 15.24 90) (layer F.SilkS))
    (fp_text user USB (at -0.0508 -16.9164 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at -7.62 -12.7 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -7.62 -10.16 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -7.62 -7.62 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -7.62 -5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -7.62 -2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(B1-Pad5)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at -7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(B1-Pad6)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -7.62 2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(B1-Pad7)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -7.62 5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad8)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -7.62 7.62 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(B1-Pad9)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -7.62 10.16 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(B1-Pad10)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -7.62 12.7 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(B1-Pad11)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -7.62 15.24 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(B1-Pad12)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 7.62 15.24 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(B1-Pad13)") (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 7.62 12.7 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(B1-Pad14)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 7.62 10.16 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(B1-Pad15)") (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 7.62 7.62 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(B1-Pad16)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 7.62 5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(B1-Pad17)") (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 7.62 2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(B1-Pad18)") (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(B1-Pad19)") (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 7.62 -2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(B1-Pad20)") (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 7.62 -5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 +5V) (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 7.62 -7.62 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(B1-Pad22)") (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 7.62 -10.16 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 7.62 -12.7 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(B1-Pad24)") (solder_mask_margin 0.1016))
  )
  (module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 5BB9A753)
    (at -1026.16 -119.38 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 16V4700 (at 11.43 5.08) (layer F.Fab) hide)
    (fp_text user %R (at 3.75 0) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6EE)
    (at -1054.1 -116.84 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 10uF (at -3.81 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 29 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5BB9A6BB)
    (at -1037.59 -116.84)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.08 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5BB9A6A0)
    (at -1007.11 -120.65 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 0 2.1 180) (layer F.Fab) hide)
    (fp_text user %R (at -3.81 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 5BB9A6A3)
    (at -993.14 -120.65)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at -3.81 0) (layer F.SilkS))
    (fp_text value 1N4007 (at 0 2.1) (layer F.Fab) hide)
    (fp_text user %R (at -3.81 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5BB9A69D)
    (at -1014.73 -120.65 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value Fuse (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 +12V))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5BB9A74B)
    (at -1024.89 -130.81 180)
    (descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J1 (at 2.54 1.27 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 0 5.08 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 3.2 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5BB98D14)
    (at -1070.61 -133.35 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 7.62 270) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(B1-Pad20)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5BB98D18)
    (at -1059.18 -133.35 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 7.62 270) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(B1-Pad19)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5BB98D1C)
    (at -1047.75 -133.35 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 7.62 270) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(B1-Pad18)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5BB9A742)
    (at -1013.46 -113.03)
    (descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J7 (at -5.08 5.08) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at -3.81 5.08) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 3.2) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 5.08 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 +12V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5BB9A746)
    (at -1000.76 -113.03)
    (descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J8 (at 10.16 -5.08) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.81 5.08) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 3.2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BB9A6AA)
    (at -1012.19 -124.46)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 2.54 -4.27) (layer F.SilkS))
    (fp_text value IRF540N (at 2.54 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BB9A6A8)
    (at -996.95 -124.46)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -4.27) (layer F.SilkS))
    (fp_text value IRF540N (at 2.54 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6B3)
    (at -1017.27 -127)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at -2.54 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 "Net-(B1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6CF)
    (at -1002.03 -127)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(B1-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6B6)
    (at -1017.27 -124.46 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 300 (at 2.54 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 "Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 "Net-(B1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6D2)
    (at -1002.03 -124.46 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 300 (at 0 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 28 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(B1-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5BB9A73F)
    (at -1061.72 -116.84 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value NCP1117-5.0_SOT223 (at -3.81 -2.54 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5BB9A6EB)
    (at -1054.1 -113.03)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F2 (at 3.81 0) (layer F.SilkS))
    (fp_text value Fuse (at 3.81 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5BB9A6E2)
    (at -1042.67 -116.84)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at -2.54 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(B1-Pad9)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6DA)
    (at -1037.59 -113.03 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 300 (at -3.81 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5BB9A6DD)
    (at -1037.59 -110.49)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 2.54) (layer F.SilkS))
    (fp_text value 10K (at 3.81 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(B1-Pad9)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5BB9AD16)
    (at -990.6 -133.35)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at -5.08 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at -5.08 -1.27) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5BB9AD1A)
    (at -1076.96 -113.03)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 5.08 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 -1.27) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5BB9ADEE)
    (at -990.6 -109.22)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5BB9ADE5)
    (at -1076.96 -128.27)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_line (start -988.06 -135.89) (end -1079.5 -135.89) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -988.06 -106.68) (end -988.06 -135.89) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -1079.5 -106.68) (end -988.06 -106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -1079.5 -135.89) (end -1079.5 -106.68) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1079.5 -135.89) (xy -1079.5 -106.68) (xy -988.06 -106.68) (xy -988.06 -135.89)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1079.5 -135.89) (xy -1079.5 -106.68) (xy -988.06 -106.68) (xy -988.06 -135.89)
      )
    )
  )
)
