(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 49)
    (no_connects 0)
    (area 121.252857 86.02 182.277143 120.455)
    (thickness 1.6)
    (drawings 26)
    (tracks 226)
    (zones 0)
    (modules 24)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 GND)
  (net 6 "Net-(C10-Pad2)")
  (net 7 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585B2788)
    (at 140.97 103.505 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value C_Small (at 1.27 15.875 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585B2B69)
    (at 146.05 103.505 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 7.62 -20.955 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585B278B)
    (at 151.765 103.505 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value C_Small (at -4.445 26.035 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585B2B8E)
    (at 157.48 103.505 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 0.635 20.955 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585B277C)
    (at 140.97 102.235 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 1.905 16.51 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.27 16.51 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585B277F)
    (at 146.05 104.775 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 1.27 -20.955 90) (layer F.SilkS))
    (fp_text value C_Small (at 1.905 -20.32 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585B2758)
    (at 151.765 102.235 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 0.635 -26.67 270) (layer F.SilkS))
    (fp_text value C_Small (at 2.54 26.67 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 585B2774)
    (at 133.985 103.505 270)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P1 (at 1.27 9.525 270) (layer F.SilkS))
    (fp_text value BNC (at 1.27 8.89 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 smd rect (at 2.54 1.778 270) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at 0 1.524 270) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -2.54 1.778 270) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 2.54 1.778 270) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -2.54 1.778 270) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 585B2736)
    (at 169.545 103.505 90)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P2 (at -0.635 8.89 90) (layer F.SilkS))
    (fp_text value BNC (at 0.635 8.89 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 smd rect (at 2.54 1.778 90) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at 0 1.524 90) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -2.54 1.778 90) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 2.54 1.778 90) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -2.54 1.778 90) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585B275C)
    (at 157.48 104.775 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 1.27 20.955 90) (layer F.SilkS))
    (fp_text value C_Small (at 1.905 20.955 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585B273A)
    (at 162.56 102.235 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 1.27 -15.875 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.27 -15.24 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585B2B6C)
    (at 138.43 98.425)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L1 (at -1.27 -0.635) (layer F.SilkS))
    (fp_text value L_Small (at 3.81 -10.795) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585B2880)
    (at 153.67 108.585 180)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L2 (at 11.43 -0.635 180) (layer F.SilkS))
    (fp_text value L_Small (at 6.35 -10.795 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585B2883)
    (at 149.86 98.425)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L3 (at 11.43 -0.635) (layer F.SilkS))
    (fp_text value L_Small (at 7.62 -10.795) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585B2887)
    (at 165.1 108.585 180)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L4 (at -1.27 -0.635 180) (layer F.SilkS))
    (fp_text value L_Small (at 3.81 -10.795 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585B26ED)
    (at 143.51 95.885 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L5 (at -0.635 -20.32 90) (layer F.SilkS))
    (fp_text value L_Small (at 0.635 -20.32 90) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585B2C5C)
    (at 148.59 111.125 270)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L6 (at 0 24.13 270) (layer F.SilkS))
    (fp_text value L_Small (at 1.27 23.495 270) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585B2C61)
    (at 154.94 95.885 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L7 (at 0.635 24.13 90) (layer F.SilkS))
    (fp_text value L_Small (at 0.635 25.4 90) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585B271C)
    (at 160.02 111.125 270)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L8 (at -0.635 -20.32 270) (layer F.SilkS))
    (fp_text value L_Small (at 0 -20.32 270) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585B278E)
    (at 162.56 103.505 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value C_Small (at -0.635 -16.51 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585B2A41)
    (at 172.72 92.71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -1.27 -5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585B2A49)
    (at 130.81 114.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585B2A45)
    (at 172.72 114.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 6.985 2.54) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585B2A72)
    (at 130.81 92.71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 3.81 -5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "mark@halibut.com  @SmittyHalibut" (at 134.62 90.17) (layer F.SilkS))
  (gr_text O (at 138.43 111.125) (layer B.Mask))
  (gr_text O (at 140.97 112.395) (layer B.Mask))
  (gr_text o (at 139.065 114.3) (layer B.Mask))
  (gr_text <>< (at 137.795 116.205) (layer B.Mask))
  (gr_text ><> (at 142.24 114.935) (layer B.Mask))
  (gr_text "HPF v1.1a" (at 134.62 114.935) (layer F.SilkS))
  (gr_text "BY-NC-SA 2016 Mark Smith" (at 134.62 116.84) (layer F.SilkS))
  (gr_arc (start 129.54 115.57) (end 129.54 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 173.99 115.57) (end 176.53 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 173.99 91.44) (end 173.99 88.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 129.54 91.44) (end 127 91.44) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 99.695) (end 127 91.44) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 99.695) (end 127 99.695) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 107.315) (end 129.54 99.695) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 107.315) (end 129.54 107.315) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 115.57) (end 127 107.315) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.99 118.11) (end 129.54 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 176.53 107.315) (end 176.53 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.99 107.315) (end 176.53 107.315) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.99 99.695) (end 173.99 107.315) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 176.53 99.695) (end 173.99 99.695) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 176.53 91.44) (end 176.53 99.695) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 88.9) (end 173.99 88.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 88.9) (xy 176.53 88.9) (xy 176.53 118.11) (xy 127 118.11)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 88.9) (xy 176.53 88.9) (xy 176.53 118.11) (xy 127 118.11)
      )
    )
  )
)
