<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="63.5" y2="0" width="0" layer="20"/>
<wire x1="63.5" y1="0" x2="66.04" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="66.04" y1="2.54" x2="66.04" y2="35.56" width="0" layer="20"/>
<wire x1="66.04" y1="35.56" x2="63.5" y2="38.1" width="0" layer="20" curve="90"/>
<wire x1="63.5" y1="38.1" x2="2.54" y2="38.1" width="0" layer="20"/>
<wire x1="2.54" y1="38.1" x2="0" y2="35.56" width="0" layer="20" curve="90"/>
<wire x1="0" y1="35.56" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<text>3V</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>5V</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>5V</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>5V</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>5V</text>
<text>SDA</text>
<text>SCL</text>
<text>3V</text>
<text>5V</text>
<text>GND</text>
<text>GP4</text>
<text>TX</text>
<text>Raspberry Pi
Edition</text>
<text>T.I.C.K.</text>
<text>by schizobovine
&lt;sean@yak.net&gt;</text>
<text>&gt;VERSION</text>
<text>&gt;VERSION</text>
<text>(T)erribly
(I)lluminated
(C)hronology
(K)eeper</text>
<text>Raspberry Pi
Edition</text>
<text>T.I.C.K.</text>
<text>(T)erribly
(I)lluminated
(C)hronology
(K)eeper</text>
<text>by schizobovine
&lt;sean@yak.net&gt;</text>
<text>T.I.C.K.</text>
<text>T.I.C.K.</text>
<text>Raspberry Pi
Edition</text>
<text>Raspberry Pi
Edition</text>
</plain>
<libraries>
<library name="a_parts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="C0805-TIGHTER">
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="2X20_PTH">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="1X04-PTH-VERT">
</package>
<package name="1X05_PTH_CENTERED_RA_FEMALE">
</package>
<package name="2X4_PTH">
</package>
<package name="1X07">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v1.0"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="a_parts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v1.0"/>
<attribute name="DESIGNER" value="sean@yak.net"/>
</element>
<element name="R1" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="a_parts" package="2X20_PTH" value="RASPBERRYPI-40-PIN-GPIO-PTH">
<attribute name="NAME"/>
</element>
<element name="C1" library="a_parts" package="C0805-TIGHTER" value="10uF"/>
<element name="C2" library="a_parts" package="C0805-TIGHTER" value="1uF"/>
<element name="Q1" library="a_parts" package="SO08" value="N6040"/>
<element name="JP3" library="a_parts" package="1X04-PTH-VERT" value="M04PTH">
<attribute name="NAME"/>
</element>
<element name="R3" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="a_parts" package="1X05_PTH_CENTERED_RA_FEMALE" value="M05PTH-CENTERED-RA-FEMALE">
<attribute name="NAME"/>
</element>
<element name="JP4" library="a_parts" package="1X04-PTH-VERT" value="M04PTH">
<attribute name="NAME"/>
</element>
<element name="JP5" library="a_parts" package="1X04-PTH-VERT" value="M04PTH">
<attribute name="NAME"/>
</element>
<element name="JP7" library="a_parts" package="2X4_PTH" value="M04X2PTH"/>
<element name="JP6" library="a_parts" package="1X07" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP1" pad="25"/>
<contactref element="JP1" pad="20"/>
<contactref element="JP1" pad="14"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="30"/>
<contactref element="JP1" pad="34"/>
<contactref element="JP1" pad="39"/>
<contactref element="JP7" pad="6"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="3.3V">
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="17"/>
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="SDA_3V">
<contactref element="JP1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="SCL_3V">
<contactref element="JP1" pad="5"/>
<contactref element="Q1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="JP7" pad="5"/>
<contactref element="JP5" pad="4"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="JP7" pad="4"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP6" pad="4"/>
</signal>
<signal name="SDA_5V">
<contactref element="Q1" pad="8"/>
<contactref element="Q1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="SCL_5V">
<contactref element="Q1" pad="5"/>
<contactref element="Q1" pad="6"/>
<contactref element="R4" pad="1"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="8"/>
<contactref element="JP7" pad="8"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="GPIO4">
<contactref element="JP1" pad="7"/>
<contactref element="JP7" pad="7"/>
<contactref element="JP6" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
