<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="16.28875" y1="60.26668125" x2="32.623959375" y2="60.26668125" width="0" layer="20"/>
<wire x1="32.623959375" y1="60.26668125" x2="32.623959375" y2="60.274459375" width="0" layer="20"/>
<wire x1="32.623959375" y1="60.274459375" x2="32.623959375" y2="79.425540625" width="0" layer="20"/>
<wire x1="32.623959375" y1="79.425540625" x2="32.623959375" y2="79.43331875" width="0" layer="20"/>
<wire x1="32.623959375" y1="79.43331875" x2="16.28875" y2="79.43331875" width="0" layer="20"/>
<wire x1="16.28875" y1="79.43331875" x2="16.28875" y2="129.74576875" width="0" layer="20"/>
<wire x1="16.28875" y1="9.95423125" x2="16.28875" y2="60.26668125" width="0" layer="20"/>
<wire x1="16.28875" y1="129.74576875" x2="157.860559375" y2="129.74576875" width="0" layer="20"/>
<wire x1="157.860559375" y1="129.74576875" x2="157.860559375" y2="80.740140625" width="0" layer="20"/>
<wire x1="157.860559375" y1="80.740140625" x2="212.31125" y2="80.740140625" width="0" layer="20"/>
<wire x1="212.31125" y1="80.740140625" x2="212.31125" y2="58.959859375" width="0" layer="20"/>
<wire x1="212.31125" y1="58.959859375" x2="157.860559375" y2="58.959859375" width="0" layer="20"/>
<wire x1="157.860559375" y1="58.959859375" x2="157.860559375" y2="9.95423125" width="0" layer="20"/>
<wire x1="157.860559375" y1="9.95423125" x2="16.28875" y2="9.95423125" width="0" layer="20"/>
<wire x1="16.368359375" y1="60.274459375" x2="32.623959375" y2="60.274459375" width="0" layer="20"/>
<wire x1="16.368359375" y1="60.274459375" x2="16.28875" y2="60.26668125" width="0" layer="20"/>
<wire x1="32.623959375" y1="79.425540625" x2="16.368359375" y2="79.425540625" width="0" layer="20"/>
<wire x1="16.368359375" y1="79.425540625" x2="16.28875" y2="79.43331875" width="0" layer="20"/>
<hole x="43.5141" y="112.97495" drill="5.7912"/>
<hole x="43.5141" y="26.72505" drill="5.7912"/>
<hole x="23.035690625" y="84.55248125" drill="4.3688"/>
<hole x="23.035690625" y="55.14751875" drill="4.3688"/>
<hole x="24.456346875" y="121.578159375" drill="3.81"/>
<hole x="149.69295" y="121.578159375" drill="3.81"/>
<hole x="123.18275" y="87.54648125" drill="3.81"/>
<hole x="123.18275" y="52.15351875" drill="3.81"/>
<hole x="149.69295" y="18.124128125" drill="3.81"/>
<hole x="24.45635" y="18.121840625" drill="3.81"/>
<text>HOT</text>
<text>GND</text>
<text>THIS PCB DESIGNED FOR:</text>
<text>Sarah Blog</text>
<text>20K</text>
<text>20K</text>
<text>25M</text>
<text>25M</text>
</plain>
<libraries>
<library name="CONRADS">
<packages>
<package name="CONRADSNEW_V1G">
</package>
<package name="SLIMMOX102">
</package>
<package name="CONRADSNEW_OHMITE-TFSF(FLAT)-SERIES">
</package>
<package name="CONN5_1814832-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="CONRADS" package="CONRADSNEW_V1G" value="V1G"/>
<element name="R1" library="CONRADS" package="SLIMMOX102" value="OHMITE_SLIMMOX102"/>
<element name="R2" library="CONRADS" package="SLIMMOX102" value="OHMITE_SLIMMOX102"/>
<element name="R3" library="CONRADS" package="CONRADSNEW_OHMITE-TFSF(FLAT)-SERIES" value="TFSF_FLAT_RESISTOR"/>
<element name="R4" library="CONRADS" package="CONRADSNEW_OHMITE-TFSF(FLAT)-SERIES" value="TFSF_FLAT_RESISTOR"/>
<element name="U1" library="CONRADS" package="CONN5_1814832-1" value="5-1814832-1">
<attribute name="MANUFACTURER_PART_NUMBER" value="518148321"/>
<attribute name="VENDOR" value="TE Connectivity"/>
</element>
</elements>
<signals>
<signal name="HOT">
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="CVR_GND">
</signal>
<signal name="GND">
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="SWITCH_HOT">
<contactref element="R3" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="LV"/>
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
