(kicad_pcb (version 20171130) (host pcbnew 5.99.0+really5.1.12+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 105)
    (tracks 375)
    (zones 0)
    (modules 2)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad24)")
  (net 2 "Net-(J1-Pad22)")
  (net 3 "Net-(J1-Pad20)")
  (net 4 "Net-(J1-Pad18)")
  (net 5 "Net-(J1-Pad16)")
  (net 6 "Net-(J1-Pad14)")
  (net 7 "Net-(J1-Pad12)")
  (net 8 "Net-(J1-Pad10)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad6)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(J1-Pad2)")
  (net 13 /50)
  (net 14 /48)
  (net 15 /46)
  (net 16 /44)
  (net 17 /42)
  (net 18 /40)
  (net 19 /38)
  (net 20 /36)
  (net 21 /34)
  (net 22 /32)
  (net 23 /30)
  (net 24 /28)
  (net 25 /26)
  (net 26 /24)
  (net 27 /22)
  (net 28 /20)
  (net 29 /18)
  (net 30 /16)
  (net 31 /14)
  (net 32 /12)
  (net 33 /10)
  (net 34 /8)
  (net 35 /6)
  (net 36 /4)
  (net 37 /2)
  (net 38 "Net-(J1-Pad50)")
  (net 39 "Net-(J1-Pad48)")
  (net 40 "Net-(J1-Pad46)")
  (net 41 "Net-(J1-Pad44)")
  (net 42 "Net-(J1-Pad42)")
  (net 43 "Net-(J1-Pad40)")
  (net 44 "Net-(J1-Pad38)")
  (net 45 "Net-(J1-Pad36)")
  (net 46 "Net-(J1-Pad34)")
  (net 47 "Net-(J1-Pad32)")
  (net 48 "Net-(J1-Pad30)")
  (net 49 "Net-(J1-Pad28)")
  (net 50 "Net-(J1-Pad26)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /10)
    (add_net /12)
    (add_net /14)
    (add_net /16)
    (add_net /18)
    (add_net /2)
    (add_net /20)
    (add_net /22)
    (add_net /24)
    (add_net /26)
    (add_net /28)
    (add_net /30)
    (add_net /32)
    (add_net /34)
    (add_net /36)
    (add_net /38)
    (add_net /4)
    (add_net /40)
    (add_net /42)
    (add_net /44)
    (add_net /46)
    (add_net /48)
    (add_net /50)
    (add_net /6)
    (add_net /8)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad42)")
    (add_net "Net-(J1-Pad44)")
    (add_net "Net-(J1-Pad46)")
    (add_net "Net-(J1-Pad48)")
    (add_net "Net-(J1-Pad50)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
  )
  (module ll:10156001051100LF (layer F.Cu) (tedit 0)
    (at 597.2 98.1 270)
    (descr 10156001-051100LF-1)
    (tags Connector)
    (attr smd)
    (fp_text reference P1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 5-104652-5 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -6 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /2))
    (pad 2 smd rect (at -5.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /4))
    (pad 3 smd rect (at -5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /6))
    (pad 4 smd rect (at -4.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /8))
    (pad 5 smd rect (at -4 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /10))
    (pad 6 smd rect (at -3.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /12))
    (pad 7 smd rect (at -3 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /14))
    (pad 8 smd rect (at -2.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /16))
    (pad 9 smd rect (at -2 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /18))
    (pad 10 smd rect (at -1.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /20))
    (pad 11 smd rect (at -1 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /22))
    (pad 12 smd rect (at -0.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /24))
    (pad 13 smd rect (at 0 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /26))
    (pad 14 smd rect (at 0.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /28))
    (pad 15 smd rect (at 1 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /30))
    (pad 16 smd rect (at 1.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /32))
    (pad 17 smd rect (at 2 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /34))
    (pad 18 smd rect (at 2.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /36))
    (pad 19 smd rect (at 3 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /38))
    (pad 20 smd rect (at 3.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /40))
    (pad 21 smd rect (at 4 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /42))
    (pad 22 smd rect (at 4.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /44))
    (pad 23 smd rect (at 5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /46))
    (pad 24 smd rect (at 5.5 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /48))
    (pad 25 smd rect (at 6 -1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /50))
    (pad 26 smd rect (at 6 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J1-Pad50)"))
    (pad 27 smd rect (at 5.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1-Pad48)"))
    (pad 28 smd rect (at 5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1-Pad46)"))
    (pad 29 smd rect (at 4.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J1-Pad44)"))
    (pad 30 smd rect (at 4 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J1-Pad42)"))
    (pad 31 smd rect (at 3.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1-Pad40)"))
    (pad 32 smd rect (at 3 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad38)"))
    (pad 33 smd rect (at 2.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J1-Pad36)"))
    (pad 34 smd rect (at 2 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J1-Pad34)"))
    (pad 35 smd rect (at 1.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J1-Pad32)"))
    (pad 36 smd rect (at 1 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J1-Pad30)"))
    (pad 37 smd rect (at 0.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J1-Pad28)"))
    (pad 38 smd rect (at 0 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J1-Pad26)"))
    (pad 39 smd rect (at -0.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad24)"))
    (pad 40 smd rect (at -1 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad22)"))
    (pad 41 smd rect (at -1.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad20)"))
    (pad 42 smd rect (at -2 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad18)"))
    (pad 43 smd rect (at -2.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad16)"))
    (pad 44 smd rect (at -3 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 45 smd rect (at -3.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 46 smd rect (at -4 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 47 smd rect (at -4.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 48 smd rect (at -5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad6)"))
    (pad 49 smd rect (at -5.5 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 50 smd rect (at -6 1.8 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (model 10156001-051100LF.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x25_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A421)
    (at 587.8 67.6)
    (descr "Through hole straight socket strip, 2x25, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x25 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.77) (layer F.SilkS))
    (fp_text value Conn_02x25_Odd_Even (at -1.27 63.73) (layer F.Fab))
    (fp_text user %R (at -1.27 30.48 90) (layer F.Fab))
    (pad 50 thru_hole oval (at -2.54 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad50)"))
    (pad 49 thru_hole oval (at 0 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /50))
    (pad 48 thru_hole oval (at -2.54 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad48)"))
    (pad 47 thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /48))
    (pad 46 thru_hole oval (at -2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad46)"))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /46))
    (pad 44 thru_hole oval (at -2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad44)"))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /44))
    (pad 42 thru_hole oval (at -2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad42)"))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /42))
    (pad 40 thru_hole oval (at -2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-Pad40)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /40))
    (pad 38 thru_hole oval (at -2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad38)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /38))
    (pad 36 thru_hole oval (at -2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-Pad36)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /36))
    (pad 34 thru_hole oval (at -2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J1-Pad34)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /34))
    (pad 32 thru_hole oval (at -2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J1-Pad32)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /32))
    (pad 30 thru_hole oval (at -2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J1-Pad30)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /30))
    (pad 28 thru_hole oval (at -2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad28)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /28))
    (pad 26 thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J1-Pad26)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /26))
    (pad 24 thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad24)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /24))
    (pad 22 thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad22)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /22))
    (pad 20 thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /20))
    (pad 18 thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /18))
    (pad 16 thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /16))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /14))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /12))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /10))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /8))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /6))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /4))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /2))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x25_P2.54mm_Vertical
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text P19 (at 591.2 113.4) (layer B.SilkS))
  (gr_text P18 (at 591.2 110.9) (layer B.SilkS))
  (gr_text P29 (at 581.8 121) (layer B.SilkS))
  (gr_text P33 (at 581.8 110.9) (layer B.SilkS))
  (gr_text P41 (at 581.8 90.6) (layer B.SilkS))
  (gr_text P46 (at 581.8 77.9) (layer B.SilkS))
  (gr_text P45 (at 581.8 80.4) (layer B.SilkS))
  (gr_text P49 (at 581.8 70.2) (layer B.SilkS))
  (gr_text P50 (at 581.8 67.8) (layer B.SilkS))
  (gr_text "P25\n" (at 591.2 128.6) (layer B.SilkS))
  (gr_text P12 (at 591.2 95.6) (layer B.SilkS))
  (gr_text P11 (at 591.2 93.1) (layer B.SilkS))
  (gr_text P14 (at 591.2 100.7) (layer B.SilkS))
  (gr_text P13 (at 591.2 98.2) (layer B.SilkS))
  (gr_text P21 (at 591.2 118.5) (layer B.SilkS))
  (gr_text "P20\n" (at 591.2 116) (layer B.SilkS))
  (gr_text P39 (at 581.8 95.6) (layer B.SilkS))
  (gr_text P1 (at 591.7 67.7) (layer B.SilkS))
  (gr_text P38 (at 581.8 98.2) (layer B.SilkS))
  (gr_text P36 (at 581.8 103.3) (layer B.SilkS))
  (gr_text P37 (at 581.8 100.7) (layer B.SilkS))
  (gr_text P48 (at 581.8 72.8) (layer B.SilkS))
  (gr_text P31 (at 581.8 116) (layer B.SilkS))
  (gr_text P32 (at 581.8 113.4) (layer B.SilkS))
  (gr_text P10 (at 591.1 90.6) (layer B.SilkS))
  (gr_text P9 (at 590.8 88) (layer B.SilkS))
  (gr_text P42 (at 581.8 88) (layer B.SilkS))
  (gr_text P43 (at 581.9 85.6) (layer B.SilkS))
  (gr_text P8 (at 590.7 85.5) (layer B.SilkS))
  (gr_text P35 (at 581.8 105.8) (layer B.SilkS))
  (gr_text P44 (at 581.9 82.9) (layer B.SilkS))
  (gr_text P15 (at 591.2 103.3) (layer B.SilkS))
  (gr_text P23 (at 591.2 123.6) (layer B.SilkS))
  (gr_text P22 (at 591.2 121) (layer B.SilkS))
  (gr_text P30 (at 581.8 118.5) (layer B.SilkS))
  (gr_text P24 (at 591.2 126.1) (layer B.SilkS))
  (gr_text P27 (at 581.8 126.2) (layer B.SilkS))
  (gr_text P28 (at 581.8 123.6) (layer B.SilkS))
  (gr_text P7 (at 590.8 82.9) (layer B.SilkS))
  (gr_text P6 (at 590.7 80.5) (layer B.SilkS))
  (gr_text P5 (at 591.7 77.9) (layer B.SilkS))
  (gr_text P26 (at 581.8 128.6) (layer B.SilkS))
  (gr_text P17 (at 591.2 108.3) (layer B.SilkS))
  (gr_text P16 (at 591.2 105.8) (layer B.SilkS))
  (gr_text P34 (at 581.8 108.3) (layer B.SilkS))
  (gr_text P40 (at 581.8 93.1) (layer B.SilkS))
  (gr_text P4 (at 591.7 75.3) (layer B.SilkS))
  (gr_text P3 (at 591.7 72.8) (layer B.SilkS))
  (gr_text P2 (at 591.7 70.3) (layer B.SilkS))
  (gr_text P47 (at 581.9 75.3) (layer B.SilkS))
  (gr_text "10156000-051100LF Breakout" (at 598.3 96.8 90) (layer B.SilkS))
  (gr_text P26 (at 581.8 128.6) (layer F.SilkS))
  (gr_text P27 (at 581.8 126.2) (layer F.SilkS))
  (gr_text P28 (at 581.8 123.6) (layer F.SilkS))
  (gr_text P29 (at 581.8 121) (layer F.SilkS))
  (gr_text P30 (at 581.8 118.5) (layer F.SilkS))
  (gr_text P31 (at 581.8 116) (layer F.SilkS))
  (gr_text P32 (at 581.8 113.4) (layer F.SilkS))
  (gr_text P33 (at 581.8 110.9) (layer F.SilkS))
  (gr_text P34 (at 581.8 108.3) (layer F.SilkS))
  (gr_text P35 (at 581.8 105.8) (layer F.SilkS))
  (gr_text P36 (at 581.8 103.3) (layer F.SilkS))
  (gr_text P37 (at 581.8 100.7) (layer F.SilkS))
  (gr_text P38 (at 581.8 98.2) (layer F.SilkS))
  (gr_text P39 (at 581.8 95.6) (layer F.SilkS))
  (gr_text P40 (at 581.8 93.1) (layer F.SilkS))
  (gr_text P41 (at 581.8 90.6) (layer F.SilkS))
  (gr_text P42 (at 581.8 88) (layer F.SilkS))
  (gr_text P43 (at 581.8 85.6) (layer F.SilkS))
  (gr_text P44 (at 581.8 82.9) (layer F.SilkS))
  (gr_text P45 (at 581.8 80.4) (layer F.SilkS))
  (gr_text P46 (at 581.8 77.9) (layer F.SilkS))
  (gr_text P47 (at 581.8 75.3) (layer F.SilkS))
  (gr_text P48 (at 581.8 72.8) (layer F.SilkS))
  (gr_text P49 (at 581.8 70.2) (layer F.SilkS))
  (gr_text P50 (at 581.8 67.8) (layer F.SilkS))
  (gr_text "P25\n" (at 591.1 128.6) (layer F.SilkS))
  (gr_text P24 (at 591.1 126.1) (layer F.SilkS))
  (gr_text P23 (at 591.1 123.6) (layer F.SilkS))
  (gr_text P22 (at 591.1 121) (layer F.SilkS))
  (gr_text P21 (at 591.1 118.5) (layer F.SilkS))
  (gr_text "P20\n" (at 591.1 116) (layer F.SilkS))
  (gr_text P19 (at 591.1 113.4) (layer F.SilkS))
  (gr_text P18 (at 591.1 110.9) (layer F.SilkS))
  (gr_text P17 (at 591.1 108.3) (layer F.SilkS))
  (gr_text P16 (at 591.1 105.8) (layer F.SilkS))
  (gr_text P15 (at 591.1 103.3) (layer F.SilkS))
  (gr_text P14 (at 591.1 100.7) (layer F.SilkS))
  (gr_text P13 (at 591.1 98.2) (layer F.SilkS))
  (gr_text P12 (at 591.1 95.6) (layer F.SilkS))
  (gr_text P11 (at 591.1 93.1) (layer F.SilkS))
  (gr_text P10 (at 591.1 90.6) (layer F.SilkS))
  (gr_text P9 (at 590.7 88) (layer F.SilkS))
  (gr_text P8 (at 590.7 85.5) (layer F.SilkS))
  (gr_text P7 (at 590.7 82.9) (layer F.SilkS))
  (gr_text P6 (at 590.7 80.5) (layer F.SilkS))
  (gr_text P5 (at 589.6 77.9) (layer F.SilkS))
  (gr_text P4 (at 589.6 75.3) (layer F.SilkS))
  (gr_text P3 (at 589.6 72.8) (layer F.SilkS))
  (gr_text P2 (at 589.6 70.3) (layer F.SilkS))
  (gr_text P1 (at 589.6 67.7) (layer F.SilkS))
  (gr_line (start 603.4 63.5) (end 603.4 132.08) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 578 63.5) (end 603.4 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 578 132.08) (end 578 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 603.4 132.08) (end 578 132.08) (layer Edge.Cuts) (width 0.1))
)
