<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.53" y2="0" width="0" layer="20"/>
<wire x1="22.53" y1="0" x2="22.53" y2="30.47" width="0" layer="20"/>
<wire x1="22.53" y1="30.47" x2="0" y2="30.47" width="0" layer="20"/>
<wire x1="0" y1="30.47" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fci-sata2">
<packages>
<package name="10067172-70CLF_PKG">
<description>&lt;b&gt;FCI&lt;/b&gt; E-SATA Connector, Receptacle, 7-Pos, Through Hole
&lt;p&gt;End user is responsible for verifying the accuracy of this library part.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ESATA1" library="fci-sata2" package="10067172-70CLF_PKG" value="10067172-70CLF"/>
<element name="ESATA2" library="fci-sata2" package="10067172-70CLF_PKG" value="10067172-70CLF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="ESATA1" pad="P1"/>
<contactref element="ESATA2" pad="P7"/>
</signal>
<signal name="N$2">
<contactref element="ESATA1" pad="P6"/>
<contactref element="ESATA2" pad="P2"/>
</signal>
<signal name="N$3">
<contactref element="ESATA1" pad="P5"/>
<contactref element="ESATA2" pad="P3"/>
</signal>
<signal name="N$4">
<contactref element="ESATA1" pad="P4"/>
<contactref element="ESATA2" pad="P4"/>
</signal>
<signal name="N$5">
<contactref element="ESATA1" pad="P3"/>
<contactref element="ESATA2" pad="P5"/>
</signal>
<signal name="N$6">
<contactref element="ESATA1" pad="P2"/>
<contactref element="ESATA2" pad="P6"/>
</signal>
<signal name="N$7">
<contactref element="ESATA1" pad="P7"/>
<contactref element="ESATA2" pad="P1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
