(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "USB Cable Tester")
    (date "2024-08-16")
    (rev "2.4")
    (company "Quesadillon LLC")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 100 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-A)")
  (net 2 "Net-(D2-A)")
  (net 3 "GND")
  (net 4 "Net-(D3-A)")
  (net 5 "Net-(D4-A)")
  (net 6 "Net-(D5-A)")
  (net 7 "Net-(D6-A)")
  (net 8 "Net-(D7-A)")
  (net 9 "Net-(D8-A)")
  (net 10 "Net-(D9-A)")
  (net 11 "+3V3")
  (net 12 "Net-(D10-A)")
  (net 13 "Net-(D11-A)")
  (net 14 "Net-(D12-A)")
  (net 15 "Net-(D13-A)")
  (net 16 "Net-(D14-A)")
  (net 17 "Net-(D15-A)")
  (net 18 "Net-(D16-A)")
  (net 19 "Net-(D17-A)")
  (net 20 "Net-(D18-A)")
  (net 21 "Net-(D19-A)")
  (net 22 "Net-(D20-A)")
  (net 23 "Net-(D21-A)")
  (net 24 "Net-(D22-A)")
  (net 25 "Net-(D23-A)")
  (net 26 "Net-(D24-A)")
  (net 27 "Net-(D25-A)")
  (net 28 "/GND_A1")
  (net 29 "/TX1+")
  (net 30 "/TX1-")
  (net 31 "/VBUS_A4")
  (net 32 "/CC1")
  (net 33 "/D+_A")
  (net 34 "/D-_A")
  (net 35 "/VBUS_B9")
  (net 36 "/VBUS_A9")
  (net 37 "/RX2-")
  (net 38 "/RX2+")
  (net 39 "/GND_A12")
  (net 40 "/GND_B1")
  (net 41 "/TX2+")
  (net 42 "/TX2-")
  (net 43 "/VBUS_B4")
  (net 44 "/CC2")
  (net 45 "/D-_B")
  (net 46 "/RX1-")
  (net 47 "/RX1+")
  (net 48 "/GND_B12")
  (net 49 "/SHLD")
  (net 50 "/SBU1")
  (net 51 "/D+_B")
  (net 52 "/SBU2")
  (net 53 "unconnected-(J3-ID-Pad4)")
  (net 54 "unconnected-(J5-ID-Pad4)")
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 66.0375 121.75)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D21" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D21-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 113.709086)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/TX2-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D4-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "snapeda:AMPHENOL_10118194-0001LF_MOD" (layer "F.Cu")
    (at 141.2 97 90)
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "10118194-0001LF")
    (property "Manufacturer" "Amphenol ICC")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr through_hole)
    (fp_text reference "J3" (at 5 -2.2 180) (layer "F.SilkS") hide)
    (fp_text value "USB_B_Micro" (at 0 4.48 90) (layer "F.Fab"))
    (fp_text user "PCB END" (at -1.95 2.1 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 -2.7 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -2.7 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -2.7 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.65 -2.7 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "unconnected-(J3-ID-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at 1.3 -2.7 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "power_out"))
    (pad "6" thru_hole oval (at -3.5 0 90) (size 0.9 1.55) (drill oval 0.5 1.15) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd roundrect (at -3.1125 0 90) (size 1.8 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.5 -2.7 90) (size 1.25 0.95) (drill oval 0.85 0.55) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1 0 90) (size 1.5 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1 0 90) (size 1.5 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.5 -2.7 90) (size 1.25 0.95) (drill oval 0.85 0.55) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd roundrect (at 3.1 0 90) (size 1.8 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 3.5 0 90) (size 0.9 1.55) (drill oval 0.5 1.15) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive"))
    (model "${ALVAROP_3D_DIR}/10118194-0001LF.step"
      (offset (xyz -75.025 3.1 -0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "snapeda:TE_1734510-1" (layer "F.Cu")
    (at 141.05 118.49225 90)
    (property "ALT MPN" "0548190519")
    (property "ALT Manufacturer" "Molex")
    (property "MPN" "1734510-1")
    (property "Manufacturer" "TE Connectivity")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Mini Type B connector")
    (property "ki_keywords" "connector USB mini")
    (attr through_hole)
    (fp_text reference "J5" (at -1.311125 -6.855945 90) (layer "F.SilkS") hide)
    (fp_text value "USB_B_Mini" (at 2.19096 4.58202 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.6 -5.05 90) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -0.8 -3.85 90) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "D-") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 0 -5.05 90) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "D+") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at 0.8 -3.85 90) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(J5-ID-Pad4)") (pinfunction "ID") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 1.6 -5.05 90) (size 1.2 1.2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "6" thru_hole oval (at -3.65 0 90) (size 1.208 2.416) (drill oval 0.7 1.9) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" thru_hole oval (at 3.65 0 90) (size 1.208 2.416) (drill oval 0.7 1.9) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Shield") (pintype "passive") (solder_mask_margin 0.102))
    (model ":ALVAROP_3D_DIR:1734510-1.step"
      (offset (xyz 0 -3.75 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 74.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/GND_B12") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(D25-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 76.173913)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D25" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(D25-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 78.945454)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/TX1+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D7-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 87.636362)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/VBUS_A4") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D20-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 91.981816)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/CC1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D16-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 102.260869)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D11-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 84.869565)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D8-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 83.290908)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/TX1-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D8-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 105.018178)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/SBU1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D17-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 118.05454)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/RX2+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D5-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Plated_Hole_D5.0mm" (layer "F.Cu")
    (at 61.5 77.25)
    (descr "Plated Hole as test Point, diameter 5.0mm")
    (tags "test point plated hole")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.948) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Plated_Hole_D5.0mm" (at 0 3.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.95) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6 6) (drill 5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "snapeda:BELFUSE_SS-52400-003" (layer "F.Cu")
    (at 60.45 109 -90)
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "SS-52400-003")
    (property "Manufacturer" "Stewart Connector")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Full-Featured Type-C Receptacle connector")
    (property "ki_keywords" "usb universal serial bus type-C full-featured")
    (attr through_hole)
    (fp_text reference "J2" (at -0.425 -9.035 90) (layer "F.SilkS") hide)
    (fp_text value "USB_C_Receptacle" (at 0 5.465 90) (layer "F.Fab"))
    (fp_text user "PCB EDGE" (at 5.3 3.3 90) (layer "F.Fab"))
    (pad "A1" smd rect (at -2.75 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/GND_A1") (pinfunction "GND") (pintype "passive"))
    (pad "A2" smd rect (at -2.25 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/TX1+") (pinfunction "TX1+") (pintype "bidirectional"))
    (pad "A3" smd rect (at -1.75 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/TX1-") (pinfunction "TX1-") (pintype "bidirectional"))
    (pad "A4" smd rect (at -1.25 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/VBUS_A4") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -0.75 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/CC1") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/D+_A") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/D-_A") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 0.75 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/SBU1") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 1.25 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/VBUS_A9") (pinfunction "VBUS") (pintype "passive"))
    (pad "A10" smd rect (at 1.75 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/RX2-") (pinfunction "RX2-") (pintype "bidirectional"))
    (pad "A11" smd rect (at 2.25 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/RX2+") (pinfunction "RX2+") (pintype "bidirectional"))
    (pad "A12" smd rect (at 2.75 -7.13 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/GND_A12") (pinfunction "GND") (pintype "passive"))
    (pad "B1" thru_hole circle (at 2.8 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 40 "/GND_B1") (pinfunction "GND") (pintype "passive"))
    (pad "B2" thru_hole circle (at 2.4 -5.17 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 41 "/TX2+") (pinfunction "TX2+") (pintype "bidirectional"))
    (pad "B3" thru_hole circle (at 1.6 -5.17 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 42 "/TX2-") (pinfunction "TX2-") (pintype "bidirectional"))
    (pad "B4" thru_hole circle (at 1.2 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 43 "/VBUS_B4") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" thru_hole circle (at 0.8 -5.17 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 44 "/CC2") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" thru_hole circle (at 0.4 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 51 "/D+_B") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" thru_hole circle (at -0.4 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 45 "/D-_B") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" thru_hole circle (at -0.8 -5.17 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 52 "/SBU2") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" thru_hole circle (at -1.2 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 35 "/VBUS_B9") (pinfunction "VBUS") (pintype "passive"))
    (pad "B10" thru_hole circle (at -1.6 -5.17 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 46 "/RX1-") (pinfunction "RX1-") (pintype "bidirectional"))
    (pad "B11" thru_hole circle (at -2.4 -5.17 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 47 "/RX1+") (pinfunction "RX1+") (pintype "bidirectional"))
    (pad "B12" thru_hole circle (at -2.8 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 48 "/GND_B12") (pinfunction "GND") (pintype "passive"))
    (pad "G1" thru_hole circle (at 2 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask"))
    (pad "G2" thru_hole circle (at -2 -5.88 270) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask"))
    (pad "G3" smd rect (at 0 -2.55 270) (size 0.2 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G4" smd rect (at 0 0.55 270) (size 0.2 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "S1" thru_hole oval (at -4.27 -4.73 270) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 49 "/SHLD") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.27 0 270) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 49 "/SHLD") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.27 -4.73 270) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 49 "/SHLD") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.27 0 270) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 49 "/SHLD") (pinfunction "SHIELD") (pintype "passive"))
    (model ":ALVAROP_3D_DIR:SS-52400-003.step"
      (offset (xyz 0 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 119.652173)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 80.521739)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D9" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D9-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" locked (layer "F.Cu")
    (at 94.5 88 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 97.913043)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D12" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D12-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 93.565217)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D16-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 122.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/GND_B1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D24-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 84.869565)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D10" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D10-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 115.304347)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 100.672724)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/D-_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D14-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 102.260869)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D14-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 109.363632)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/VBUS_B4") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "snapeda:BELFUSE_SS-52400-003" (layer "F.Cu")
    (at 139.4625 107.4 90)
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "SS-52400-003")
    (property "Manufacturer" "Stewart Connector")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Full-Featured Type-C Receptacle connector")
    (property "ki_keywords" "usb universal serial bus type-C full-featured")
    (attr through_hole)
    (fp_text reference "J1" (at 5.9 -4.4625 180) (layer "F.SilkS") hide)
    (fp_text value "USB_C_Receptacle" (at 0 5.465 90) (layer "F.Fab"))
    (fp_text user "PCB EDGE" (at 5.3 3.3 90) (layer "F.Fab"))
    (pad "A1" smd rect (at -2.75 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "passive"))
    (pad "A2" smd rect (at -2.25 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "TX1+") (pintype "bidirectional"))
    (pad "A3" smd rect (at -1.75 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "TX1-") (pintype "bidirectional"))
    (pad "A4" smd rect (at -1.25 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -0.75 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 0.75 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 1.25 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "passive"))
    (pad "A10" smd rect (at 1.75 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "RX2-") (pintype "bidirectional"))
    (pad "A11" smd rect (at 2.25 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "RX2+") (pintype "bidirectional"))
    (pad "A12" smd rect (at 2.75 -7.13 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "passive"))
    (pad "B1" thru_hole circle (at 2.8 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "passive"))
    (pad "B2" thru_hole circle (at 2.4 -5.17 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "TX2+") (pintype "bidirectional"))
    (pad "B3" thru_hole circle (at 1.6 -5.17 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "TX2-") (pintype "bidirectional"))
    (pad "B4" thru_hole circle (at 1.2 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" thru_hole circle (at 0.8 -5.17 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" thru_hole circle (at 0.4 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" thru_hole circle (at -0.4 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" thru_hole circle (at -0.8 -5.17 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" thru_hole circle (at -1.2 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "passive"))
    (pad "B10" thru_hole circle (at -1.6 -5.17 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "RX1-") (pintype "bidirectional"))
    (pad "B11" thru_hole circle (at -2.4 -5.17 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "RX1+") (pintype "bidirectional"))
    (pad "B12" thru_hole circle (at -2.8 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "passive"))
    (pad "G1" thru_hole circle (at 2 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask"))
    (pad "G2" thru_hole circle (at -2 -5.88 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask"))
    (pad "G3" smd rect (at 0 -2.55 90) (size 0.2 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G4" smd rect (at 0 0.55 90) (size 0.2 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "S1" thru_hole oval (at -4.27 -4.73 90) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.27 0 90) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.27 -4.73 90) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.27 0 90) (size 1.05 2.1) (drill oval 0.65 1.25) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SHIELD") (pintype "passive"))
    (model ":ALVAROP_3D_DIR:SS-52400-003.step"
      (offset (xyz 0 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 96.32727)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/D-_B") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D13-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 89.217391)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 106.608695)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D15-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "snapeda:AMPHENOL_GSB3211311WEU" (layer "F.Cu")
    (at 135.35 83.5 90)
    (property "ALT MPN" "E8199-030-03")
    (property "ALT Manufacturer" "Pulse Electronics")
    (property "MPN" "GSB3211311WEU")
    (property "Manufacturer" "Amphenol ICC")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB 3.0 B connector")
    (property "ki_keywords" "usb universal serial bus")
    (attr through_hole)
    (fp_text reference "J4" (at 8 -6.85) (layer "F.SilkS") hide)
    (fp_text value "USB3_B" (at 7.56676 -16.67393 270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 1.25 -4.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "VBUS") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -1.25 -4.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "D-") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at -1.25 -2.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "D+") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at 1.25 -2.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "GND") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at -4.25 -6.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SSTX-") (pintype "output") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at -2.5 -6.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SSTX+") (pintype "output") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at 0 -6.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "DRAIN") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at 2.5 -6.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SSRX-") (pintype "input") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at 4.25 -6.71 90) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SSRX+") (pintype "input") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at -6.02 0 90) (size 3.416 3.416) (drill 2.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 6.02 0 90) (size 3.416 3.416) (drill 2.4) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
    (model ":ALVAROP_3D_DIR:GSB3211311WEU.step"
      (offset (xyz 0 7.75 5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 76.173913)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D22" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D22-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "snapeda:BAT_BU2032SM-BT-GTR" locked (layer "F.Cu")
    (at 100 101.5 -90)
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "BU2032SM-BT-GTR")
    (property "Manufacturer" "Memory Protection Devices")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr smd)
    (fp_text reference "BT1" (at -12.81935 -7.62 90) (layer "F.SilkS") hide)
    (fp_text value "CR2032" (at -3.93386 9.46116 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -14.65 0 270) (size 3.2 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+3V3") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect locked (at 14.65 0 270) (size 3.2 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.102))
    (model ":ALVAROP_3D_DIR:BU2032SM-BT-GTR.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 91.981816)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/SBU2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D18-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 121 122.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/GND_A12") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D23-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 115.304347)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "snapeda:AMPHENOL_GSB311131HR" (layer "F.Cu")
    (at 67.7575 92.01 -90)
    (property "ALT MPN" "SS-52000-001")
    (property "ALT Manufacturer" "Stewart Connector")
    (property "MPN" "GSB311131HR")
    (property "Manufacturer" "Amphenol ICC")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB 3.0 A connector")
    (property "ki_keywords" "usb universal serial bus")
    (attr through_hole)
    (fp_text reference "J6" (at -4.46621 -4.21387 -90) (layer "F.SilkS") hide)
    (fp_text value "USB3_A" (at 0 14.61964 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.5 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 31 "/VBUS_A4") (pinfunction "VBUS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -1 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 34 "/D-_A") (pinfunction "D-") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 1 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 33 "/D+_A") (pinfunction "D+") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at 3.5 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 28 "/GND_A1") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 4 -1.5 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "/RX2-") (pinfunction "SSRX-") (pintype "output") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at 2 -1.5 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 38 "/RX2+") (pinfunction "SSRX+") (pintype "output") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at 0 -1.5 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 39 "/GND_A12") (pinfunction "DRAIN") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at -2 -1.5 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 30 "/TX1-") (pinfunction "SSTX-") (pintype "input") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at -4 -1.5 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 29 "/TX1+") (pinfunction "SSTX+") (pintype "input") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at -6.57 2 270) (size 3.316 3.316) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 49 "/SHLD") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 6.57 2 270) (size 3.316 3.316) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 49 "/SHLD") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
    (model ":ALVAROP_3D_DIR:GSB311131HR.step"
      (offset (xyz 0 -5.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 89.217391)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D20" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D20-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 87.636362)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/VBUS_B9") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 106.608695)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D17" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D17-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 83.290908)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/RX1-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D10-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 118.05454)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/TX2+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D3-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 124)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D23" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D23-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 109.363632)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/VBUS_A9") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D19-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 96.32727)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/D+_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D12-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 78.945454)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/RX1+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D9-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 110.956521)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 121 74.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/GND_A1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D22-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 110.956521)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D19" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D19-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 105.018178)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/CC2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D15-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 121 80.521739)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 66.0375 120)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/SHLD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D21-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 119.652173)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 124)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D24" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D24-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 97.913043)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D13-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 120.96 113.709086)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/RX2-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D6-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" locked (layer "F.Cu")
    (at 78 100.672724)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/D+_B") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D11-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" locked (layer "F.Cu")
    (at 78 93.565217)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "ALT MPN" "")
    (property "ALT Manufacturer" "")
    (property "MPN" "")
    (property "Manufacturer" "")
    (property "Sheetfile" "usb_c_cable_tester.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D18" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D18-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Logo_11.4x12mm_SilkScreen" locked (layer "B.Cu")
    (at 100.25 81 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Logo_11.4x12mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (gr_line locked (start 57.2 123.81) (end 57.2 76.19)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 57.2 76.19) (mid 58.1314 73.9414) (end 60.38 73.01)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 60.38 126.99) (mid 58.1314 126.0586) (end 57.2 123.81)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 142.8 123.81) (mid 141.8686 126.0586) (end 139.62 126.99)
    (layer "Edge.Cuts"))
  (gr_line locked (start 139.62 126.99) (end 60.38 126.99)
    (layer "Edge.Cuts"))
  (gr_arc locked (start 139.62 73.01) (mid 141.8686 73.9414) (end 142.8 76.19)
    (layer "Edge.Cuts"))
  (gr_line locked (start 142.8 76.19) (end 142.8 123.81)
    (layer "Edge.Cuts"))
  (gr_line locked (start 60.38 73.01) (end 139.62 73.01)
    (layer "Edge.Cuts"))
  (gr_text "Connect USB cable to both sides \nof the board. The LED of each \nconnected signal will light up." (at 100 117.5) (layer "B.SilkS"))
  (gr_text "WARNING\nFOR CABLE USE ONLY\nDO NOT CONNECT TO ANY DEVICE!\nIT WILL BREAK IT" (at 100 100) (layer "B.SilkS"))
  (gr_text "VBUS" (at 115.058334 88.972727) (layer "F.SilkS"))
  (gr_text "A12" (at 125.272619 123.7) (layer "F.SilkS"))
  (gr_text "TX1+" (at 115.004762 80.290909) (layer "F.SilkS"))
  (gr_text "B2" (at 74.314286 119.35909) (layer "F.SilkS"))
  (gr_text "D+" (at 82.689285 102.109086) (layer "F.SilkS"))
  (gr_text "CC1" (at 116.076191 93.313636) (layer "F.SilkS"))
  (gr_text "RX2-" (at 114.736905 115.018181) (layer "F.SilkS"))
  (gr_text "B5" (at 74.314286 106.336363) (layer "F.SilkS"))
  (gr_text "SBU2" (at 84.617857 93.472724) (layer "F.SilkS"))
  (gr_text "B10" (at 73.6 84.631818) (layer "F.SilkS"))
  (gr_text "VBUS" (at 84.510714 89.154543) (layer "F.SilkS"))
  (gr_text "SBU1" (at 114.951191 106.336363) (layer "F.SilkS"))
  (gr_text "GND" (at 83.6 76.2) (layer "F.SilkS"))
  (gr_text "B6" (at 74.314286 101.995454) (layer "F.SilkS"))
  (gr_text "A2" (at 124.558334 80.290909) (layer "F.SilkS"))
  (gr_text "TX2-" (at 84.564285 115.063629) (layer "F.SilkS"))
  (gr_text "B1" (at 74.469048 123.7) (layer "F.SilkS"))
  (gr_text "GND" (at 115.969048 75.95) (layer "F.SilkS"))
  (gr_text "GND" (at 115.969048 123.7) (layer "F.SilkS"))
  (gr_text "A1" (at 124.558334 75.95) (layer "F.SilkS"))
  (gr_text "A11" (at 125.272619 119.35909) (layer "F.SilkS"))
  (gr_text "B12" (at 73.6 75.95) (layer "F.SilkS"))
  (gr_text "A3" (at 124.558334 84.631818) (layer "F.SilkS"))
  (gr_text "TX2+" (at 84.564285 119.38181) (layer "F.SilkS"))
  (gr_text "A4" (at 124.558334 88.972727) (layer "F.SilkS"))
  (gr_text "Alvaro Prieto\nalvarop.com" (at 100 122.75) (layer "F.SilkS"))
  (gr_text "D-" (at 82.689285 97.790905) (layer "F.SilkS"))
  (gr_text "D-" (at 116.879762 101.995454) (layer "F.SilkS"))
  (gr_text "VBUS" (at 115.058334 110.677272) (layer "F.SilkS"))
  (gr_text "B7" (at 74.314286 97.654545) (layer "F.SilkS"))
  (gr_text "B3" (at 74.314286 115.018181) (layer "F.SilkS"))
  (gr_text "A6" (at 124.558334 97.654545) (layer "F.SilkS"))
  (gr_text "A5" (at 124.558334 93.313636) (layer "F.SilkS"))
  (gr_text "RX1-" (at 84.832143 84.836362) (layer "F.SilkS"))
  (gr_text "TX1-" (at 115.004762 84.631818) (layer "F.SilkS"))
  (gr_text "DO NOT CONNECT TO\nDEVICE!!!" (at 131 90 90) (layer "F.SilkS"))
  (gr_text "A8" (at 124.558334 106.336363) (layer "F.SilkS"))
  (gr_text "VBUS" (at 84.510714 110.745448) (layer "F.SilkS"))
  (gr_text "B8" (at 74.314286 93.313636) (layer "F.SilkS"))
  (gr_text "CC2" (at 83.492857 106.427267) (layer "F.SilkS"))
  (gr_text "USB Cable\nTester" (at 100 78) (layer "F.SilkS"))
  (gr_text "GND" (at 83.6 123.7) (layer "F.SilkS"))
  (gr_text "A7" (at 124.558334 101.995454) (layer "F.SilkS"))
  (gr_text "RX2+" (at 114.736905 119.35909) (layer "F.SilkS"))
  (gr_text "A10" (at 125.272619 115.018181) (layer "F.SilkS"))
  (gr_text "A9" (at 124.558334 110.677272) (layer "F.SilkS"))
  (gr_text "D+" (at 116.879762 97.654545) (layer "F.SilkS"))
  (gr_text "B4" (at 74.314286 110.677272) (layer "F.SilkS"))
  (gr_text "RX1+" (at 84.832143 80.518181) (layer "F.SilkS"))
  (gr_text "B9" (at 74.314286 88.972727) (layer "F.SilkS"))
  (gr_text "B11" (at 73.6 80.290909) (layer "F.SilkS"))
  (gr_text "SHIELD" (at 66.1375 123.85) (layer "F.SilkS"))
  (gr_text "v${REVISION}" (at 99.75 82.5) (layer "F.SilkS"))
  (zone locked (net 3) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 143 127)
        (xy 57 127)
        (xy 57 73)
        (xy 143 73)
      )
    )
  )
)
