(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 191)
    (no_connects 0)
    (area 115.424999 69.924999 200.575001 125.075001)
    (thickness 1.6)
    (drawings 183)
    (tracks 638)
    (zones 0)
    (modules 82)
    (nets 44)
  )
  (page A4)
  (title_block
    (title "Universal Atmega328 Platform")
    (rev 0)
    (company -)
  )
  (layers
    (0 Top_Copper signal)
    (31 Back_Copper signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.152)
    (zone_clearance 0.15)
    (zone_45_only yes)
    (trace_min 0.152)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1)
    (pcb_text_size 0.8 0.8)
    (mod_edge_width 0.1)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.1)
    (pad_size 0.6 0.6)
    (pad_drill 0.35)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 25.4 187.96)
    (visible_elements 7FFFEF6F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/V1.2/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /XTAL1)
  (net 3 /XTAL2)
  (net 4 /RST)
  (net 5 /D5)
  (net 6 /D6)
  (net 7 /MISO-D12)
  (net 8 /SCK-D13)
  (net 9 /MOSI-D11)
  (net 10 /SDA-A4)
  (net 11 /SCL-A5)
  (net 12 "Net-(BT1-Pad1)")
  (net 13 /D2-INT0)
  (net 14 /VCC_SD)
  (net 15 /A7)
  (net 16 /VREG_3V3)
  (net 17 /SELECT_SD)
  (net 18 /ENABLE_SD)
  (net 19 "Net-(D1-Pad3)")
  (net 20 /VRAW)
  (net 21 /D3-INT1)
  (net 22 /V_RTC_PIN)
  (net 23 "Net-(C2-Pad1)")
  (net 24 /AREF)
  (net 25 /VCC_SD_TPS27082)
  (net 26 "Net-(J20-Pad2)")
  (net 27 "Net-(J21-Pad2)")
  (net 28 "Net-(J22-Pad2)")
  (net 29 "Net-(J23-Pad2)")
  (net 30 "Net-(J24-Pad2)")
  (net 31 "Net-(J25-Pad2)")
  (net 32 "Net-(R19-Pad1)")
  (net 33 "Net-(J3-Pad1)")
  (net 34 "Net-(J3-Pad2)")
  (net 35 /V_BLE_PIN)
  (net 36 /TX_BLE)
  (net 37 /RX_BLE)
  (net 38 /LED1)
  (net 39 /LED2)
  (net 40 /D4)
  (net 41 "Net-(BT2-Pad1)")
  (net 42 "Net-(C5-Pad2)")
  (net 43 "Net-(R6-Pad1)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.152)
    (trace_width 0.2)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /AREF)
    (add_net /D2-INT0)
    (add_net /D3-INT1)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /ENABLE_SD)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /MISO-D12)
    (add_net /MOSI-D11)
    (add_net /RST)
    (add_net /RX_BLE)
    (add_net /SCK-D13)
    (add_net /SCL-A5)
    (add_net /SDA-A4)
    (add_net /SELECT_SD)
    (add_net /TX_BLE)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J20-Pad2)")
    (add_net "Net-(J21-Pad2)")
    (add_net "Net-(J22-Pad2)")
    (add_net "Net-(J23-Pad2)")
    (add_net "Net-(J24-Pad2)")
    (add_net "Net-(J25-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R6-Pad1)")
  )
  (net_class Spannungen ""
    (clearance 0.152)
    (trace_width 0.4)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A7)
    (add_net /VCC_SD)
    (add_net /VCC_SD_TPS27082)
    (add_net /VRAW)
    (add_net /VREG_3V3)
    (add_net /V_BLE_PIN)
    (add_net /V_RTC_PIN)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT2-Pad1)")
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 117.983 94.234)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 121.92 93.599)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 154.9908 95.3008)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 157.226 87.757)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 156.9974 84.201)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 189.4205 106.172)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 190.6 114.4)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 167.9 119.6)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 158 80.6)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Sockel__MicroSD_Sockel_ATTEND_1121-TXAR-R (layer Top_Copper) (tedit 5AFDB5C2)
    (at 192.4 107.5)
    (autoplace_cost180 10)
    (fp_text reference J9 (at 4.3 7.5) (layer F.SilkS) hide)
    (fp_text value SD-Card (at 0.4 -0.8) (layer F.Fab) hide)
    (fp_text user microSD (at 0 11) (layer F.SilkS))
    (pad 8 smd rect (at -4.75 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask))
    (pad 7 smd rect (at -3.65 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask)
      (net 7 /MISO-D12))
    (pad 6 smd rect (at -2.55 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.45 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask)
      (net 8 /SCK-D13))
    (pad 3 smd rect (at 0.75 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask)
      (net 9 /MOSI-D11))
    (pad 1 smd rect (at 2.95 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask))
    (pad 4 smd rect (at -0.35 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask)
      (net 14 /VCC_SD))
    (pad 2 smd rect (at 1.85 -3) (size 0.7 2) (layers Top_Copper F.Paste F.Mask)
      (net 17 /SELECT_SD))
    (pad 9 smd rect (at 4.2 -3) (size 0.85 2) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 5.35 -3) (size 0.85 2) (layers Top_Copper F.Paste F.Mask))
    (pad 9 smd rect (at 6.65 5.45) (size 1.5 2) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -6.7 5.45) (size 1.5 2) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Attend_1121_uSDslot.wrl
      (at (xyz 0 -0.145 0.06))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz 90 180 180))
    )
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 158.1 96.5)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 155.5 87)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 169 74)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 165.4 73.2)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 168.9 87.1)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 165.1 86)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 152.75 107.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value 100N (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 178.5 121)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value SDA_pullup (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 10 /SDA-A4))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:SOIC_normal+narrow.Pitch1.27 (layer Back_Copper) (tedit 5AE36AF0)
    (at 164.135 92.81 180)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 3.556 180) (layer B.SilkS) hide)
    (fp_text value 24XXYYYY (at 0 -3.68 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.175 1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 29 "Net-(J23-Pad2)"))
    (pad 2 smd rect (at -3.175 0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 30 "Net-(J24-Pad2)"))
    (pad 3 smd rect (at -3.175 -0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 31 "Net-(J25-Pad2)"))
    (pad 4 smd rect (at -3.175 -1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.175 1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 7 smd rect (at 3.175 0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.175 -0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 11 /SCL-A5))
    (pad 5 smd rect (at 3.175 -1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 10 /SDA-A4))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 196.6 108.7)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 15-33K (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 17 /SELECT_SD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:HM-11 (layer Top_Copper) (tedit 5AF829EB)
    (at 145.75 101 270)
    (fp_text reference U7 (at -0.25 -11.85 270) (layer F.SilkS) hide)
    (fp_text value HM-11 (at 0.05 -9.75 270) (layer F.Fab) hide)
    (fp_text user 8 (at -5.3 -1.7 270) (layer F.SilkS))
    (fp_text user 1 (at -5.3 -12.2 270) (layer F.SilkS))
    (fp_text user 9 (at 5.3 -1.8 270) (layer F.SilkS))
    (fp_text user 16 (at 5.1 -12.2 270) (layer F.SilkS))
    (pad 9 smd rect (at 7 -1.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask)
      (net 35 /V_BLE_PIN))
    (pad 1 smd rect (at -7 -12.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 2 smd rect (at -7 -10.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask)
      (net 36 /TX_BLE))
    (pad 3 smd rect (at -7 -9.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 4 smd rect (at -7 -7.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask)
      (net 37 /RX_BLE))
    (pad 5 smd rect (at -7 -6.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 6 smd rect (at -7 -4.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 7 smd rect (at -7 -3.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 8 smd rect (at -7 -1.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 10 smd rect (at 7 -3.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 11 smd rect (at 7 -4.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 12 smd rect (at 7 -6.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 7 -7.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 14 smd rect (at 7 -9.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 15 smd rect (at 7 -10.75 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
    (pad 16 smd rect (at 7 -12.25 270) (size 1.5 1.2) (layers Top_Copper F.Paste F.Mask))
  )
  (module SMD_Packages:SO-16-L (layer Back_Copper) (tedit 5A9F2241)
    (at 148.2 78.1 90)
    (attr smd)
    (fp_text reference U4 (at 0 -1.524 90) (layer B.SilkS) hide)
    (fp_text value DS3231 (at 0.381 1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -4.445 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 32 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at -3.175 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 22 /V_RTC_PIN))
    (pad 3 smd rect (at -1.905 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 13 /D2-INT0))
    (pad 4 smd rect (at -0.635 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask))
    (pad 5 smd rect (at 0.635 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.905 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.175 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 4.445 -5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 3.175 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 1.905 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 0.635 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -0.635 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.905 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 12 "Net-(BT1-Pad1)"))
    (pad 15 smd rect (at -3.175 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 10 /SDA-A4))
    (pad 16 smd rect (at -4.445 5.08 90) (size 0.635 1.905) (layers Back_Copper B.Paste B.Mask)
      (net 11 /SCL-A5))
    (model SMD_Packages.3dshapes/SO-16-L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:Resonator_SMD_muRata_CSTCC (layer Back_Copper) (tedit 5A9F0911)
    (at 144.75 108 315)
    (descr "SMD Resomator/Filter Murata SFECV, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 6.9x2.9mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 2.358 2.942 315) (layer B.SilkS) hide)
    (fp_text value RES8-16Mhz (at 0 -3 315) (layer B.Fab))
    (fp_text user %R (at 0 0 315) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0 315) (size 1.5 4) (layers Back_Copper B.Paste B.Mask)
      (net 3 /XTAL2))
    (pad 2 smd rect (at 0 0 315) (size 1.5 4) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.5 0 315) (size 1.5 4) (layers Back_Copper B.Paste B.Mask)
      (net 2 /XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Resonator_SMD_muRata_SFECV-3pin_6.9x2.9mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:LED_3528_handlötbar (layer Top_Copper) (tedit 5A9EE93E)
    (at 137.65 107.1)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference D1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value LED_Dual_AACC (at 0 4) (layer F.Fab) hide)
    (pad 1 smd rect (at 1.75 -0.85) (size 1.6 1) (layers Top_Copper F.Paste F.Mask)
      (net 38 /LED1))
    (pad 2 smd rect (at 1.75 0.85) (size 1.6 1) (layers Top_Copper F.Paste F.Mask)
      (net 39 /LED2))
    (pad 3 smd rect (at -1.75 -0.85) (size 1.6 1) (layers Top_Copper F.Paste F.Mask)
      (net 19 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at -1.75 0.85) (size 1.6 1) (layers Top_Copper F.Paste F.Mask)
      (net 19 "Net-(D1-Pad3)"))
    (model LEDs.3dshapes/LED_PLCC_2835.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.38 0.38 0.38))
      (rotate (xyz 0 0 180))
    )
  )
  (module 000EigeneFootprints:Taster_SMD_eBay4,5x3mm (layer Top_Copper) (tedit 5AE72C1C)
    (at 190.2 100.2)
    (tags Testpoint)
    (fp_text reference SW1 (at 0 3.7) (layer F.SilkS) hide)
    (fp_text value Reset (at 0 -4.2) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 2) (layers Top_Copper F.Paste F.Mask)
      (net 4 /RST))
    (pad 2 smd rect (at 2 0 90) (size 2 2) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:C_1206_handlötbar (layer Top_Copper) (tedit 5AA313A7)
    (at 120.5 105.222 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -1.249999 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 2.000001 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.270001 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.778 0 90) (size 1.5 1.6) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.778 0 90) (size 1.5 1.6) (layers Top_Copper F.Paste F.Mask)
      (net 20 /VRAW))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:C_1206_handlötbar (layer Top_Copper) (tedit 5AA313A7)
    (at 131 105.222 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 2 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.778 0 270) (size 1.5 1.6) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.778 0 270) (size 1.5 1.6) (layers Top_Copper F.Paste F.Mask)
      (net 16 /VREG_3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer Top_Copper) (tedit 5AFDED55)
    (at 139 99 180)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at -0.068 1 180) (layer F.SilkS) hide)
    (fp_text value ISCP (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54 180) (size 3.15 1) (layers Top_Copper F.Paste F.Mask)
      (net 7 /MISO-D12))
    (pad 2 smd rect (at 2.525 -2.54 180) (size 3.15 1) (layers Top_Copper F.Paste F.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at -2.525 0 180) (size 3.15 1) (layers Top_Copper F.Paste F.Mask)
      (net 8 /SCK-D13))
    (pad 4 smd rect (at 2.525 0 180) (size 3.15 1) (layers Top_Copper F.Paste F.Mask)
      (net 9 /MOSI-D11))
    (pad 5 smd rect (at -2.525 2.54 180) (size 3.15 1) (layers Top_Copper F.Paste F.Mask)
      (net 4 /RST))
    (pad 6 smd rect (at 2.525 2.54 180) (size 3.15 1) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer Top_Copper) (tedit 5AF86EC9)
    (at 127.16 95.1 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value AREF_ext (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /AREF))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:TQFP-32_7x7mm_Pitch0.8mm_INDEXDOT (layer Back_Copper) (tedit 5AA314F5)
    (at 150.75 100.6 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value ATMEGA328P-AU (at 0 -6.6 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 21 /D3-INT1))
    (pad 2 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 40 /D4))
    (pad 3 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 5 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 7 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 2 /XTAL1))
    (pad 8 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 3 /XTAL2))
    (pad 9 smd rect (at -2.8 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 5 /D5))
    (pad 10 smd rect (at -2 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 6 /D6))
    (pad 11 smd rect (at -1.2 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 39 /LED2))
    (pad 12 smd rect (at -0.4 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 17 /SELECT_SD))
    (pad 13 smd rect (at 0.4 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 22 /V_RTC_PIN))
    (pad 14 smd rect (at 1.2 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 38 /LED1))
    (pad 15 smd rect (at 2 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 9 /MOSI-D11))
    (pad 16 smd rect (at 2.8 -4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 7 /MISO-D12))
    (pad 17 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 43 "Net-(R6-Pad1)"))
    (pad 18 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 23 "Net-(C2-Pad1)"))
    (pad 19 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask))
    (pad 20 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 24 /AREF))
    (pad 21 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 15 /A7))
    (pad 23 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 35 /V_BLE_PIN))
    (pad 24 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 36 /TX_BLE))
    (pad 25 smd rect (at 2.8 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 37 /RX_BLE))
    (pad 26 smd rect (at 2 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 18 /ENABLE_SD))
    (pad 27 smd rect (at 1.2 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 10 /SDA-A4))
    (pad 28 smd rect (at 0.4 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 11 /SCL-A5))
    (pad 29 smd rect (at -0.4 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 4 /RST))
    (pad 30 smd rect (at -1.2 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 33 "Net-(J3-Pad1)"))
    (pad 31 smd rect (at -2 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 34 "Net-(J3-Pad2)"))
    (pad 32 smd rect (at -2.8 4.25) (size 1.6 0.55) (layers Back_Copper B.Paste B.Mask)
      (net 13 /D2-INT0))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:SOIC_normal+narrow.Pitch1.27 (layer Back_Copper) (tedit 5AE36AF0)
    (at 164.135 79.895 180)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 3.556 180) (layer B.SilkS) hide)
    (fp_text value 24XXYYYY (at 0 -3.68 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.175 1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 26 "Net-(J20-Pad2)"))
    (pad 2 smd rect (at -3.175 0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 27 "Net-(J21-Pad2)"))
    (pad 3 smd rect (at -3.175 -0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 28 "Net-(J22-Pad2)"))
    (pad 4 smd rect (at -3.175 -1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.175 1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 7 smd rect (at 3.175 0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.175 -0.635 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 11 /SCL-A5))
    (pad 5 smd rect (at 3.175 -1.905 180) (size 3 0.65) (layers Back_Copper B.Paste B.Mask)
      (net 10 /SDA-A4))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 141.75 97)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 15-33K (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 7 /MISO-D12))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 152.5 87)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 100N (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 15 /A7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 151.1 93.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 100N (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 24 /AREF))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 139.7 76.6 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 1.75 90) (layer B.SilkS) hide)
    (fp_text value INT/SQW_PUP (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 22 /V_RTC_PIN))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 13 /D2-INT0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 139.7 81.1 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 1.75 90) (layer B.SilkS) hide)
    (fp_text value INT/SQW_PUP (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 32 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 22 /V_RTC_PIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 152.5 89 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value 1M5 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 15 /A7))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 152.499999 91)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 4M7 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 20 /VRAW))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 15 /A7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Top_Copper) (tedit 5AA31355)
    (at 190.2 96.7 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 27-50K (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Top_Copper F.Paste F.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Top_Copper F.Paste F.Mask)
      (net 4 /RST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 189.9 116.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value "125K min" (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 42 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 189.25 113 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.75 270) (layer B.SilkS) hide)
    (fp_text value 33K (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 18 /ENABLE_SD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 148.000001 91)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 100N (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 23 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 141.75 99)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 15-33K (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 9 /MOSI-D11))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 164.5 120.98307 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value Rs2 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 21 /D3-INT1))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 132 121 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value Rs2 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 6 /D6))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 142 121 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value Rs2 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 5 /D5))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 152.25 121 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value Rs2 (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 40 /D4))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Top_Copper) (tedit 5AA31355)
    (at 137.55 104.3 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value R_LED (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Top_Copper F.Paste F.Mask)
      (net 19 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 171.25 121)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value SCL_pullup (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 11 /SCL-A5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 195.8 113 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.75 270) (layer B.SilkS) hide)
    (fp_text value 2,5N (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 25 /VCC_SD_TPS27082))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 42 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 148 89)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 23 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:Pin_Header_RxTxGND_2.54 (layer Top_Copper) (tedit 5AF0B803)
    (at 184.5 102.54 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value RxTxGND_Connector (at 0 7.41 180) (layer F.Fab))
    (fp_text user Rx (at 2.2 0 450) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (fp_text user Tx (at 2.2 2.5 270) (layer F.SilkS))
    (fp_text user GND (at 2.2 5.08 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 192.5 108.75)
    (fp_text reference J8 (at 3.089 -0.4) (layer B.SilkS) hide)
    (fp_text value SD_VCC_Select (at 0 5.715) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 14 /VCC_SD))
    (pad 1 smd rect (at -0.889 0) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 25 /VCC_SD_TPS27082))
    (pad 3 smd rect (at 0.889 0) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 167.495 74.816 90)
    (fp_text reference J20 (at 3.089 -0.4 90) (layer B.SilkS) hide)
    (fp_text value GS3 (at 0 5.715 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0 90) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 26 "Net-(J20-Pad2)"))
    (pad 1 smd rect (at -0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at 0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 164.135 74.816 90)
    (fp_text reference J21 (at 3.089 -0.4 90) (layer B.SilkS) hide)
    (fp_text value GS3 (at 0 5.715 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0 90) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 27 "Net-(J21-Pad2)"))
    (pad 1 smd rect (at -0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at 0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 160.96 74.816 90)
    (fp_text reference J22 (at 3.089 -0.4 90) (layer B.SilkS) hide)
    (fp_text value GS3 (at 0 5.715 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0 90) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 28 "Net-(J22-Pad2)"))
    (pad 1 smd rect (at -0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at 0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 167.31 88 90)
    (fp_text reference J23 (at 3.089 -0.4 90) (layer B.SilkS) hide)
    (fp_text value GS3 (at 0 5.715 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0 90) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 29 "Net-(J23-Pad2)"))
    (pad 1 smd rect (at -0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at 0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 164.052 88 90)
    (fp_text reference J24 (at 3.089 -0.4 90) (layer B.SilkS) hide)
    (fp_text value GS3 (at 0 5.715 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0 90) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 30 "Net-(J24-Pad2)"))
    (pad 1 smd rect (at -0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at 0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:SolderJumper_3way (layer Back_Copper) (tedit 5AF8AE51)
    (at 161 88 90)
    (fp_text reference J25 (at 3.089 -0.4 90) (layer B.SilkS) hide)
    (fp_text value GS3 (at 0 5.715 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0 90) (size 0.6 1.5) (layers Back_Copper B.Mask)
      (net 31 "Net-(J25-Pad2)"))
    (pad 1 smd rect (at -0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 16 /VREG_3V3))
    (pad 3 smd rect (at 0.889 0 90) (size 0.6 1.2) (layers Back_Copper B.Mask)
      (net 1 GND))
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 159.5 120.98307)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value Rs2 (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 21 /D3-INT1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:Via_Stitch_0.6mm (layer Top_Copper) (tedit 5AFDD22E)
    (at 192.6 98.1)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value Via_Stitch_0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.35) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer Back_Copper) (tedit 0)
    (at 129.8 80.9 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer Back_Copper) (tedit 0)
    (at 131 74.1 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer Top_Copper) (tedit 5B02F373)
    (at 117.5 90.1 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value ON/OFF (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /VRAW))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(BT2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 137.6 81.1 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.75 90) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 22 /V_RTC_PIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:C_1206_handlötbar (layer Back_Copper) (tedit 5AA313A7)
    (at 195.7 116.5 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 1.25 180) (layer B.SilkS) hide)
    (fp_text value 1u (at 0 -2 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.778 0 180) (size 1.5 1.6) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.778 0 180) (size 1.5 1.6) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.8 (layer Back_Copper) (tedit 5B07FD40)
    (at 128.7 102.4 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.8")
    (attr smd)
    (fp_text reference C10 (at 0 -4.56 180) (layer B.SilkS) hide)
    (fp_text value CP1_Small (at 0 4.56 180) (layer B.Fab))
    (fp_text user + (at -1.75 0.08 180) (layer B.Fab))
    (fp_text user + (at -4.28 -3.01 180) (layer B.SilkS))
    (fp_text user %R (at 0 -4.56 180) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Top_Copper) (tedit 5AA31355)
    (at 130.2 101.4)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1.3 1.3) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1.3 1.3) (layers Top_Copper F.Paste F.Mask)
      (net 16 /VREG_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 141.7 94 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.75 180) (layer B.SilkS) hide)
    (fp_text value 22R (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 43 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 8 /SCK-D13))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 155.4 90 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 1.75 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 35 /V_BLE_PIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:R_0805_HandSoldering_Eigener (layer Back_Copper) (tedit 5AA31355)
    (at 189.23 108.601 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 1.75 90) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 25 /VCC_SD_TPS27082))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.3) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:Keystone_18650_1043 (layer Top_Copper) (tedit 5B095CB5)
    (at 158 81.5 180)
    (fp_text reference BT2 (at -34 8 180) (layer F.SilkS) hide)
    (fp_text value 18650 (at 0 8 180) (layer F.Fab))
    (fp_text user "Keystone 1043" (at 0 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -36.11 0 180) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 36.11 0 180) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask)
      (net 41 "Net-(BT2-Pad1)"))
    (pad "" np_thru_hole circle (at -27.6 8 180) (size 3.55 3.55) (drill 3.55) (layers *.Cu))
    (pad "" np_thru_hole circle (at 27.6 -8 180) (size 3.55 3.55) (drill 3.55) (layers *.Cu))
    (pad "" np_thru_hole circle (at 36.11 8 180) (size 2.4 2.4) (drill 2.4) (layers *.Cu))
  )
  (module 000EigeneFootprints:TSOP-6_1.65x3.05mm_Pitch0.95mm_handsoldering (layer Back_Copper) (tedit 5B082A4F)
    (at 192.5 112.776 270)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U2 (at 0 2.45 270) (layer B.SilkS) hide)
    (fp_text value TPS27082L (at 0 -2.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.145756 540) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95 270) (size 1.1 0.6) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.1 0.6) (layers Back_Copper B.Paste B.Mask)
      (net 25 /VCC_SD_TPS27082))
    (pad 3 smd rect (at -1.35 -0.95 270) (size 1.1 0.6) (layers Back_Copper B.Paste B.Mask)
      (net 25 /VCC_SD_TPS27082))
    (pad 4 smd rect (at 1.35 -0.95 270) (size 1.1 0.6) (layers Back_Copper B.Paste B.Mask)
      (net 16 /VREG_3V3))
    (pad 5 smd rect (at 1.35 0 270) (size 1.1 0.6) (layers Back_Copper B.Paste B.Mask)
      (net 18 /ENABLE_SD))
    (pad 6 smd rect (at 1.35 0.95 270) (size 1.1 0.6) (layers Back_Copper B.Paste B.Mask)
      (net 42 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSOP-6_1.65x3.05mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:Renata_1225 (layer Back_Copper) (tedit 5B095A44)
    (at 178.9 83.5 270)
    (descr "Renata Knopfzellenhalter 1225")
    (tags "Keystone type 3034 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 1.2 7.6 270) (layer B.SilkS) hide)
    (fp_text value RTC_Backup (at 0 -11.5 270) (layer B.Fab) hide)
    (fp_text user + (at -8.2 -2.4 270) (layer B.SilkS))
    (fp_text user %R (at 4.4 7.6 270) (layer B.Fab) hide)
    (fp_text user - (at 0 -5.4 270) (layer B.SilkS))
    (fp_text user + (at 8.2 -2.4 270) (layer B.SilkS))
    (pad 2 smd circle (at 0 0 270) (size 10 10) (layers Back_Copper B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at 8.05 0 270) (size 3.5 3.5) (layers Back_Copper B.Paste B.Mask)
      (net 12 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -8.05 0 270) (size 3.5 3.5) (layers Back_Copper B.Paste B.Mask)
      (net 12 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery_Holders.3dshapes/Keystone_3034_1x20mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer Top_Copper) (tedit 58CE4E7E)
    (at 125.7 104.85 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value MCP1703A-3302_SOT223 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 90) (size 2 3.8) (layers Top_Copper F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers Top_Copper F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers Top_Copper F.Paste F.Mask)
      (net 16 /VREG_3V3))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers Top_Copper F.Paste F.Mask)
      (net 20 /VRAW))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000EigeneFootprints:WAGO250-402 (layer Top_Copper) (tedit 5B1BFE81)
    (at 123.5 117.5)
    (fp_text reference J17 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value "3xAA IN" (at -2.25 -8.5) (layer F.Fab))
    (fp_text user "Wago 250-402" (at -4.3 -0.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(BT2-Pad1)"))
    (pad 2 thru_hole circle (at -2.5 -5) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-402.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (module 000EigeneFootprints:WAGO250-403 (layer Top_Copper) (tedit 5B1BFE9B)
    (at 135.5 117.5)
    (fp_text reference J5 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at -3.75 -9.25) (layer F.Fab))
    (fp_text user "Wago 250-403" (at -7.05 -0.15 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D6))
    (pad 2 thru_hole circle (at -2.5 -5) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 16 /VREG_3V3))
    (pad 3 thru_hole circle (at -5 0) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-403.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (module 000EigeneFootprints:WAGO250-403 (layer Top_Copper) (tedit 5B1BFE9B)
    (at 165.58 117.5)
    (fp_text reference J10 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at -3.75 -9.25) (layer F.Fab))
    (fp_text user "Wago 250-403" (at -7.05 -0.15 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D3-INT1))
    (pad 2 thru_hole circle (at -2.5 -5) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 16 /VREG_3V3))
    (pad 3 thru_hole circle (at -5 0) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-403.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (module 000EigeneFootprints:WAGO250-403 (layer Top_Copper) (tedit 5B1BFE9B)
    (at 145.58 117.5)
    (fp_text reference J4 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at -3.75 -9.25) (layer F.Fab))
    (fp_text user "Wago 250-403" (at -7.05 -0.15 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D5))
    (pad 2 thru_hole circle (at -2.5 -5) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 16 /VREG_3V3))
    (pad 3 thru_hole circle (at -5 0) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-403.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (module 000EigeneFootprints:WAGO250-403 (layer Top_Copper) (tedit 5B1BFE9B)
    (at 155.58 117.5)
    (fp_text reference J2 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at -3.75 -9.25) (layer F.Fab))
    (fp_text user "Wago 250-403" (at -7.05 -0.15 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D4))
    (pad 2 thru_hole circle (at -2.5 -5) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 16 /VREG_3V3))
    (pad 3 thru_hole circle (at -5 0) (size 2 2) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-403.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (module 000EigeneFootprints:WAGO250-404 (layer Top_Copper) (tedit 5B1BFEB6)
    (at 179.58 117.5)
    (fp_text reference J6 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value I2C1 (at -2.25 -8.5) (layer F.Fab))
    (fp_text user "Wago 250-404" (at -9.8 -0.15 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SDA-A4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCL-A5))
    (pad 3 thru_hole circle (at -5.08 0) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 /VREG_3V3))
    (pad 4 thru_hole circle (at -7.62 -5.08) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-404.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (module 000EigeneFootprints:WAGO250-404 (layer Top_Copper) (tedit 5B1BFEB6)
    (at 179.58 102.5)
    (fp_text reference J7 (at -3.75 6.5) (layer F.SilkS) hide)
    (fp_text value I2C2 (at -2.25 -8.5) (layer F.Fab))
    (fp_text user "Wago 250-404" (at -9.8 -0.15 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SDA-A4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCL-A5))
    (pad 3 thru_hole circle (at -5.08 0) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 /VREG_3V3))
    (pad 4 thru_hole circle (at -7.62 -5.08) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../../../../../../Users/gerd/Documents/KiCAD-Projekte/000_Eigene_Symbole/3D-Modelle/Wago250-404.wrl
      (at (xyz 0.047 0 0))
      (scale (xyz 0.397 0.397 0.397))
      (rotate (xyz -90 0 90))
    )
  )
  (gr_text GND (at 134.239 96.52 90) (layer F.SilkS))
  (gr_text 3V3 (at 134.239 101.473 90) (layer F.SilkS))
  (gr_text GND (at 194.056 79.5) (layer B.SilkS))
  (gr_text "3V3 programming only!" (at 144.145 100.584 90) (layer F.SilkS))
  (gr_text Ø4 (at 192.151 93.345) (layer F.SilkS))
  (gr_text Ø7 (at 194.564 93.345) (layer F.SilkS))
  (gr_arc (start 200 100.5) (end 200 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 200 95.5) (end 200.5 95.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 116 100) (end 115.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 116 95) (end 116 95.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Renata 100380" (at 172.8978 83.5152 270) (layer B.SilkS))
  (gr_text "https://hackaday.io/project/78326-upower-beehive-sd-logger\nV1.2.1 (09.06.2018)\nby J-G W." (at 199.3138 72.263) (layer B.SilkS))
  (gr_text A7 (at 134.3152 88.2142) (layer B.SilkS))
  (gr_text 100n (at 156.972 90.043 270) (layer B.SilkS))
  (gr_text "supply sense voltage divider:\nV_raw―R17―R18―GND" (at 139.446 86.106) (layer B.SilkS))
  (gr_text R17 (at 154.6098 93.599) (layer B.SilkS))
  (gr_text "put cap only if\nVCC is unstable" (at 133.5 107.1) (layer B.SilkS))
  (gr_text "ca. 30k" (at 142.5 71.8) (layer B.SilkS))
  (gr_text "ca. 30k" (at 136.6 84.2) (layer B.SilkS))
  (gr_text "ca. 30k" (at 137 99) (layer B.SilkS))
  (gr_text "ca. 30k" (at 137 97) (layer B.SilkS))
  (gr_text "ca. 30k" (at 196.6 107.2) (layer B.SilkS))
  (gr_text 22-27R (at 137.1 94) (layer B.SilkS))
  (gr_text "ca. 30k" (at 185.2 113 270) (layer B.SilkS))
  (gr_text 125k (at 187 116.5 270) (layer B.SilkS))
  (gr_text 1µ (at 199.136 116.332 270) (layer B.SilkS))
  (gr_text 2n5 (at 197.231 112.903 270) (layer B.SilkS))
  (gr_text 100n (at 187.071 108.585 270) (layer B.SilkS))
  (gr_text 100n (at 152.527 85.598) (layer B.SilkS))
  (gr_text 1-1k5 (at 134.1 106.8 90) (layer F.SilkS))
  (gr_text 100n (at 130.2 99.9) (layer F.SilkS))
  (gr_text "ca. 100µ" (at 129.4 98.2) (layer B.SilkS))
  (gr_text 100n (at 136 81.1 270) (layer B.SilkS))
  (gr_text "ca. 4k7" (at 174.8 119.5) (layer B.SilkS))
  (gr_text "ca. 30k" (at 190.2 95.1) (layer F.SilkS))
  (gr_text "MCP1700 (max. 6.5V)\nMCP1703 (max. 16V)" (at 126.1 123.7 90) (layer F.SilkS))
  (gr_text R18 (at 148 86.8) (layer B.SilkS))
  (gr_text V_raw (at 121.9 79.5) (layer B.SilkS))
  (gr_text ON/OFF (at 118.37 92.8) (layer F.SilkS))
  (dimension 55 (width 0.1) (layer F.Fab)
    (gr_text "55,000 mm" (at 204.5 97.5 90) (layer F.Fab))
    (feature1 (pts (xy 200.5 70) (xy 205.1 70)))
    (feature2 (pts (xy 200.5 125) (xy 205.1 125)))
    (crossbar (pts (xy 203.9 125) (xy 203.9 70)))
    (arrow1a (pts (xy 203.9 70) (xy 204.486421 71.126504)))
    (arrow1b (pts (xy 203.9 70) (xy 203.313579 71.126504)))
    (arrow2a (pts (xy 203.9 125) (xy 204.486421 123.873496)))
    (arrow2b (pts (xy 203.9 125) (xy 203.313579 123.873496)))
  )
  (gr_text "if #: don't\nplace framed\ncomponents" (at 199.39 120.396) (layer B.SilkS))
  (gr_text TPS27082 (at 196.25 110.3) (layer B.SilkS))
  (gr_text "I2C global pullups" (at 174.775 124) (layer B.SilkS))
  (gr_text "place only ONE" (at 161.75 124) (layer B.SilkS))
  (gr_text "use V_in OR 18650 cell! " (at 116.8 114.65 90) (layer F.SilkS))
  (gr_text "18650 cell\n" (at 118.8 74.2 90) (layer F.SilkS))
  (gr_text "dual LED" (at 137.7 109.3) (layer F.SilkS))
  (gr_text "microSD socket\nAttend\n1121-TXAR-R" (at 192.5 111.85) (layer F.SilkS))
  (gr_text "MCP1700\nMCP1703\nSOT-223" (at 125.75 104.902) (layer F.SilkS))
  (gr_text 1µ (at 131 108.75) (layer F.SilkS))
  (gr_text 1µ (at 120.5 108.75) (layer F.SilkS))
  (gr_text 8MHz (at 141.75 105 45) (layer B.SilkS))
  (gr_text Resonator (at 146.75 106 315) (layer B.SilkS))
  (gr_text DS3231 (at 150.241 72.263) (layer B.SilkS))
  (gr_text "10µH or 47R" (at 141.6 89.05) (layer B.SilkS))
  (gr_text 100n (at 151.1 94.9) (layer B.SilkS))
  (gr_text 100n (at 144.1 90.7) (layer B.SilkS))
  (gr_text 100n (at 152.85 108.95) (layer B.SilkS))
  (gr_text "SD VCC select\n*  on/off via pin A3\n#  tied to 3V3" (at 199.4 103.45) (layer B.SilkS))
  (gr_text "#" (at 193 106.75) (layer B.SilkS))
  (gr_text * (at 191.95 107) (layer B.SilkS))
  (gr_text "CR1225 (3V)" (at 186.1566 83.5152 270) (layer B.SilkS))
  (gr_text "Address select" (at 171.35 77.05 270) (layer B.SilkS))
  (gr_text A1 (at 167.5 72.6) (layer B.SilkS))
  (gr_text A2 (at 164.15 72.6) (layer B.SilkS))
  (gr_text + (at 159.5 75.65) (layer B.SilkS))
  (gr_text - (at 159.5 73.85) (layer B.SilkS))
  (gr_text A3 (at 160.95 72.6) (layer B.SilkS))
  (gr_text A3 (at 161 85.85) (layer B.SilkS))
  (gr_text A2 (at 164.05 85.85) (layer B.SilkS))
  (gr_text A1 (at 167.3 85.85) (layer B.SilkS))
  (gr_text - (at 159.45 87.1) (layer B.SilkS))
  (gr_text + (at 159.45 88.9) (layer B.SilkS))
  (gr_text "EEPROM 2" (at 162.433 83.566) (layer B.SilkS))
  (gr_text "EEPROM 1" (at 162.306 96.393) (layer B.SilkS))
  (gr_text ICSP (at 139 94) (layer F.SilkS))
  (gr_text RESET (at 190.25 102.25) (layer F.SilkS))
  (gr_text I2C (at 181.25 106.25 90) (layer F.SilkS))
  (gr_text I2C (at 181.25 121.5 90) (layer F.SilkS))
  (gr_text "- V_in +" (at 121.5 123.5) (layer F.SilkS))
  (gr_text "+ V_in -" (at 121.5 123.5) (layer B.SilkS))
  (gr_text GND (at 127.6 97.9 315) (layer F.SilkS))
  (gr_text AREF (at 130.6 98.1 315) (layer F.SilkS))
  (gr_text Pullup (at 171.2 122.9) (layer B.SilkS))
  (gr_text Pullup (at 178.5 122.9) (layer B.SilkS))
  (gr_text "D6 Pullup" (at 132 123) (layer B.SilkS))
  (gr_text "D5 Pullup" (at 142 123) (layer B.SilkS))
  (gr_text "D4 Pullup" (at 152.25 123) (layer B.SilkS))
  (gr_text Pulld. (at 159.5 123) (layer B.SilkS))
  (gr_text Pullup (at 164.5 123) (layer B.SilkS))
  (gr_text GND (at 170.25 108.25) (layer F.SilkS))
  (gr_text SDA (at 179.5 108.25) (layer F.SilkS))
  (gr_text SCL (at 176.5 108.25) (layer F.SilkS))
  (gr_text 3V3 (at 173.5 108.25) (layer F.SilkS))
  (gr_text SDA (at 179.5 123.5) (layer F.SilkS))
  (gr_text SCL (at 176.5 123.5) (layer F.SilkS))
  (gr_text 3V3 (at 173.5 123.5) (layer F.SilkS))
  (gr_text GND (at 170.25 123.5) (layer F.SilkS))
  (gr_text INT1 (at 165.5 123.5) (layer F.SilkS))
  (gr_text 3V3 (at 162.25 123.5) (layer F.SilkS))
  (gr_text GND (at 159 123.5) (layer F.SilkS))
  (gr_text D4 (at 156 123.5) (layer F.SilkS))
  (gr_text 3V3 (at 152.65 123.5) (layer F.SilkS))
  (gr_text GND (at 149 123.5) (layer F.SilkS))
  (gr_text D5 (at 146 123.5) (layer F.SilkS))
  (gr_text 3V3 (at 142.55 123.5) (layer F.SilkS))
  (gr_text GND (at 139 123.5) (layer F.SilkS))
  (gr_text D6 (at 135.75 123.5) (layer F.SilkS))
  (gr_text 3V3 (at 132.55 123.5) (layer F.SilkS))
  (gr_text GND (at 129 123.5) (layer F.SilkS))
  (gr_arc (start 117 123.5) (end 117 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 199 123.5) (end 200.5 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 199 71.5) (end 199 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117 71.5) (end 115.5 71.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.5 123.5) (end 200.5 100.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 197.5 98) (end 197.500001 100.000001) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 96) (end 197.500002 96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 100) (end 197.500001 100.000001) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.5 100) (end 115.5 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.5 97.5) (end 118.5 95.5) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116 99.5) (end 118.5 99.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116 95.5) (end 118.5 95.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.5 95.5) (end 200.5 71.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117 125) (end 199 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.5 71.5) (end 115.5 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199 70) (end 117 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Top_Copper) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.4) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 115.5 70) (xy 200.5 70) (xy 200.5 95.5) (xy 195 95.5) (xy 195 100.5)
        (xy 200.5 100.5) (xy 200.5 125) (xy 115.5 125) (xy 115.5 100) (xy 121 100)
        (xy 121 95) (xy 115.5 95)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Back_Copper) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.4) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 115.5 70) (xy 200.5 70) (xy 200.5 95.5) (xy 195 95.5) (xy 195 100.5)
        (xy 200.5 100.5) (xy 200.5 125) (xy 115.5 125) (xy 115.5 100) (xy 121 100)
        (xy 121 95) (xy 115.5 95)
      )
    )
  )
)
