(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 439)
    (zones 0)
    (modules 43)
    (nets 71)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.1778)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 1.016 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0381)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00008_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 USB_C_D_N)
  (net 2 USB_C_D_P)
  (net 3 +3V3)
  (net 4 "Net-(L1-Pad2)")
  (net 5 +5V)
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(JP2-Pad1)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(D2-Pad1)")
  (net 11 "Net-(C4-Pad1)")
  (net 12 "Net-(R11-Pad1)")
  (net 13 GND)
  (net 14 "Net-(R10-Pad2)")
  (net 15 "Net-(R9-Pad2)")
  (net 16 "Net-(R1-Pad1)")
  (net 17 "Net-(J2-PadB5)")
  (net 18 "Net-(J2-PadA5)")
  (net 19 "Net-(R5-Pad2)")
  (net 20 "Net-(R6-Pad2)")
  (net 21 "Net-(JP1-Pad2)")
  (net 22 "Net-(R7-Pad2)")
  (net 23 "Net-(J1-Pad1)")
  (net 24 "Net-(D1-Pad1)")
  (net 25 "Net-(U3-Pad2)")
  (net 26 "Net-(U3-Pad3)")
  (net 27 "Net-(U3-Pad6)")
  (net 28 "Net-(U3-Pad9)")
  (net 29 "Net-(U3-Pad10)")
  (net 30 "Net-(U3-Pad11)")
  (net 31 "Net-(U3-Pad12)")
  (net 32 "Net-(U3-Pad13)")
  (net 33 "Net-(U3-Pad14)")
  (net 34 "Net-(C1-Pad1)")
  (net 35 "Net-(U3-Pad22)")
  (net 36 "Net-(U3-Pad23)")
  (net 37 "Net-(U3-Pad27)")
  (net 38 "Net-(U3-Pad28)")
  (net 39 "Net-(U5-Pad7)")
  (net 40 "Net-(U5-Pad8)")
  (net 41 "Net-(C6-Pad1)")
  (net 42 "Net-(U2-Pad15)")
  (net 43 "Net-(U2-Pad14)")
  (net 44 "Net-(U2-Pad11)")
  (net 45 "Net-(D3-Pad1)")
  (net 46 "Net-(U2-Pad8)")
  (net 47 "Net-(U2-Pad5)")
  (net 48 "Net-(U2-Pad4)")
  (net 49 "Net-(U2-Pad1)")
  (net 50 "Net-(J1-Pad4)")
  (net 51 "Net-(J2-PadA2)")
  (net 52 "Net-(J2-PadA3)")
  (net 53 "Net-(J2-PadA10)")
  (net 54 "Net-(J2-PadA8)")
  (net 55 "Net-(J2-PadA11)")
  (net 56 "Net-(J2-PadB2)")
  (net 57 "Net-(J2-PadB3)")
  (net 58 "Net-(J2-PadB8)")
  (net 59 "Net-(J2-PadB10)")
  (net 60 "Net-(J2-PadB11)")
  (net 61 /Sheet5C4CE702/USB_B_P)
  (net 62 /Sheet5C4CE702/USB2_P)
  (net 63 /Sheet5C4CE702/USB2_N)
  (net 64 /Sheet5C4CE702/USB_B_N)
  (net 65 /Sheet5C4CE702/USB1_N)
  (net 66 /Sheet5C4CE702/USB1_P)
  (net 67 UART_RX_MIO14)
  (net 68 UART_TX_MIO15)
  (net 69 /Sheet5C4CE702/USB_P)
  (net 70 /Sheet5C4CE702/USB_N)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.2032)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.1778)
    (diff_pair_width 0.2794)
    (add_net +3V3)
    (add_net +5V)
    (add_net /Sheet5C4CE702/USB1_N)
    (add_net /Sheet5C4CE702/USB1_P)
    (add_net /Sheet5C4CE702/USB2_N)
    (add_net /Sheet5C4CE702/USB2_P)
    (add_net /Sheet5C4CE702/USB_B_N)
    (add_net /Sheet5C4CE702/USB_B_P)
    (add_net /Sheet5C4CE702/USB_N)
    (add_net /Sheet5C4CE702/USB_P)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-PadA10)")
    (add_net "Net-(J2-PadA11)")
    (add_net "Net-(J2-PadA2)")
    (add_net "Net-(J2-PadA3)")
    (add_net "Net-(J2-PadA5)")
    (add_net "Net-(J2-PadA8)")
    (add_net "Net-(J2-PadB10)")
    (add_net "Net-(J2-PadB11)")
    (add_net "Net-(J2-PadB2)")
    (add_net "Net-(J2-PadB3)")
    (add_net "Net-(J2-PadB5)")
    (add_net "Net-(J2-PadB8)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net UART_RX_MIO14)
    (add_net UART_TX_MIO15)
  )
  (net_class diffp ""
    (clearance 0.1778)
    (trace_width 0.2794)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.1778)
    (diff_pair_width 0.2794)
    (add_net USB_C_D_N)
    (add_net USB_C_D_P)
  )
  (module Package_SO:SSOP-28_5.3x10.2mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 132.08 131.318 180)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (solder_paste_margin -0.0508)
    (attr smd)
    (fp_text reference U3 (at -0.508 5.969 180) (layer F.SilkS))
    (fp_text value FT232RL (at 0 6.25 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 67 UART_RX_MIO14))
    (pad 2 smd rect (at -3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at -3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 68 UART_TX_MIO15))
    (pad 6 smd rect (at -3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 8 smd rect (at -3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at -3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at -3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U3-Pad11)"))
    (pad 12 smd rect (at -3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at -3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U3-Pad13)"))
    (pad 14 smd rect (at -3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 69 /Sheet5C4CE702/USB_P))
    (pad 16 smd rect (at 3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 70 /Sheet5C4CE702/USB_N))
    (pad 17 smd rect (at 3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad1)"))
    (pad 18 smd rect (at 3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 19 smd rect (at 3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R7-Pad2)"))
    (pad 20 smd rect (at 3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 21 smd rect (at 3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 22 smd rect (at 3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U3-Pad22)"))
    (pad 23 smd rect (at 3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U3-Pad23)"))
    (pad 24 smd rect (at 3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 26 smd rect (at 3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 27 smd rect (at 3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U3-Pad27)"))
    (pad 28 smd rect (at 3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U3-Pad28)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-28_5.3x10.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 149.733 114.935)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.445 121.793 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.413 0.254 270) (layer F.SilkS))
    (fp_text value 100nF_603 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.238 130.175 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -3.175 -0.381 270) (layer F.SilkS))
    (fp_text value 100nF_603 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.875 129.032 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 9.271 -0.635 180) (layer F.SilkS))
    (fp_text value 100nF_603 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.683 124.079 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.127 -1.27 180) (layer F.SilkS))
    (fp_text value 100nF_603 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.414 122.682 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.54 -0.889 180) (layer F.SilkS))
    (fp_text value 100nF_603 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1812_4532Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.127 119.634 270)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.794 -2.921) (layer F.SilkS))
    (fp_text value 22uF_lo_ESR (at 0 2.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -2.1375 0 270) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 5 +5V))
    (pad 2 smd roundrect (at 2.1375 0 270) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 13 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1812_4532Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.224 122.428 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.016 2.667 180) (layer F.SilkS))
    (fp_text value 22uF_lo_ESR (at 0 2.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 2.1375 0 180) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 13 GND))
    (pad 1 smd roundrect (at -2.1375 0 180) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1812_4532Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.478 116.205 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.286 2.921 180) (layer F.SilkS))
    (fp_text value 22uF_lo_ESR (at 0 2.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.1375 0 90) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 2.1375 0 90) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 13 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 139.0269 135.0391 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 8.7249 2.9591 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125.476 135.128 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at -2.286 3.175) (layer F.SilkS))
    (fp_text value Jumper_3_Bridged12 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 147.193 114.935)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at -2.667 0.762 90) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 UART_RX_MIO14))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 UART_TX_MIO15))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Amphenol_12401610E4-2A_CircularHoles (layer F.Cu) (tedit 5A142044)
    (at 118.872 119.126 270)
    (descr "USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A")
    (tags "USB C Type-C Receptacle SMD")
    (attr smd)
    (fp_text reference J2 (at 6.096 4.699) (layer F.SilkS))
    (fp_text value USB_C_Receptacle (at 0 6.14 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad S1 thru_hole circle (at -4.13 -3.11 270) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad A1 smd rect (at -2.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad A2 smd rect (at -2.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J2-PadA2)"))
    (pad A3 smd rect (at -1.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J2-PadA3)"))
    (pad A4 smd rect (at -1.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad A5 smd rect (at -0.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-PadA5)"))
    (pad A6 smd rect (at -0.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 USB_C_D_P))
    (pad A7 smd rect (at 0.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 USB_C_D_N))
    (pad A12 smd rect (at 2.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad A10 smd rect (at 1.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J2-PadA10)"))
    (pad A9 smd rect (at 1.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad A8 smd rect (at 0.75 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J2-PadA8)"))
    (pad A11 smd rect (at 2.25 -5.02 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J2-PadA11)"))
    (pad B1 smd rect (at 2.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad S1 thru_hole circle (at 4.13 -3.11 270) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad S1 thru_hole circle (at 4.49 2.84 270) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad S1 thru_hole circle (at -4.49 2.84 270) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad "" np_thru_hole circle (at 3.6 -4.36 270) (size 0.95 0.95) (drill 0.95) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.6 -4.36 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad B2 smd rect (at 2 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J2-PadB2)"))
    (pad B3 smd rect (at 1.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J2-PadB3)"))
    (pad B4 smd rect (at 1 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad B5 smd rect (at 0.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-PadB5)"))
    (pad B6 smd rect (at 0 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 USB_C_D_P))
    (pad B7 smd rect (at -0.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 USB_C_D_N))
    (pad B8 smd rect (at -1 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J2-PadB8)"))
    (pad B9 smd rect (at -1.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad B10 smd rect (at -2 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J2-PadB10)"))
    (pad B11 smd rect (at -2.5 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J2-PadB11)"))
    (pad B12 smd rect (at -3 -3.32 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Amphenol_12401610E4-2A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 5A1DC0BD)
    (at 115.824 132.207 270)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J1 (at 0.889 -3.556 180) (layer F.SilkS))
    (fp_text value USB_miniB (at 0 4.6 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -0.65 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 64 /Sheet5C4CE702/USB_B_N))
    (pad 3 smd rect (at 0 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 61 /Sheet5C4CE702/USB_B_P))
    (pad 4 smd rect (at 0.65 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd rect (at -2.4625 -1.1 270) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd rect (at 2.4625 -1.1 270) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd rect (at -2.91 1.2 270) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd rect (at 2.91 1.2 270) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd rect (at -0.84 1.2 270) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd rect (at 0.84 1.2 270) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.51 135.255 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at -0.254 -11.811 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.098 132.08 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at -0.254 2.032 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.859 135.2295 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at -0.1525 -11.557 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(D3-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5C3AA3BE)
    (at 139.827 128.524 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (solder_paste_margin -0.03048)
    (attr smd)
    (fp_text reference U2 (at -2.667 1.524) (layer F.SilkS))
    (fp_text value UTC2000 (at 0 2.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at -0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 13 GND))
    (pad "" smd rect (at -0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad15)"))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-Pad14)"))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R11-Pad1)"))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-Pad11)"))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-Pad8)"))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R5-Pad2)"))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R6-Pad2)"))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-Pad5)"))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad4)"))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R9-Pad2)"))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R10-Pad2)"))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5A650279)
    (at 134.493 122.428)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (solder_paste_margin -0.03048)
    (attr smd)
    (fp_text reference U5 (at 0.127 2.794) (layer F.SilkS))
    (fp_text value SC185 (at 0 2.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad1)"))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad1)"))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U5-Pad7)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U5-Pad8)"))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C6-Pad1)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(L1-Pad2)"))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(L1-Pad2)"))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(L1-Pad2)"))
    (pad "" smd rect (at -0.45 0.45) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 13 GND))
    (pad "" smd rect (at 0.45 0.45) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 -0.45) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.45 -0.45) (size 0.73 0.73) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:UQFN-10_1.6x2.1mm_P0.5mm (layer F.Cu) (tedit 5B5C1E86)
    (at 122.555 128.651 270)
    (descr "UQFN, 10 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/00001725D.pdf (Page 12)), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "UQFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at -1.905 1.651) (layer F.SilkS))
    (fp_text value USB3740B-AI9 (at 0 2.35 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.625 -0.25 270) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /Sheet5C4CE702/USB1_N))
    (pad 2 smd roundrect (at -0.625 0.25 270) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /Sheet5C4CE702/USB1_P))
    (pad 3 smd roundrect (at -0.5 1 270) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 4 smd roundrect (at 0 1 270) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R1-Pad1)"))
    (pad 5 smd roundrect (at 0.5 1 270) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 6 smd roundrect (at 0.625 0.25 270) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /Sheet5C4CE702/USB2_P))
    (pad 7 smd roundrect (at 0.625 -0.25 270) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /Sheet5C4CE702/USB2_N))
    (pad 8 smd roundrect (at 0.5 -1 270) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 9 smd roundrect (at 0 -1 270) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /Sheet5C4CE702/USB_N))
    (pad 10 smd roundrect (at -0.5 -1 270) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /Sheet5C4CE702/USB_P))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-10_1.6x2.1mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 149.479 134.874 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 4.445 1.397 90) (layer F.SilkS))
    (fp_text value 74LVC1G00 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.761 128.905 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.524 1.651) (layer F.SilkS))
    (fp_text value R100k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(J1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.812 130.429 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 1.397 9.271) (layer F.SilkS))
    (fp_text value 35k7 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.714 132.588)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.127 -3.175) (layer F.SilkS))
    (fp_text value R10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.952 130.937)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.889 -2.794) (layer F.SilkS))
    (fp_text value R4k7 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.746 123.444)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.54 2.032) (layer F.SilkS))
    (fp_text value R10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(J2-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.746 124.968)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.778 1.651) (layer F.SilkS))
    (fp_text value R10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J2-PadA5)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.492 115.824 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.413 0.127 180) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J2-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.3683 114.1857)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.4257 -0.1397) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(J2-PadB5)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 115.189 126.492)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0.762 -1.27) (layer F.SilkS))
    (fp_text value R100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.51 125.222 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -0.889 8.001 180) (layer F.SilkS))
    (fp_text value R10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.51 126.746 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -1.27 8.255 180) (layer F.SilkS))
    (fp_text value R10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.399 129.032 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -9.144 -0.381) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.921 121.793 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.794 -0.127 90) (layer F.SilkS))
    (fp_text value 1 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.288 135.128 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -0.127 12.319 270) (layer F.SilkS))
    (fp_text value R100k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.51 132.207 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -6.35 -2.159 270) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 141.859 132.207 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -6.35 1.27) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.812 134.493 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -0.762 12.7 270) (layer F.SilkS))
    (fp_text value R100k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.923 132.08)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -0.381 -8.255 180) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module proj_footprints:L_CDMC6D28 (layer F.Cu) (tedit 5C36D1E6)
    (at 135.255 116.84 180)
    (fp_text reference L1 (at 4.572 1.397 180) (layer F.SilkS))
    (fp_text value 1uH (at 0 -2.75 180) (layer F.Fab))
    (pad 1 smd roundrect (at -2.85 0 180) (size 2 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 2.85 0 180) (size 2 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(L1-Pad2)"))
  )
  (module proj_footprints:WE_CNSW (layer F.Cu) (tedit 5C36D7E2)
    (at 118.491 125.857)
    (fp_text reference FL1 (at 2.794 -0.254) (layer F.SilkS))
    (fp_text value EMI_Filter_LL_14 (at 0 3.6) (layer F.Fab))
    (pad 4 smd roundrect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 USB_C_D_N))
    (pad 3 smd roundrect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /Sheet5C4CE702/USB1_N))
    (pad 2 smd roundrect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /Sheet5C4CE702/USB1_P))
    (pad 1 smd roundrect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 USB_C_D_P))
  )
  (module proj_footprints:WE_CNSW (layer F.Cu) (tedit 5C36D7E2)
    (at 120.142 131.826)
    (fp_text reference FL2 (at 1.27 -1.27) (layer F.SilkS))
    (fp_text value EMI_Filter_LL_14 (at 0 3.6) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /Sheet5C4CE702/USB_B_P))
    (pad 2 smd roundrect (at 0.85 0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /Sheet5C4CE702/USB2_P))
    (pad 3 smd roundrect (at 0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /Sheet5C4CE702/USB2_N))
    (pad 4 smd roundrect (at -0.85 -0.4) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /Sheet5C4CE702/USB_B_N))
  )
  (gr_line (start 113.284 136.906) (end 113.284 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.6888 136.906) (end 113.284 136.906) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.6888 113.03) (end 151.6888 136.906) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.284 113.03) (end 151.6888 113.03) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name "Net-(L1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.731 121.158) (xy 131.5339 118.2116) (xy 131.5212 115.3668) (xy 133.7437 115.3668) (xy 134.874 120.4468)
        (xy 134.8994 121.158)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 137.033 115.062) (xy 142.493899 115.092651) (xy 144.78 115.062) (xy 144.78 113.792) (xy 148.59 113.792)
        (xy 148.59 118.491) (xy 144.78 118.491) (xy 144.78 124.079) (xy 141.986 124.0663) (xy 140.5763 119.8245)
        (xy 137.0838 119.8118)
      )
    )
  )
  (zone (net 13) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 151.257 136.525) (xy 113.665 136.525) (xy 113.665 113.411) (xy 151.257 113.411)
      )
    )
    (polygon
      (pts
        (xy 130.302 114.3) (xy 130.302 118.618) (xy 130.81 120.142) (xy 132.207 120.142) (xy 132.588 121.412)
        (xy 135.001 121.412) (xy 135.001 114.3)
      )
    )
  )
  (zone (net 5) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 125.603 117.221) (xy 129.286 117.221) (xy 130.937 120.523) (xy 132.08 120.523) (xy 133.35 121.539)
        (xy 133.35 122.428) (xy 129.54 122.428) (xy 125.73 120.65)
      )
    )
  )
  (zone (net 5) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 141.80644 127.541197) (xy 141.224 127.508) (xy 141.224 126.619) (xy 145.288 126.619) (xy 145.288 131.445)
        (xy 144.272 131.445)
      )
    )
  )
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 113.665 113.411) (xy 151.257 113.411) (xy 151.257 136.525) (xy 113.665 136.525)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.302 114.3) (xy 135.001 114.3) (xy 135.001 121.412) (xy 132.588 121.412) (xy 132.207 120.142)
        (xy 130.81 120.142) (xy 130.302 118.491)
      )
    )
  )
)
