(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6002)
    (drawings 46)
    (tracks 28)
    (zones 0)
    (modules 18)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +24V)
  (net 2 GND)
  (net 3 /SENSOR1_INT_L)
  (net 4 +3V3)
  (net 5 /SENSOR2_INT_L)
  (net 6 "Net-(J11-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +24V)
    (add_net +3V3)
    (add_net /SENSOR1_INT_L)
    (add_net /SENSOR2_INT_L)
    (add_net GND)
    (add_net "Net-(J11-Pad4)")
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer F.Cu) (tedit 5AE50EF0)
    (at 97.162 80.274 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C1 (at 3.75 -2.67 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.75 2.67 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer F.Cu) (tedit 5AE50EF0)
    (at 125.902 84.866 270)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C2 (at 3.75 -2.67 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.75 2.67 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer F.Cu) (tedit 5AE50EF0)
    (at 141.562 84.276 270)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C3 (at 3.75 -2.67 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.75 2.67 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 7.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 104.112 77.704 90)
    (descr "Molex SPOX Connector System, 5267-02A, 2 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J1 (at 1.25 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical (layer F.Cu) (tedit 5B783167)
    (at 97.254 106.38 90)
    (descr "Molex PicoBlade Connector System, 53047-0410, 4 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (fp_text reference J2 (at 1.88 -3.25 90) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 1.88 2.35 90) (layer F.Fab))
    (fp_text user %R (at 1.88 -1.35 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.25 0 90) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /SENSOR1_INT_L))
    (pad 3 thru_hole oval (at 2.5 0 90) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 /SENSOR2_INT_L))
    (pad 4 thru_hole oval (at 3.75 0 90) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 152.422 99.06 270)
    (descr "Molex SPOX Connector System, 5267-03A, 3 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J3 (at 2.5 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 /SENSOR1_INT_L))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 133.272 86.986 270)
    (descr "Molex SPOX Connector System, 5267-02A, 2 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J4 (at 1.25 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2.4 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 147.442 86.856 270)
    (descr "Molex SPOX Connector System, 5267-02A, 2 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J5 (at 6.108 0.122 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 142.922 99.1 270)
    (descr "Molex SPOX Connector System, 5267-03A, 3 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J6 (at 2.5 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -2.4 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 /SENSOR1_INT_L))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer F.Cu) (tedit 5AE50EF0)
    (at 148.5392 79.756 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C4 (at 3.75 -2.67 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.75 2.67 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal (layer F.Cu) (tedit 5AE50EF0)
    (at 133.3754 80.2132 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (fp_text reference C5 (at 3.75 -2.67 90) (layer F.SilkS))
    (fp_text value 0.1u (at 3.75 2.67 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 124.2314 99.0638 270)
    (descr "Molex SPOX Connector System, 5267-03A, 3 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J7 (at 2.5 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 /SENSOR2_INT_L))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 133.0198 99.06 270)
    (descr "Molex SPOX Connector System, 5267-03A, 3 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J8 (at 2.5 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -2.4 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 /SENSOR2_INT_L))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-03A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 126.8476 77.557 90)
    (descr "Molex SPOX Connector System, 5267-02A, 2 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J9 (at 1.25 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7833F7)
    (at 141.9098 77.2922 90)
    (descr "Molex SPOX Connector System, 5267-02A, 2 Pins per row (http://www.molex.com/pdm_docs/sd/022035035_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SPOX side entry")
    (fp_text reference J10 (at 1.25 -4.3 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2.4 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.85) (drill 0.85) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_SPOX_5267-02A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 103.3018 106.6038 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SENSOR1_INT_L))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SENSOR2_INT_L))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J11-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 167.894 88.392)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 94.234 88.392)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 162.56 111.76) (end 172.72 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162.306 68.58) (end 172.72 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_text "RX Ap1" (at 148.082 109.474) (layer F.SilkS))
  (gr_text "RX Ap2" (at 129.032 109.728) (layer F.SilkS))
  (gr_text "TX Ap2" (at 120.65 88.138 90) (layer F.SilkS))
  (gr_text "TX Ap1" (at 120.65 75.946 90) (layer F.SilkS))
  (gr_text GND (at 106.934 106.68) (layer F.SilkS))
  (gr_text SENSOR1_INT_L (at 110.998 104.14) (layer F.SilkS))
  (gr_text SENSOR2_INT_L (at 110.998 101.346) (layer F.SilkS))
  (gr_text "SIG Out" (at 96.774 97.79) (layer F.SilkS))
  (gr_text "PWR In\n(V24)" (at 103.632 82.804 180) (layer F.SilkS))
  (gr_line (start 172.72 68.58) (end 172.72 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.154 68.58) (end 162.56 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.154 71.374) (end 89.154 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.154 81.534) (end 89.154 71.374) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.154 111.76) (end 162.56 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.154 81.534) (end 89.154 111.76) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.194 87.884) (xy 101.854 87.884) (xy 94.742 82.042) (xy 94.742 76.454) (xy 112.014 76.454)
        (xy 140.716 76.2) (xy 155.194 76.2)
      )
    )
  )
  (zone (net 1) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.544 102.87) (xy 125.222 102.87) (xy 124.206 102.108) (xy 124.206 100.838) (xy 125.222 100.33)
        (xy 154.178 100.33) (xy 154.178 76.2) (xy 161.544 76.2)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.212 111.252) (xy 89.408 111.506) (xy 89.408 68.834) (xy 172.212 68.834)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.212 75.692) (xy 89.408 75.692) (xy 89.408 68.834) (xy 172.212 68.834)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.212 111.252) (xy 89.408 111.506) (xy 89.408 101.6) (xy 95.504 101.6) (xy 95.504 105.664)
        (xy 104.394 105.664) (xy 105.41 104.902) (xy 115.062 104.902) (xy 120.142 109.982) (xy 138.684 109.982)
        (xy 143.002 106.426) (xy 150.876 106.426) (xy 154.432 106.172) (xy 154.432 103.378) (xy 162.052 103.378)
        (xy 162.052 75.692) (xy 172.212 75.692)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 99.822) (xy 122.936 99.822) (xy 120.65 102.108) (xy 105.664 102.108) (xy 105.664 97.028)
        (xy 101.346 97.028) (xy 95.504 101.6) (xy 89.408 101.6) (xy 89.408 93.472) (xy 95.25 93.472)
        (xy 101.854 88.392) (xy 153.67 88.392)
      )
    )
  )
)
