(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo8+1)
  (general
    (links 154)
    (no_connects 0)
    (area 107.224919 92.9002 176.629509 117.068201)
    (thickness 1.6)
    (drawings 7)
    (tracks 308)
    (zones 0)
    (modules 119)
    (nets 44)
  )
  (page A4)
  (title_block
    (title "Isolon Reworked")
    (date 2018-03-04)
    (rev 0.3)
    (company BITFixIT)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 25.4)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFCDFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 Earth)
  (net 4 VDD)
  (net 5 VEE)
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(C8-Pad2)")
  (net 10 "Net-(L1-Pad1)")
  (net 11 "Net-(L2-Pad1)")
  (net 12 /SCL)
  (net 13 /SDA)
  (net 14 "Net-(J2-Pad1)")
  (net 15 "Net-(R5-Pad2)")
  (net 16 "Net-(R6-Pad2)")
  (net 17 "Net-(R10-Pad2)")
  (net 18 "Net-(R9-Pad1)")
  (net 19 "Net-(R10-Pad1)")
  (net 20 /21)
  (net 21 /~RESET)
  (net 22 /AREF)
  (net 23 /12)
  (net 24 /VBAT)
  (net 25 /EN)
  (net 26 /VUSB)
  (net 27 /13)
  (net 28 /27)
  (net 29 /33)
  (net 30 /15)
  (net 31 /32)
  (net 32 /14)
  (net 33 /A0)
  (net 34 /A1)
  (net 35 /A2)
  (net 36 /A3)
  (net 37 /A4)
  (net 38 /A5)
  (net 39 /SCK)
  (net 40 /MOSI)
  (net 41 /MISO)
  (net 42 /RX)
  (net 43 /TX)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net /12)
    (add_net /13)
    (add_net /14)
    (add_net /15)
    (add_net /21)
    (add_net /27)
    (add_net /32)
    (add_net /33)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /EN)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net /VBAT)
    (add_net /VUSB)
    (add_net /~RESET)
    (add_net Earth)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net VCC)
    (add_net VDD)
    (add_net VEE)
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.0833 109.9185)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.1186 108.8898)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 138.6586 110.1598)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module wq-boardv2:bitfixitlogoflipped (layer F.Cu) (tedit 0)
    (at 147.828 101.1936)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 147.0787 112.9538)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 149.733 109.0549)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 160.8455 96.8248)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 163.4363 98.7044)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 162.8521 104.9528)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 162.8521 107.6579)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 162.8521 110.4773)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 163.3982 113.2586)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 161.1757 111.7473)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 159.1183 113.284)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 157.4546 105.4481)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 154.5717 104.267)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 151.7396 111.0361)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 144.2847 111.7473)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 144.1704 109.2708)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 142.0876 109.2708)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 141.1732 113.284)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 138.6586 112.6998)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.144 113.284)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.5786 112.6998)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.0132 114.0968)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 127.5588 114.0968)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 141.1986 111.4298)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.8806 111.2266)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.0386 111.4298)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 110.1598)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 125.9586 111.4298)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 123.4186 110.1598)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 138.5189 106.5911)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.6294 107.8992)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.0386 108.8898)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 107.6198)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 125.9586 108.8898)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 123.4186 107.6198)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.144 105.8418)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.5913 105.3084)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.2291 105.9688)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 105.0798)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 125.9586 106.3498)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 123.4186 105.0798)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 138.2522 101.8794)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 135.9408 103.2383)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.5786 102.5398)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.0386 103.8098)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 102.5398)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 125.9586 103.8098)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 123.4186 102.5398)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 142.1892 101.473)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 138.6586 99.9998)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.5377 101.5619)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.0198 99.7204)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.0386 101.2698)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 99.9998)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 125.9586 101.2698)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 123.4186 99.9998)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 141.1986 98.7298)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 138.6586 97.4598)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.1186 98.7298)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.5786 97.4598)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 131.0386 98.7298)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 97.4598)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 125.9586 99.0727)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 142.9766 96.8248)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 136.1186 96.1898)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 133.5786 94.9198)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 130.9751 96.6724)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACD17C)
    (at 128.4986 94.9198)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 Earth) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 172.4406 111.8616)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 172.4533 109.5629)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 172.4406 107.0229)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 172.4406 104.1781)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 166.9796 114.0968)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 164.7571 113.2205)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 169.0878 111.887)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 164.6936 110.5027)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 167.4114 109.2708)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 164.6682 107.6198)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 167.767 106.5276)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 164.6682 105.0798)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 167.8432 103.8606)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 164.6682 102.5398)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 163.83 101.0412 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ADUM1250ARZ (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9FC074)
    (at 166.4208 97.5868 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.1016 0 180) (layer F.SilkS))
    (fp_text value 3K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A9C722B)
    (at 151.7904 112.6744)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at -0.1016 0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A9FC081)
    (at 156.5148 98.3996 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0.1016 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0.12192 -0.04572 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VEE))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A9C722F)
    (at 148.3868 111.1504 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0.0762 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9FC067)
    (at 170.0784 101.1428 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.0508 -0.0508 90) (layer F.SilkS))
    (fp_text value 3K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9BDC8F)
    (at 171.704 101.1428 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.0508 0.0635 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /21))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9BBE9F)
    (at 151.2316 97.4852)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.7 1.52) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9BE7F0)
    (at 146.8628 97.4852 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.8956 -0.0762 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.4244 99.2632 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9BE7F3)
    (at 143.8148 107.8992 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.8956 0.0254 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6_Handsoldering (layer F.Cu) (tedit 58CE4E7F)
    (at 149.1996 100.0252 180)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (attr smd)
    (fp_text reference U3 (at 0 -2 180) (layer F.SilkS))
    (fp_text value MCP4017 (at 0 2 360) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.33 -0.65 180) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at -1.33 0 180) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 3 smd rect (at -1.33 0.65 180) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (pad 4 smd rect (at 1.33 0.65 180) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at 1.33 0 180) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 6 smd rect (at 1.33 -0.65 180) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A9BE79C)
    (at 144.526 110.6424 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U5 (at 1.7526 -1.2192 180) (layer F.SilkS))
    (fp_text value REF3130 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5A9BE458)
    (at 153.5684 108.2548 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U6 (at 1.4478 -2.4384 270) (layer F.SilkS))
    (fp_text value MCP3221 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.9804 107.8992 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 3K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 149.9616 103.6828 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:Inductor_Murata_8200 (layer F.Cu) (tedit 5A9FC096)
    (at 156.21 101.6508 90)
    (descr "Inductor Murata 8200")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L2 (at 0.1524 0.0508 90) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.143 0 90) (size 1.524 3.048) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.143 0 90) (size 1.524 3.048) (layers F.Cu F.Paste F.Mask)
      (net 5 VEE))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:Inductor_Murata_8200 (layer F.Cu) (tedit 5A9C0DD6)
    (at 156.4132 112.395 180)
    (descr "Inductor Murata 8200")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L1 (at 0 -2.7 180) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.7 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.143 0 180) (size 1.524 3.048) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.143 0 180) (size 1.524 3.048) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:C_0603_HandSoldering (layer F.Cu) (tedit 5A9C15AE)
    (at 144.4244 100.8888)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 0.1016 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:C_0603_HandSoldering (layer F.Cu) (tedit 5A9C15AE)
    (at 143.6624 113.3348 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 0.1016 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:C_0603_HandSoldering (layer F.Cu) (tedit 5A9C15AE)
    (at 156.464 108.0008 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 0.1016 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:C_0603_HandSoldering (layer F.Cu) (tedit 5A9C15AE)
    (at 168.5036 101.1428 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 0.1016 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:C_0603_HandSoldering (layer F.Cu) (tedit 5A9C15AE)
    (at 158.9532 101.4476 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0.1016 450) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:C_0603_HandSoldering (layer F.Cu) (tedit 5A9C15AE)
    (at 150.8252 108.0008 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 0.1016 270) (layer F.SilkS))
    (fp_text value 220pF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:5pinMTU (layer F.Cu) (tedit 5A9C19E9)
    (at 163.4744 107.95 90)
    (fp_text reference U1 (at -4.74 0 180) (layer F.SilkS))
    (fp_text value MTU1D0305MC (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at -2.54 -3.25 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(L1-Pad1)"))
    (pad 1 smd rect (at -2.54 3.25 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 5 smd rect (at 0 -3.25 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 4 smd rect (at 2.54 -3.25 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(L2-Pad1)"))
    (pad 3 smd rect (at 2.54 3.25 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A9FC092)
    (at 153.416 103.6828 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.1524 0 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 170.5991 110.3884 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (zone_connect 2)
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /21) (zone_connect 2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 151.6888 103.6828 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 500R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:SOP-8L (layer F.Cu) (tedit 5A9BBD81)
    (at 145.3896 104.394 270)
    (descr "SOP-8L Surface Mount Small Outline Package 8pin")
    (tags "jfet opamp")
    (fp_text reference U4 (at 0 0 270) (layer F.SilkS))
    (fp_text value TL072 (at 0 0 270) (layer F.Fab))
    (pad 1 smd oval (at -1.905 2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd oval (at -0.635 2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 3 smd oval (at 0.635 2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 4 smd oval (at 1.905 2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VEE))
    (pad 5 smd oval (at 1.905 -2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R9-Pad1)"))
    (pad 6 smd oval (at 0.635 -2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R10-Pad2)"))
    (pad 7 smd oval (at -0.635 -2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R10-Pad1)"))
    (pad 8 smd oval (at -1.905 -2.7 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
  )
  (module kicad-library:Via_0.6mm (layer F.Cu) (tedit 5AACC030)
    (at 164.6682 99.9998)
    (zone_connect 2)
    (fp_text reference REF** (at 0.3048 1.1176) (layer F.SilkS) hide)
    (fp_text value Via_0.6mm (at 0 -1.0922) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module wq-boardv2:oshw_all_13mm (layer B.Cu) (tedit 0)
    (at 163.4744 102.743 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 127.1778 105.4989 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 90) (layer B.Fab) hide)
  )
  (module kicad-library:BNC_Socket_Gmod (layer F.Cu) (tedit 5AB57471)
    (at 134.1528 105.4862 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference J2 (at 0.508 9.652 90) (layer F.SilkS))
    (fp_text value BNC (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at -5.08 0.82 90) (size 2.01 2.01) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0.82 90) (size 2.01 2.01) (drill 2.01) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 5.9 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 5.9 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-library:FeatherWing (layer F.Cu) (tedit 5AB56D48)
    (at 147.9296 105.4608)
    (fp_text reference J3 (at 19.05 8.636) (layer F.Fab))
    (fp_text value FEATHER (at 0 0) (layer F.Fab))
    (fp_arc (start 22.86 8.89) (end 22.86 11.43) (angle -90) (layer Edge.Cuts) (width 0.05))
    (fp_text user %R (at 20.32 8.89) (layer F.Fab))
    (fp_arc (start -22.86 -8.89) (end -25.4 -8.89) (angle 90) (layer Edge.Cuts) (width 0.05))
    (fp_arc (start -22.86 8.89) (end -22.86 11.43) (angle 90) (layer Edge.Cuts) (width 0.05))
    (fp_arc (start 22.86 -8.89) (end 22.86 -11.43) (angle 90) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -25.4 -8.89) (end -25.4 8.89) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -22.86 11.43) (end 22.86 11.43) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 25.4 8.89) (end 25.4 -8.89) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 22.86 -11.43) (end -22.86 -11.43) (layer Edge.Cuts) (width 0.05))
    (pad 17 thru_hole circle (at -8.89 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /VBAT))
    (pad 18 thru_hole circle (at -6.35 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /EN))
    (pad 19 thru_hole circle (at -3.81 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /VUSB))
    (pad 20 thru_hole circle (at -1.27 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /13))
    (pad 21 thru_hole circle (at 1.27 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /12))
    (pad 22 thru_hole circle (at 3.81 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /27))
    (pad 23 thru_hole circle (at 6.35 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /33))
    (pad 24 thru_hole circle (at 8.89 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /15))
    (pad 25 thru_hole circle (at 11.43 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /32))
    (pad 26 thru_hole circle (at 13.97 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /14))
    (pad 27 thru_hole circle (at 16.51 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /SCL))
    (pad 28 thru_hole circle (at 19.05 -10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (pad 1 thru_hole circle (at -19.05 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /~RESET))
    (pad 2 thru_hole circle (at -16.51 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -13.97 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /AREF))
    (pad 4 thru_hole circle (at -11.43 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -8.89 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /A0))
    (pad 6 thru_hole circle (at -6.35 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /A1))
    (pad 7 thru_hole circle (at -3.81 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /A2))
    (pad 8 thru_hole circle (at -1.27 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /A3))
    (pad 9 thru_hole circle (at 1.27 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /A4))
    (pad 10 thru_hole circle (at 3.81 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /A5))
    (pad 11 thru_hole circle (at 6.35 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /SCK))
    (pad 12 thru_hole circle (at 8.89 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 /MOSI))
    (pad 13 thru_hole circle (at 11.43 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /MISO))
    (pad 14 thru_hole circle (at 13.97 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /RX))
    (pad "" np_thru_hole circle (at -22.86 -8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 22.86 -8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -22.86 8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 22.86 8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 19.05 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /21))
    (pad 15 thru_hole circle (at 16.51 10.16) (size 1.616 1.616) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /TX))
  )
  (gr_text "IsoISE\nFeather" (at 134.5565 105.3846) (layer B.SilkS))
  (gr_text BitFIXit (at 147.8534 107.7341) (layer B.SilkS))
  (gr_text git.io/vx4da (at 155.575 113.2205) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.7576 112.3188) (xy 168.7576 114.554) (xy 164.211 114.554) (xy 164.211 96.3676) (xy 168.8592 96.3676)
        (xy 168.8592 98.6028) (xy 172.8978 98.6028) (xy 172.8978 112.3188)
      )
    )
    (polygon
      (pts        (xy 165.354 98.2218) (xy 166.3192 100.4824) (xy 166.7256 101.2444) (xy 170.2308 101.2698) (xy 168.5544 98.0694)
        (xy 165.3286 98.1964)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.8592 112.3188) (xy 168.8592 114.554) (xy 164.211 114.554) (xy 164.211 96.3676) (xy 168.7576 96.3676)
        (xy 168.7576 98.6028) (xy 172.8978 98.6028) (xy 172.8978 112.3188)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.890612 96.3676) (xy 163.890612 114.5286) (xy 127.111412 114.554) (xy 127.111412 112.3442) (xy 122.945812 112.3188)
        (xy 122.945812 98.6028) (xy 127.086012 98.6028) (xy 127.086012 94.4626) (xy 137.957212 94.4626) (xy 137.957212 96.3676)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.9062 96.3676) (xy 163.9062 114.554) (xy 127.1016 114.554) (xy 127.1016 112.3188) (xy 122.9614 112.3188)
        (xy 122.9614 98.6028) (xy 127.1016 98.6028) (xy 127.1016 94.4626) (xy 137.9728 94.4626) (xy 137.9728 96.3676)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.891 104.7496) (xy 143.891 105.3084) (xy 143.4592 105.7402) (xy 141.224 105.7402) (xy 141.224 105.9688)
        (xy 140.5382 106.6546) (xy 139.573 106.6546) (xy 138.8872 105.9688) (xy 138.8872 105.0036) (xy 139.573 104.3178)
        (xy 143.4592 104.3178)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.573 104.3178) (xy 140.5382 104.3178) (xy 141.224 105.0036) (xy 141.224 105.9688) (xy 140.5382 106.6546)
        (xy 139.573 106.6546) (xy 138.8872 105.9688) (xy 138.8872 105.0036)
      )
    )
  )
)
