(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "" (layer "F.Cu")
    (at 10.5 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.31 1.31) (drill 0.73) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 4 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.28 1.28) (drill 0.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 18.5 -6.5)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.39 1.39) (drill 0.81) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 2 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.28 1.28) (drill 0.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 19 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.26 1.26) (drill 0.68) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 12.5 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.23 1.23) (drill 0.65) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 10.5 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.23 1.23) (drill 0.65) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 6 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.62) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 4 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.62) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 21 -6.5)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.41 1.41) (drill 0.83) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 10.5 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.15 1.15) (drill 0.57) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 14.5 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.31 1.31) (drill 0.73) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 23.5 -6.5)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.43 1.43) (drill 0.85) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 23.5 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.49 1.49) (drill 0.91) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 2 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.62) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 18.5 -9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.33 1.33) (drill 0.75) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 19 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.18 1.18) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 12.5 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.15 1.15) (drill 0.57) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 4 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.13 1.13) (drill 0.55) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 6 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.28 1.28) (drill 0.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 22.986703 -19.983527)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.18 1.18) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 21 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.47 1.47) (drill 0.89) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 23.5 -9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.37 1.37) (drill 0.79) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 6 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.13 1.13) (drill 0.55) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 12.5 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.31 1.31) (drill 0.73) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 18.5 -4)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.45 1.45) (drill 0.87) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 21 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.18 1.18) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 23 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.26 1.26) (drill 0.68) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 21 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.26 1.26) (drill 0.68) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 14.5 -20)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.15 1.15) (drill 0.57) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 21 -9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.35 1.35) (drill 0.77) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Ray Library 1:ADOM_MEDIUM_PIN" (layer "F.Cu")
    (at 2 -20)
    (attr through_hole)
    (fp_text reference "PIN**" (at 0 -1.4 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ADOM_MEDIUM_PIN" (at 0 -2 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.13 1.13) (drill 0.55) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/Ray/Documents/KiCad Projects/KiCad Library/Ray Library 1.pretty/1PIN MEDIUM v3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 14.5 -11.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.23 1.23) (drill 0.65) (layers "*.Cu" "*.Mask"))
  )
  (gr_line (start 0 0) (end 25 0)
    (layer "Edge.Cuts"))
  (gr_line (start 0 -27) (end 0 0)
    (layer "Edge.Cuts"))
  (gr_line (start 25 0) (end 25 -27)
    (layer "Edge.Cuts"))
  (gr_line (start 25 -27) (end 0 -27)
    (layer "Edge.Cuts"))
  (gr_text "0.68" (at 17.5 -13.25) (layer "F.SilkS"))
  (gr_text "1.28" (at 0.5 -7.75) (layer "F.SilkS"))
  (gr_text "1.13" (at 0.5 -24) (layer "F.SilkS"))
  (gr_text "1.20" (at 0.5 -15.75) (layer "F.SilkS"))
  (gr_text "1.31" (at 9 -7.75) (layer "F.SilkS"))
  (gr_text "0.73" (at 9 -5.25) (layer "F.SilkS"))
  (gr_text "1.18" (at 17.5 -24) (layer "F.SilkS"))
  (gr_text "0.70" (at 0.5 -5.25) (layer "F.SilkS"))
  (gr_text "0.57" (at 9 -21.5) (layer "F.SilkS"))
  (gr_text "1.15" (at 9 -24) (layer "F.SilkS"))
  (gr_text "1.26" (at 17.5 -15.75) (layer "F.SilkS"))
  (gr_text "0.65" (at 9 -13.25) (layer "F.SilkS"))
  (gr_text "1.23" (at 9 -15.75) (layer "F.SilkS"))
  (gr_text "0.60" (at 17.5 -21.5) (layer "F.SilkS"))
  (gr_text "Adom Medium Pin Size Tests v1" (at 0.25 -0.5) (layer "F.SilkS"))
  (gr_text "0.55" (at 0.5 -21.5) (layer "F.SilkS"))
  (gr_text "0.62" (at 0.5 -13.25) (layer "F.SilkS"))
)
