(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 41)
    (tracks 639)
    (zones 0)
    (modules 99)
    (nets 48)
  )
  (page USLetter)
  (title_block
    (title "Furnace Logger PCB")
    (date 2019-10-07)
    (rev 3)
    (company "Montana State University Capstone")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 1.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.25)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.55 1.55)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C102-Pad1)")
  (net 4 "Net-(C103-Pad1)")
  (net 5 PWR)
  (net 6 +5V)
  (net 7 "Net-(C204-Pad1)")
  (net 8 "Net-(C301-Pad1)")
  (net 9 "Net-(C302-Pad1)")
  (net 10 AIN1)
  (net 11 "Net-(C306-Pad1)")
  (net 12 "Net-(C307-Pad2)")
  (net 13 "Net-(C307-Pad1)")
  (net 14 AIN0)
  (net 15 "Net-(C310-Pad2)")
  (net 16 "Net-(D101-Pad1)")
  (net 17 "Net-(D201-Pad1)")
  (net 18 "Net-(D301-Pad1)")
  (net 19 "Net-(D302-Pad1)")
  (net 20 "Net-(FB301-Pad1)")
  (net 21 "Net-(J101-Pad2)")
  (net 22 "Net-(J102-Pad2)")
  (net 23 SDA)
  (net 24 SCL)
  (net 25 TX)
  (net 26 RX)
  (net 27 PPS)
  (net 28 STATE_CNHG)
  (net 29 DQ)
  (net 30 "Net-(J201-Pad2)")
  (net 31 "Net-(J202-PadSH)")
  (net 32 "Net-(J301-Pad2)")
  (net 33 "Net-(J303-Pad2)")
  (net 34 "Net-(JP303-Pad2)")
  (net 35 "Net-(R103-Pad1)")
  (net 36 "Net-(R104-Pad2)")
  (net 37 "Net-(R105-Pad2)")
  (net 38 "Net-(R106-Pad2)")
  (net 39 "Net-(R202-Pad1)")
  (net 40 "Net-(R307-Pad1)")
  (net 41 "Net-(R309-Pad1)")
  (net 42 "Net-(R310-Pad2)")
  (net 43 SCL_5V)
  (net 44 SDA_5V)
  (net 45 "Net-(BT101-Pad1)")
  (net 46 AIN2)
  (net 47 "Net-(TP307-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.25)
    (diff_pair_gap 0.25)
    (add_net AIN0)
    (add_net AIN1)
    (add_net AIN2)
    (add_net DQ)
    (add_net GND)
    (add_net "Net-(BT101-Pad1)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C204-Pad1)")
    (add_net "Net-(C301-Pad1)")
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C306-Pad1)")
    (add_net "Net-(C307-Pad1)")
    (add_net "Net-(C307-Pad2)")
    (add_net "Net-(C310-Pad2)")
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D201-Pad1)")
    (add_net "Net-(D301-Pad1)")
    (add_net "Net-(D302-Pad1)")
    (add_net "Net-(FB301-Pad1)")
    (add_net "Net-(J101-Pad2)")
    (add_net "Net-(J102-Pad2)")
    (add_net "Net-(J201-Pad2)")
    (add_net "Net-(J202-PadSH)")
    (add_net "Net-(J301-Pad2)")
    (add_net "Net-(J303-Pad2)")
    (add_net "Net-(JP303-Pad2)")
    (add_net "Net-(R103-Pad1)")
    (add_net "Net-(R104-Pad2)")
    (add_net "Net-(R105-Pad2)")
    (add_net "Net-(R106-Pad2)")
    (add_net "Net-(R202-Pad1)")
    (add_net "Net-(R307-Pad1)")
    (add_net "Net-(R309-Pad1)")
    (add_net "Net-(R310-Pad2)")
    (add_net "Net-(TP307-Pad1)")
    (add_net PPS)
    (add_net RX)
    (add_net SCL)
    (add_net SCL_5V)
    (add_net SDA)
    (add_net SDA_5V)
    (add_net STATE_CNHG)
    (add_net TX)
  )
  (net_class 5/3V ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.3)
    (diff_pair_gap 0.25)
    (add_net +3V3)
    (add_net +5V)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 1.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.25)
    (diff_pair_gap 0.25)
    (add_net PWR)
  )
  (module Logos:BobcatLogo (layer B.Cu) (tedit 0)
    (at 172 111.25 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module FurnaceLogger:LDO03C-005W05-VJ (layer F.Cu) (tedit 5DD58625)
    (at 122 94 180)
    (fp_text reference U202 (at 2.5 1.75) (layer F.SilkS))
    (fp_text value LDO03C-005W05-VJ (at 0 -6.8) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.7 0 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 5 PWR))
    (pad 1 thru_hole rect (at 3.4 0 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 4 thru_hole circle (at -1.7 0 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C204-Pad1)"))
    (pad 5 thru_hole circle (at -3.4 0 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(R202-Pad1)"))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_OKI-78SR_Vertical.wrl
      (offset (xyz -3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Logos:MSU (layer F.Cu) (tedit 0)
    (at 163 81)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Logos:RextorSilk (layer F.Cu) (tedit 0)
    (at 163.5 88.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Batteries:BATTCON-6.8MM (layer F.Cu) (tedit 5DD34578)
    (at 158.9 107.4 90)
    (descr "PART#: MS621FE-FL11E")
    (tags "PART#: MS621FE-FL11E")
    (attr smd)
    (fp_text reference BT101 (at 4.9 2.1 270) (layer F.SilkS))
    (fp_text value MS412FE-FL26E (at -3.1 0.1 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 4.86918 0.7493 270) (size 2.2479 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at 4.86918 -0.7493 270) (size 2.2479 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(BT101-Pad1)") (solder_mask_margin 0.1016))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Seiko_MS621F.step
      (offset (xyz 4 0 0))
      (scale (xyz 0.7 0.7 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5DD2EB88)
    (at 154.6 81.6)
    (fp_text reference TP307 (at 3.4 -1.6) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "Net-(TP307-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5DD2EB88)
    (at 166 76.2)
    (fp_text reference TP306 (at -4 0.05) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 AIN2))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5DD2EB88)
    (at 112.87512 74.06512 180)
    (fp_text reference TP104 (at -2.37488 0.06512 90) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 SCL))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5DD2EB88)
    (at 112.87512 77.2 180)
    (fp_text reference TP103 (at 0.12512 -2.05 180) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 SDA))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5DD2EB88)
    (at 130.2 95.4)
    (fp_text reference TP102 (at -2.2 0.1 90) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 RX))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5DD2EB88)
    (at 133.4 95.4)
    (fp_text reference TP101 (at 2.35 0.1 90) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 TX))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 153.14488 77.93488)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R314 (at 4.35512 0.06512) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 46 AIN2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 153.14488 74.64488)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R313 (at 4.35512 0.10512) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 46 AIN2))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 159.65 65.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CB9)
    (at 101.65 114.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 159.65 114.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 101.65 65.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module digikey-footprints:SOT-223 (layer F.Cu) (tedit 5D28A60E)
    (at 122.841 86.831 180)
    (attr smd)
    (fp_text reference U203 (at -4.159 -1.169 90) (layer F.SilkS))
    (fp_text value NCP1117ST33T3G (at 0.15 5.65) (layer F.Fab))
    (fp_text user %R (at -0.05 0.025) (layer F.Fab))
    (pad 3 smd rect (at 2.3 3.15 180) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR))
    (pad 2 smd rect (at 0 3.15 180) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -2.3 3.15 180) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 -3.15 180) (size 3.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 137.061 113.15 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C101 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 139.54 92.525 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C102 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100p (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(C102-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 154.614 115.186 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C103 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C103-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 153.184 99.884 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C104 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 45 "Net-(BT101-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 150.677 115.186 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C105 (at 0 1.777 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C103-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 147.2875 71.6 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C106 (at 0 1.75) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 112.862 88.821 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C201 (at -0.571 -1.888 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 PWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 107.655 90.5355 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C202 (at 0.155 -1.9645) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 PWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 112.862 82.471 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C203 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 115.5 102.8405 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C204 (at 4.5085 -0.1905 90) (layer F.SilkS))
    (fp_text value 22u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(C204-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 112.884 102.8405 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C205 (at 4.5085 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(C204-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 117.761 83.021 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C206 (at -0.521 1.761 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 PWR))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 122.333 80.862)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C207 (at 1.167 -1.862) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 PWR))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 117.761 88.5185 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C208 (at 0.2685 -1.761 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 170.345 103.255 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C301 (at 0 -1.995) (layer F.SilkS))
    (fp_text value 470p (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C301-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 176.15 103.35 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C302 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 "Net-(C302-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 134.3875 76.9 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C303 (at -3.2625 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 178.65 103.35 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C304 (at 0.1 1.85 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 "Net-(C302-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 152.8875 92)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C305 (at 1.1125 -1.905) (layer F.SilkS))
    (fp_text value 22u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 AIN1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 171.715 76.17 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C306 (at 0.065 -1.73) (layer F.SilkS))
    (fp_text value 6u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 "Net-(C306-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 178.065 83.79)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C307 (at 3.335 0.11 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 "Net-(C307-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(C307-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 176.922 94.839)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C308 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 0.01u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 171.715 92.68 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C309 (at 0 -2.28 90) (layer F.SilkS))
    (fp_text value ECP-U1C105MA5 (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 AIN0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 139.3495 87.064 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C310 (at -0.381 2.0955 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(C310-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 587CCEF9)
    (at 153.184 109.9)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D101 (at -2.534 0 90) (layer F.SilkS))
    (fp_text value ZHCS500TA (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad "" smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D101-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:1206 (layer F.Cu) (tedit 5D288D46)
    (at 108.6 114 270)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/LTST-C230KFKT_5-24-06.pdf)
    (attr smd)
    (fp_text reference D201 (at 3.5 0.6 180) (layer F.SilkS))
    (fp_text value LTST-C150KGKT (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.8 0 270) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D201-Pad1)"))
    (pad 2 smd rect (at 1.8 0 270) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 171.715 72.995 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D301 (at 0 1.595) (layer F.SilkS))
    (fp_text value SP4020-01FTG (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D301-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 129.4 76.9 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D302 (at 0 -1.75) (layer F.SilkS))
    (fp_text value SP4020-01FTG (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D302-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 146.994 115.186 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference FB101 (at 0.036 -1.844 90) (layer F.SilkS))
    (fp_text value MI1206K601R-10 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C103-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 151.605 81.73 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference FB301 (at 2.77 -1.395 180) (layer F.SilkS))
    (fp_text value MMZ2012Y152BT000 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 "Net-(FB301-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 140.81 74.745 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference FB302 (at 0.06 1.745 180) (layer F.SilkS))
    (fp_text value MMZ2012Y152BT000 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 +5V))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(C310-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Coax_Conn_U.FL (layer F.Cu) (tedit 5D288EC0)
    (at 141.35 114.65 180)
    (descr https://media.digikey.com/pdf/Data%20Sheets/Hirose%20PDFs/UFL%20Series.pdf)
    (attr smd)
    (fp_text reference J101 (at -0.05 -2.5) (layer F.SilkS))
    (fp_text value U_FL-R-SMT-1_10_ (at 0.01 3.15) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5 180) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J101-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x02_P5.08mm_Drill1.5mm (layer F.Cu) (tedit 5AEE5F19)
    (at 166 71.6 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J102 (at 8 0 180) (layer F.SilkS) hide)
    (fp_text value "Wire Pads (Virtual Component)" (at 2.54 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 22 "Net-(J102-Pad2)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 106.52 67.175 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J104 (at 1.27 -2.5 90) (layer F.SilkS) hide)
    (fp_text value RASPBERRYPI-40-PIN-GPIO_PTH (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 SDA))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 SCL))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 DQ))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 TX))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 RX))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 PPS))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 STATE_CNHG))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Micro-Fit_3.0_43045-0200_2x01_P3.00mm_Horizontal (layer F.Cu) (tedit 5B799D96)
    (at 106.4 103.65 90)
    (descr "Molex Micro-Fit 3.0 Connector System, 43045-0200 (compatible alternatives: 43045-0201, 43045-0202), 1 Pins per row (https://www.molex.com/pdm_docs/sd/430450200_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Micro-Fit_3.0 top entry")
    (fp_text reference J201 (at -2.85 2.35 270) (layer F.SilkS))
    (fp_text value 0430450200 (at 0 5.7 90) (layer F.Fab))
    (fp_text user %R (at 0 -8.22 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -4.32 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask) (roundrect_rratio 0.166667)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(J201-Pad2)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.8 0.9))
      (rotate (xyz 0 0 180))
    )
  )
  (module digikey-footprints:USB_A_Female_UE27AC54100 (layer F.Cu) (tedit 5DA36A4C)
    (at 118.4 109.9)
    (fp_text reference J202 (at 0.6 -4.851) (layer F.SilkS))
    (fp_text value UE27AC54100 (at 0 12) (layer F.Fab))
    (fp_text user %R (at -0.025 0.975) (layer F.Fab))
    (pad SH thru_hole circle (at -6.57 0) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 31 "Net-(J202-PadSH)"))
    (pad SH thru_hole circle (at 6.57 0) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 31 "Net-(J202-PadSH)"))
    (pad 1 thru_hole circle (at -3.5 -2.71) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask)
      (net 7 "Net-(C204-Pad1)"))
    (pad 2 thru_hole circle (at -1 -2.71) (size 1.8 1.8) (drill 0.92) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1 -2.71) (size 1.8 1.8) (drill 0.92) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.5 -2.71) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Mini-B_Lumberg_2486_01_Horizontal.step
      (offset (xyz 0 -2.5 0))
      (scale (xyz 1.5 1.4 1.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x03_P4.445mm_Drill1.5mm (layer F.Cu) (tedit 5AEE5F77)
    (at 130.15 90.595 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J301 (at 4.695 3 90) (layer F.SilkS) hide)
    (fp_text value "Wire Pads " (at 4.445 3.81 90) (layer F.Fab))
    (fp_text user %R (at 4.445 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4.445 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 32 "Net-(J301-Pad2)"))
    (pad 3 thru_hole circle (at 8.89 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 +3V3))
  )
  (module Connector_Wire:SolderWirePad_1x03_P4.445mm_Drill1.5mm (layer F.Cu) (tedit 5AEE5F77)
    (at 125.455 72.65)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J302 (at 11.945 0.25 90) (layer F.SilkS) hide)
    (fp_text value "Wire Pads " (at 4.445 3.81) (layer F.Fab))
    (fp_text user %R (at 4.445 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 8.89 0) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 4.445 0) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 32 "Net-(J301-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_JST:JST_SH_BM02B-SRSS-TB_1x02-1MP_P1.00mm_Vertical (layer F.Cu) (tedit 5B78AD87)
    (at 174.9 65.65)
    (descr "JST SH series connector, BM02B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (attr smd)
    (fp_text reference J303 (at -3.65 0.1 270) (layer F.SilkS))
    (fp_text value "BM02B-SRSS-TB(LF)(SN)" (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 -0.25) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 1.325) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.5 1.325) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J303-Pad2)"))
    (pad MP smd roundrect (at -1.8 -1.2) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 1.8 -1.2) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.step
      (offset (xyz -0.5 1 0))
      (scale (xyz 0.7 0.8 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 101.9 75.65 270)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J304 (at 4.6 0.65 180) (layer F.SilkS))
    (fp_text value "SM04B-SRSS-TB(LF)(SN)" (at 0 3.98 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 SCL))
    (pad 2 smd roundrect (at -0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 SDA))
    (pad 3 smd roundrect (at 0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 4 smd roundrect (at 1.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad MP smd roundrect (at -2.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 2.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal.step
      (offset (xyz -1.5 1.5 0))
      (scale (xyz 0.5 0.7 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.65 97.9 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP201 (at 2.4 1.15 270) (layer F.SilkS))
    (fp_text value M20-9990246 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 PWR))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J201-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 177.43 79.98 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP301 (at -2.17 0.97 180) (layer F.SilkS))
    (fp_text value M20-9990246 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C306-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C307-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 172.985 79.98 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP302 (at 2.17 1.585 180) (layer F.SilkS))
    (fp_text value M20-9990246 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 AIN2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C306-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 175.525 98.395 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP303 (at -0.005 5.125 90) (layer F.SilkS))
    (fp_text value M20-9990246 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(JP303-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 140.4 111.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L101 (at 4 0) (layer F.SilkS))
    (fp_text value LQG18HN33NJ00D (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J101-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 149.446 88.08 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R101 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 200k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(C102-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 153.184 105.15 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R102 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 45 "Net-(BT101-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(D101-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 152.9 94.65)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R103 (at 0 1.905) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 35 "Net-(R103-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 133.15 113.15 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R104 (at -3.35 0.85 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 36 "Net-(R104-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 133.55 100.3 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R105 (at 4.45 -0.2 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 37 "Net-(R105-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 130.05 100.3 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R106 (at 4.45 0.05 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 26 RX))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 38 "Net-(R106-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 108.22 77.2 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R107 (at -0.03 4.95) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 23 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 108.2 74.2 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R108 (at 0.2 -5.05) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 24 SCL))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 106.2 114 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R201 (at 3.5 0.8 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(D201-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 122.4 102.8 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R202 (at -0.05 -1.85 90) (layer F.SilkS))
    (fp_text value 267 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 39 "Net-(R202-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 135.65 80.9 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R301 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 "Net-(J301-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 177.43 71.725 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R302 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(D301-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 33 "Net-(J303-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 118.65 77.15)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R303 (at 0 2) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 "Net-(D302-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 "Net-(J301-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 158.6 99.4)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R304 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C301-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 AIN1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 118.65 74.4)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R305 (at 0 -1.765) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 "Net-(D302-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 29 DQ))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 180.605 74.9 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R306 (at -0.25 1.795 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(D301-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 "Net-(C306-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 172.985 83.79 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R307 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 40 "Net-(R307-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 179.97 88.6525 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R308 (at 0.1525 2.03 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 40 "Net-(R307-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 148.049 81.603 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R309 (at -0.127 1.851 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 "Net-(FB301-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 41 "Net-(R309-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 145.255 76.65 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R310 (at 0 -1.895 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(C310-Pad2)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 42 "Net-(R310-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 135.73 87.064 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R311 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(C310-Pad2)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 43 SCL_5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 140.81 78.555)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R312 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 44 SDA_5V))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(C310-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 129.6 113.8 180)
    (fp_text reference TP201 (at 0.1 -2.7) (layer F.SilkS))
    (fp_text value 5002 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 119 102.8 90)
    (fp_text reference TP202 (at 2.337 -0.127 180) (layer F.SilkS))
    (fp_text value 5000 (at 0 3.93 90) (layer F.Fab))
    (fp_text user %R (at 0 2.41 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 "Net-(C204-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 167.4 98.4 180)
    (fp_text reference TP301 (at 1.4 -2.35) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 "Net-(C301-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 180.4 70.65 180)
    (fp_text reference TP302 (at -0.1 2.25) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(D301-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 177.43 76.17 90)
    (fp_text reference TP303 (at -2.23 -0.03) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93 90) (layer F.Fab))
    (fp_text user %R (at 0 2.41 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 "Net-(C306-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 158.6 93.2 180)
    (fp_text reference TP304 (at 0 -2.55) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93) (layer F.Fab))
    (fp_text user %R (at 0 2.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 AIN1))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Test_Point_D1.02mm (layer F.Cu) (tedit 5A43AEC6)
    (at 171.08 98.395 90)
    (fp_text reference TP305 (at -2.355 0.17 180) (layer F.SilkS))
    (fp_text value 5011 (at 0 3.93 90) (layer F.Fab))
    (fp_text user %R (at 0 2.41 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 AIN0))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.4mm_Beaded.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOIC-8_W3.9mm (layer F.Cu) (tedit 5D28A544)
    (at 145.001 89.35)
    (attr smd)
    (fp_text reference U101 (at 0.01778 4.445 180) (layer F.SilkS))
    (fp_text value PCA9306D_118 (at 0.06604 4.80314) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.905 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.635 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at 1.905 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 23 SDA))
    (pad 5 smd rect (at 1.905 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 44 SDA_5V))
    (pad 6 smd rect (at 0.635 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 43 SCL_5V))
    (pad 7 smd rect (at -0.635 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 8 smd rect (at -1.905 -2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 3 smd rect (at 0.635 2.45) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 24 SCL))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module GPS:TITAN_X1_GPS (layer F.Cu) (tedit 5962901B)
    (at 143.15 102.9 90)
    (attr smd)
    (fp_text reference U102 (at 7.15 5.35) (layer F.SilkS))
    (fp_text value XA1110_GPS (at 0 -0.127 180) (layer F.SilkS))
    (pad 1 smd rect (at -6.2484 -2.99974 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -6.2484 -1.79832 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J101-Pad2)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -6.2484 -0.59944 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -6.2484 0.59944 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -6.2484 1.79832 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at -6.2484 2.99974 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -3.59918 6.2484 180) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad1)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -2.39776 6.2484 180) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(BT101-Pad1)") (solder_mask_margin 0.1016))
    (pad 9 smd rect (at -1.19888 6.2484 180) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 1.19888 6.2484 180) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 2.39776 6.2484 180) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 3.59918 6.2484 180) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R103-Pad1)") (solder_mask_margin 0.1016))
    (pad 13 smd rect (at 6.2484 2.99974 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 14 smd rect (at 6.2484 1.79832 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 15 smd rect (at 6.2484 0.59944 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 smd rect (at 6.2484 -0.59944 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 17 smd rect (at 6.2484 -1.79832 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 18 smd rect (at 6.2484 -2.99974 90) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 19 smd rect (at 3.59918 -6.2484) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R106-Pad2)") (solder_mask_margin 0.1016))
    (pad 20 smd rect (at 2.39776 -6.2484) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R105-Pad2)") (solder_mask_margin 0.1016))
    (pad 21 smd rect (at 1.19888 -6.2484) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 27 PPS) (solder_mask_margin 0.1016))
    (pad 22 smd rect (at -1.19888 -6.2484) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R104-Pad2)") (solder_mask_margin 0.1016))
    (pad 23 smd rect (at -2.39776 -6.2484) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 24 smd rect (at -3.59918 -6.2484) (size 1.99898 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-S-8-1EP_6x5mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 2.1 2.5 4.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-143-4 (layer F.Cu) (tedit 5D28A606)
    (at 160.4 71.4 90)
    (descr http://datasheets.maximintegrated.com/en/ds/MAX6816-MAX6818.pdf)
    (attr smd)
    (fp_text reference U103 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value MAX6816EUS_T (at 0 3 90) (layer F.Fab))
    (pad 4 smd rect (at -0.96 -1 90) (size 0.55 1.31) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -0.76 1 90) (size 0.94 1.31) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.96 1 90) (size 0.55 1.31) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J102-Pad2)"))
    (pad 3 smd rect (at 0.96 -1 90) (size 0.55 1.31) (layers F.Cu F.Paste F.Mask)
      (net 28 STATE_CNHG))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-343_SC-70-4.step
      (at (xyz 0 0 0))
      (scale (xyz 1.6 1.4 1.2))
      (rotate (xyz 0 0 -90))
    )
  )
  (module digikey-footprints:SOT-223 (layer F.Cu) (tedit 5D28A60E)
    (at 107.655 84.376)
    (attr smd)
    (fp_text reference U201 (at -3.155 6.374 90) (layer F.SilkS))
    (fp_text value NCP1117ST50T3G (at 0.15 5.65) (layer F.Fab))
    (fp_text user %R (at -0.05 0.025) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.15) (size 3.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 1 smd rect (at -2.3 3.15) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 3.15) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 3 smd rect (at 2.3 3.15) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module FurnaceLogger:8BSOP (layer F.Cu) (tedit 5D9C04B9)
    (at 172.9 111.4 180)
    (descr "SOP, 8 Pin (http://www.ti.com/lit/ds/symlink/iso1050.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (attr smd)
    (fp_text reference U301 (at 7.75 5.75 180) (layer F.SilkS))
    (fp_text value MPXV7002DP (at 0 9.12) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -8.38 -3.81 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -8.38 -1.27 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 3 smd roundrect (at -8.38 1.27 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -8.38 3.81 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C301-Pad1)"))
    (pad 5 smd roundrect (at 8.38 3.81 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 8.38 1.27 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 8.38 -1.27 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 8.38 -3.81 180) (size 2.35 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 3.7 3.6 6.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TSSOP-8_W3mm (layer F.Cu) (tedit 5D28AC6D)
    (at 176.668 88.997 180)
    (descr http://www.ti.com/lit/ds/symlink/ina333.pdf)
    (attr smd)
    (fp_text reference U302 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value LTC1966CMS8_PBF (at 0 4.58) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.975 2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05))
    (pad 2 smd rect (at -0.325 2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C307-Pad1)") (solder_mask_margin 0.05))
    (pad 3 smd rect (at 0.325 2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R307-Pad1)") (solder_mask_margin 0.05))
    (pad 4 smd rect (at 0.975 2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05))
    (pad 5 smd rect (at 0.975 -2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 14 AIN0) (solder_mask_margin 0.05))
    (pad 6 smd rect (at 0.325 -2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05))
    (pad 7 smd rect (at -0.325 -2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V) (solder_mask_margin 0.05))
    (pad 8 smd rect (at -0.975 -2.2 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(JP303-Pad2)") (solder_mask_margin 0.05))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.5 1.2))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Package_SO:TSSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 143.477 82.238 180)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U303 (at 0 -2.55) (layer F.SilkS))
    (fp_text value ADS1015IDGS (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.15 -1 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R309-Pad1)"))
    (pad 2 smd rect (at -2.15 -0.5 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R310-Pad2)"))
    (pad 3 smd rect (at -2.15 0 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.15 0.5 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 AIN0))
    (pad 5 smd rect (at -2.15 1 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 AIN1))
    (pad 6 smd rect (at 2.15 1 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 AIN2))
    (pad 7 smd rect (at 2.15 0.5 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(TP307-Pad1)"))
    (pad 8 smd rect (at 2.15 0 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C310-Pad2)"))
    (pad 9 smd rect (at 2.15 -0.5 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 SDA_5V))
    (pad 10 smd rect (at 2.15 -1 180) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 SCL_5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Sponsored by\nDennis and Amy Heidner" (at 154.5 86.25) (layer B.SilkS))
  (gr_text "Ryan McCarty\nJames Eaton\nKaitlyn Icopini \nFranki Taylor" (at 141.5 104.5) (layer B.SilkS))
  (gr_text "13.8VDC Max" (at 103.25 108.8) (layer F.SilkS))
  (gr_line (start 160.15 118.4) (end 180.4 118.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.15 62.4) (end 180.4 62.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.15 98.9) (end 102.15 98.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.15 82.9) (end 103.15 97.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 183.4 65.4) (end 183.4 115.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.15 65.4) (end 98.15 80.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.15 99.9) (end 98.15 115.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.15 81.9) (end 102.15 81.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.15 118.4) (end 160.15 118.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 180.4 115.4) (end 183.4 115.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 5 (width 0.15) (layer Dwgs.User)
    (gr_text "5 mm" (at 185.5 71.5) (layer Dwgs.User))
    (feature1 (pts (xy 181.75 73.5) (xy 181.75 68.8)))
    (feature2 (pts (xy 176.75 73.5) (xy 176.75 68.8)))
    (crossbar (pts (xy 176.75 71.5) (xy 181.75 71.5)))
    (arrow1a (pts (xy 181.75 71.5) (xy 180.623496 72.086421)))
    (arrow1b (pts (xy 181.75 71.5) (xy 180.623496 70.913579)))
    (arrow2a (pts (xy 176.75 71.5) (xy 177.876504 72.086421)))
    (arrow2b (pts (xy 176.75 71.5) (xy 177.876504 70.913579)))
  )
  (gr_arc (start 102.15 97.9) (end 103.15 97.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 99.15 99.9) (end 98.15 99.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 187 101.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 183.75 110) (xy 189.45 110)))
    (feature2 (pts (xy 183.75 106.5) (xy 189.45 106.5)))
    (crossbar (pts (xy 186.75 106.5) (xy 186.75 110)))
    (arrow1a (pts (xy 186.75 110) (xy 186.163579 108.873496)))
    (arrow1b (pts (xy 186.75 110) (xy 187.336421 108.873496)))
    (arrow2a (pts (xy 186.75 106.5) (xy 186.163579 107.626504)))
    (arrow2b (pts (xy 186.75 106.5) (xy 187.336421 107.626504)))
  )
  (dimension 29 (width 0.15) (layer Dwgs.User)
    (gr_text "29 mm" (at 194.75 65.349999) (layer Dwgs.User))
    (feature1 (pts (xy 209.25 61.5) (xy 209.25 66.699999)))
    (feature2 (pts (xy 180.25 61.5) (xy 180.25 66.699999)))
    (crossbar (pts (xy 180.25 63.999999) (xy 209.25 63.999999)))
    (arrow1a (pts (xy 209.25 63.999999) (xy 208.123496 64.58642)))
    (arrow1b (pts (xy 209.25 63.999999) (xy 208.123496 63.413578)))
    (arrow2a (pts (xy 180.25 63.999999) (xy 181.376504 64.58642)))
    (arrow2b (pts (xy 180.25 63.999999) (xy 181.376504 63.413578)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 185.25 113.5) (layer Dwgs.User))
    (feature1 (pts (xy 180.25 111) (xy 180.25 116.2)))
    (feature2 (pts (xy 176.75 111) (xy 176.75 116.2)))
    (crossbar (pts (xy 176.75 113.5) (xy 180.25 113.5)))
    (arrow1a (pts (xy 180.25 113.5) (xy 179.123496 114.086421)))
    (arrow1b (pts (xy 180.25 113.5) (xy 179.123496 112.913579)))
    (arrow2a (pts (xy 176.75 113.5) (xy 177.876504 114.086421)))
    (arrow2b (pts (xy 176.75 113.5) (xy 177.876504 112.913579)))
  )
  (dimension 58 (width 0.15) (layer Dwgs.User)
    (gr_text "58 mm" (at 209.25 48.65) (layer Dwgs.User))
    (feature1 (pts (xy 238.25 52.5) (xy 238.25 47.3)))
    (feature2 (pts (xy 180.25 52.5) (xy 180.25 47.3)))
    (crossbar (pts (xy 180.25 50) (xy 238.25 50)))
    (arrow1a (pts (xy 238.25 50) (xy 237.123496 50.586421)))
    (arrow1b (pts (xy 238.25 50) (xy 237.123496 49.413579)))
    (arrow2a (pts (xy 180.25 50) (xy 181.376504 50.586421)))
    (arrow2b (pts (xy 180.25 50) (xy 181.376504 49.413579)))
  )
  (gr_arc (start 102.15 82.9) (end 102.15 81.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 99.15 80.9) (end 99.15 81.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 19.5 (width 0.15) (layer Dwgs.User)
    (gr_text "19.5 mm" (at 171.4 100.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 175.75 110) (xy 170.05 110)))
    (feature2 (pts (xy 175.75 90.5) (xy 170.05 90.5)))
    (crossbar (pts (xy 172.75 90.5) (xy 172.75 110)))
    (arrow1a (pts (xy 172.75 110) (xy 172.163579 108.873496)))
    (arrow1b (pts (xy 172.75 110) (xy 173.336421 108.873496)))
    (arrow2a (pts (xy 172.75 90.5) (xy 172.163579 91.626504)))
    (arrow2b (pts (xy 172.75 90.5) (xy 173.336421 91.626504)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 228.1 98.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 223.75 107) (xy 229.45 107)))
    (feature2 (pts (xy 223.75 90) (xy 229.45 90)))
    (crossbar (pts (xy 226.75 90) (xy 226.75 107)))
    (arrow1a (pts (xy 226.75 107) (xy 226.163579 105.873496)))
    (arrow1b (pts (xy 226.75 107) (xy 227.336421 105.873496)))
    (arrow2a (pts (xy 226.75 90) (xy 226.163579 91.126504)))
    (arrow2b (pts (xy 226.75 90) (xy 227.336421 91.126504)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 186.1 82 270) (layer Dwgs.User))
    (feature1 (pts (xy 182.75 90.5) (xy 187.45 90.5)))
    (feature2 (pts (xy 182.75 73.5) (xy 187.45 73.5)))
    (crossbar (pts (xy 184.75 73.5) (xy 184.75 90.5)))
    (arrow1a (pts (xy 184.75 90.5) (xy 184.163579 89.373496)))
    (arrow1b (pts (xy 184.75 90.5) (xy 185.336421 89.373496)))
    (arrow2a (pts (xy 184.75 73.5) (xy 184.163579 74.626504)))
    (arrow2b (pts (xy 184.75 73.5) (xy 185.336421 74.626504)))
  )
  (gr_arc (start 101.15 115.4) (end 101.15 118.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 65 (width 0.15) (layer Dwgs.User)
    (gr_text "65 mm" (at 209.25 44.15) (layer Dwgs.User))
    (feature1 (pts (xy 241.75 52.5) (xy 241.75 42.8)))
    (feature2 (pts (xy 176.75 52.5) (xy 176.75 42.8)))
    (crossbar (pts (xy 176.75 45.5) (xy 241.75 45.5)))
    (arrow1a (pts (xy 241.75 45.5) (xy 240.623496 46.086421)))
    (arrow1b (pts (xy 241.75 45.5) (xy 240.623496 44.913579)))
    (arrow2a (pts (xy 176.75 45.5) (xy 177.876504 46.086421)))
    (arrow2b (pts (xy 176.75 45.5) (xy 177.876504 44.913579)))
  )
  (dimension 11.5 (width 0.15) (layer Dwgs.User)
    (gr_text "11.5 mm" (at 215.900001 104.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 219.75 110) (xy 214.550001 110)))
    (feature2 (pts (xy 219.75 98.5) (xy 214.550001 98.5)))
    (crossbar (pts (xy 217.250001 98.5) (xy 217.250001 110)))
    (arrow1a (pts (xy 217.250001 110) (xy 216.66358 108.873496)))
    (arrow1b (pts (xy 217.250001 110) (xy 217.836422 108.873496)))
    (arrow2a (pts (xy 217.250001 98.5) (xy 216.66358 99.626504)))
    (arrow2b (pts (xy 217.250001 98.5) (xy 217.836422 99.626504)))
  )
  (gr_arc (start 101.15 65.4) (end 98.15 65.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.15 62.4) (end 160.15 62.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 56 (width 0.15) (layer Dwgs.User)
    (gr_text "56 mm (Thru-hole socket J2)" (at 283.6 81.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 274.25 109.75) (xy 284.95 109.75)))
    (feature2 (pts (xy 274.25 53.75) (xy 284.95 53.75)))
    (crossbar (pts (xy 282.25 53.75) (xy 282.25 109.75)))
    (arrow1a (pts (xy 282.25 109.75) (xy 281.663579 108.623496)))
    (arrow1b (pts (xy 282.25 109.75) (xy 282.836421 108.623496)))
    (arrow2a (pts (xy 282.25 53.75) (xy 281.663579 54.876504)))
    (arrow2b (pts (xy 282.25 53.75) (xy 282.836421 54.876504)))
  )
  (gr_arc (start 180.4 65.4) (end 180.4 62.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 2 (width 0.15) (layer Dwgs.User)
    (gr_text "2 mm" (at 226.5 86.5) (layer Dwgs.User))
    (feature1 (pts (xy 222.75 89) (xy 222.75 83.800001)))
    (feature2 (pts (xy 220.75 89) (xy 220.75 83.800001)))
    (crossbar (pts (xy 220.75 86.500001) (xy 222.75 86.500001)))
    (arrow1a (pts (xy 222.75 86.500001) (xy 221.623496 87.086422)))
    (arrow1b (pts (xy 222.75 86.500001) (xy 221.623496 85.91358)))
    (arrow2a (pts (xy 220.75 86.500001) (xy 221.876504 87.086422)))
    (arrow2b (pts (xy 220.75 86.500001) (xy 221.876504 85.91358)))
  )
  (gr_text + (at 132.5 81.75) (layer F.SilkS))
  (gr_text DQ (at 133 86.5 90) (layer F.SilkS))
  (gr_text - (at 132.5 91 90) (layer F.SilkS))
  (gr_text + (at 134.5 75.25) (layer F.SilkS))
  (gr_text - (at 125.5 75.25) (layer F.SilkS))
  (gr_text DQ (at 128.75 75.25) (layer F.SilkS))
  (gr_text "Field-Observation Furnace Logger Rev 4" (at 122 69.75) (layer F.SilkS))
  (gr_text "POWER OUT\n ONLY" (at 130.75 109) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.2 61.8) (xy 184.6 61.4) (xy 184.4 121.6) (xy 95 121.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94 61.4) (xy 185.6 60.8) (xy 186.4 124) (xy 93.6 122.8)
      )
    )
  )
)
