(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 84.575 106.55)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (gr_circle (center 105.125 113.25) (end 105.125 112.925) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 111.45) (end 105.025 111.45) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 66.525 84.973717) (end 67.25 85.623717) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 108.95) (end 105.025 108.95) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 110.45) (end 105.025 110.45) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_poly
    (pts
      (xy 64.475 81.55)
      (xy 70.625 82.55)
      (xy 75.275 83.25)
      (xy 75.65 83.275)
      (xy 77 83.3)
      (xy 78.275 83.525)
      (xy 79.4 84)
      (xy 80.575 84.85)
      (xy 81.35 85.575)
      (xy 82.325 86.625)
      (xy 82.675 87.075)
      (xy 82.825 87.775)
      (xy 82.825 88.625)
      (xy 82.975 89.625)
      (xy 83.025 89.65)
      (xy 84.125 89.75)
      (xy 84.875 89.825)
      (xy 85.325 89.95)
      (xy 86.625 90.65)
      (xy 87.8 91.325)
      (xy 88.55 91.9)
      (xy 88.75 92.025)
      (xy 89.075 92.375)
      (xy 89.15 92.575)
      (xy 89.225 93.875)
      (xy 89.275 99.275)
      (xy 89.25 104.125)
      (xy 89.25 107.675)
      (xy 103.65 107.675)
      (xy 103.65 107.175)
      (xy 103.775 107.175)
      (xy 104.125 107.675)
      (xy 106.125 107.675)
      (xy 106.475 107.175)
      (xy 106.6 107.175)
      (xy 106.6 107.675)
      (xy 113.5 107.675)
      (xy 113.5 113.225)
      (xy 106.6 113.225)
      (xy 106.6 113.725)
      (xy 106.475 113.725)
      (xy 106.125 113.225)
      (xy 104.125 113.225)
      (xy 103.775 113.725)
      (xy 103.65 113.725)
      (xy 103.65 113.225)
      (xy 83.6 113.225)
      (xy 81.65 112.225)
      (xy 81.325 112)
      (xy 80.85 112)
      (xy 80.325 112)
      (xy 79.4 112)
      (xy 76.375 112)
      (xy 75.125 112)
      (xy 74.6 111.95)
      (xy 74.25 111.9)
      (xy 74.025 111.85)
      (xy 73.675 111.75)
      (xy 73.225 111.55)
      (xy 72.925 111.375)
      (xy 72.625 111.15)
      (xy 72.275 110.85)
      (xy 71.925 110.5)
      (xy 71.6 110.1)
      (xy 71.375 109.725)
      (xy 71.25 109.45)
      (xy 71 108.85)
      (xy 70.425 107.05)
      (xy 70.2 106.375)
      (xy 70.15 105.6)
      (xy 70.125 103)
      (xy 70.1 102.75)
      (xy 70.075 102.7)
      (xy 70.025 102.65)
      (xy 69.875 102.625)
      (xy 69.425 102.6)
      (xy 67.15 102.525)
      (xy 66.725 102.5)
      (xy 66.325 102.45)
      (xy 65.95 102.375)
      (xy 65.625 102.275)
      (xy 65.15 102.075)
      (xy 64.475 101.725)
      (xy 64.1 101.5)
      (xy 63.775 101.25)
      (xy 63.55 101.05)
      (xy 62.85 100.35)
      (xy 62.6 100.05)
      (xy 62.3 99.625)
      (xy 62.1 99.25)
      (xy 61.95 98.9)
      (xy 61.825 98.525)
      (xy 61.75 98.2)
      (xy 61.675 97.8)
      (xy 61.575 96.95)
      (xy 61.5 96.5)
      (xy 61.475 96.4)
      (xy 61.425 96.125)
      (xy 61.375 95.75)
      (xy 61.325 95.3)
      (xy 61.3 95.15)
      (xy 61.275 95.025)
      (xy 61.25 94.95)
      (xy 61.2 94.9)
      (xy 61.175 94.825)
      (xy 61.15 94.55)
      (xy 61.15 94.3)
      (xy 61.125 94.1)
      (xy 61.075 93.95)
      (xy 60.95 93.775)
      (xy 60.75 93.525)
      (xy 60.525 93.275)
      (xy 60.35 93.075)
      (xy 59.85 92.525)
      (xy 59.3 91.925)
      (xy 59.05 91.65)
      (xy 58.775 91.35)
      (xy 58.475 91.025)
      (xy 58.45 91)
      (xy 57.9 90.4)
      (xy 57.175 89.6)
      (xy 56.65 89)
      (xy 56.225 88.475)
      (xy 56.075 88.275)
      (xy 55.9 88.025)
      (xy 55.775 87.825)
      (xy 55.625 87.55)
      (xy 55.4 87)
      (xy 55.2 86.35)
      (xy 55.175 86.225)
      (xy 55.15 86.075)
      (xy 55.125 85.725)
      (xy 55.15 85.325)
      (xy 55.2 84.925)
      (xy 55.3 84.45)
      (xy 55.375 84.2)
      (xy 55.55 83.775)
      (xy 55.825 83.2)
      (xy 56.025 82.85)
      (xy 56.35 82.4)
      (xy 56.85 81.9)
      (xy 57.3 81.55)
      (xy 63.080606 81.480073)
      (xy 63.5 81.475)
    ) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 112.45) (end 105.025 112.45) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 109.95) (end 105.025 109.95) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 76.3 96.325) (end 78.325 96.5) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 110.95) (end 105.025 110.95) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 111.95) (end 105.025 111.95) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 84.575 106.55) (end 85.2 107.375) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 108.45) (end 105.025 108.45) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 107.65) (end 105.125 107.975) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_circle (center 105.125 109.45) (end 105.025 109.45) (layer "Edge.Cuts") (width 0.05) (fill none))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 76.825 102.075)
        (xy 77.375 102.2)
        (xy 77.9 102.475)
        (xy 78.4 102.875)
        (xy 78.875 103.45)
        (xy 79.175 103.925)
        (xy 79.375 104.575)
        (xy 79.4 104.925)
        (xy 79.4 105)
        (xy 76.55 105)
        (xy 76.25 105.25)
        (xy 76.275 108.35)
        (xy 75.475 108.275)
        (xy 74.775 108)
        (xy 74.15 107.55)
        (xy 73.775 107.175)
        (xy 73.375 106.525)
        (xy 73.15 105.9)
        (xy 73.075 105.4)
        (xy 73.05 105.025)
        (xy 76.225 105.025)
        (xy 76.225 102.025)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 59.325 84.45)
        (xy 59.05 84.475)
        (xy 58.925 84.8)
        (xy 55.8 84.8)
        (xy 56 86.725)
        (xy 57 88.075)
        (xy 58.7 88.825)
        (xy 59.7 88.525)
        (xy 59.7 85.6)
        (xy 60.2 85.175)
        (xy 63.05 85.175)
        (xy 62.977161 83.901066)
        (xy 62.030848 82.326536)
        (xy 59.9 81.525)
        (xy 63.5 81.475)
        (xy 64.475 81.55)
        (xy 69.829172 82.425)
        (xy 75.275 83.25)
        (xy 77 83.3)
        (xy 78.225 83.525)
        (xy 77.625 84.275)
        (xy 75.952539 83.99998)
        (xy 75.975 86.875)
        (xy 75.725 86.875)
        (xy 75.575 87.275)
        (xy 73.025 87.225)
        (xy 72.525 87.25)
        (xy 72.644257 88.703041)
        (xy 73.73277 90.759122)
        (xy 75.1 91.35)
        (xy 76.45 91.475)
        (xy 76.475 90.85)
        (xy 76.425 88.1)
        (xy 76.85 87.7)
        (xy 79.9 87.75)
        (xy 79.7 86.25)
        (xy 78.775 84.9)
        (xy 77.7 84.325)
        (xy 78.3 83.525)
        (xy 79.425 84)
        (xy 80.575 84.85)
        (xy 81.35 85.6)
        (xy 82.3 86.6)
        (xy 82.675 87.075)
        (xy 82.825 87.775)
        (xy 82.825 88.625)
        (xy 82.975 89.625)
        (xy 83.025 89.65)
        (xy 84.9 89.825)
        (xy 85.375 89.975)
        (xy 87.825 91.325)
        (xy 88.75 92.025)
        (xy 89.075 92.375)
        (xy 89.175 92.6)
        (xy 89.25 96.5)
        (xy 88.825 96.475)
        (xy 87.9 93.575)
        (xy 84.8 92.55)
        (xy 84.725 95.7)
        (xy 84.45 96)
        (xy 81.825 95.975)
        (xy 81.825 95.825)
        (xy 81.25 96.025)
        (xy 81.7 98.5)
        (xy 83.225 100.075)
        (xy 85.35 100.325)
        (xy 85.375 96.925)
        (xy 85.75 96.575)
        (xy 89.25 96.575)
        (xy 89.275 107.625)
        (xy 89.25 113.225)
        (xy 83.6 113.225)
        (xy 81.65 112.225)
        (xy 81.325 112)
        (xy 75.125 112)
        (xy 74.25 111.9)
        (xy 74.025 111.85)
        (xy 73.675 111.75)
        (xy 73.375 111.625)
        (xy 74.525 108.475)
        (xy 75.798633 108.756192)
        (xy 76.425 108.775)
        (xy 76.375 105.575)
        (xy 76.85 105.225)
        (xy 79.9 105.225)
        (xy 79.8 104.025)
        (xy 79.225 102.925)
        (xy 78.325 102)
        (xy 76.975 101.55)
        (xy 76 101.5)
        (xy 76.05 104.425)
        (xy 75.675 104.75)
        (xy 72.525 104.75)
        (xy 72.745473 106.425596)
        (xy 73.365024 107.485707)
        (xy 74.4 108.45)
        (xy 73.325 111.6)
        (xy 72.9 111.35)
        (xy 72.275 110.85)
        (xy 71.925 110.5)
        (xy 71.6 110.1)
        (xy 71.35 109.675)
        (xy 70.975 108.775)
        (xy 70.2 106.375)
        (xy 70.15 105.575)
        (xy 70.125 103)
        (xy 70.1 102.725)
        (xy 70.025 102.65)
        (xy 69.825 102.625)
        (xy 67.45 102.525)
        (xy 66.7 102.5)
        (xy 66.225 102.425)
        (xy 65.95 102.375)
        (xy 65.625 102.275)
        (xy 65.15 102.075)
        (xy 64.45 101.7)
        (xy 64.075 101.475)
        (xy 63.6 101.1)
        (xy 65.225 99.45)
        (xy 66.124145 99.854195)
        (xy 67.575 100.15)
        (xy 67.6 96.85)
        (xy 67.875 96.775)
        (xy 68 96.45)
        (xy 71.25 96.475)
        (xy 70.925 94.675)
        (xy 69.4 93.025)
        (xy 67.15 92.55)
        (xy 67.175 95.7)
        (xy 66.775 96.075)
        (xy 63.825 95.931518)
        (xy 63.95 97.875)
        (xy 65.125 99.375)
        (xy 63.525 101.025)
        (xy 62.85 100.35)
        (xy 62.6 100.05)
        (xy 62.3 99.625)
        (xy 62.1 99.25)
        (xy 61.95 98.9)
        (xy 61.825 98.5)
        (xy 61.75 98.175)
        (xy 61.675 97.8)
        (xy 61.575 96.95)
        (xy 61.5 96.5)
        (xy 61.475 96.4)
        (xy 61.425 96.125)
        (xy 61.325 95.3)
        (xy 61.275 95.05)
        (xy 61.25 94.95)
        (xy 61.2 94.9)
        (xy 61.175 94.823943)
        (xy 61.15 94.55)
        (xy 61.15 94.3)
        (xy 61.125 94.099589)
        (xy 61.05 93.9)
        (xy 60.75 93.525)
        (xy 56.7 89.05)
        (xy 56.4 88.7)
        (xy 55.925 88.075)
        (xy 55.625 87.55)
        (xy 55.4 86.975)
        (xy 55.2 86.35)
        (xy 55.15 86.05)
        (xy 55.125 85.725)
        (xy 55.2 84.9)
        (xy 55.375 84.2)
        (xy 55.525 83.825)
        (xy 55.975 82.9)
        (xy 56.375 82.35)
        (xy 56.875 81.875)
        (xy 57.325 81.55)
        (xy 59.325 81.525)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 68 93.35)
        (xy 68.55 93.475)
        (xy 69.075 93.75)
        (xy 69.575 94.15)
        (xy 70.05 94.725)
        (xy 70.35 95.2)
        (xy 70.55 95.85)
        (xy 70.575 96.2)
        (xy 70.575 96.275)
        (xy 67.725 96.275)
        (xy 67.425 96.525)
        (xy 67.45 99.625)
        (xy 66.65 99.55)
        (xy 65.95 99.275)
        (xy 65.325 98.825)
        (xy 64.95 98.45)
        (xy 64.55 97.8)
        (xy 64.325 97.175)
        (xy 64.25 96.675)
        (xy 64.225 96.3)
        (xy 67.4 96.3)
        (xy 67.4 93.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads no (clearance 0.0255))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 113.225)
        (xy 106.6 113.25)
        (xy 106.599977 113.726706)
        (xy 106.475 113.725)
        (xy 106.125 113.25)
        (xy 105.25 113.25)
        (xy 105.25 107.65)
        (xy 106.125 107.65)
        (xy 106.475 107.175)
        (xy 106.6 107.175)
        (xy 106.6 107.65)
        (xy 113.5 107.65)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 85.6 93.325)
        (xy 86.15 93.45)
        (xy 86.675 93.725)
        (xy 87.175 94.125)
        (xy 87.65 94.7)
        (xy 87.95 95.175)
        (xy 88.15 95.825)
        (xy 88.175 96.175)
        (xy 88.175 96.25)
        (xy 85.325 96.25)
        (xy 85.025 96.5)
        (xy 85.05 99.6)
        (xy 84.25 99.525)
        (xy 83.55 99.25)
        (xy 82.925 98.8)
        (xy 82.55 98.425)
        (xy 82.15 97.775)
        (xy 81.925 97.15)
        (xy 81.85 96.65)
        (xy 81.825 96.275)
        (xy 85 96.275)
        (xy 85 93.275)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 60.075 82.05)
        (xy 60.625 82.175)
        (xy 61.15 82.45)
        (xy 61.65 82.85)
        (xy 62.125 83.425)
        (xy 62.425 83.9)
        (xy 62.625 84.55)
        (xy 62.65 84.9)
        (xy 62.65 84.975)
        (xy 59.8 84.975)
        (xy 59.5 85.225)
        (xy 59.525 88.325)
        (xy 58.725 88.25)
        (xy 58.025 87.975)
        (xy 57.4 87.525)
        (xy 57.025 87.15)
        (xy 56.625 86.5)
        (xy 56.4 85.875)
        (xy 56.325 85.375)
        (xy 56.3 85)
        (xy 59.475 85)
        (xy 59.475 82)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 76.825 84.575)
        (xy 77.375 84.7)
        (xy 77.9 84.975)
        (xy 78.4 85.375)
        (xy 78.875 85.95)
        (xy 79.175 86.425)
        (xy 79.375 87.075)
        (xy 79.4 87.425)
        (xy 79.4 87.5)
        (xy 76.55 87.5)
        (xy 76.25 87.75)
        (xy 76.275 90.85)
        (xy 75.475 90.775)
        (xy 74.775 90.5)
        (xy 74.15 90.05)
        (xy 73.775 89.675)
        (xy 73.375 89.025)
        (xy 73.15 88.4)
        (xy 73.075 87.9)
        (xy 73.05 87.525)
        (xy 76.225 87.525)
        (xy 76.225 84.525)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.0255))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.515619 113.218088)
        (xy 106.615619 113.243088)
        (xy 106.6 113.725)
        (xy 106.474416 113.730027)
        (xy 106.124416 113.255027)
        (xy 105.240619 113.243088)
        (xy 105.240619 107.643088)
        (xy 106.136354 107.639947)
        (xy 106.486354 107.164947)
        (xy 106.615619 107.168088)
        (xy 106.615619 107.643088)
        (xy 113.515619 107.643088)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 108.4)
        (xy 100 108.4)
        (xy 100 108)
        (xy 105 108)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 111.9)
        (xy 100 111.9)
        (xy 100 111.5)
        (xy 105 111.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 108.9)
        (xy 100 108.9)
        (xy 100 108.5)
        (xy 105 108.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 110.4)
        (xy 100 110.4)
        (xy 100 110)
        (xy 105 110)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 112.9)
        (xy 100 112.9)
        (xy 100 112.5)
        (xy 105 112.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 112.4)
        (xy 100 112.4)
        (xy 100 112)
        (xy 105 112)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 109.4)
        (xy 100 109.4)
        (xy 100 109)
        (xy 105 109)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 110.9)
        (xy 100 110.9)
        (xy 100 110.5)
        (xy 105 110.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 109.9)
        (xy 100 109.9)
        (xy 100 109.5)
        (xy 105 109.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.0255))
    (min_thickness 0.0255) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.0255) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 105 111.4)
        (xy 100 111.4)
        (xy 100 111)
        (xy 105 111)
      )
    )
  )
)
