(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 63)
    (no_connects 0)
    (area 132.813667 54.073666 161.032715 99.8982)
    (thickness 1.6)
    (drawings 21)
    (tracks 440)
    (zones 0)
    (modules 20)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D101-Pad1)")
  (net 2 "Net-(D102-Pad1)")
  (net 3 "Net-(D103-Pad1)")
  (net 4 VDD)
  (net 5 "Net-(R101-Pad2)")
  (net 6 GND)
  (net 7 /DIO0)
  (net 8 /SSEL)
  (net 9 /SCLK)
  (net 10 /MISO)
  (net 11 /MOSI)
  (net 12 /LED1)
  (net 13 /LED2)
  (net 14 /DIO1)
  (net 15 /TX)
  (net 16 /RX)
  (net 17 /DIO2)
  (net 18 /DIO3)
  (net 19 /SWDIO)
  (net 20 /SWCLK)
  (net 21 /DIO5)
  (net 22 /LED3)
  (net 23 /RESET)
  (net 24 /BOOT0)
  (net 25 /MODEM_RESET)
  (net 26 /ANT)
  (net 27 /BUTTON)
  (net 28 /PA1)
  (net 29 /PB4)
  (net 30 /PB5)
  (net 31 /PB6)
  (net 32 /PB7)
  (net 33 /PF0)
  (net 34 /PF1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ANT)
    (add_net /BOOT0)
    (add_net /BUTTON)
    (add_net /DIO0)
    (add_net /DIO1)
    (add_net /DIO2)
    (add_net /DIO3)
    (add_net /DIO5)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LED3)
    (add_net /MISO)
    (add_net /MODEM_RESET)
    (add_net /MOSI)
    (add_net /PA1)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /PF0)
    (add_net /PF1)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SCLK)
    (add_net /SSEL)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D102-Pad1)")
    (add_net "Net-(D103-Pad1)")
    (add_net "Net-(R101-Pad2)")
    (add_net VDD)
  )
  (module Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 148.4884 66.802 90)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 7 x 7 x 1.4 mm (see NXP sot358-1_po.pdf and sot358-1_fr.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U101 (at 0 -5.85 90) (layer F.Fab))
    (fp_text value STM32F051K8Tx_u (at 0 5.85 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /PF0))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /PF1))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /RESET))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /BUTTON))
    (pad 7 smd rect (at -4.25 2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /PA1))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /MODEM_RESET))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /DIO0))
    (pad 10 smd rect (at -2 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /SSEL))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCLK))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /LED1))
    (pad 15 smd rect (at 2 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /LED2))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 18 smd rect (at 4.25 2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /DIO1))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /TX))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /RX))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /DIO2))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /DIO3))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /SWDIO))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /SWCLK))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /DIO5))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /LED3))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /PB4))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /PB5))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /PB6))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /PB7))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /BOOT0))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RFM12:RFM12B (layer F.Cu) (tedit 55FB358D)
    (at 149.4536 81.6864)
    (fp_text reference U102 (at 0 1) (layer F.Fab))
    (fp_text value RFM12 (at 0 -1) (layer F.Fab))
    (pad 1 smd rect (at -8 -6) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 2 smd rect (at -8 -4) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /DIO0))
    (pad 3 smd rect (at -8 -2) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /DIO2))
    (pad 4 smd rect (at -8 0) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /DIO1))
    (pad 5 smd rect (at -8 2) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /DIO5))
    (pad 6 smd rect (at -8 4) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /MODEM_RESET))
    (pad 7 smd rect (at -8 6) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 8 smd rect (at 8 6) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /ANT))
    (pad 9 smd rect (at 8 4) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 10 smd rect (at 8 2) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 11 smd rect (at 8 0) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /DIO3))
    (pad 12 smd rect (at 8 -2) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 13 smd rect (at 8 -4) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCLK))
    (pad 14 smd rect (at 8 -6) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /SSEL))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 156.972 68.4276 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D101 (at 0 -1.5 180) (layer F.Fab))
    (fp_text value Led_Small (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LED1))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D101-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 156.972 65.2272 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D102 (at 0 -1.5 180) (layer F.Fab))
    (fp_text value Led_Small (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LED2))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D102-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 156.972 62.0268 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D103 (at 0 -1.5 180) (layer F.Fab))
    (fp_text value Led_Small (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 22 /LED3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D103-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B)
    (at 140.208 67.818 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P101 (at 0 -5.1 180) (layer F.Fab))
    (fp_text value CONN_02X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VDD))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /RESET))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /SWCLK))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SWDIO))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 149.9108 94.0308 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R101 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value R_Small (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R101-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 149.9108 96.6216 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R102 (at 0 -1.8 270) (layer F.Fab))
    (fp_text value R_Small (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R101-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 156.5148 70.0532 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R103 (at 0 -1.8 180) (layer F.Fab))
    (fp_text value R_Small (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 156.5148 66.802 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R104 (at 0 -1.8 180) (layer F.Fab))
    (fp_text value R_Small (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D102-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 156.5148 63.6016 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R105 (at 0 -1.8 180) (layer F.Fab))
    (fp_text value R_Small (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D103-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 153.7208 59.182 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P102 (at 0 -5.1 270) (layer F.Fab))
    (fp_text value CONN_01X06 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VDD))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /BOOT0))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /TX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /RX))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /RESET))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ekoeppen_parts:SMA_PTH (layer F.Cu) (tedit 586D1006)
    (at 154.5336 94.488)
    (fp_text reference AE101 (at 0.13 -2) (layer F.Fab))
    (fp_text value Antenna (at 0 -3.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask)
      (net 26 /ANT))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 140.716 71.628 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.27 90) (layer F.Fab))
    (fp_text value C_Small (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 145.034 72.644 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27 180) (layer F.Fab))
    (fp_text value C_Small (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 153.12 61.6712 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -1.27 180) (layer F.Fab))
    (fp_text value C_Small (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 138.176 71.6788 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.27 180) (layer F.Fab))
    (fp_text value C_Small (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 138.2268 70.4596 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.27 180) (layer F.Fab))
    (fp_text value C_Small (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h4.3mm (layer F.Cu) (tedit 58134DDE)
    (at 141.224 92.2232)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW101 (at 3.25 -2) (layer F.Fab))
    (fp_text value SW_PUSH (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R101-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /BUTTON))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R101-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /BUTTON))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h4.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x09 (layer F.Cu) (tedit 0)
    (at 137.922 76.2)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P103 (at 0 -5.1) (layer F.Fab))
    (fp_text value CONN_01X09 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VDD))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /PA1))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /PB4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /PB5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /PB6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /PB7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /PF0))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /PF1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x09.wrl
      (at (xyz 0 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text PF1 (at 144.526 96.266) (layer B.SilkS))
  (gr_text PF0 (at 144.526 94.0308) (layer B.SilkS))
  (gr_text PB7 (at 144.4752 91.2368) (layer B.SilkS))
  (gr_text PB6 (at 141.6304 88.9508) (layer B.SilkS))
  (gr_text PB5 (at 141.6812 86.4108) (layer B.SilkS))
  (gr_text PB4 (at 141.6304 83.9216) (layer B.SilkS))
  (gr_text PA1 (at 141.6304 81.3816) (layer B.SilkS))
  (gr_text VDD (at 141.6812 78.994) (layer B.SilkS))
  (gr_text GND (at 141.7828 76.454) (layer B.SilkS))
  (gr_text RESET (at 141.8844 63.6524 90) (layer B.SilkS))
  (gr_text GND (at 143.9164 62.5856 90) (layer B.SilkS))
  (gr_text RX (at 146.1516 61.9252 90) (layer B.SilkS))
  (gr_text TX (at 148.844 61.8744 90) (layer B.SilkS))
  (gr_text BOOT0 (at 151.2824 64.1096 90) (layer B.SilkS))
  (gr_text 20180411 (at 157.0228 83.3628 90) (layer B.SilkS))
  (gr_text VDD (at 153.8224 62.8904 90) (layer B.SilkS))
  (gr_line (start 159 99) (end 136 99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 57) (end 159 99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136 57) (end 159 57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136 99) (end 136 57) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.0932 57.15) (xy 158.9024 57.15) (xy 159.004 99.0092) (xy 136.0424 99.0092)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.144 57.2008) (xy 158.8516 57.15) (xy 158.9024 99.0092) (xy 136.0932 98.9076) (xy 136.1948 57.2516)
      )
    )
  )
)
