(kicad_pcb (version 4) (host pcbnew 4.0.1-4.201602090852+6195~38~ubuntu14.04.1-stable)
  (general
    (links 48)
    (no_connects 8)
    (area 148.224999 51.424999 217.275001 105.175001)
    (thickness 1.6)
    (drawings 13)
    (tracks 129)
    (zones 0)
    (modules 8)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 1.2)
    (uvia_drill 0.8)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "test gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 BATTERY)
  (net 3 "Net-(J2-Pad1)")
  (net 4 3.3VOLT)
  (net 5 UART_ARDUINO_TO_RADIO)
  (net 6 UART_RADIO_TO_ARDUINO)
  (net 7 /AD_P8)
  (net 8 /AD_P9)
  (net 9 /AD_P10)
  (net 10 /AD_P11)
  (net 11 "Net-(J3-Pad1)")
  (net 12 RN_RESET)
  (net 13 /HW_RX)
  (net 14 /HW_TX)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 1.2)
    (uvia_drill 0.8)
    (add_net /AD_P10)
    (add_net /AD_P11)
    (add_net /AD_P8)
    (add_net /AD_P9)
    (add_net /HW_RX)
    (add_net /HW_TX)
    (add_net 3.3VOLT)
    (add_net BATTERY)
    (add_net GND)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net RN_RESET)
    (add_net UART_ARDUINO_TO_RADIO)
    (add_net UART_RADIO_TO_ARDUINO)
  )
  (net_class Thin ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 1.2)
    (uvia_drill 0.8)
  )
  (module freetronics_footprints:ARDUINO_SHIELD (layer F.Cu) (tedit 0)
    (at 148.5011 105.0036)
    (descr http://www.thingiverse.com/thing:9630)
    (fp_text reference SHIELD1 (at 5.715 -57.15) (layer F.SilkS))
    (fp_text value ARDUINO_SHIELD (at 10.16 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 3.3VOLT))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /HW_RX))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /HW_TX))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /AD_P8))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /AD_P9))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /AD_P10))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /AD_P11))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RN_RESET))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 BATTERY))
    (pad "" np_thru_hole circle (at 66.04 -7.62 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 66.04 -35.56 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 15.24 -50.8 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 13.97 -2.54 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad SDA thru_hole oval (at 21.336 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SCL thru_hole oval (at 18.796 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad IO_R thru_hole oval (at 30.48 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad NC thru_hole oval (at 27.94 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SP1 thru_hole circle (at 63.5 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SP2 thru_hole circle (at 66.04 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SP3 thru_hole circle (at 63.5 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SP4 thru_hole circle (at 66.04 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SP5 thru_hole circle (at 63.5 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SP6 thru_hole circle (at 66.04 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 195.58 62.23 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /HW_RX))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /HW_TX))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /AD_P8))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /AD_P9))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /AD_P10))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /AD_P11))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 195.58 59.69 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 UART_ARDUINO_TO_RADIO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 UART_ARDUINO_TO_RADIO))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 UART_ARDUINO_TO_RADIO))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 UART_ARDUINO_TO_RADIO))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 UART_ARDUINO_TO_RADIO))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 UART_ARDUINO_TO_RADIO))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 195.58 64.77 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 UART_RADIO_TO_ARDUINO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 UART_RADIO_TO_ARDUINO))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 UART_RADIO_TO_ARDUINO))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 UART_RADIO_TO_ARDUINO))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 UART_RADIO_TO_ARDUINO))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 UART_RADIO_TO_ARDUINO))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module freetronics_footprints:SCREWTERMINAL-5MM-2 (layer F.Cu) (tedit 54779580)
    (at 213.36 88.265 270)
    (fp_text reference J1 (at 0 -2.4 270) (layer Eco1.User))
    (fp_text value SCREW_TERMINAL (at 0 -1.8 270) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at -2.5 0 270) (size 1.94564 1.94564) (drill 1.29794) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.94564 1.94564) (drill 1.29794) (layers *.Cu *.Mask)
      (net 2 BATTERY))
  )
  (module MyFootprints:SMA_BOARD_UPRIGHT (layer F.Cu) (tedit 5643618C)
    (at 153.67 77.47 90)
    (fp_text reference J2 (at -1.4 4.8 90) (layer F.SilkS))
    (fp_text value SMA (at 4.3 -4.8 90) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.54 2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 2.54 -2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at -2.54 -2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.6 2.6) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J2-Pad1)"))
  )
  (module MyFootprints:SMA_BOARD_UPRIGHT (layer F.Cu) (tedit 5643618C)
    (at 153.67 88.265 90)
    (fp_text reference J3 (at -1.4 4.8 90) (layer F.SilkS))
    (fp_text value SMA (at 4.3 -4.8 90) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.54 2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 2.54 -2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at -2.54 -2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.6 2.6) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J3-Pad1)"))
  )
  (module MyFootprints:RN2483 (layer F.Cu) (tedit 5643193A)
    (at 187.96 87.63 90)
    (fp_text reference U1 (at 2.8956 -1.4478 90) (layer F.SilkS))
    (fp_text value RN2483 (at 4.7752 -24.2062 90) (layer F.Fab) hide)
    (pad 47 smd rect (at 0 -1.27 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at 0 -2.54 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 45 smd rect (at 0 -3.81 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at 0 -5.08 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at 0 -6.35 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0 -7.62 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0 -8.89 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 0 -10.16 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 0 -11.43 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 0 -12.7 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 0 -13.97 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 0 -15.24 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 0 -16.51 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 0 -17.78 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 4 3.3VOLT))
    (pad 33 smd rect (at 0 -19.05 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 0 -20.32 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 12 RN_RESET))
    (pad 31 smd rect (at 0 -21.59 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 0 -22.86 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 0 -24.13 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0 -25.4 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 17.78 -25.4 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 5.08 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 6.35 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at 7.62 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 24 smd rect (at 8.89 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 10.16 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 22 smd rect (at 11.43 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 12.7 -26.67 90) (size 1.016 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 17.78 -24.13 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 17.78 -22.86 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 17.78 -21.59 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 17.78 -20.32 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 17.78 -19.05 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 17.78 -17.78 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 17.78 -16.51 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 17.78 -15.24 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 4 3.3VOLT))
    (pad 11 smd rect (at 17.78 -13.97 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 17.78 -12.7 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 17.78 -11.43 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 17.78 -10.16 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 17.78 -8.89 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 5 UART_ARDUINO_TO_RADIO))
    (pad 6 smd rect (at 17.78 -7.62 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 6 UART_RADIO_TO_ARDUINO))
    (pad 5 smd rect (at 17.78 -6.35 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 17.78 -5.08 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 17.78 -3.81 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 17.78 -2.54 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 17.78 -1.27 90) (size 1.524 1.016) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text "RN2483 shield\nJP Meijers" (at 191.135 76.835) (layer F.Cu))
  (dimension 53.6 (width 0.3) (layer Margin)
    (gr_text "53,600 mm" (at 137.750001 78.3 270) (layer Margin))
    (feature1 (pts (xy 148.3 105.1) (xy 136.400001 105.1)))
    (feature2 (pts (xy 148.3 51.5) (xy 136.400001 51.5)))
    (crossbar (pts (xy 139.100001 51.5) (xy 139.100001 105.1)))
    (arrow1a (pts (xy 139.100001 105.1) (xy 138.51358 103.973496)))
    (arrow1b (pts (xy 139.100001 105.1) (xy 139.686422 103.973496)))
    (arrow2a (pts (xy 139.100001 51.5) (xy 138.51358 52.626504)))
    (arrow2b (pts (xy 139.100001 51.5) (xy 139.686422 52.626504)))
  )
  (dimension 68.9 (width 0.3) (layer Margin)
    (gr_text "68,900 mm" (at 182.75 42.35) (layer Margin))
    (feature1 (pts (xy 148.3 67.3) (xy 148.3 41)))
    (feature2 (pts (xy 217.2 67.3) (xy 217.2 41)))
    (crossbar (pts (xy 217.2 43.7) (xy 148.3 43.7)))
    (arrow1a (pts (xy 148.3 43.7) (xy 149.426504 43.113579)))
    (arrow1b (pts (xy 148.3 43.7) (xy 149.426504 44.286421)))
    (arrow2a (pts (xy 217.2 43.7) (xy 216.073496 43.113579)))
    (arrow2b (pts (xy 217.2 43.7) (xy 216.073496 44.286421)))
  )
  (gr_line (start 213.3 51.5) (end 148.3 51.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.4 51.6) (end 213.3 51.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.7 52.9) (end 213.4 51.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.7 64.3) (end 214.7 52.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.2 66.8) (end 214.7 64.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.2 100) (end 217.2 66.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.7 102.5) (end 217.2 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.7 105.1) (end 214.7 102.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.3 105.1) (end 214.7 105.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.3 51.5) (end 148.3 105.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 71.12) (xy 162.56 86.36) (xy 187.96 86.36) (xy 187.96 71.12)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.6) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 148.3 51.5) (xy 148.3 105.1) (xy 214.7 105.1) (xy 214.7 102.5) (xy 217.2 100)
        (xy 217.2 66.8) (xy 214.7 64.3) (xy 214.7 52.9) (xy 213.3 51.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.6) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 148.3 51.5) (xy 148.3 105.1) (xy 214.7 105.1) (xy 214.7 102.5) (xy 217.2 100)
        (xy 217.2 66.8) (xy 214.7 64.3) (xy 214.7 52.9) (xy 213.3 51.5)
      )
    )
  )
)
