(kicad_pcb (version 4) (host pcbnew 4.0.1-3.201512221401+6198~38~ubuntu15.10.1-stable)
  (general
    (links 12)
    (no_connects 0)
    (area 11.205538 8.2676 38.768302 52.416601)
    (thickness 1.6)
    (drawings 4)
    (tracks 63)
    (zones 0)
    (modules 5)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x030f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad3)")
  (net 3 "Net-(U1-Pad4)")
  (net 4 "Net-(U1-Pad5)")
  (net 5 "Net-(U1-Pad6)")
  (net 6 "Net-(U1-Pad7)")
  (net 7 "Net-(U1-Pad16)")
  (net 8 +3V3)
  (net 9 GND)
  (net 10 "Net-(P1-Pad1)")
  (net 11 /SCK)
  (net 12 /MISO)
  (net 13 /MOSI)
  (net 14 /IRQ)
  (net 15 /CSN)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CSN)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 569FEB7C)
    (at 19.658 42.96 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U2 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value NRF24L01 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(U1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /CSN))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCK))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /MOSI))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /MISO))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /IRQ))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 29.9704 21.0652 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value CP (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer B.Cu) (tedit 569FEB72)
    (at 17.9572 18.564 270)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U1 (at 0.254 1.778 270) (layer B.SilkS) hide)
    (fp_text value RFM69HW (at 8.382 -7.112 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.4 0 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -1.4 -2 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 14 /IRQ))
    (pad 3 smd rect (at -1.4 -4 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.4 -6 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -1.4 -8 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -1.4 -10 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -1.4 -12 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -1.4 -14 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
    (pad 9 smd rect (at 18.3 -14 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 9 GND))
    (pad 10 smd rect (at 18.3 -12 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (pad 11 smd rect (at 18.3 -10 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 9 GND))
    (pad 12 smd rect (at 18.3 -8 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCK))
    (pad 13 smd rect (at 18.3 -6 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 /MISO))
    (pad 14 smd rect (at 18.3 -4 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 13 /MOSI))
    (pad 15 smd rect (at 18.3 -2 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 15 /CSN))
    (pad 16 smd rect (at 18.3 0 270) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U1-Pad16)"))
    (model mysensors.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals_Oscillators_SMD.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen_BIG (layer F.Cu) (tedit 569FEB60)
    (at 24.6872 8.7716)
    (descr "Symbol, OSHW-Logo, Silk Screen, BIG")
    (tags "Symbol, OSHW-Logo, Silk Screen, BIG")
    (fp_text reference REF** (at -0.29972 11.50112) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen_BIG (at 0.29972 32.10052) (layer F.Fab))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 31.1896 41.5376)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 16.7116 14.9) (end 16.7116 44.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33.1708 14.9) (end 16.7116 14.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33.1708 44.9) (end 33.1708 14.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 16.7116 44.9) (end 33.1708 44.9) (layer Edge.Cuts) (width 0.15))
  (zone (net 9) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.7 14.9) (xy 33.2 14.9) (xy 33.2 44.9) (xy 16.7 44.9)
      )
    )
  )
)
