(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-dev-496-g41c1657eb)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 61)
    (zones 0)
    (modules 18)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 120.65 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 /SDA)
  (net 4 /SCL)
  (net 5 "Net-(U1-Pad3)")
  (net 6 "Net-(U1-Pad5)")
  (net 7 "Net-(U1-Pad8)")
  (net 8 +5V)
  (net 9 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad1)")
  )
  (net_class signals ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SCL)
    (add_net /SDA)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B098A9B)
    (at 143.51 99.06)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B098A96)
    (at 123.19 99.06)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B098A91)
    (at 123.19 78.74)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B098A87)
    (at 143.51 78.74)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 5A042B2C)
    (at 139.065 77.47)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 5A042B16)
    (at 127.635 100.33)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 5A042B16)
    (at 139.065 100.33)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 5A042B2C)
    (at 127.635 77.47)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 5A042B1F)
    (at 121.92 94.615)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57D2B7A7)
    (at 137.16 83.185 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 4k7 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57D2B7B3)
    (at 133.35 88.9)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -5.08 1.905 270) (layer F.SilkS))
    (fp_text value AS5601 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad8)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57D2B7A2)
    (at 131.445 83.185 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57D2B79E)
    (at 128.905 83.185 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 57D2B795)
    (at 133.985 93.98 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.635 3.81 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 3.81 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57D2B79A)
    (at 134.62 83.185 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 4k7 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer B.Cu) (tedit 57D2C3EA)
    (at 142.875 83.82 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 5.1 180) (layer B.SilkS) hide)
    (fp_text value CONN_02X05 (at 0 3.1 180) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(P1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(P1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 +5V))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /SCL))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /SCL))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /SDA))
    (pad 10 thru_hole oval (at 2.54 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /SDA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 5A042BF8)
    (at 128.905 92.71 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference "©2017 LSF" (at 2.54 6.985 270) (layer B.SilkS))
    (fp_text value SatNOGS-Encoder (at 4.445 4.445 270) (layer B.SilkS))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 5A042B26)
    (at 121.92 83.185)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (gr_text SDA (at 136.525 93.98) (layer B.SilkS))
  (gr_text SCL (at 136.525 91.44) (layer B.SilkS))
  (gr_text GND|+5V (at 134.62 88.9) (layer B.SilkS))
  (gr_text GND|+5V (at 134.62 86.36) (layer B.SilkS))
  (gr_text GND|+5V (at 134.62 83.82) (layer B.SilkS))
  (gr_line (start 120.65 76.2) (end 120.65 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 76.2) (end 120.65 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 101.6) (end 146.05 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.65 101.6) (end 146.05 101.6) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.8) (thermal_bridge_width 0.8) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 120.65 101.6) (xy 120.65 76.2) (xy 146.05 76.2) (xy 146.05 101.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.4)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 120.65 101.6) (xy 120.65 76.2) (xy 146.05 76.2) (xy 146.05 101.6)
      )
    )
  )
)
