<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="4.318" y1="21.475825" x2="4.318" y2="9.398" width="0.1524" layer="20"/>
<wire x1="4.318" y1="9.398" x2="5.588" y2="8.382" width="0.1524" layer="20" curve="90"/>
<wire x1="5.588" y1="8.382" x2="21.379590625" y2="8.382" width="0.1524" layer="20"/>
<wire x1="21.379590625" y1="8.382" x2="22.86" y2="10.370409375" width="0.1524" layer="20" curve="90"/>
<wire x1="22.86" y1="10.370409375" x2="22.86" y2="21.218121875" width="0.1524" layer="20"/>
<wire x1="22.86" y1="21.218121875" x2="21.472121875" y2="23.114" width="0.1524" layer="20" curve="90"/>
<wire x1="21.472121875" y1="23.114" x2="5.956175" y2="23.114" width="0.1524" layer="20"/>
<wire x1="5.956175" y1="23.114" x2="4.318" y2="21.475825" width="0.1524" layer="20" curve="90"/>
<text>Mobius Strip
Technologies</text>
<text>TE/PC-GT
Video Mod v1.0</text>
<text>Connect to HuC6260
Lift and Ground Pins
19, 25, 29, 32, and 39

Transistors: MMBT3904
or equivalent</text>
<text>SMD Package Size 0805</text>
<text>Original Circuit Schematic by thesteve of PCEngineFX Forums</text>
</plain>
<libraries>
<library name="transistor-neu-to92">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="COMPVID" library="transistor-neu-to92" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VIDOUT" library="transistor-neu-to92" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="27K" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="8.2K" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="6.3K" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4.7K" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="220" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1K" library="eagle-ltspice" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PIN20" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PIN26" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PIN33" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PIN40" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TO-SCREEN" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TO-AV-JACK" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="27K" pad="2"/>
<contactref element="PIN20" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="8.2K" pad="2"/>
<contactref element="PIN26" pad="1"/>
</signal>
<signal name="S$3">
<contactref element="6.3K" pad="2"/>
<contactref element="PIN33" pad="1"/>
</signal>
<signal name="S$4">
<contactref element="4.7K" pad="2"/>
<contactref element="PIN40" pad="1"/>
</signal>
<signal name="S$5">
<contactref element="8.2K" pad="1"/>
<contactref element="27K" pad="1"/>
<contactref element="6.3K" pad="1"/>
<contactref element="4.7K" pad="1"/>
<contactref element="COMPVID" pad="1"/>
</signal>
<signal name="S$7">
</signal>
<signal name="S$11">
</signal>
<signal name="S$6">
<contactref element="COMPVID" pad="3"/>
<contactref element="5V" pad="1"/>
<contactref element="220" pad="1"/>
</signal>
<signal name="S$8">
<contactref element="VIDOUT" pad="3"/>
<contactref element="220" pad="2"/>
</signal>
<signal name="S$9">
<contactref element="TO-SCREEN" pad="1"/>
<contactref element="COMPVID" pad="2"/>
<contactref element="1K" pad="1"/>
</signal>
<signal name="S$10">
<contactref element="VIDOUT" pad="1"/>
<contactref element="1K" pad="2"/>
</signal>
<signal name="S$13">
<contactref element="TO-AV-JACK" pad="1"/>
<contactref element="VIDOUT" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
