(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 67)
    (no_connects 0)
    (area 104.064999 48.819999 191.845001 90.880001)
    (thickness 1.6)
    (drawings 31)
    (tracks 226)
    (zones 0)
    (modules 27)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 2.159)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 146.685 57.785)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +5V)
  (net 4 //MCLR)
  (net 5 "Net-(U1-Pad12)")
  (net 6 /ICSPCLK)
  (net 7 /ICSPDAT)
  (net 8 /LBUS)
  (net 9 /OUT_1)
  (net 10 /OUT_2)
  (net 11 /OUT_3)
  (net 12 /OUT_4)
  (net 13 /12V_UNPROTECTED)
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad2)")
  (net 16 "Net-(D5-Pad2)")
  (net 17 "Net-(D6-Pad2)")
  (net 18 /CMD_1)
  (net 19 /CMD_2)
  (net 20 /CMD_3)
  (net 21 /CMD_4)
  (net 22 /A0)
  (net 23 /A1)
  (net 24 /A2)
  (net 25 /A3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.508)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net //MCLR)
    (add_net /12V_UNPROTECTED)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /CMD_1)
    (add_net /CMD_2)
    (add_net /CMD_3)
    (add_net /CMD_4)
    (add_net /ICSPCLK)
    (add_net /ICSPDAT)
    (add_net /LBUS)
    (add_net /OUT_1)
    (add_net /OUT_2)
    (add_net /OUT_3)
    (add_net /OUT_4)
    (add_net GND)
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(U1-Pad12)")
  )
  (module Mounting_Holes:MountingHole_2.7mm_Pad_Via (layer F.Cu) (tedit 5844A543)
    (at 188.595 87.63)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_Pad_Via (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_Pad_Via (layer F.Cu) (tedit 5844A546)
    (at 107.315 87.63)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_Pad_Via (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_Pad_Via (layer F.Cu) (tedit 5844A533)
    (at 188.595 52.07)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_Pad_Via (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 151.765 66.548)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q2 (at 0 -0.762) (layer F.SilkS))
    (fp_text value Q_NMOS_GDSD (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 /OUT_2))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 /OUT_2))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 153.035 79.629 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.254 -1.905 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn_ribbon:SOD-323_HandSoldering (layer F.Cu) (tedit 57E36C55)
    (at 146.685 67.691 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /LBUS))
    (pad 2 smd rect (at 1.055 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model /home/cpriscal/Projets/lin_modules/13a_switch/sod323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 541A9C39)
    (at 146.685 73.66 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at -4.445 -0.635 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.7 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 136.525 74.295 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 13 /12V_UNPROTECTED))
    (model /home/cpriscal/Projets/lin_modules/13a_switch/sod-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 131.445 66.675)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q4 (at 0 -0.762) (layer F.SilkS))
    (fp_text value Q_NMOS_GDSD (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 12 /OUT_4))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 12 /OUT_4))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 161.925 66.548)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 -0.762) (layer F.SilkS))
    (fp_text value Q_NMOS_GDSD (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 /OUT_1))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 /OUT_1))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 151.765 75.438)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.175 0.127) (layer F.SilkS))
    (fp_text value 150 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /CMD_2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 161.925 75.438)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.175 0.127) (layer F.SilkS))
    (fp_text value 150 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /CMD_1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 141.605 66.675)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q3 (at 0 -0.762) (layer F.SilkS))
    (fp_text value Q_NMOS_GDSD (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 11 /OUT_3))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 11 /OUT_3))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D6-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 141.605 75.565)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.175 0) (layer F.SilkS))
    (fp_text value 150 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /CMD_3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 131.445 75.565)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.255 0) (layer F.SilkS))
    (fp_text value 150 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /CMD_4))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 54EA0684)
    (at 151.765 88.9 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 12.7 270) (layer F.SilkS))
    (fp_text value MOLEX-22-28-6050 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 //MCLR))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /ICSPDAT))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /ICSPCLK))
    (model /home/cpriscal/Projets/lin_modules/common/3d/molex-22-28-6050.wrl
      (at (xyz 0 0 0))
      (scale (xyz -1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-20_5.3x7.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 146.685 81.28 180)
    (descr "20-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.75 180) (layer F.SilkS))
    (fp_text value PIC16F1829LIN (at 0 4.75 180) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /CMD_1))
    (pad 4 smd rect (at -3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 //MCLR))
    (pad 5 smd rect (at -3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /CMD_2))
    (pad 6 smd rect (at -3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /CMD_4))
    (pad 7 smd rect (at -3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /CMD_3))
    (pad 8 smd rect (at -3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /LBUS))
    (pad 10 smd rect (at -3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 11 smd rect (at 3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 12 smd rect (at 3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad12)"))
    (pad 14 smd rect (at 3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 /A3))
    (pad 15 smd rect (at 3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 /A2))
    (pad 16 smd rect (at 3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 /A1))
    (pad 17 smd rect (at 3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 /A0))
    (pad 18 smd rect (at 3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 /ICSPCLK))
    (pad 19 smd rect (at 3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /ICSPDAT))
    (pad 20 smd rect (at 3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SSOP.3dshapes/SSOP-20_5.3x7.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock (layer F.Cu) (tedit 5794C14F)
    (at 121.08 62.535 270)
    (descr "Sabre™ Right Angle Header, 43160-XX03, http://www.molex.com/pdm_docs/sd/431601102_sd.pdf")
    (tags "connector molex sabre 43160")
    (fp_text reference P1 (at -5 0 270) (layer F.SilkS))
    (fp_text value MOLEX-0431603103 (at 7.49 17.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 1 thru_hole rect (at 0 -3.18 270) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 2 thru_hole circle (at 7.49 0 270) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 8 /LBUS))
    (pad 2 thru_hole circle (at 7.49 -3.18 270) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 8 /LBUS))
    (pad 3 thru_hole circle (at 14.98 0 270) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 14.98 -3.18 270) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at -4.75 13.13 270) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 19.73 13.13 270) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (model ../../../../../home/cpriscal/Projets/lin_modules/lin_bluetooth_gateway/Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock (layer F.Cu) (tedit 5794C14F)
    (at 175.26 77.515 90)
    (descr "Sabre™ Right Angle Header, 43160-XX03, http://www.molex.com/pdm_docs/sd/431601102_sd.pdf")
    (tags "connector molex sabre 43160")
    (fp_text reference P2 (at -5 0 90) (layer F.SilkS))
    (fp_text value MOLEX-0431603103 (at 7.49 17.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 1 thru_hole rect (at 0 -3.18 90) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 2 thru_hole circle (at 7.49 0 90) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 8 /LBUS))
    (pad 2 thru_hole circle (at 7.49 -3.18 90) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 8 /LBUS))
    (pad 3 thru_hole circle (at 14.98 0 90) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 14.98 -3.18 90) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at -4.75 13.13 90) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 19.73 13.13 90) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (model /home/cpriscal/Projets/lin_modules/lin_bluetooth_gateway/Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier4 (layer F.Cu) (tedit 0)
    (at 139.065 57.785 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P4 (at 0 -3.175 180) (layer F.SilkS))
    (fp_text value TE-282836-4 (at 0 5.08 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 11 /OUT_3))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 12 /OUT_4))
    (model /home/cpriscal/Projets/lin_modules/common/3d/te-282836-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 131.445 73.025 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value LITEON-LTST-C170KGKT (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 161.925 72.898 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 3.175 -0.127 180) (layer F.SilkS))
    (fp_text value LITEON-LTST-C170KGKT (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 151.765 72.898 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at -3.175 -0.127 180) (layer F.SilkS))
    (fp_text value LITEON-LTST-C170KGKT (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 141.605 73.025 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D6 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value LITEON-LTST-C170KGKT (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier4 (layer F.Cu) (tedit 0)
    (at 159.385 57.785 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.175 180) (layer F.SilkS))
    (fp_text value TE-282836-4 (at 0 5.08 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 9 /OUT_1))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 13 /12V_UNPROTECTED))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 10 /OUT_2))
    (model /home/cpriscal/Projets/lin_modules/common/3d/te-282836-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Copal_CHS-04TB (layer F.Cu) (tedit 584490CC)
    (at 136.525 81.28 180)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference S1 (at 0 -4.191 180) (layer F.SilkS))
    (fp_text value DIP_SWITCH_4 (at 0 4.318 180) (layer F.Fab))
    (fp_text user N (at 2.032 -1.143 180) (layer F.Fab))
    (fp_text user O (at 2.032 -2.413 180) (layer F.Fab))
    (fp_text user 1 (at -1.905 -1.905 180) (layer F.Fab))
    (fp_text user 2 (at -1.905 -0.635 180) (layer F.Fab))
    (fp_text user 3 (at -1.905 0.635 180) (layer F.Fab))
    (fp_text user 4 (at -1.905 1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 /A0))
    (pad 3 smd rect (at -3.65 -0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 /A1))
    (pad 5 smd rect (at -3.65 0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 24 /A2))
    (pad 7 smd rect (at -3.65 1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 /A3))
    (pad 8 smd rect (at 3.65 1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.65 0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 3.65 -0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.65 -1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model /home/cpriscal/Projets/lin_modules/common/3d/copal-chs-04tb.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_Pad_Via (layer F.Cu) (tedit 5844A549)
    (at 107.315 52.07)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_Pad_Via (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (gr_text "2016 Cedric Priscal" (at 123.825 88.9) (layer F.SilkS))
  (gr_text GND (at 172.72 59.69 360) (layer F.SilkS))
  (gr_text LIN (at 172.72 67.31 360) (layer F.SilkS))
  (gr_text 12V (at 172.72 74.93 360) (layer F.SilkS))
  (gr_text A3 (at 130.175 79.375) (layer F.SilkS))
  (gr_text A0 (at 130.175 83.185) (layer F.SilkS))
  (gr_text 4 (at 133.985 50.8 180) (layer F.SilkS))
  (gr_text - (at 131.445 52.705 180) (layer F.SilkS))
  (gr_text + (at 136.525 52.705 180) (layer F.SilkS))
  (gr_text 3 (at 144.145 50.8 180) (layer F.SilkS))
  (gr_text - (at 141.605 52.705 180) (layer F.SilkS))
  (gr_text + (at 146.685 52.705 180) (layer F.SilkS))
  (gr_text 2 (at 154.305 50.8 180) (layer F.SilkS))
  (gr_text - (at 151.765 52.705 180) (layer F.SilkS))
  (gr_text + (at 156.845 52.705 180) (layer F.SilkS))
  (gr_text + (at 167.005 52.705 180) (layer F.SilkS))
  (gr_text - (at 161.925 52.705 180) (layer F.SilkS))
  (gr_text 1 (at 164.465 50.8 180) (layer F.SilkS))
  (gr_line (start 104.14 90.805) (end 104.14 48.895) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 90.805) (end 104.14 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 48.895) (end 191.77 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 48.895) (end 191.77 48.895) (layer Edge.Cuts) (width 0.15))
  (gr_text "4x13A switch rev 2" (at 169.545 88.9) (layer F.SilkS))
  (gr_text 12V (at 123.825 59.69) (layer F.SilkS))
  (gr_text LIN (at 123.825 67.31) (layer F.SilkS))
  (gr_text GND (at 123.825 74.93) (layer F.SilkS))
)
