(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 70)
    (zones 0)
    (modules 14)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad12)")
  (net 2 "Net-(J1-Pad11)")
  (net 3 "Net-(J1-Pad10)")
  (net 4 "Net-(J1-Pad9)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad1)")
  (net 13 "Net-(J2-Pad12)")
  (net 14 "Net-(J2-Pad11)")
  (net 15 "Net-(J2-Pad10)")
  (net 16 "Net-(J2-Pad9)")
  (net 17 "Net-(J2-Pad8)")
  (net 18 "Net-(J2-Pad7)")
  (net 19 "Net-(J2-Pad6)")
  (net 20 "Net-(J2-Pad5)")
  (net 21 "Net-(J2-Pad4)")
  (net 22 "Net-(J2-Pad3)")
  (net 23 "Net-(J2-Pad2)")
  (net 24 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module DMack_Custom_Footprints_Library:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 92.71 102.87)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module DMack_Custom_Footprints_Library:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 123.19 102.87)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module DMack_Custom_Footprints_Library:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 123.19 72.39)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module DMack_Custom_Footprints_Library:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 92.71 72.39)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module DMack_Custom_Footprints_Library:LargePushButton_W12mm_H12mm_P2.54mm (layer F.Cu) (tedit 621BD342)
    (at 110.49 125.73)
    (descr "large push buttons with color caps")
    (fp_text reference SW4 (at 6.35 2.54) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 1 thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 1 thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:LargePushButton_W12mm_H12mm_P2.54mm (layer F.Cu) (tedit 621BD342)
    (at 92.71 125.73)
    (descr "large push buttons with color caps")
    (fp_text reference SW3 (at 6.35 2.54) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 1 thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 1 thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:LargePushButton_W12mm_H12mm_P2.54mm (layer F.Cu) (tedit 621BD342)
    (at 110.49 110.49)
    (descr "large push buttons with color caps")
    (fp_text reference SW2 (at 6.35 2.54) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad5)"))
    (pad 1 thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad5)"))
    (pad 1 thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:LargePushButton_W12mm_H12mm_P2.54mm (layer F.Cu) (tedit 621BD342)
    (at 92.71 110.49)
    (descr "large push buttons with color caps")
    (fp_text reference SW1 (at 6.35 2.54) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad6)"))
    (pad 1 thru_hole oval (at 0 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad6)"))
    (pad 1 thru_hole oval (at 12.5 0) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:Resistor_L6.3mm_D2.5mm_P7.62mm_Horizontal_Axial (layer F.Cu) (tedit 621BD393)
    (at 121.92 96.52 90)
    (descr "standard resistor")
    (fp_text reference 10K (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:Resistor_L6.3mm_D2.5mm_P7.62mm_Horizontal_Axial (layer F.Cu) (tedit 621BD393)
    (at 121.92 85.09 90)
    (descr "standard resistor")
    (fp_text reference 10K (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:Resistor_L6.3mm_D2.5mm_P7.62mm_Horizontal_Axial (layer F.Cu) (tedit 621BD393)
    (at 93.98 96.52 90)
    (descr "standard resistor")
    (fp_text reference 10K (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:Resistor_L6.3mm_D2.5mm_P7.62mm_Horizontal_Axial (layer F.Cu) (tedit 621BD393)
    (at 93.98 85.09 90)
    (descr "standard resistor")
    (fp_text reference 10K (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:FemaleHeader_1x12_P2.54mm (layer F.Cu) (tedit 621BD2ED)
    (at 116.84 100.33 180)
    (descr "12-pin female header")
    (fp_text reference J2 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value "Photon 12-pin Header" (at 0 30.71) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMack_Custom_Footprints_Library:FemaleHeader_1x12_P2.54mm (layer F.Cu) (tedit 621BD2ED)
    (at 99.06 72.39)
    (descr "12-pin female header")
    (fp_text reference J1 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value "Photon 12-pin Header" (at 0 30.71) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "DMack, Mar 2022" (at 107.95 120.65) (layer B.SilkS))
  (gr_text "version 01" (at 107.95 83.82) (layer B.SilkS))
  (gr_text "Keyboard\nEmulator" (at 107.95 78.74) (layer B.SilkS))
  (gr_text PHOTON (at 106.68 87.63 90) (layer F.SilkS))
  (gr_text D0 (at 114.3 100.33) (layer F.SilkS))
  (gr_text D1 (at 114.3 97.79) (layer F.SilkS))
  (gr_text D2 (at 114.3 95.25) (layer F.SilkS))
  (gr_text D3 (at 114.3 92.71) (layer F.SilkS))
  (gr_text D4 (at 114.3 90.17) (layer F.SilkS))
  (gr_text D5 (at 114.3 87.63) (layer F.SilkS))
  (gr_text D6 (at 114.3 85.09) (layer F.SilkS))
  (gr_text D7 (at 114.3 82.55) (layer F.SilkS))
  (gr_text GND (at 114.3 80.01) (layer F.SilkS))
  (gr_text VBAT (at 114.3 77.47) (layer F.SilkS))
  (gr_text RST (at 114.3 74.93) (layer F.SilkS))
  (gr_text 3V3 (at 114.3 72.39) (layer F.SilkS))
  (gr_line (start 127 68.58) (end 88.9 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 135.89) (end 127 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 135.89) (end 127 135.89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 68.58) (end 88.9 135.89) (layer Edge.Cuts) (width 0.05))
)
