(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 496)
    (no_connects 2)
    (area 22.890479 27.985719 206.108301 189.542421)
    (thickness 1.6002)
    (drawings 39)
    (tracks 1195)
    (zones 0)
    (modules 65)
    (nets 66)
  )
  (page A4)
  (layers
    (0 Front signal hide)
    (31 Back signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.6)
    (user_trace_width 0.03302)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (trace_clearance 0.3048)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.0254)
    (segment_width 0.3048)
    (edge_width 0.381)
    (via_size 0.6096)
    (via_drill 0.508)
    (via_min_size 0.4064)
    (via_min_drill 0.2032)
    (user_via 0.6096 0.3048)
    (user_via 0.8128 0.508)
    (user_via 1.27 0.762)
    (user_via 1.651 0.9906)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.6096)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 6.3754 6.3754)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2032)
    (aux_axis_origin 0 0)
    (grid_origin 77.47 50.8)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 100)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /COL0)
  (net 2 /COL1)
  (net 3 /COL10)
  (net 4 /COL11)
  (net 5 /COL4)
  (net 6 /COL5)
  (net 7 /COL6)
  (net 8 /LED_A)
  (net 9 /LED_B)
  (net 10 /LED_C)
  (net 11 /ROW0)
  (net 12 /ROW1)
  (net 13 /ROW2)
  (net 14 /ROW3)
  (net 15 /ROW4)
  (net 16 /ROW5)
  (net 17 /SCLM)
  (net 18 /SDAM)
  (net 19 GND)
  (net 20 N-000001)
  (net 21 N-000003)
  (net 22 N-000011)
  (net 23 N-000012)
  (net 24 N-000013)
  (net 25 N-000015)
  (net 26 N-000016)
  (net 27 N-000017)
  (net 28 N-000018)
  (net 29 N-000026)
  (net 30 N-000027)
  (net 31 N-000030)
  (net 32 N-000033)
  (net 33 N-000034)
  (net 34 N-000035)
  (net 35 N-000036)
  (net 36 N-000037)
  (net 37 N-000038)
  (net 38 N-000039)
  (net 39 N-000040)
  (net 40 N-000041)
  (net 41 N-000042)
  (net 42 N-000043)
  (net 43 N-000044)
  (net 44 N-000045)
  (net 45 N-000046)
  (net 46 N-000047)
  (net 47 N-000048)
  (net 48 N-000049)
  (net 49 N-000050)
  (net 50 N-000051)
  (net 51 N-000052)
  (net 52 N-000055)
  (net 53 N-000056)
  (net 54 N-000057)
  (net 55 N-000058)
  (net 56 N-000059)
  (net 57 N-000060)
  (net 58 N-000063)
  (net 59 N-000064)
  (net 60 N-000065)
  (net 61 N-000067)
  (net 62 N-000068)
  (net 63 N-000069)
  (net 64 N-000072)
  (net 65 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.3048)
    (trace_width 0.6)
    (via_dia 0.6096)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /COL0)
    (add_net /COL1)
    (add_net /COL10)
    (add_net /COL11)
    (add_net /COL4)
    (add_net /COL5)
    (add_net /COL6)
    (add_net /LED_A)
    (add_net /LED_B)
    (add_net /LED_C)
    (add_net /ROW0)
    (add_net /ROW1)
    (add_net /ROW2)
    (add_net /ROW3)
    (add_net /ROW4)
    (add_net /ROW5)
    (add_net /SCLM)
    (add_net /SDAM)
    (add_net GND)
    (add_net N-000001)
    (add_net N-000003)
    (add_net N-000011)
    (add_net N-000012)
    (add_net N-000013)
    (add_net N-000015)
    (add_net N-000016)
    (add_net N-000017)
    (add_net N-000018)
    (add_net N-000026)
    (add_net N-000027)
    (add_net N-000030)
    (add_net N-000033)
    (add_net N-000034)
    (add_net N-000035)
    (add_net N-000036)
    (add_net N-000037)
    (add_net N-000038)
    (add_net N-000039)
    (add_net N-000040)
    (add_net N-000041)
    (add_net N-000042)
    (add_net N-000043)
    (add_net N-000044)
    (add_net N-000045)
    (add_net N-000046)
    (add_net N-000047)
    (add_net N-000048)
    (add_net N-000049)
    (add_net N-000050)
    (add_net N-000051)
    (add_net N-000052)
    (add_net N-000055)
    (add_net N-000056)
    (add_net N-000057)
    (add_net N-000058)
    (add_net N-000059)
    (add_net N-000060)
    (add_net N-000063)
    (add_net N-000064)
    (add_net N-000065)
    (add_net N-000067)
    (add_net N-000068)
    (add_net N-000069)
    (add_net N-000072)
    (add_net VCC)
  )
  (module "ErgoDOX pcb:STAR" (layer Front) (tedit 582CF5BC)
    (at 94.9325 142.5575)
    (fp_text reference STAR_1 (at 0 5) (layer F.SilkS) hide)
    (fp_text value STAR_FRONT (at 0 3) (layer F.SilkS) hide)
    (pad 0 smd circle (at 2.8448 0) (size 1.27 1.27) (layers Front))
    (pad 0 smd circle (at 1.4224 2.46126) (size 1.27 1.27) (layers Front))
    (pad 0 smd circle (at -1.41986 2.46126) (size 1.27 1.27) (layers Front))
    (pad 0 smd circle (at -2.8448 0) (size 1.27 1.27) (layers Front))
    (pad 0 smd circle (at -1.4224 -2.46126) (size 1.27 1.27) (layers Front))
    (pad 0 smd circle (at 1.41986 -2.46126) (size 1.27 1.27) (layers Front))
    (pad 1 smd circle (at 5.08 1.75768) (size 0.508 0.508) (layers Front))
    (pad 1 smd circle (at 1.016 5.27812) (size 0.508 0.508) (layers Front))
    (pad 1 smd circle (at -4.06146 3.5179) (size 0.508 0.508) (layers Front))
    (pad 1 smd circle (at -5.08 -1.75768) (size 0.508 0.508) (layers Front))
    (pad 1 smd circle (at -1.016 -5.27812) (size 0.508 0.508) (layers Front))
    (pad 1 smd circle (at 4.06146 -3.5179) (size 0.508 0.508) (layers Front))
    (pad 2 smd circle (at 4.064 3.5179) (size 0.508 0.508) (layers Front))
    (pad 2 smd circle (at -1.01346 5.27812) (size 0.508 0.508) (layers Front))
    (pad 2 smd circle (at -5.08 1.75768) (size 0.508 0.508) (layers Front))
    (pad 2 smd circle (at -4.064 -3.5179) (size 0.508 0.508) (layers Front))
    (pad 2 smd circle (at 1.01346 -5.27812) (size 0.508 0.508) (layers Front))
    (pad 2 smd circle (at 5.07746 -1.75768) (size 0.508 0.508) (layers Front))
    (pad 3 smd circle (at 7.112 1.75768) (size 0.3048 0.3048) (layers Front))
    (pad 3 smd circle (at 2.032 7.03834) (size 0.3048 0.3048) (layers Front))
    (pad 3 smd circle (at -5.07746 5.27812) (size 0.3048 0.3048) (layers Front))
    (pad 3 smd circle (at -7.112 -1.75768) (size 0.3048 0.3048) (layers Front))
    (pad 3 smd circle (at -2.032 -7.03834) (size 0.3048 0.3048) (layers Front))
    (pad 3 smd circle (at 5.07746 -5.27812) (size 0.3048 0.3048) (layers Front))
    (pad 4 smd circle (at 5.08 5.27812) (size 0.3048 0.3048) (layers Front))
    (pad 4 smd circle (at -2.02946 7.03834) (size 0.3048 0.3048) (layers Front))
    (pad 4 smd circle (at -7.112 1.75768) (size 0.3048 0.3048) (layers Front))
    (pad 4 smd circle (at -5.08 -5.27812) (size 0.3048 0.3048) (layers Front))
    (pad 4 smd circle (at 2.02946 -7.03834) (size 0.3048 0.3048) (layers Front))
    (pad 4 smd circle (at 7.10946 -1.75768) (size 0.3048 0.3048) (layers Front))
    (pad 5 smd circle (at 8.128 3.5179) (size 0.2032 0.2032) (layers Front))
    (pad 5 smd circle (at 1.016 8.79856) (size 0.2032 0.2032) (layers Front))
    (pad 5 smd circle (at -7.10946 5.27812) (size 0.2032 0.2032) (layers Front))
    (pad 5 smd circle (at -8.128 -3.5179) (size 0.2032 0.2032) (layers Front))
    (pad 5 smd circle (at -1.016 -8.79856) (size 0.2032 0.2032) (layers Front))
    (pad 5 smd circle (at 7.10946 -5.27812) (size 0.2032 0.2032) (layers Front))
    (pad 6 smd circle (at 7.112 5.27812) (size 0.2032 0.2032) (layers Front))
    (pad 6 smd circle (at -1.01346 8.79856) (size 0.2032 0.2032) (layers Front))
    (pad 6 smd circle (at -8.128 3.5179) (size 0.2032 0.2032) (layers Front))
    (pad 6 smd circle (at -7.112 -5.27812) (size 0.2032 0.2032) (layers Front))
    (pad 6 smd circle (at 1.01346 -8.79856) (size 0.2032 0.2032) (layers Front))
    (pad 6 smd circle (at 8.128 -3.5179) (size 0.2032 0.2032) (layers Front))
  )
  (module "ErgoDOX pcb:STAR" (layer Back) (tedit 582CF58F)
    (at 94.9325 142.5575 180)
    (fp_text reference STAR_2 (at 0 5 180) (layer B.SilkS) hide)
    (fp_text value STAR_BACK (at 0 3 180) (layer B.SilkS) hide)
    (pad 0 smd circle (at 2.8448 0 180) (size 1.27 1.27) (layers Back))
    (pad 0 smd circle (at 1.4224 -2.46126 180) (size 1.27 1.27) (layers Back))
    (pad 0 smd circle (at -1.41986 -2.46126 180) (size 1.27 1.27) (layers Back))
    (pad 0 smd circle (at -2.8448 0 180) (size 1.27 1.27) (layers Back))
    (pad 0 smd circle (at -1.4224 2.46126 180) (size 1.27 1.27) (layers Back))
    (pad 0 smd circle (at 1.41986 2.46126 180) (size 1.27 1.27) (layers Back))
    (pad 1 smd circle (at 5.08 -1.75768 180) (size 0.508 0.508) (layers Back))
    (pad 1 smd circle (at 1.016 -5.27812 180) (size 0.508 0.508) (layers Back))
    (pad 1 smd circle (at -4.06146 -3.5179 180) (size 0.508 0.508) (layers Back))
    (pad 1 smd circle (at -5.08 1.75768 180) (size 0.508 0.508) (layers Back))
    (pad 1 smd circle (at -1.016 5.27812 180) (size 0.508 0.508) (layers Back))
    (pad 1 smd circle (at 4.06146 3.5179 180) (size 0.508 0.508) (layers Back))
    (pad 2 smd circle (at 4.064 -3.5179 180) (size 0.508 0.508) (layers Back))
    (pad 2 smd circle (at -1.01346 -5.27812 180) (size 0.508 0.508) (layers Back))
    (pad 2 smd circle (at -5.08 -1.75768 180) (size 0.508 0.508) (layers Back))
    (pad 2 smd circle (at -4.064 3.5179 180) (size 0.508 0.508) (layers Back))
    (pad 2 smd circle (at 1.01346 5.27812 180) (size 0.508 0.508) (layers Back))
    (pad 2 smd circle (at 5.07746 1.75768 180) (size 0.508 0.508) (layers Back))
    (pad 3 smd circle (at 7.112 -1.75768 180) (size 0.3048 0.3048) (layers Back))
    (pad 3 smd circle (at 2.032 -7.03834 180) (size 0.3048 0.3048) (layers Back))
    (pad 3 smd circle (at -5.07746 -5.27812 180) (size 0.3048 0.3048) (layers Back))
    (pad 3 smd circle (at -7.112 1.75768 180) (size 0.3048 0.3048) (layers Back))
    (pad 3 smd circle (at -2.032 7.03834 180) (size 0.3048 0.3048) (layers Back))
    (pad 3 smd circle (at 5.07746 5.27812 180) (size 0.3048 0.3048) (layers Back))
    (pad 4 smd circle (at 5.08 -5.27812 180) (size 0.3048 0.3048) (layers Back))
    (pad 4 smd circle (at -2.02946 -7.03834 180) (size 0.3048 0.3048) (layers Back))
    (pad 4 smd circle (at -7.112 -1.75768 180) (size 0.3048 0.3048) (layers Back))
    (pad 4 smd circle (at -5.08 5.27812 180) (size 0.3048 0.3048) (layers Back))
    (pad 4 smd circle (at 2.02946 7.03834 180) (size 0.3048 0.3048) (layers Back))
    (pad 4 smd circle (at 7.10946 1.75768 180) (size 0.3048 0.3048) (layers Back))
    (pad 5 smd circle (at 8.128 -3.5179 180) (size 0.2032 0.2032) (layers Back))
    (pad 5 smd circle (at 1.016 -8.79856 180) (size 0.2032 0.2032) (layers Back))
    (pad 5 smd circle (at -7.10946 -5.27812 180) (size 0.2032 0.2032) (layers Back))
    (pad 5 smd circle (at -8.128 3.5179 180) (size 0.2032 0.2032) (layers Back))
    (pad 5 smd circle (at -1.016 8.79856 180) (size 0.2032 0.2032) (layers Back))
    (pad 5 smd circle (at 7.10946 5.27812 180) (size 0.2032 0.2032) (layers Back))
    (pad 6 smd circle (at 7.112 -5.27812 180) (size 0.2032 0.2032) (layers Back))
    (pad 6 smd circle (at -1.01346 -8.79856 180) (size 0.2032 0.2032) (layers Back))
    (pad 6 smd circle (at -8.128 -3.5179 180) (size 0.2032 0.2032) (layers Back))
    (pad 6 smd circle (at -7.112 5.27812 180) (size 0.2032 0.2032) (layers Back))
    (pad 6 smd circle (at 1.01346 8.79856 180) (size 0.2032 0.2032) (layers Back))
    (pad 6 smd circle (at 8.128 3.5179 180) (size 0.2032 0.2032) (layers Back))
  )
  (module DIP28_300 (layer Back) (tedit 5114C046)
    (at 178.435 41.275)
    (fp_text reference U2 (at 0 0) (layer B.SilkS) hide)
    (fp_text value MCP23018 (at 0 0) (layer B.SilkS))
    (pad 2 thru_hole circle (at -13.97 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 3 thru_hole circle (at -11.43 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 16 /ROW5))
    (pad 4 thru_hole circle (at -8.89 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 15 /ROW4))
    (pad 5 thru_hole circle (at -6.35 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 14 /ROW3))
    (pad 6 thru_hole circle (at -3.81 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 13 /ROW2))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ROW1))
    (pad 8 thru_hole circle (at 1.27 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ROW0))
    (pad 9 thru_hole circle (at 3.81 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 11 thru_hole circle (at 8.89 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 65 VCC))
    (pad 12 thru_hole circle (at 11.43 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 17 /SCLM))
    (pad 13 thru_hole circle (at 13.97 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 18 /SDAM))
    (pad 14 thru_hole circle (at 16.51 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -16.51 -3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
    (pad 15 thru_hole circle (at 16.51 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
    (pad 16 thru_hole circle (at 13.97 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 65 VCC))
    (pad 17 np_thru_hole circle (at 11.43 3.81) (size 1.0922 1.0922) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 18 np_thru_hole circle (at 8.89 3.81) (size 1.0922 1.0922) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 19 np_thru_hole circle (at 6.35 3.81) (size 1.0922 1.0922) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 20 thru_hole circle (at 3.81 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 1 /COL0))
    (pad 21 thru_hole circle (at 1.27 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 2 /COL1))
    (pad 22 thru_hole circle (at -1.27 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 4 /COL11))
    (pad 23 thru_hole circle (at -3.81 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 3 /COL10))
    (pad 24 thru_hole circle (at -6.35 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 5 /COL4))
    (pad 25 thru_hole circle (at -8.89 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 6 /COL5))
    (pad 26 thru_hole circle (at -11.43 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 7 /COL6))
    (pad 27 thru_hole circle (at -13.97 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 28 thru_hole circle (at -16.51 3.81) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  )
  (module DIODE (layer Front) (tedit 4E0F7A99)
    (at 56.7944 145.57756 25)
    (fp_text reference D1:7 (at 0 0 25) (layer F.SilkS) hide)
    (fp_text value D (at 0 0 25) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 31 N-000030))
    (pad 99 smd rect (at -1.6637 0 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 0 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 2 thru_hole rect (at 3.81 0 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 7 /COL6))
    (pad 99 smd rect (at 1.6637 0 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 0 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module DIODE (layer Front) (tedit 4E0F7A99)
    (at 74.05878 137.52576 25)
    (fp_text reference D1:8 (at 0 0 25) (layer F.SilkS) hide)
    (fp_text value D (at 0 0 25) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 25 N-000015))
    (pad 99 smd rect (at -1.6637 0 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 0 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 2 thru_hole rect (at 3.81 0 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 6 /COL5))
    (pad 99 smd rect (at 1.6637 0 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 0 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module MX_LED (layer Front) (tedit 4EC3E7B7)
    (at 72.39 117.48516 90)
    (fp_text reference LED_C1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LEDc (at 0 10.16 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 61 N-000067))
    (pad 2 thru_hole rect (at 1.27 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
  )
  (module MX_LED (layer Front) (tedit 4EC3E7B7)
    (at 72.39 88.91016 90)
    (fp_text reference LED_B1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LEDb (at 0 10.16 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 62 N-000068))
    (pad 2 thru_hole rect (at 1.27 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
  )
  (module MX_LED (layer Front) (tedit 4EC3E7B7)
    (at 72.39 65.1002)
    (fp_text reference LED_A1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LEDa (at 0 10.16) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 63 N-000069))
    (pad 2 thru_hole rect (at 1.27 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
  )
  (module USBMINImod (layer Front) (tedit 4FDC5756)
    (at 137.6426 30.48 270)
    (fp_text reference J1 (at 0 0 360) (layer F.SilkS) hide)
    (fp_text value USB (at 2.54 0 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 6.79958 -1.6002 270) (size 1.651 1.143) (drill 0.762 (offset 0.27432 0)) (layers *.Cu *.Mask F.SilkS)
      (net 65 VCC))
    (pad 2 thru_hole oval (at 5.6007 -0.8001 270) (size 1.651 1.143) (drill 0.762 (offset -0.27432 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 6.79958 0 270) (size 1.651 1.143) (drill 0.762 (offset 0.27432 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 5.6007 0.8001 270) (size 1.651 1.143) (drill 0.762 (offset -0.27432 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 6.79958 1.6002 270) (size 1.651 1.143) (drill 0.762 (offset 0.27432 0)) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
    (pad 6 thru_hole oval (at 1.75006 3.64744 270) (size 2.794 1.7018) (drill oval 1.905 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
    (pad 6 thru_hole oval (at 1.75006 -3.64744 270) (size 2.794 1.7018) (drill oval 1.905 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
    (pad 1 thru_hole circle (at 9.779 -2.413 270) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 65 VCC))
    (pad 2 thru_hole circle (at 3.937 -5.715 270) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 9.779 0 270) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 3.937 5.715 270) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 9.779 2.413 270) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
  )
  (module MX_FLIP (layer Front) (tedit 4FD81CDD)
    (at 77.2795 144.43202 25)
    (fp_text reference SX1:8 (at 0 3.302 25) (layer F.SilkS))
    (fp_text value SX1:5 (at 0 3.302 25) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 25 N-000015))
    (pad 0 np_thru_hole circle (at 0 0 25) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 25 N-000015))
  )
  (module MX_FLIP (layer Front) (tedit 4FD81CDD)
    (at 60.01512 152.48382 25)
    (fp_text reference SX1:7 (at 0 3.302 25) (layer F.SilkS))
    (fp_text value SX1:6 (at 0 3.302 25) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 31 N-000030))
    (pad 0 np_thru_hole circle (at 0 0 25) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 31 N-000030))
  )
  (module MX_FLIP (layer Front) (tedit 4FD81CDD)
    (at 85.3313 161.69894 205)
    (fp_text reference SX0:10 (at 0 3.302 205) (layer F.SilkS))
    (fp_text value SX0:3 (at 0 3.302 205) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 30 N-000027))
    (pad 0 np_thru_hole circle (at 0 0 205) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 205) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 205) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 30 N-000027))
  )
  (module MX_FLIP (layer Front) (tedit 4FD81CDD)
    (at 68.06438 169.7482 205)
    (fp_text reference SX0:11 (at 0 3.302 205) (layer F.SilkS))
    (fp_text value SX0:2 (at 0 3.302 205) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 64 N-000072))
    (pad 0 np_thru_hole circle (at 0 0 205) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 205) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 205) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 205) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 64 N-000072))
  )
  (module RESISTOR (layer Front) (tedit 4E0F7A99)
    (at 148.9075 45.4025 225)
    (fp_text reference RA1 (at 0 0 225) (layer F.SilkS) hide)
    (fp_text value LEDa (at 0 0 225) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 225) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 8 /LED_A))
    (pad 2 thru_hole circle (at 5.08 0 225) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 63 N-000069))
  )
  (module RESISTOR (layer Front) (tedit 4E0F7A99)
    (at 147.0025 43.4975 225)
    (fp_text reference RB1 (at 0 0 225) (layer F.SilkS) hide)
    (fp_text value LEDb (at 0 0 225) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 225) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 9 /LED_B))
    (pad 2 thru_hole circle (at 5.08 0 225) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 62 N-000068))
  )
  (module RESISTOR (layer Front) (tedit 4E0F7A99)
    (at 125.4125 46.99 180)
    (fp_text reference RC1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value LEDc (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 10 /LED_C))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 61 N-000067))
  )
  (module RESISTOR (layer Front) (tedit 4E0F7A99)
    (at 105.41 40.3225 315)
    (fp_text reference R1 (at 0 0 315) (layer F.SilkS) hide)
    (fp_text value 2.2kΩ (at 0 0 315) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 315) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 65 VCC))
    (pad 2 thru_hole circle (at 5.08 0 315) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 18 /SDAM))
  )
  (module RESISTOR (layer Front) (tedit 4E0F7A99)
    (at 102.235 41.5925 315)
    (fp_text reference R2 (at 0 0 315) (layer F.SilkS) hide)
    (fp_text value 2.2kΩ (at 0 0 315) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 315) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 65 VCC))
    (pad 2 thru_hole circle (at 5.08 0 315) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 17 /SCLM))
  )
  (module 100PITCH1X3 (layer Front) (tedit 4F8E9504)
    (at 78.74 37.465 90)
    (fp_text reference J4 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value JMP (at 0 3.048 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 65 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 20 N-000001))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
  )
  (module 100PITCH1X3 (layer Back) (tedit 4F8E9504)
    (at 93.98 37.465 90)
    (fp_text reference J3 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value JMP (at 0 -3.048 90) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask B.SilkS)
      (net 65 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask B.SilkS)
      (net 21 N-000003))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask B.SilkS)
      (net 19 GND))
  )
  (module TEENSY_2.0 (layer Front) (tedit 501A4641)
    (at 175.895 42.545)
    (fp_text reference U1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TEENSY2.0 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -13.97 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND))
    (pad 2 thru_hole circle (at -11.43 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 7 /COL6))
    (pad 3 thru_hole circle (at -8.89 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 6 /COL5))
    (pad 4 thru_hole circle (at -6.35 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 5 /COL4))
    (pad 5 thru_hole circle (at -3.81 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 3 /COL10))
    (pad 6 thru_hole circle (at -1.27 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 10 /LED_C))
    (pad 7 thru_hole circle (at 1.27 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 17 /SCLM))
    (pad 8 thru_hole circle (at 3.81 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 18 /SDAM))
    (pad 9 thru_hole circle (at 6.35 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 4 /COL11))
    (pad 10 thru_hole circle (at 8.89 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 2 /COL1))
    (pad 11 thru_hole circle (at 11.43 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 1 /COL0))
    (pad 12 thru_hole circle (at 13.97 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 18 thru_hole circle (at 13.97 -7.62) (size 1.7526 1.7526) (drill 1.08966) (layers *.Cu *.SilkS *.Mask)
      (net 19 GND) (zone_connect 0))
    (pad 19 thru_hole circle (at 11.43 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
    (pad 20 thru_hole circle (at 8.89 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 65 VCC))
    (pad 21 thru_hole circle (at 6.35 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 8 /LED_A))
    (pad 22 thru_hole circle (at 3.81 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 9 /LED_B))
    (pad 23 thru_hole circle (at 1.27 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ROW0))
    (pad 24 thru_hole circle (at -1.27 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ROW1))
    (pad 27 thru_hole circle (at -8.89 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 15 /ROW4))
    (pad 28 thru_hole circle (at -11.43 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 16 /ROW5))
    (pad 29 thru_hole circle (at -13.97 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 65 VCC))
    (pad 25 thru_hole circle (at -3.81 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 13 /ROW2))
    (pad 26 thru_hole circle (at -6.35 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 14 /ROW3))
  )
  (module GAP (layer Back) (tedit 501A4626)
    (at 192.7225 34.925 270)
    (fp_text reference JP2 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value JUMPER (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0 0.635 270) (size 2.032 1.016) (layers Back B.Paste B.Mask)
      (net 19 GND) (zone_connect 0))
    (pad 1 smd rect (at 0 -0.635 270) (size 2.032 1.016) (layers Back B.Paste B.Mask)
      (net 19 GND))
  )
  (module GAP (layer Front) (tedit 500D0F18)
    (at 187.325 40.9575)
    (fp_text reference JP1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -0.635) (size 2.032 1.016) (layers Front F.Paste F.Mask)
      (net 65 VCC))
    (pad 1 smd rect (at 0 0.635) (size 2.032 1.016) (layers Front F.Paste F.Mask)
      (net 65 VCC))
  )
  (module 4pin35mmAudio (layer Front) (tedit 4FD999CA)
    (at 86.3092 30.48 270)
    (fp_text reference J2 (at 1.27 0 360) (layer F.SilkS) hide)
    (fp_text value 3.5mm (at 5.715 0 360) (layer F.SilkS))
    (fp_text user 3.5mm (at 5.715 0 360) (layer B.SilkS))
    (pad 1 thru_hole oval (at 2.8956 -4.6482 270) (size 1.7526 2.0574) (drill oval 1.0922 1.397) (layers *.Cu *.Mask F.SilkS)
      (net 21 N-000003))
    (pad 2 thru_hole circle (at 7.8994 3.6068 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.Mask F.SilkS)
      (net 18 /SDAM))
    (pad 3 thru_hole circle (at 10.9982 -1.6002 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SCLM))
    (pad 4 thru_hole oval (at 2.8956 4.6482 270) (size 1.7526 2.0574) (drill oval 1.0922 1.397) (layers *.Cu *.Mask F.SilkS)
      (net 20 N-000001))
    (pad 5 thru_hole circle (at 10.9982 1.6002 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SCLM))
    (pad 6 thru_hole circle (at 7.8994 -3.6068 270) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.Mask F.SilkS)
      (net 18 /SDAM))
    (pad HOLE np_thru_hole circle (at 2.8956 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad HOLE np_thru_hole circle (at 7.8994 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module STAB_PCB940 (layer Front) (tedit 4D9C8C49)
    (at 81.30286 153.06548 295)
    (solder_mask_margin -0.254)
    (zone_connect 2)
    (fp_text reference S2 (at 0 0 295) (layer B.SilkS) hide)
    (fp_text value STAB200 (at 0 0 295) (layer B.SilkS) hide)
    (pad 0 np_thru_hole circle (at -11.938 6.985 295) (size 3.048 3.048) (drill 3.048) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 11.938 6.985 295) (size 3.048 3.048) (drill 3.048) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
    (pad 0 np_thru_hole circle (at -11.938 -8.255 295) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 11.938 -8.255 295) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
  )
  (module STAB_PCB940 (layer Front) (tedit 4D9C8C49)
    (at 64.03848 161.11728 115)
    (solder_mask_margin -0.254)
    (zone_connect 2)
    (fp_text reference S1 (at 0 0 115) (layer B.SilkS) hide)
    (fp_text value STAB200 (at 0 0 115) (layer B.SilkS) hide)
    (pad 0 np_thru_hole circle (at -11.938 6.985 115) (size 3.048 3.048) (drill 3.048) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 11.938 6.985 115) (size 3.048 3.048) (drill 3.048) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
    (pad 0 np_thru_hole circle (at -11.938 -8.255 115) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 11.938 -8.255 115) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu)
      (net 19 GND) (zone_connect 2))
  )
  (module ErgoDOXmech (layer Front) (tedit 4FDC5756)
    (at 50.8 177.8)
    (fp_text reference H99 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value MECHANICAL (at 0 0 90) (layer F.SilkS) hide)
    (pad 0 np_thru_hole circle (at 3.0988 -11.9634) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 8.8646 -56.134) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 54.6354 -20.0406) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 150.9776 -37.7444) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 88.2396 -86.2076) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 150.3426 -140.6652) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 67.4116 -140.6652) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
    (pad 0 np_thru_hole circle (at 16.6116 -140.6652) (size 6.3754 6.3754) (drill 6.3754) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND) (solder_mask_margin -0.254) (zone_connect 2))
  )
  (module "ErgoDOX pcb:MX_FLIP_XX" (layer Front) (tedit 582D0414)
    (at 191.4525 86.05266)
    (fp_text reference SW4:13 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW4:0 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 47 N-000048))
    (pad "" thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.28346 2.28346) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 47 N-000048))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 47 N-000048))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 47 N-000048))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 1 thru_hole circle (at -9.8425 -2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 1 thru_hole circle (at -7.3025 -3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -7.3025 3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 47 N-000048))
    (pad 2 thru_hole circle (at -9.8425 2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 47 N-000048))
    (pad 2 thru_hole oval (at -2.38252 0) (size 8.7503 3.9878) (drill oval 8.7503 3.9878) (layers *.Cu *.Mask)
      (net 47 N-000048) (zone_connect 2))
    (pad 3 thru_hole circle (at -4.7625 5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 47 N-000048) (zone_connect 2))
    (pad 2 thru_hole circle (at -4.7625 -5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 47 N-000048) (zone_connect 2))
  )
  (module "ErgoDOX pcb:MX_FLIP_XX" locked (layer Front) (tedit 582D0414)
    (at 191.4525 124.15266)
    (fp_text reference SW2:13 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW2:0 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 46 N-000047))
    (pad "" thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.28346 2.28346) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 46 N-000047))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 46 N-000047))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 46 N-000047))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 1 thru_hole circle (at -9.8425 -2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 1 thru_hole circle (at -7.3025 -3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -7.3025 3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 46 N-000047))
    (pad 2 thru_hole circle (at -9.8425 2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 46 N-000047))
    (pad 2 thru_hole oval (at -2.38252 0) (size 8.7503 3.9878) (drill oval 8.7503 3.9878) (layers *.Cu *.Mask)
      (net 46 N-000047) (zone_connect 2))
    (pad 3 thru_hole circle (at -4.7625 5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 46 N-000047) (zone_connect 2))
    (pad 2 thru_hole circle (at -4.7625 -5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 46 N-000047) (zone_connect 2))
  )
  (module "ErgoDOX pcb:MX_FLIP_XX" locked (layer Front) (tedit 582D0414)
    (at 191.4525 67.0052)
    (fp_text reference SW5:13 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:0 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 42 N-000043))
    (pad "" thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.28346 2.28346) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 42 N-000043))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 42 N-000043))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 42 N-000043))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 1 thru_hole circle (at -9.8425 -2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 1 thru_hole circle (at -7.3025 -3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -7.3025 3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 42 N-000043))
    (pad 2 thru_hole circle (at -9.8425 2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 42 N-000043))
    (pad 2 thru_hole oval (at -2.38252 0) (size 8.7503 3.9878) (drill oval 8.7503 3.9878) (layers *.Cu *.Mask)
      (net 42 N-000043) (zone_connect 2))
    (pad 3 thru_hole circle (at -4.7625 5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 42 N-000043) (zone_connect 2))
    (pad 2 thru_hole circle (at -4.7625 -5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 42 N-000043) (zone_connect 2))
  )
  (module "ErgoDOX pcb:MX_FLIP_XX" locked (layer Front) (tedit 582D0414)
    (at 191.4525 105.10266)
    (fp_text reference SW3:13 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW3:0 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 48 N-000049))
    (pad "" thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.28346 2.28346) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 48 N-000049))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 48 N-000049))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 48 N-000049))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 1 thru_hole circle (at -9.8425 -2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 1 thru_hole circle (at -7.3025 -3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -7.3025 3.81) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 48 N-000049))
    (pad 2 thru_hole circle (at -9.8425 2.54) (size 2.28092 2.28092) (drill 1.4986) (layers *.Cu *.Mask)
      (net 48 N-000049))
    (pad 2 thru_hole oval (at -2.38252 0) (size 8.7503 3.9878) (drill oval 8.7503 3.9878) (layers *.Cu *.Mask)
      (net 48 N-000049) (zone_connect 2))
    (pad 3 thru_hole circle (at -4.7625 5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 48 N-000049) (zone_connect 2))
    (pad 2 thru_hole circle (at -4.7625 -5.08 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 48 N-000049) (zone_connect 2))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 91.44 65.1002)
    (fp_text reference SW5:8 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:5 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 23 N-000012))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 23 N-000012))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 N-000012))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 N-000012))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 148.59 82.87766)
    (fp_text reference SW4:11 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW4:2 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 44 N-000045))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 44 N-000045))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 44 N-000045))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 44 N-000045))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 64.03848 161.11728 115)
    (fp_text reference SW0:11 (at 0 3.302 115) (layer F.SilkS))
    (fp_text value SW0:2 (at 0 3.302 115) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 64 N-000072))
    (pad 0 thru_hole circle (at 0 0 115) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 115) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 115) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 64 N-000072))
    (pad 3 thru_hole circle (at -3.81 5.08 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 64 N-000072))
    (pad 4 thru_hole rect (at 3.81 5.08 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 3 thru_hole circle (at -3.81 7.62 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 64 N-000072))
    (pad 4 thru_hole rect (at 3.81 7.62 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 99 smd rect (at -1.6637 7.62 115) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 115) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 115) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 115) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 81.30286 153.06548 115)
    (fp_text reference SW0:10 (at 0 3.302 115) (layer F.SilkS))
    (fp_text value SW0:3 (at 0 3.302 115) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 30 N-000027))
    (pad 0 thru_hole circle (at 0 0 115) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 115) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 115) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 115) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 30 N-000027))
    (pad 3 thru_hole circle (at -3.81 5.08 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 30 N-000027))
    (pad 4 thru_hole rect (at 3.81 5.08 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 3 thru_hole circle (at -3.81 7.62 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 30 N-000027))
    (pad 4 thru_hole rect (at 3.81 7.62 115) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 99 smd rect (at -1.6637 7.62 115) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 115) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 115) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 115) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 110.49 140.02766)
    (fp_text reference SW1:9 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW1:4 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 29 N-000026))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 29 N-000026))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 29 N-000026))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 29 N-000026))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 129.54 138.43)
    (fp_text reference SW1:10 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW1:3 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 40 N-000041))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 40 N-000041))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 40 N-000041))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 40 N-000041))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 167.64 143.20266)
    (fp_text reference SW1:12 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW1:1 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 54 N-000057))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 54 N-000057))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 54 N-000057))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 54 N-000057))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 91.44 122.24766)
    (fp_text reference SW2:8 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW2:5 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 36 N-000037))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 36 N-000037))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 36 N-000037))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 36 N-000037))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 110.49 120.97766)
    (fp_text reference SW2:9 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW2:4 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 37 N-000038))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 37 N-000038))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 37 N-000038))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 37 N-000038))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 129.54 119.38)
    (fp_text reference SW2:10 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW2:3 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 32 N-000033))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 32 N-000033))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 32 N-000033))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 32 N-000033))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 148.59 120.97766)
    (fp_text reference SW2:11 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW2:2 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 38 N-000039))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 38 N-000039))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 38 N-000039))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 38 N-000039))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 167.64 124.15266)
    (fp_text reference SW2:12 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW2:1 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 41 N-000042))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 41 N-000042))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 41 N-000042))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 41 N-000042))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 91.44 103.19766)
    (fp_text reference SW3:8 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW3:5 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 34 N-000035))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 34 N-000035))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 34 N-000035))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 34 N-000035))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 110.49 101.92766)
    (fp_text reference SW3:9 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW3:4 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 33 N-000034))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 33 N-000034))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 33 N-000034))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 33 N-000034))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 129.54 100.33)
    (fp_text reference SW3:10 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW3:3 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 51 N-000052))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 51 N-000052))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 51 N-000052))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 51 N-000052))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 148.59 101.92766)
    (fp_text reference SW3:11 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW3:2 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 50 N-000051))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 50 N-000051))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 50 N-000051))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 50 N-000051))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 110.49 82.87766)
    (fp_text reference SW4:9 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW4:4 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 43 N-000044))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 43 N-000044))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 43 N-000044))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 43 N-000044))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 129.54 81.28)
    (fp_text reference SW4:10 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW4:3 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 60 N-000065))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 60 N-000065))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 60 N-000065))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 60 N-000065))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 167.64 86.05266)
    (fp_text reference SW4:12 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW4:1 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 45 N-000046))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 45 N-000046))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 45 N-000046))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 45 N-000046))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 148.59 140.02766)
    (fp_text reference SW1:11 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW1:2 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 39 N-000040))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 39 N-000040))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 39 N-000040))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 39 N-000040))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 110.49 63.82766)
    (fp_text reference SW5:9 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:4 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 26 N-000016))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 26 N-000016))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 N-000016))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 N-000016))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 129.54 62.23)
    (fp_text reference SW5:10 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:3 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 27 N-000017))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 27 N-000017))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 N-000017))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 N-000017))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 /COL10))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 148.59 63.82766)
    (fp_text reference SW5:11 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:2 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 28 N-000018))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 28 N-000018))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 N-000018))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 N-000018))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 /COL11))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 167.64 67.0052)
    (fp_text reference SW5:12 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:1 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 22 N-000011))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 22 N-000011))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 N-000011))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 N-000011))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 51.96332 135.21944 25)
    (fp_text reference SW0:8 (at 0 3.302 25) (layer F.SilkS))
    (fp_text value SW0:5 (at 0 3.302 25) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 52 N-000055))
    (pad 0 thru_hole circle (at 0 0 25) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 52 N-000055))
    (pad 3 thru_hole circle (at -3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 52 N-000055))
    (pad 4 thru_hole rect (at 3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 3 thru_hole circle (at -3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 52 N-000055))
    (pad 4 thru_hole rect (at 3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 34.69894 143.2687 25)
    (fp_text reference SW0:7 (at 0 3.302 25) (layer F.SilkS))
    (fp_text value SW0:6 (at 0 3.302 25) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 57 N-000060))
    (pad 0 thru_hole circle (at 0 0 25) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 57 N-000060))
    (pad 3 thru_hole circle (at -3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 57 N-000060))
    (pad 4 thru_hole rect (at 3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 3 thru_hole circle (at -3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 57 N-000060))
    (pad 4 thru_hole rect (at 3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 50.8 177.8 25)
    (fp_text reference SW0:12 (at 0 3.302 25) (layer F.SilkS))
    (fp_text value SW0:1 (at 0 3.302 25) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 55 N-000058))
    (pad 0 thru_hole circle (at 0 0 25) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 55 N-000058))
    (pad 3 thru_hole circle (at -3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 55 N-000058))
    (pad 4 thru_hole rect (at 3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 55 N-000058))
    (pad 4 thru_hole rect (at 3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 42.7482 160.53308 25)
    (fp_text reference SW0:9 (at 0 3.302 25) (layer F.SilkS))
    (fp_text value SW0:4 (at 0 3.302 25) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 56 N-000059))
    (pad 0 thru_hole circle (at 0 0 25) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 25) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 11 /ROW0))
    (pad 2 thru_hole circle (at -2.54 -5.08 25) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 56 N-000059))
    (pad 3 thru_hole circle (at -3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 56 N-000059))
    (pad 4 thru_hole rect (at 3.81 5.08 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 3 thru_hole circle (at -3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 56 N-000059))
    (pad 4 thru_hole rect (at 3.81 7.62 25) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 /COL4))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 25) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 91.44 84.14766)
    (fp_text reference SW4:8 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW4:5 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 59 N-000064))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 59 N-000064))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 59 N-000064))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 59 N-000064))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 /COL5))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 186.69 143.20266)
    (fp_text reference SW1:13 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW1:0 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 53 N-000056))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /ROW1))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 53 N-000056))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 53 N-000056))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 53 N-000056))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 /COL0))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 72.39 117.48516 90)
    (fp_text reference SW2:7 (at 0 3.302 90) (layer F.SilkS))
    (fp_text value SW2:6 (at 0 3.302 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 35 N-000036))
    (pad 0 thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 13 /ROW2))
    (pad 2 thru_hole circle (at -2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 35 N-000036))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 35 N-000036))
    (pad 4 thru_hole rect (at 3.81 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 3 thru_hole circle (at -3.81 7.62 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 35 N-000036))
    (pad 4 thru_hole rect (at 3.81 7.62 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 99 smd rect (at -1.6637 7.62 90) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 90) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 90) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 90) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 72.39 88.91016 90)
    (fp_text reference SW4:7 (at 0 3.302 90) (layer F.SilkS))
    (fp_text value SW4:6 (at 0 3.302 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 58 N-000063))
    (pad 0 thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0 90) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 15 /ROW4))
    (pad 2 thru_hole circle (at -2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 58 N-000063))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 58 N-000063))
    (pad 4 thru_hole rect (at 3.81 5.08 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 3 thru_hole circle (at -3.81 7.62 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 58 N-000063))
    (pad 4 thru_hole rect (at 3.81 7.62 90) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 99 smd rect (at -1.6637 7.62 90) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62 90) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62 90) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62 90) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 72.39 65.1002)
    (fp_text reference SW5:7 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW5:6 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 24 N-000013))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 16 /ROW5))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 24 N-000013))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 N-000013))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 N-000013))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL6))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (module "ErgoDOX pcb:MX_FLIP_DIODE" (layer Front) (tedit 582D0751)
    (at 167.64 105.10266)
    (fp_text reference SW3:12 (at 0 3.302) (layer F.SilkS))
    (fp_text value SW3:1 (at 0 3.302) (layer B.SilkS))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 49 N-000050))
    (pad 0 thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 0 thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (net 19 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 14 /ROW3))
    (pad 2 thru_hole circle (at -2.54 -5.08) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 49 N-000050))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 49 N-000050))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 49 N-000050))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Front F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers Back B.Paste B.Mask))
  )
  (gr_text "Revision 2016-11-18" (at 178.435 127 90) (layer F.SilkS))
  (gr_text ID (at 129.794 34.544) (layer F.SilkS))
  (gr_text D+ (at 137.668 42.164) (layer F.SilkS))
  (gr_text GND (at 132.207 40.386) (layer F.SilkS))
  (gr_text 5V (at 142.494 40.386) (layer F.SilkS))
  (gr_text D- (at 146.30146 34.544) (layer F.SilkS))
  (gr_text ErgoDox (at 113.03 48.895) (layer B.SilkS))
  (gr_text "Components are intended to be\nplaced on the side they are drawn. It is however possible to\ninvert the design. See the webpage for further instructions.\nhttp://ergodox.io" (at 66.04 50.8) (layer F.SilkS))
  (gr_text "RIGHT\nHAND" (at 67.31 100.965) (layer F.SilkS))
  (gr_text "LEFT\nHAND" (at 78.105 100.965) (layer B.SilkS))
  (gr_text "FR4 Tg170° Laminate\n24mil traces on 1oz copper " (at 191.77 54.61) (layer B.SilkS))
  (gr_text "FR4 Tg170° Laminate\n24mil traces on 1oz copper " (at 160.655 54.61) (layer F.SilkS))
  (gr_text "Drawn in KiCAD by Fredrik Atmer, Bathroom Epiphanies" (at 201.93 127 90) (layer F.SilkS))
  (gr_text "Design by Dominic Beauchamp, based on the Key64 by  Nestor A. Diaz" (at 201.93 91.44 270) (layer B.SilkS))
  (gr_line (start 127.1524 152.908) (end 196.3928 152.908) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 196.3928 152.908) (end 205.9178 143.383) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 205.9178 143.383) (end 205.9178 35.433) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 205.9178 35.433) (end 202.7428 32.258) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 202.7428 32.258) (end 143.4084 32.258) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 143.4084 32.258) (end 143.4084 30.48) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 143.4084 30.48) (end 131.9022 30.48) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 131.9022 30.48) (end 131.9022 32.258) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 131.9022 32.258) (end 95.0468 32.258) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 95.0468 32.258) (end 95.0468 30.48) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 95.0468 30.48) (end 88.7095 30.48) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 88.7095 30.48) (end 88.7095 31.75) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 88.7095 31.75) (end 84.2137 31.75) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 84.2137 31.75) (end 84.2137 30.48) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 84.2137 30.48) (end 77.8764 30.48) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 77.8764 30.48) (end 77.8764 32.258) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 77.8764 32.258) (end 65.8114 32.258) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 65.8114 32.258) (end 62.611 35.433) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 62.611 35.433) (end 62.611 121.666) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 62.611 121.666) (end 57.7088 121.666) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 57.7088 121.666) (end 24.61768 137.0965) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 24.61768 137.0965) (end 23.08098 141.31544) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 23.08098 141.31544) (end 44.76496 187.81776) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 44.76496 187.81776) (end 48.9839 189.35192) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 48.9839 189.35192) (end 127.1524 152.908) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 19) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3048)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.6096))
    (polygon
      (pts
        (xy 48.9839 189.35192) (xy 127.1524 152.908) (xy 196.3928 152.908) (xy 205.9178 143.383) (xy 205.9178 35.433)
        (xy 202.7428 32.258) (xy 143.4084 32.258) (xy 143.4084 30.48) (xy 131.9022 30.48) (xy 131.9022 32.258)
        (xy 95.0468 32.258) (xy 95.0468 30.48) (xy 88.7095 30.48) (xy 88.7095 31.75) (xy 84.2137 31.75)
        (xy 84.2137 30.48) (xy 77.8764 30.48) (xy 77.8764 32.258) (xy 65.8114 32.258) (xy 62.611 35.433)
        (xy 62.611 121.666) (xy 57.7088 121.666) (xy 24.61768 137.0965) (xy 23.08098 141.31544) (xy 44.76496 187.81776)
      )
    )
  )
  (zone (net 19) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3048)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.6096))
    (polygon
      (pts
        (xy 48.9839 189.35192) (xy 127.1524 152.908) (xy 196.3928 152.908) (xy 205.9178 143.383) (xy 205.9178 35.433)
        (xy 202.7428 32.258) (xy 143.4084 32.258) (xy 143.4084 30.48) (xy 131.9022 30.48) (xy 131.9022 32.258)
        (xy 95.0468 32.258) (xy 95.0468 30.48) (xy 88.7095 30.48) (xy 88.7095 31.75) (xy 84.2137 31.75)
        (xy 84.2137 30.48) (xy 77.8764 30.48) (xy 77.8764 32.258) (xy 65.8114 32.258) (xy 62.611 35.433)
        (xy 62.611 121.666) (xy 57.7088 121.666) (xy 24.61768 137.0965) (xy 23.08098 141.31544) (xy 44.76496 187.81776)
      )
    )
  )
)
