(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 54)
    (zones 0)
    (modules 38)
    (nets 32)
  )
  (page A4)
  (title_block
    (title "Osborne 1 Floppy Adapter")
    (date 2020-07-13)
    (rev 1.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 10 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J11-Pad1)")
  (net 2 "Net-(J13-Pad1)")
  (net 3 "Net-(J14-Pad1)")
  (net 4 "Net-(J15-Pad1)")
  (net 5 "Net-(J16-Pad1)")
  (net 6 "Net-(J17-Pad1)")
  (net 7 "Net-(J21-Pad1)")
  (net 8 "Net-(J23-Pad1)")
  (net 9 "Net-(J25-Pad1)")
  (net 10 "Net-(J32-Pad1)")
  (net 11 "Net-(J34-Pad1)")
  (net 12 "Net-(FLOPPY1-Pad34)")
  (net 13 "Net-(FLOPPY1-Pad1)")
  (net 14 "Net-(FLOPPY1-Pad32)")
  (net 15 "Net-(FLOPPY1-Pad30)")
  (net 16 "Net-(FLOPPY1-Pad28)")
  (net 17 "Net-(FLOPPY1-Pad26)")
  (net 18 "Net-(FLOPPY1-Pad24)")
  (net 19 "Net-(FLOPPY1-Pad22)")
  (net 20 "Net-(FLOPPY1-Pad20)")
  (net 21 "Net-(FLOPPY1-Pad18)")
  (net 22 "Net-(FLOPPY1-Pad16)")
  (net 23 "Net-(FLOPPY1-Pad10)")
  (net 24 "Net-(FLOPPY1-Pad8)")
  (net 25 "Net-(FLOPPY1-Pad6)")
  (net 26 "Net-(FLOPPY1-Pad4)")
  (net 27 "Net-(FLOPPY1-Pad2)")
  (net 28 "Net-(FLOPPY1-Pad14)")
  (net 29 "Net-(FLOPPY1-Pad12)")
  (net 30 "Net-(J10-Pad1)")
  (net 31 "Net-(J12-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(FLOPPY1-Pad1)")
    (add_net "Net-(FLOPPY1-Pad10)")
    (add_net "Net-(FLOPPY1-Pad12)")
    (add_net "Net-(FLOPPY1-Pad14)")
    (add_net "Net-(FLOPPY1-Pad16)")
    (add_net "Net-(FLOPPY1-Pad18)")
    (add_net "Net-(FLOPPY1-Pad2)")
    (add_net "Net-(FLOPPY1-Pad20)")
    (add_net "Net-(FLOPPY1-Pad22)")
    (add_net "Net-(FLOPPY1-Pad24)")
    (add_net "Net-(FLOPPY1-Pad26)")
    (add_net "Net-(FLOPPY1-Pad28)")
    (add_net "Net-(FLOPPY1-Pad30)")
    (add_net "Net-(FLOPPY1-Pad32)")
    (add_net "Net-(FLOPPY1-Pad34)")
    (add_net "Net-(FLOPPY1-Pad4)")
    (add_net "Net-(FLOPPY1-Pad6)")
    (add_net "Net-(FLOPPY1-Pad8)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J23-Pad1)")
    (add_net "Net-(J25-Pad1)")
    (add_net "Net-(J32-Pad1)")
    (add_net "Net-(J34-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 99.568 81.28 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference PWR1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x01 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.016) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J21-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 90.932 75.184)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 106.68)
    (fp_text reference J1 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 104.14)
    (fp_text reference J3 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 101.6)
    (fp_text reference J5 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 99.06)
    (fp_text reference J7 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 96.52)
    (fp_text reference J9 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 93.98)
    (fp_text reference J11 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +12V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 1 "Net-(J11-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 91.44)
    (fp_text reference J13 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +12V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 2 "Net-(J13-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 88.9)
    (fp_text reference J15 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +12V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 4 "Net-(J15-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 86.36)
    (fp_text reference J17 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +12V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 6 "Net-(J17-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 83.82)
    (fp_text reference J19 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 81.28)
    (fp_text reference J21 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +5V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 7 "Net-(J21-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 78.74)
    (fp_text reference J23 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +5V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 8 "Net-(J23-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 73.66)
    (fp_text reference J27 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 71.12)
    (fp_text reference J29 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 68.58)
    (fp_text reference J31 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 66.04)
    (fp_text reference J33 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value GND (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 104.14)
    (fp_text reference J4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 26 "Net-(FLOPPY1-Pad4)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 106.68)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 27 "Net-(FLOPPY1-Pad2)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 101.6)
    (fp_text reference J6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 25 "Net-(FLOPPY1-Pad6)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 99.06)
    (fp_text reference J8 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value INDEX (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 24 "Net-(FLOPPY1-Pad8)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 96.52)
    (fp_text reference J10 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value DS1 (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 30 "Net-(J10-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 93.98)
    (fp_text reference J12 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value DS2 (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 31 "Net-(J12-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 91.44)
    (fp_text reference J14 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NC (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 3 "Net-(J14-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 88.9)
    (fp_text reference J16 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 4MHz (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 5 "Net-(J16-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 86.36)
    (fp_text reference J18 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value DIR (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 21 "Net-(FLOPPY1-Pad18)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 83.82)
    (fp_text reference J20 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value STEP (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 20 "Net-(FLOPPY1-Pad20)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 81.28)
    (fp_text reference J22 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value WD (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 19 "Net-(FLOPPY1-Pad22)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 78.74)
    (fp_text reference J24 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value WG (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 18 "Net-(FLOPPY1-Pad24)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer B.Cu) (tedit 5F0A61A3)
    (at 106.68 76.2)
    (fp_text reference J25 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value +5V (at 0 0.5) (layer B.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers B.Cu B.Mask)
      (net 9 "Net-(J25-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 76.2)
    (fp_text reference J26 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TRK00 (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 17 "Net-(FLOPPY1-Pad26)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 73.66)
    (fp_text reference J28 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value WP (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 16 "Net-(FLOPPY1-Pad28)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 68.58)
    (fp_text reference J32 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value SS (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 10 "Net-(J32-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 71.12)
    (fp_text reference J30 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value RD (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 15 "Net-(FLOPPY1-Pad30)") (zone_connect 2))
  )
  (module wayne_footprints:EdgeFinger (layer F.Cu) (tedit 5F0A61A3)
    (at 106.68 66.04)
    (fp_text reference J34 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value LATE (at 0 -0.5) (layer F.Fab))
    (pad 1 connect rect (at 0 0) (size 10 1.5) (drill (offset 5 0)) (layers F.Cu F.Mask)
      (net 11 "Net-(J34-Pad1)") (zone_connect 2))
  )
  (module wayne_footprints:PPPC172LJBN-RC (layer F.Cu) (tedit 5F0A5D5D)
    (at 83.82 106.68)
    (fp_text reference FLOPPY (at 5.08 -1.27 90) (layer F.SilkS))
    (fp_text value "IDC 34 Pin" (at -2.54 -20.955 90) (layer F.Fab))
    (fp_text user 1 (at -2.032 0) (layer F.SilkS))
    (pad 34 thru_hole circle (at 2.54 -40.64) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 "Net-(FLOPPY1-Pad34)"))
    (pad 33 thru_hole circle (at 0 -40.64) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 32 thru_hole circle (at 2.54 -38.1) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "Net-(FLOPPY1-Pad32)"))
    (pad 31 thru_hole circle (at 0 -38.1) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 30 thru_hole circle (at 2.54 -35.56) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 "Net-(FLOPPY1-Pad30)"))
    (pad 29 thru_hole circle (at 0 -35.56) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 28 thru_hole circle (at 2.54 -33.02) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 "Net-(FLOPPY1-Pad28)"))
    (pad 27 thru_hole circle (at 0 -33.02) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 26 thru_hole circle (at 2.54 -30.48) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "Net-(FLOPPY1-Pad26)"))
    (pad 25 thru_hole circle (at 0 -30.48) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 24 thru_hole circle (at 2.54 -27.94) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(FLOPPY1-Pad24)"))
    (pad 23 thru_hole circle (at 0 -27.94) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 22 thru_hole circle (at 2.54 -25.4) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "Net-(FLOPPY1-Pad22)"))
    (pad 21 thru_hole circle (at 0 -25.4) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 20 thru_hole circle (at 2.54 -22.86) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "Net-(FLOPPY1-Pad20)"))
    (pad 19 thru_hole circle (at 0 -22.86) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 18 thru_hole circle (at 2.54 -20.32) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "Net-(FLOPPY1-Pad18)"))
    (pad 17 thru_hole circle (at 0 -20.32) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 16 thru_hole circle (at 2.54 -17.78) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "Net-(FLOPPY1-Pad16)"))
    (pad 15 thru_hole circle (at 0 -17.78) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 14 thru_hole circle (at 2.54 -15.24) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "Net-(FLOPPY1-Pad14)"))
    (pad 13 thru_hole circle (at 0 -15.24) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 12 thru_hole circle (at 2.54 -12.7) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(FLOPPY1-Pad12)"))
    (pad 11 thru_hole circle (at 0 -12.7) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 10 thru_hole circle (at 2.54 -10.16) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 "Net-(FLOPPY1-Pad10)"))
    (pad 9 thru_hole circle (at 0 -10.16) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 8 thru_hole circle (at 2.54 -7.62) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 "Net-(FLOPPY1-Pad8)"))
    (pad 7 thru_hole circle (at 0 -7.62) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 6 thru_hole circle (at 2.54 -5.08) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 "Net-(FLOPPY1-Pad6)"))
    (pad 5 thru_hole circle (at 0 -5.08) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 "Net-(FLOPPY1-Pad4)"))
    (pad 3 thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 "Net-(FLOPPY1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(FLOPPY1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 97.028 96.52 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference DRV_SEL (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 2.286 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J12-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(FLOPPY1-Pad12)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 94.488 96.52) (layer F.SilkS))
  (gr_text 2 (at 94.488 93.98) (layer F.SilkS))
  (gr_text 3 (at 94.488 91.44) (layer F.SilkS))
  (gr_text "OSBORNE 1\nFLOPPY ADAPTER\nRev 1.1\nWAYNE VISSER, 2020" (at 88.392 68.58) (layer F.SilkS))
  (gr_text "1-2: \"A\"\n2-3: \"B\"" (at 93.98 101.346) (layer F.SilkS))
  (gr_text 33 (at 105.41 66.04) (layer B.SilkS))
  (gr_text 1 (at 105.41 106.68) (layer B.SilkS))
  (gr_text 34 (at 105.41 66.04) (layer F.SilkS))
  (gr_text 2 (at 105.41 106.68) (layer F.SilkS))
  (gr_text GND (at 93.98 81.28) (layer F.SilkS))
  (gr_text +5V (at 102.362 81.28) (layer F.SilkS))
  (gr_line (start 117.602 103.2256) (end 117.602 108.1405) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.68 103.2256) (end 117.602 103.2256) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.68 102.5144) (end 106.68 103.2256) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.602 102.5144) (end 106.68 102.5144) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.602 64.5795) (end 116.586 63.5635) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.602 108.1405) (end 116.586 109.1565) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.586 109.1565) (end 80.264 109.1565) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80.264 63.5635) (end 80.264 109.1565) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.586 63.5635) (end 80.264 63.5635) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.602 102.5144) (end 117.602 64.5795) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.856 109.22) (xy 106.68 109.22) (xy 106.68 63.5) (xy 117.856 63.5)
      )
    )
  )
  (zone (net 13) (net_name "Net-(FLOPPY1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.75))
    (polygon
      (pts
        (xy 118.6815 109.777185) (xy 79.4385 109.780416) (xy 79.502 62.995231) (xy 118.745 62.995231)
      )
    )
  )
  (zone (net 13) (net_name "Net-(FLOPPY1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.75))
    (polygon
      (pts
        (xy 118.364 110.236) (xy 79.756 110.236) (xy 79.756 62.992) (xy 118.364 62.992)
      )
    )
  )
)
