(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "Net-(H1-Pad1)")
  (net 2 "Net-(D4K1-Pad1)")
  (net 3 "Net-(D4K1-Pad2)")
  (net 4 "Net-(D4K1-Pad3)")
  (net 5 "Net-(D4K1-Pad4)")
  (net 6 "Net-(D4K1-Pad5)")
  (net 7 "Net-(D4K1-Pad6)")
  (net 8 "Net-(D4K1-Pad7)")
  (net 9 "Net-(D4K1-Pad8)")
  (net 10 "Net-(D4K1-Pad9)")
  (net 11 "Net-(D4K1-Pad10)")
  (net 12 "Net-(D4K1-Pad11)")
  (net 13 "Net-(D4K1-Pad12)")
  (net 14 "unconnected-(D4K1-Pad13)")
  (net 15 "Net-(D4K1-Pad14)")
  (net 16 "Net-(D4K1-Pad15)")
  (net 17 "Net-(D4K1-Pad16)")
  (net 18 "Net-(D4K1-Pad17)")
  (net 19 "Net-(D4K1-Pad18)")
  (net 20 "Net-(D4K1-Pad19)")
  (net 21 "Net-(D4K1-Pad20)")
  (net 22 "Net-(D4K1-Pad21)")
  (net 23 "Net-(D4K1-Pad22)")
  (net 24 "Net-(D4K1-Pad23)")
  (net 25 "Net-(D4K1-Pad24)")
  (net 26 "Net-(D4K1-Pad25)")
  (net 27 "unconnected-(D4K1-PadMH1)")
  (net 28 "unconnected-(D4K1-PadMH2)")
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 258.7625 85.852)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R52" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 3 "Net-(D4K1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 16 "Net-(D4K1-Pad15)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 258.7625 44.9805)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R58" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 2 "Net-(D4K1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 15 "Net-(D4K1-Pad14)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 228.2825 85.852)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 9 "Net-(D4K1-Pad8)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 22 "Net-(D4K1-Pad21)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 207.9625 85.852)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R47" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 13 "Net-(D4K1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 26 "Net-(D4K1-Pad25)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 207.9625 100.7495)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R50" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D4K1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D4K1-Pad25)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 258.7625 100.7495)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R55" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D4K1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D4K1-Pad15)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 248.6025 100.7495)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D4K1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D4K1-Pad17)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 228.2825 50.673)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 8 "Net-(D4K1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 21 "Net-(D4K1-Pad20)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 258.7625 96.387)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R54" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D4K1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D4K1-Pad15)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 238.4425 50.673)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 6 "Net-(D4K1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 19 "Net-(D4K1-Pad18)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 238.4425 91.5445)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 7 "Net-(D4K1-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 20 "Net-(D4K1-Pad19)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 228.2825 40.138)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D4K1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D4K1-Pad20)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 258.7625 57.15)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R56" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 2 "Net-(D4K1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 15 "Net-(D4K1-Pad14)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 248.6025 40.138)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D4K1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D4K1-Pad16)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 218.1225 100.7495)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R40" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D4K1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D4K1-Pad23)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 207.7702 50.673)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R42" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 12 "Net-(D4K1-Pad11)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 25 "Net-(D4K1-Pad24)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 238.4425 40.138)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D4K1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D4K1-Pad18)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 218.1225 35.7755)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D4K1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D4K1-Pad22)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 228.2825 79.375)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 9 "Net-(D4K1-Pad8)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 22 "Net-(D4K1-Pad21)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 248.6025 35.7755)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D4K1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D4K1-Pad16)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 238.4425 85.852)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 7 "Net-(D4K1-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 20 "Net-(D4K1-Pad19)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 248.6025 96.387)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D4K1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D4K1-Pad17)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 207.772 44.9805)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 12 "Net-(D4K1-Pad11)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 25 "Net-(D4K1-Pad24)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 238.4425 44.9805)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 6 "Net-(D4K1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 19 "Net-(D4K1-Pad18)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 218.1225 50.673)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 10 "Net-(D4K1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 23 "Net-(D4K1-Pad22)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 258.7625 50.673)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R57" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 2 "Net-(D4K1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 15 "Net-(D4K1-Pad14)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 248.6025 50.673)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 4 "Net-(D4K1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 17 "Net-(D4K1-Pad16)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 218.1225 44.9805)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 10 "Net-(D4K1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 23 "Net-(D4K1-Pad22)") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_ISO7380_Pad" (layer "F.Cu")
    (at 199.39 31.115)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -0.127 4.8514) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0.01 -5.015) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 228.2825 96.387)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D4K1-Pad8)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D4K1-Pad21)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 248.6025 57.15)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 4 "Net-(D4K1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 17 "Net-(D4K1-Pad16)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 238.4425 100.7495)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D4K1-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D4K1-Pad19)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 238.4425 79.375)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 7 "Net-(D4K1-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 20 "Net-(D4K1-Pad19)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 207.9625 96.387)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R49" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D4K1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D4K1-Pad25)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 207.9625 79.375)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R46" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 13 "Net-(D4K1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 26 "Net-(D4K1-Pad25)") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_ISO7380_Pad" (layer "F.Cu")
    (at 198.755 105.41)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.8) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 4.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 218.1225 57.15)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 10 "Net-(D4K1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 23 "Net-(D4K1-Pad22)") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_ISO7380_Pad" (layer "F.Cu")
    (at 267.335 105.41)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.8) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 4.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_ISO7380_Pad" (layer "F.Cu")
    (at 267.335 31.115)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0.1016 5.0038) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0.015 -5.065) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 218.1225 79.375)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 11 "Net-(D4K1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 24 "Net-(D4K1-Pad23)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 258.7625 40.138)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R59" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D4K1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D4K1-Pad14)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 228.2825 57.15)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 8 "Net-(D4K1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 21 "Net-(D4K1-Pad20)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 238.4425 35.7755)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D4K1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D4K1-Pad18)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 228.2825 91.5445)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 9 "Net-(D4K1-Pad8)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 22 "Net-(D4K1-Pad21)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 218.1225 96.387)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R39" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D4K1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D4K1-Pad23)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 218.1225 40.138)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D4K1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D4K1-Pad22)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 248.6025 91.5445)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 5 "Net-(D4K1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 18 "Net-(D4K1-Pad17)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 248.6025 79.375)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 5 "Net-(D4K1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 18 "Net-(D4K1-Pad17)") (pintype "passive"))
  )
  (footprint "KiCad:MDM25SBSP" (layer "F.Cu")
    (at 248.666 67.5894)
    (descr "MDM-25SBSP-4")
    (tags "Connector")
    (property "Description" "D-Sub Micro-D Connectors")
    (property "Height" "14.1")
    (property "Manufacturer_Name" "")
    (property "Manufacturer_Part_Number" "")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "D-Sub Micro-D Connectors")
    (attr through_hole)
    (fp_text reference "D4K1" (at 10.6426 -0.1016) (layer "F.SilkS"))
    (fp_text value "MDM-25SBSP" (at 14.6812 1.8542) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 10.6426 -0.1016) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D4K1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D4K1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D4K1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -7.62 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D4K1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -10.16 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D4K1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -12.7 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D4K1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -15.24 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D4K1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -17.78 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D4K1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -20.32 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4K1-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at -22.86 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D4K1-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at -25.4 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D4K1-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at -27.94 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D4K1-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at -30.48 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(D4K1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -1.27 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D4K1-Pad14)") (pinfunction "14") (pintype "passive"))
    (pad "15" thru_hole circle (at -3.81 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D4K1-Pad15)") (pinfunction "15") (pintype "passive"))
    (pad "16" thru_hole circle (at -6.35 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D4K1-Pad16)") (pinfunction "16") (pintype "passive"))
    (pad "17" thru_hole circle (at -8.89 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D4K1-Pad17)") (pinfunction "17") (pintype "passive"))
    (pad "18" thru_hole circle (at -11.43 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D4K1-Pad18)") (pinfunction "18") (pintype "passive"))
    (pad "19" thru_hole circle (at -13.97 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D4K1-Pad19)") (pinfunction "19") (pintype "passive"))
    (pad "20" thru_hole circle (at -16.51 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(D4K1-Pad20)") (pinfunction "20") (pintype "passive"))
    (pad "21" thru_hole circle (at -19.05 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D4K1-Pad21)") (pinfunction "21") (pintype "passive"))
    (pad "22" thru_hole circle (at -21.59 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(D4K1-Pad22)") (pinfunction "22") (pintype "passive"))
    (pad "23" thru_hole circle (at -24.13 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(D4K1-Pad23)") (pinfunction "23") (pintype "passive"))
    (pad "24" thru_hole circle (at -26.67 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(D4K1-Pad24)") (pinfunction "24") (pintype "passive"))
    (pad "25" thru_hole circle (at -29.21 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(D4K1-Pad25)") (pinfunction "25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 3.81 1.27) (size 4.155 4.155) (drill 2.77) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(D4K1-PadMH1)") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at -34.29 1.27) (size 4.155 4.155) (drill 2.77) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(D4K1-PadMH2)") (pinfunction "MH2") (pintype "passive"))
    (model "MDM-25SBSP.stp"
      (offset (xyz -15.23999954 -1.299999933 6.760000127))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 228.2825 100.7495)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D4K1-Pad8)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D4K1-Pad21)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 248.6025 44.9805)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 4 "Net-(D4K1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 17 "Net-(D4K1-Pad16)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 207.9625 91.5445)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R48" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 13 "Net-(D4K1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 26 "Net-(D4K1-Pad25)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 228.2825 35.7755)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D4K1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D4K1-Pad20)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 218.1225 91.5445)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 11 "Net-(D4K1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 24 "Net-(D4K1-Pad23)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 228.2825 44.9805)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 8 "Net-(D4K1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 21 "Net-(D4K1-Pad20)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 207.772 35.7755)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R45" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D4K1-Pad11)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D4K1-Pad24)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 238.4425 96.387)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D4K1-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D4K1-Pad19)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0402_Hybrid" (layer "F.Cu")
    (at 258.7625 35.7755)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R60" (at 0 -1 unlocked) (layer "F.Fab") hide)
    (fp_text value "0402" (at 0 1.2 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D4K1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 0) (size 0.56 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D4K1-Pad14)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 218.1225 85.852)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R37" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 11 "Net-(D4K1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 24 "Net-(D4K1-Pad23)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 258.7625 79.375)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R51" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 3 "Net-(D4K1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 16 "Net-(D4K1-Pad15)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 207.5815 57.15)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R41" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 12 "Net-(D4K1-Pad11)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 25 "Net-(D4K1-Pad24)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1210_1206_Hybrid" (layer "F.Cu")
    (at 248.6025 85.852)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -2.2 unlocked) (layer "F.Fab") hide)
    (fp_text value "1210/1206" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785713043)
      (net 5 "Net-(D4K1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 18 "Net-(D4K1-Pad17)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_1812_Hybrid" (layer "F.Cu")
    (at 238.4425 57.15)
    (descr "Generalized 1812 Pad")
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 -2.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "1812" (at 0 2.65 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 6 "Net-(D4K1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222221429)
      (net 19 "Net-(D4K1-Pad18)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0805_Hybrid" (layer "F.Cu")
    (at 258.7625 91.5445)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R53" (at 0 -1.6 unlocked) (layer "F.Fab") hide)
    (fp_text value "0805" (at 0 1.7 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 3 "Net-(D4K1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9125 0) (size 1.025 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 16 "Net-(D4K1-Pad15)") (pintype "passive"))
  )
  (footprint "Hybrid_RC_Pads:RC_0603_Hybrid" (layer "F.Cu")
    (at 207.772 40.138)
    (property "Sheetfile" "SPLENDOR_Component_Test_Board_v1.2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R44" (at 0 -1.3 unlocked) (layer "F.Fab") hide)
    (fp_text value "0603" (at 0 1.4 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D4K1-Pad11)") (pintype "passive"))
    (pad "2" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D4K1-Pad24)") (pintype "passive"))
  )
  (gr_rect (start 193.675 25.4) (end 273.05 111.125)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "(12,25)" (at 207.9625 75.565) (layer "F.SilkS"))
  (gr_text "(2,15)\n" (at 258.7625 75.565) (layer "F.SilkS"))
  (gr_text "(4,17)" (at 248.6025 75.565) (layer "F.SilkS"))
  (gr_text "(8,21)\n" (at 228.2825 75.565) (layer "F.SilkS"))
  (gr_text "(9,22)\n" (at 218.1225 61.595) (layer "F.SilkS"))
  (gr_text "(1,14)" (at 258.7625 61.595) (layer "F.SilkS"))
  (gr_text "(3,16)\n" (at 248.6025 61.595) (layer "F.SilkS"))
  (gr_text "(10,23)\n" (at 218.1225 75.565) (layer "F.SilkS"))
  (gr_text "(7,20)" (at 228.2825 61.595) (layer "F.SilkS"))
  (gr_text "(11,24)\n" (at 207.9625 61.595) (layer "F.SilkS"))
  (gr_text "(6,19)" (at 238.4425 75.565) (layer "F.SilkS"))
  (gr_text "Cold Component Testing PCB v1.2\n07/18/2023\nRiley Carpenter\n" (at 233.375 109.475) (layer "F.SilkS"))
  (gr_text "(5,18)" (at 238.4425 61.595) (layer "F.SilkS"))
  (zone (net 1) (net_name "Net-(H1-Pad1)") (layers "F&B.Cu") (name "Thermal Frame") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999997))
    (polygon
      (pts
        (xy 193.675 25.4)
        (xy 273.05 25.4)
        (xy 273.05 111.125)
        (xy 193.675 111.125)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu" "Dwgs.User") (name "Center Window") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 203.125 34.225)
        (xy 263.6 34.225)
        (xy 263.6 102.95)
        (xy 203.125 102.95)
      )
    )
  )
)
