<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="53" x2="0" y2="3" width="0" layer="20"/>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3" y1="0" x2="42.648" y2="0" width="0" layer="20"/>
<wire x1="42.648" y1="0" x2="42.648" y2="56" width="0" layer="20"/>
<wire x1="42.648" y1="56" x2="3" y2="56" width="0" layer="20"/>
<wire x1="3" y1="56" x2="0" y2="53" width="0" layer="20" curve="90"/>
<hole x="3.5" y="52.5" drill="2.75"/>
<hole x="3.5" y="3.5" drill="2.75"/>
<text>l1+l2 5v</text>
<text>l1g</text>
<text>l1r</text>
<text>l2g</text>
<text>l2r</text>
<text>GND mosfet</text>
<text>d1s</text>
<text>l1s</text>
<text>l2s</text>
<text>bewator s</text>
<text>inputs</text>
<text>d1s+bew g</text>
<text>g</text>
<text>5v</text>
<text>gnd</text>
<text>12v</text>
<text>input pulled high</text>
<text>input pulled high</text>
<text>input pulled high</text>
<text>output switch to gnd</text>
<text>12v output</text>
<text>gnd output</text>
<text>gnd output</text>
<text>dc 12v
2.1x5.5mm</text>
<text>3.5mm stereo
siren</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="PJ-102A">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
</package>
<package name="1X04_NO_SILK">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X14">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X16/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R8" library="adafruit" package="M0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="M0805" value="10k"/>
<element name="R12" library="adafruit" package="M0805" value="10k"/>
<element name="R13" library="adafruit" package="M0805" value="10k"/>
<element name="R14" library="adafruit" package="M0805" value="10k"/>
<element name="R15" library="adafruit" package="M0805" value="10k"/>
<element name="JP5" library="pinhead" package="2X14" value=""/>
<element name="Q1" library="adafruit" package="SOT23-W" value=""/>
<element name="Q2" library="adafruit" package="SOT23-W" value=""/>
<element name="Q3" library="adafruit" package="SOT23-W" value=""/>
<element name="Q4" library="adafruit" package="SOT23-W" value=""/>
<element name="JP2" library="pinhead" package="1X16/90" value=""/>
<element name="JP8" library="SparkFun-Connectors" package="AUDIO-JACK" value=""/>
<element name="U$1" library="adafruit" package="PJ-102A" value="2.1MMJACKTHM"/>
<element name="JP3" library="pinhead" package="1X04" value=""/>
<element name="JP4" library="pinhead" package="1X04" value=""/>
<element name="R1" library="adafruit" package="M0805" value="1k"/>
<element name="R2" library="adafruit" package="M0805" value="1k"/>
<element name="R3" library="adafruit" package="M0805" value="1k"/>
<element name="R4" library="adafruit" package="M0805" value="1k"/>
<element name="R5" library="adafruit" package="M0805" value="1k"/>
<element name="R6" library="adafruit" package="M0805" value="10k"/>
<element name="R7" library="adafruit" package="M0805" value="1k"/>
<element name="R16" library="adafruit" package="M0805" value="10k"/>
<element name="R17" library="adafruit" package="M0805" value="1k"/>
<element name="R18" library="adafruit" package="M0805" value="10k"/>
<element name="Q9" library="adafruit" package="SOT23-W" value=""/>
<element name="R19" library="adafruit" package="M0805" value="10k"/>
<element name="Q10" library="adafruit" package="SOT23-W" value=""/>
<element name="R20" library="adafruit" package="M0805" value="10k"/>
<element name="Q11" library="adafruit" package="SOT23-W" value=""/>
<element name="R21" library="adafruit" package="M0805" value="10k"/>
<element name="R22" library="adafruit" package="M0805" value="10k"/>
<element name="JP7" library="pinhead" package="2X05/90" value=""/>
<element name="R23" library="adafruit" package="M0805" value="180"/>
<element name="Q12" library="adafruit" package="SOT23-W" value=""/>
<element name="R24" library="adafruit" package="M0805" value="180"/>
<element name="Q13" library="adafruit" package="SOT23-W" value=""/>
<element name="R25" library="adafruit" package="M0805" value="180"/>
<element name="JP9" library="SparkFun-Connectors" package="1X04_NO_SILK" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP5" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="3"/>
<contactref element="R12" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="16"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="JP5" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="JP5" pad="8"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R13" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="N$9">
<contactref element="R11" pad="1"/>
<contactref element="JP2" pad="11"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R12" pad="2"/>
<contactref element="JP2" pad="10"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="2"/>
<contactref element="JP5" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="R14" pad="2"/>
<contactref element="JP2" pad="9"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="2"/>
<contactref element="JP5" pad="11"/>
</signal>
<signal name="N$15">
<contactref element="JP2" pad="8"/>
<contactref element="R15" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="2"/>
<contactref element="JP5" pad="12"/>
</signal>
<signal name="N$18">
<contactref element="R7" pad="2"/>
<contactref element="JP5" pad="13"/>
</signal>
<signal name="N$17">
<contactref element="JP2" pad="7"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="JP2" pad="6"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R17" pad="2"/>
<contactref element="JP5" pad="16"/>
</signal>
<signal name="N$21">
<contactref element="Q1" pad="3"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="JP5" pad="15"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="Q2" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="JP5" pad="18"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="3"/>
<contactref element="Q9" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="JP5" pad="19"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="JP2" pad="2"/>
<contactref element="Q10" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="JP5" pad="22"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="Q11" pad="3"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="JP5" pad="21"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="Q2" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="Q9" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="Q10" pad="1"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="Q11" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="U$1" pad="TIP"/>
<contactref element="JP8" pad="RING"/>
<contactref element="JP7" pad="8"/>
<contactref element="JP7" pad="7"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="JP8" pad="SLEEVE"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="Q3" pad="1"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R22" pad="2"/>
<contactref element="JP5" pad="23"/>
</signal>
<signal name="N$31">
<contactref element="Q4" pad="1"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="Q4" pad="2"/>
<contactref element="JP7" pad="5"/>
<contactref element="JP7" pad="6"/>
</signal>
<signal name="N$35">
<contactref element="R23" pad="1"/>
<contactref element="JP5" pad="24"/>
</signal>
<signal name="N$36">
<contactref element="Q12" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="Q12" pad="3"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="N$38">
<contactref element="R24" pad="1"/>
<contactref element="JP5" pad="26"/>
</signal>
<signal name="N$39">
<contactref element="Q13" pad="1"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="Q13" pad="3"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="R25" pad="1"/>
<contactref element="JP5" pad="25"/>
</signal>
<signal name="N$42">
<contactref element="JP5" pad="28"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="JP5" pad="27"/>
<contactref element="JP9" pad="4"/>
</signal>
<signal name="N$49">
<contactref element="JP9" pad="2"/>
<contactref element="JP9" pad="1"/>
<contactref element="U$1" pad="RING_SW"/>
<contactref element="U$1" pad="RING"/>
<contactref element="Q3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP5" pad="6"/>
<contactref element="R13" pad="1"/>
<contactref element="JP5" pad="5"/>
<contactref element="R11" pad="2"/>
<contactref element="JP2" pad="14"/>
<contactref element="JP2" pad="13"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q9" pad="2"/>
<contactref element="Q10" pad="2"/>
<contactref element="Q11" pad="2"/>
<contactref element="JP7" pad="10"/>
<contactref element="JP7" pad="9"/>
<contactref element="Q12" pad="2"/>
<contactref element="Q13" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
