(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Node_Controller")
		(date "2025-09-05")
		(rev "RevA")
		(company "VTNSI")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 114.3 101.6)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(A1-GND-Pad16)")
	(net 2 "GND")
	(net 3 "+3.3V")
	(net 4 "DIO_MODE_TTL1")
	(net 5 "Vdd_rf")
	(net 6 "VBUS")
	(net 7 "~{TEMP_ADC_AR}")
	(net 8 "DIO_MODE_TTL0")
	(net 9 "SCL")
	(net 10 "+5V")
	(net 11 "SDA")
	(net 12 "~{PA_CURR_ALERT}")
	(net 13 "u3V3")
	(net 14 "+28V")
	(net 15 "unconnected-(A1-~{RESET}-Pad1)")
	(net 16 "unconnected-(A1-EN-Pad27)")
	(net 17 "Net-(JP5-C)")
	(net 18 "unconnected-(A1-AREF-Pad3)")
	(net 19 "+12V")
	(net 20 "unconnected-(D2-NC-Pad2)")
	(net 21 "Net-(D2-A)")
	(net 22 "Net-(JP2-A)")
	(net 23 "Net-(D4-A)")
	(net 24 "Net-(D5-A)")
	(net 25 "Net-(D1-K)")
	(net 26 "unconnected-(D3-NC-Pad2)")
	(net 27 "Net-(D3-A)")
	(net 28 "unconnected-(D5-NC-Pad2)")
	(net 29 "+28V_IN")
	(net 30 "RF_FWD_POW")
	(net 31 "/rf_power_sensor/ADC_RF0_1")
	(net 32 "/rf_power_sensor/ADC_RF0_2")
	(net 33 "/rf_power_sensor/ADC_RF0_3")
	(net 34 "Net-(JP4-C)")
	(net 35 "RF_REV_POW")
	(net 36 "Net-(Q6-D)")
	(net 37 "Net-(Q7-D)")
	(net 38 "Net-(Q8-D)")
	(net 39 "Net-(Q9-D)")
	(net 40 "Net-(Q10-D)")
	(net 41 "/rf_power_sensor/ADC_RF1_1")
	(net 42 "/rf_power_sensor/ADC_RF1_2")
	(net 43 "PA_28V_SEND")
	(net 44 "/USRP GPIO Interface/gpio_7")
	(net 45 "Net-(JP1-A)")
	(net 46 "/USRP GPIO Interface/gpio_4")
	(net 47 "/USRP GPIO Interface/gpio_5")
	(net 48 "/rf_power_sensor/ADC_RF1_3")
	(net 49 "PA_FET_DIS")
	(net 50 "LNA_12V")
	(net 51 "~{XFER_PTT}")
	(net 52 "/RF Switch Control/XFER_COIL_28V")
	(net 53 "~{LNA_PTT}")
	(net 54 "~{LNA_EN}")
	(net 55 "/power_amp_interface/PA_28V")
	(net 56 "/W6PQL_Sequencer/~{PTT}")
	(net 57 "Net-(D8-A)")
	(net 58 "unconnected-(D8-NC-Pad2)")
	(net 59 "Net-(D9-A)")
	(net 60 "unconnected-(D9-NC-Pad2)")
	(net 61 "Net-(D10-A)")
	(net 62 "unconnected-(D10-NC-Pad2)")
	(net 63 "Net-(D16-A)")
	(net 64 "LNA0_VDD")
	(net 65 "USRP_GPIO_5")
	(net 66 "USRP_GPIO_0")
	(net 67 "USRP_GPIO_4")
	(net 68 "USRP_GPIO_6")
	(net 69 "USRP_GPIO_3")
	(net 70 "USRP_GPIO_1")
	(net 71 "USRP_GPIO_7")
	(net 72 "USRP_GPIO_2")
	(net 73 "LNA1_VDD")
	(net 74 "LNA2_VDD")
	(net 75 "LNA3_VDD")
	(net 76 "Net-(JP6-C)")
	(net 77 "unconnected-(D4-NC-Pad2)")
	(net 78 "Net-(D7-A)")
	(net 79 "unconnected-(D7-NC-Pad2)")
	(net 80 "Net-(D10-K)")
	(net 81 "/RF Switch Control/SP4T0_TTL0")
	(net 82 "/RF Switch Control/SP4T0_TTL1")
	(net 83 "/RF Switch Control/SP4T1_TTL1")
	(net 84 "/RF Switch Control/SP4T1_TTL0")
	(net 85 "Net-(Q1-B)")
	(net 86 "Net-(Q1-C)")
	(net 87 "Net-(Q3-D)")
	(net 88 "Net-(Q11-C)")
	(net 89 "Net-(Q11-B)")
	(net 90 "Net-(Q12-G)")
	(net 91 "Net-(Q4-D)")
	(net 92 "Net-(Q5-D)")
	(net 93 "~{PA_FET_DIS}")
	(net 94 "~{PA_FET_PTT}")
	(net 95 "~{RF_ADC0_AR}")
	(net 96 "~{RF_ADC1_AR}")
	(net 97 "Net-(R23-Pad2)")
	(net 98 "Net-(R24-Pad2)")
	(net 99 "Net-(R25-Pad2)")
	(net 100 "Net-(R26-Pad2)")
	(net 101 "Net-(R27-Pad2)")
	(net 102 "Net-(R28-Pad2)")
	(net 103 "Net-(R29-Pad2)")
	(net 104 "Net-(R30-Pad2)")
	(net 105 "USRP_MODE_0")
	(net 106 "USRP_PTT")
	(net 107 "USRP_MODE_1")
	(net 108 "MODE_0")
	(net 109 "MODE_1")
	(net 110 "/USRP GPIO Interface/gpio_3")
	(net 111 "DIO_SRC_SELECT")
	(net 112 "DIO_PTT")
	(net 113 "USRP_NOTIFY")
	(net 114 "unconnected-(D11-NC-Pad2)")
	(net 115 "Net-(D12-A)")
	(net 116 "unconnected-(D12-NC-Pad2)")
	(net 117 "unconnected-(D13-NC-Pad2)")
	(net 118 "Net-(D13-K)")
	(net 119 "Net-(D14-A)")
	(net 120 "unconnected-(D14-NC-Pad2)")
	(net 121 "Net-(D15-K)")
	(net 122 "unconnected-(D15-NC-Pad2)")
	(net 123 "unconnected-(D16-NC-Pad2)")
	(net 124 "Net-(D18-A)")
	(net 125 "unconnected-(D17-NC-Pad2)")
	(net 126 "unconnected-(D18-NC-Pad2)")
	(net 127 "PTT")
	(net 128 "PA_28V_RTN")
	(net 129 "Net-(Q13-C)")
	(net 130 "DIO_PA_PTT")
	(net 131 "DIO_USRP")
	(net 132 "DIO_XFER_PTT")
	(net 133 "DIO_LNA_PTT")
	(net 134 "Net-(Q13-B)")
	(net 135 "Net-(Q14-G)")
	(net 136 "Net-(Q17-B)")
	(net 137 "Net-(R52-Pad2)")
	(net 138 "Net-(R62-Pad1)")
	(net 139 "Net-(R63-Pad1)")
	(net 140 "Net-(R64-Pad1)")
	(net 141 "Net-(R65-Pad1)")
	(net 142 "Net-(U20-EN)")
	(net 143 "Net-(U21-EN)")
	(net 144 "unconnected-(U20-~{FLT}-Pad3)")
	(net 145 "unconnected-(U21-~{FLT}-Pad3)")
	(net 146 "/Preamp_Control/LNA_5V")
	(net 147 "Net-(C51-Pad1)")
	(net 148 "Net-(U15-EN)")
	(net 149 "/power_amp_interface/TEMP_PA")
	(net 150 "/power_amp_interface/TEMP_COMP")
	(net 151 "Net-(U4-BP)")
	(net 152 "~{XFER_DIS}")
	(net 153 "Net-(U15-BP)")
	(net 154 "Net-(U4-EN)")
	(net 155 "Net-(U22A-+)")
	(net 156 "Net-(U22B-+)")
	(net 157 "Net-(U22C-+)")
	(net 158 "Net-(U22D-+)")
	(net 159 "Net-(U22A--)")
	(net 160 "Net-(U22B--)")
	(net 161 "Net-(U22C--)")
	(net 162 "Net-(U22D--)")
	(net 163 "unconnected-(U1-NC-Pad13)")
	(net 164 "unconnected-(U1-ALERT-Pad7)")
	(net 165 "unconnected-(U9-NC-Pad1)")
	(net 166 "unconnected-(U9-NC-Pad5)")
	(net 167 "unconnected-(U10-NC-Pad13)")
	(net 168 "Net-(U13-Pad3)")
	(net 169 "Net-(U13-Pad10)")
	(net 170 "Net-(U14-Pad3)")
	(net 171 "Net-(U14-Pad10)")
	(net 172 "Net-(U16-~{Y2})")
	(net 173 "Net-(U16-~{Y3})")
	(net 174 "Net-(U16-~{Y1})")
	(net 175 "Net-(U16-~{Y0})")
	(net 176 "Net-(U19-EN)")
	(net 177 "Net-(U18-EN)")
	(net 178 "unconnected-(U18-~{FLT}-Pad3)")
	(net 179 "unconnected-(U19-~{FLT}-Pad3)")
	(net 180 "unconnected-(U23-Pad7)")
	(net 181 "unconnected-(U23-Pad4)")
	(net 182 "unconnected-(U23-Pad6)")
	(net 183 "unconnected-(U23-Pad5)")
	(net 184 "LNA_EN")
	(net 185 "Net-(Q21-G)")
	(net 186 "RX{slash}D0")
	(net 187 "D13")
	(net 188 "Net-(D19-K)")
	(net 189 "Net-(JP10-A)")
	(net 190 "Net-(JP11-A)")
	(net 191 "POW_FWD")
	(net 192 "POW_REV")
	(net 193 "Net-(U5A--)")
	(net 194 "Net-(R75-Pad2)")
	(net 195 "Net-(U25A-+)")
	(net 196 "Net-(U5B--)")
	(net 197 "Net-(R79-Pad2)")
	(net 198 "Net-(R80-Pad2)")
	(net 199 "Net-(U25A--)")
	(net 200 "unconnected-(U25B---Pad6)")
	(net 201 "unconnected-(U25-Pad7)")
	(net 202 "unconnected-(U25B-+-Pad5)")
	(net 203 "TX{slash}D1")
	(net 204 "D12")
	(net 205 "Net-(Q22-D)")
	(net 206 "Net-(D20-K)")
	(net 207 "Net-(D21-A)")
	(net 208 "Net-(D21-K)")
	(net 209 "Net-(D22-A)")
	(net 210 "Net-(D22-K)")
	(net 211 "Net-(Q2-G)")
	(net 212 "TEMP_PCB")
	(net 213 "/power_amp_interface/TEMP_CASE")
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 149.225 142.875 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP10"
			(at 0 -2.148 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ADC_RF1_2"
			(at 0 2.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 48 "/rf_power_sensor/ADC_RF1_3")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 125.095 90.805)
		(property "Reference" "R61"
			(at 3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "Net-(U22D--)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 142.875 135.89)
		(descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
		(tags "SSOP 0.5")
		(property "Reference" "U7"
			(at -2.54 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115IDGS"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1.71 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 -1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "SDA")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.15 -0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "~{RF_ADC1_AR}")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -2.15 0)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -2.15 0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 190 "Net-(JP11-A)")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.15 1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/rf_power_sensor/ADC_RF1_1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.15 1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/rf_power_sensor/ADC_RF1_2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.15 0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/rf_power_sensor/ADC_RF1_3")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.15 0)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(JP4-C)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 2.15 -0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 2.15 -1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 90.9 74.295)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D6"
			(at 4.445 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "US1M"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds16008.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V, 1A, General Purpose Rectifier Diode, SMA(DO-214AC)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.635 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 52 "/RF Switch Control/XFER_COIL_28V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 71.125 -90)
		(property "Reference" "R22"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "/USRP GPIO Interface/gpio_7")
			(pintype "passive")
		)
	)
	(footprint "Module:Adafruit_Feather"
		(layer "F.Cu")
		(at 164.465 108.585 -90)
		(descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
		(tags "Adafruit Feather")
		(property "Reference" "A1"
			(at 10.16 -7.62 90)
			(layer "F.SilkS")
		)
		(property "Value" "Adafruit_Feather_M0_Basic_Proto"
			(at 10.16 45.72 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-basic-proto.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Adafruit*Feather*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(clearance 0.2)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 19.05 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 15 "unconnected-(A1-~{RESET}-Pad1)")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 13 "u3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-AREF-Pad3)")
			(pinfunction "AREF")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "Net-(A1-GND-Pad16)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 131 "DIO_USRP")
			(pinfunction "DAC0/A0")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 112 "DIO_PTT")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "DIO_MODE_TTL0")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 4 "DIO_MODE_TTL1")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 111 "DIO_SRC_SELECT")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 133 "DIO_LNA_PTT")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 184 "LNA_EN")
			(pinfunction "SCK/D24")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 132 "DIO_XFER_PTT")
			(pinfunction "MOSI/D23")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 130 "DIO_PA_PTT")
			(pinfunction "MISO/D22")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 186 "RX{slash}D0")
			(pinfunction "RX/D0")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 203 "TX{slash}D1")
			(pinfunction "TX/D1")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "Net-(A1-GND-Pad16)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 20.32 38.1 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 11 "SDA")
			(pinfunction "SDA/D20")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole oval
			(at 20.32 35.56 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 9 "SCL")
			(pinfunction "SCL/D21")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 20.32 33.02 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "~{TEMP_ADC_AR}")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at 20.32 30.48 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "~{PA_CURR_ALERT}")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 20.32 27.94 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 49 "PA_FET_DIS")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 20.32 25.4 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 95 "~{RF_ADC0_AR}")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 20.32 22.86 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 96 "~{RF_ADC1_AR}")
			(pinfunction "D11")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole oval
			(at 20.32 20.32 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 204 "D12")
			(pinfunction "D12")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 20.32 17.78 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 187 "D13")
			(pinfunction "D13")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 20.32 15.24 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "VBUS")
			(pinfunction "USB")
			(pintype "power_in")
		)
		(pad "27" thru_hole oval
			(at 20.32 12.7 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-EN-Pad27)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 20.32 10.16 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 10 "+5V")
			(pinfunction "VBAT")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 101.6 132.715 180)
		(property "Reference" "R71"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "Net-(Q21-G)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 73.66 100.33)
		(property "Reference" "C5"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 130.81 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP24"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LNA2"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 74 "LNA2_VDD")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:VSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 145.415 102.235)
		(descr "VSSOP, 10 Pin (http://www.ti.com/lit/ds/symlink/ads1115.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "VSSOP SO")
		(property "Reference" "U24"
			(at 0 2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "TS5A23159DGS"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a23159.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual SPDT 1ohm Bidirectional Analog Switch with Off protection, VSSOP-10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VSSOP*3x3mm*P0.5mm*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.2 -1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "DIO_SRC_SELECT")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.2 -0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "DIO_MODE_TTL1")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.2 0)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.2 0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "DIO_MODE_TTL0")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -2.2 1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "DIO_SRC_SELECT")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.2 1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "MODE_0")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.2 0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "USRP_MODE_0")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.2 0)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "Net-(JP6-C)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.2 -0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "USRP_MODE_1")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 2.2 -1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "MODE_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 99.695 141.605 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP13"
			(at 0 -2.148 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_COMP"
			(at 0 2.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 150 "/power_amp_interface/TEMP_COMP")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 74.935 -90)
		(property "Reference" "R21"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "USRP_NOTIFY")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 93.985 -90)
		(property "Reference" "R16"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "USRP_GPIO_1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 74.295 76.2 90)
		(property "Reference" "R31"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "20k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(D5-A)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 98.425 104.775 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP30"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SP4T_+5V"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 85.31 81.28 180)
		(property "Reference" "C36"
			(at 0 -1.84 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 152 "~{XFER_DIS}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 97.155 80.645 -90)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D7"
			(at 0 1.905 90)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "unconnected-(D7-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "~{LNA_PTT}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 121.285 90.17 180)
		(property "Reference" "R65"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "Net-(R65-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "Net-(D18-A)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 80.645 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP40"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPI_6"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 68 "USRP_GPIO_6")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 69.85 139.7)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MH"
			(at 0 4.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "digikey-footprints:SOT-23-3"
		(layer "F.Cu")
		(at 111.125 83.82 90)
		(property "Reference" "Q17"
			(at -2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT2907A-TP"
			(at 0.025 3.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOT-23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mccsemi.com/pdf/Products/MMBT2907A(SOT-23).pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TRANS PNP 60V 0.6A SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MMBT2907A-TPMSCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MMBT2907A-TP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Discrete Semiconductor Products"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Transistors - Bipolar (BJT) - Single"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "https://www.mccsemi.com/pdf/Products/MMBT2907A(SOT-23).pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/micro-commercial-co/MMBT2907A-TP/MMBT2907A-TPMSCT-ND/1220289"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "TRANS PNP 60V 0.6A SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Micro Commercial Co"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.125 0.15 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 136 "Net-(Q17-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -1.05 0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "Net-(D10-A)")
			(pinfunction "C")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at 1.05 0 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pinfunction "E")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 79.375 94.615 -90)
		(property "Reference" "C10"
			(at 3.615 -0.08 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 120.396 74.168 90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U20"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2065CDBV"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "LNA2_VDD")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "unconnected-(U20-~{FLT}-Pad3)")
			(pinfunction "~{FLT}")
			(pintype "open_collector")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 142 "Net-(U20-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "/Preamp_Control/LNA_5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 114.3 65.7075 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D21"
			(at -1.3185 -2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 208 "Net-(D21-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 207 "Net-(D21-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 128.905 124.875 -90)
		(property "Reference" "R1"
			(at -2.955 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "SCL")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 83.82 132.08 180)
		(property "Reference" "R10"
			(at 0.635 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "6k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "Net-(Q1-B)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 99.695 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP34"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPO_0"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 66 "USRP_GPIO_0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 79.375 90.805 90)
		(property "Reference" "C11"
			(at 3.615 -0.08 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 140.335 97.155)
		(property "Reference" "R69"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "DIO_SRC_SELECT")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 85.725 90.805 90)
		(property "Reference" "C13"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(JP2-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 81.915 141.605 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP12"
			(at 0 -2.148 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_CASE"
			(at 0 2.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 213 "/power_amp_interface/TEMP_CASE")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 88.265 95.25 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP2"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "3V3"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 22 "Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "+3.3V")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 188 "Net-(D19-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 81.915 66.895 90)
		(property "Reference" "R37"
			(at 0.22 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "13k"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "Net-(Q12-G)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "Net-(Q11-C)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 88.9 70.485)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP33"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "XFER_28V"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 52 "/RF Switch Control/XFER_COIL_28V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 82.555 180)
		(property "Reference" "R23"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(Q7-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "Net-(R23-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 137.795 142.875)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP20"
			(at 0 5.715 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RF_POW_REV"
			(at 0 4.445 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 35 "RF_REV_POW")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 132.715 89.52)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D9"
			(at 0 -1.89 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(D9-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(D9-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/W6PQL_Sequencer/~{PTT}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.03 75.565 -90)
		(property "Reference" "C48"
			(at 3.175 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "/Preamp_Control/LNA_5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 97.409 90.551 90)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D17"
			(at -2.032 0.142 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 133 "DIO_LNA_PTT")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "unconnected-(D17-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 113.03 122.555 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D22"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 210 "Net-(D22-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 209 "Net-(D22-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 101.2675 85.725 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q20"
			(at -1.9535 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D10-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "~{LNA_PTT}")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 126.365 142.875 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP5"
			(at 0 -4.445 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ADC_RF0_1"
			(at 0 -4.445 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 31 "/rf_power_sensor/ADC_RF0_1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 111.795 132.715)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U5"
			(at -2.575 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "TLC277"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc272.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual LinCMOS Precision Dual Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 194 "Net-(R75-Pad2)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "Net-(U5A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 191 "POW_FWD")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "POW_REV")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 196 "Net-(U5B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "Net-(R79-Pad2)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 108.585 69.435 -90)
		(property "Reference" "R45"
			(at -3.141 2.159 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "LNA_12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "Net-(U15-EN)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 119.38 101.6)
		(property "Reference" "R59"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "Net-(U22B--)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "Net-(U22C--)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 98.425 108.585 90)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP31"
			(at 0 -2.148 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SP4T_GND"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 73.66 102.235 180)
		(property "Reference" "C3"
			(at 3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 117.475 142.875 90)
		(property "Reference" "R77"
			(at 0 1.397 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.4k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 192 "POW_REV")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 91.445 180)
		(property "Reference" "R25"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "Net-(Q4-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "Net-(R25-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 80.015 180)
		(property "Reference" "R28"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(Q8-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "Net-(R28-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 113.665 107.95 180)
		(property "Reference" "U14"
			(at 5.08 -0.16 -90)
			(layer "F.SilkS")
		)
		(property "Value" "74HC00"
			(at 0.635 1.11 180)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOIC-14_W3.9mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc00"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SO14*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "MODE_0")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "MODE_0")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(U14-Pad3)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(U14-Pad3)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(U14-Pad3)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "/RF Switch Control/SP4T1_TTL0")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "/RF Switch Control/SP4T1_TTL1")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "Net-(U14-Pad10)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "Net-(U14-Pad10)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "Net-(U14-Pad10)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "MODE_1")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "MODE_1")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 108.585 127 90)
		(property "Reference" "R76"
			(at 2.54 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 194 "Net-(R75-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 199 "Net-(U25A--)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 164.465 113.445 -90)
		(property "Reference" "C14"
			(at 0 -1.905 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "u3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 150.495 100.33 180)
		(property "Reference" "C54"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "Net-(JP6-C)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 103.505 141.605 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP11"
			(at 0 -2.148 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_PA"
			(at 0 2.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 149 "/power_amp_interface/TEMP_PA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 87.63 128.27 180)
		(property "Reference" "R13"
			(at 0 1.27 180)
			(layer "F.SilkS")
		)
		(property "Value" "13k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "Net-(Q2-G)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "Net-(Q1-C)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 99.695 73.025 90)
		(property "Reference" "R42"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "Net-(Q13-B)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 71.755 90.17 180)
		(property "Reference" "C4"
			(at 3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 90.175 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q5"
			(at 1.5725 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "USRP_GPIO_2")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 92 "Net-(Q5-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 77.47 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP41"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPI_7"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 71 "USRP_GPIO_7")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 78.105 72.39 -90)
		(property "Reference" "R35"
			(at 3.175 -0.254 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "Net-(Q11-B)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 104.775 121.285 180)
		(property "Reference" "R80"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "Net-(R79-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 198 "Net-(R80-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 83.82 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP39"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPO_5"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 65 "USRP_GPIO_5")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 123.19 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP16"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LNA_GND"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 103.505 89.17 -90)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D10"
			(at 2.27 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(D10-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "unconnected-(D10-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 142.875 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP17"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GND"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 116.84 133.13 90)
		(property "Reference" "R79"
			(at -3.175 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 196 "Net-(U5B--)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "Net-(R79-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 106.045 116.205 90)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP27"
			(at 0 -2.148 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SP4T0_TTL1"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 82 "/RF Switch Control/SP4T0_TTL1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 100.965 80.645 90)
		(property "Reference" "R40"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "Net-(D7-A)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 142.24 139.065 180)
		(property "Reference" "C23"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/rf_power_sensor/ADC_RF1_1")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 103.505 95.885 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "C51"
			(at -2.54 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "Net-(C51-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5mm"
		(layer "F.Cu")
		(at 84.535 122.775)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx0162.pdf")
		(property "Reference" "J7"
			(at 2.7 -4.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "PA_28V"
			(at 2.05 5.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 43 "PA_28V_SEND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 128 "PA_28V_RTN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:TO-252-3"
		(layer "F.Cu")
		(at 72.39 82.805 180)
		(descr "http://www.digikey.com/products/en?keywords=MC7805BDTRKGOSCT-ND")
		(property "Reference" "U3"
			(at 5.08 -4.19 0)
			(layer "F.SilkS")
		)
		(property "Value" "MC7805BDTRKG"
			(at 0 5.1 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:TO-252-3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7800-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC REG LINEAR 5V 1A DPAK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MC7805BDTRKGOSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MC7805BDTRKG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits (ICs)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "PMIC - Voltage Regulators - Linear"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.onsemi.com/pub/Collateral/MC7800-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/MC7805BDTRKG/MC7805BDTRKGOSCT-ND/1139742"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.03 -0.12 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.08 -2.285)
			(size 3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pinfunction "IN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -4.08 2.285)
			(size 3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(JP1-A)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd rect
			(at 3.09 0)
			(size 6.2 5.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
	)
	(footprint "digikey-footprints:SOT-23-3"
		(layer "F.Cu")
		(at 102.87 76.835 90)
		(property "Reference" "Q13"
			(at 1.905 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "MMBTA06LT1G"
			(at 0.025 3.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOT-23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MMBTA05LT1-D.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TRANS NPN 80V 0.5A SOT23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MMBTA06LT1GOSCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MMBTA06LT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Discrete Semiconductor Products"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Transistors - Bipolar (BJT) - Single"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.onsemi.com/pub/Collateral/MMBTA05LT1-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/MMBTA06LT1G/MMBTA06LT1GOSCT-ND/1139832"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "TRANS NPN 80V 0.5A SOT23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.125 0.15 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "Net-(Q13-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -1.05 0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "Net-(D8-A)")
			(pinfunction "E")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at 1.05 0 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "Net-(Q13-C)")
			(pinfunction "C")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.258 134.112 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP48"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "D13"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 187 "D13")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 86.365 180)
		(property "Reference" "R27"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.81 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(Q6-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "Net-(R27-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 131.064 83.312)
		(property "Reference" "C45"
			(at 0 1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 122.555 139.7 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP10"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Vdd_RF"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 189 "Net-(JP10-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "RF_FWD_POW")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 191 "POW_FWD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 92.71 70.485)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP32"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "XFER_RTN"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 107.95 75.565 90)
		(property "Reference" "C40"
			(at 3.175 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "~{LNA_EN}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 74.935 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q9"
			(at 1.5725 -1.41 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 -1.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "USRP_NOTIFY")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "Net-(Q9-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 116.84 122.555 180)
		(property "Reference" "R84"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 210 "Net-(D22-K)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 107.315 141.605 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP15"
			(at 0 -5.715 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_GND"
			(at 0 2.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 78.105 141.605)
		(property "Reference" "C32"
			(at 0 -1.27 360)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "/power_amp_interface/TEMP_CASE")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 94.488 123.825)
		(property "Reference" "R6"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "20k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "+28V_IN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(D3-A)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.665 94.615)
		(property "Reference" "R53"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "Net-(C51-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "Net-(U22A-+)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 137.795 137.16)
		(property "Reference" "C22"
			(at 0 -1.84 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 190 "Net-(JP11-A)")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 165.1 69.85)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H4"
			(at 4.445 -3.81 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MH"
			(at 0 4.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 96.52 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP35"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPO_1"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 70 "USRP_GPIO_1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 120.015 132.08 180)
		(property "Reference" "R78"
			(at 0.508 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 196 "Net-(U5B--)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 80.01 72.39 -90)
		(property "Reference" "R32"
			(at 3.175 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.5k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 91.44 128.27 180)
		(property "Reference" "R12"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "+28V_IN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "Net-(Q2-G)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 130.175 142.875 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP6"
			(at 0 -4.445 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ADC_RF0_2"
			(at 0 -4.445 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 32 "/rf_power_sensor/ADC_RF0_2")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 136.525 85.725)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D12"
			(at -0.381 -1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "Net-(D12-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "unconnected-(D12-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "USRP_NOTIFY")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 127.635 135.89)
		(descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
		(tags "SSOP 0.5")
		(property "Reference" "U6"
			(at -1.905 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115IDGS"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 -1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Vdd_rf")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.15 -0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "~{RF_ADC0_AR}")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -2.15 0)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -2.15 0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 189 "Net-(JP10-A)")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.15 1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/rf_power_sensor/ADC_RF0_1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.15 1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/rf_power_sensor/ADC_RF0_2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.15 0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/rf_power_sensor/ADC_RF0_3")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.15 0)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Vdd_rf")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 2.15 -0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 2.15 -1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 132.35 100.315 180)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D15"
			(at 0.27 -1.92 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.65 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "DIO_XFER_PTT")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "unconnected-(D15-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "Net-(D15-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 136.525 92.71 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q16"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "PTT")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/W6PQL_Sequencer/~{PTT}")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 99.695 76.835 90)
		(property "Reference" "R41"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "6k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "Net-(D7-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "Net-(Q13-B)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 114.935 140.97 90)
		(property "Reference" "R73"
			(at 0 1.397 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.4k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 191 "POW_FWD")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 84.7875 70.485)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q12"
			(at 0.9375 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLML9301"
			(at 0 -0.775 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml9301pbf.pdf?fileId=5546d462533600a401535668e5e42640"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-3.6A Id, -30V Vds, 64mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "Net-(Q12-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "+28V")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/RF Switch Control/XFER_COIL_28V")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:1206"
		(layer "F.Cu")
		(at 156.845 113.665 90)
		(descr "http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/LTST-C230KFKT_5-24-06.pdf")
		(property "Reference" "FB2"
			(at 0 -1.905 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:1206"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.8 0 90)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.8 0 90)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(A1-GND-Pad16)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 146.685 139.065 180)
		(property "Reference" "C24"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.905 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/rf_power_sensor/ADC_RF1_2")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "F.Cu")
		(at 95.885 87.085 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP12"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "~{XFER}_~{LNA}"
			(at 0 2.63 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.725 0 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 53 "~{LNA_PTT}")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.725 0 270)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 51 "~{XFER_PTT}")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0) (xy -0.65 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 71.125 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q10"
			(at 2.2075 -1.41 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 -1.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/USRP GPIO Interface/gpio_7")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(Q10-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 125.73 87.63 180)
		(property "Reference" "R49"
			(at 3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "Net-(D9-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 136 "Net-(Q17-B)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 163.83 75.565)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP54"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NOTIFY"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 113 "USRP_NOTIFY")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 153.67 103.505 90)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D11"
			(at -1.905 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "DIO_USRP")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 114 "unconnected-(D11-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "USRP_NOTIFY")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 136.525 89.535)
		(property "Reference" "C50"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "/W6PQL_Sequencer/~{PTT}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.115 128.27)
		(property "Reference" "C1"
			(at 0 -1.84 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.045 131.445 180)
		(property "Reference" "R75"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 193 "Net-(U5A--)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 194 "Net-(R75-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:SOT-23-3"
		(layer "F.Cu")
		(at 83.82 128.905 90)
		(property "Reference" "Q1"
			(at 1.27 -1.27 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBTA06LT1G"
			(at 0.025 3.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOT-23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MMBTA05LT1-D.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TRANS NPN 80V 0.5A SOT23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MMBTA06LT1GOSCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MMBTA06LT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Discrete Semiconductor Products"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Transistors - Bipolar (BJT) - Single"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.onsemi.com/pub/Collateral/MMBTA05LT1-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/MMBTA06LT1G/MMBTA06LT1GOSCT-ND/1139832"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "TRANS NPN 80V 0.5A SOT23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.125 0.15 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -1.05 0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(D3-A)")
			(pinfunction "E")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at 1.05 0 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 120.65 118.11)
		(property "Reference" "R88"
			(at 0 1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "MODE_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 90.805 76.835)
		(property "Reference" "C38"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/RF Switch Control/XFER_COIL_28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 132.588 74.0465 -90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U19"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2065CDBV"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.635 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "LNA1_VDD")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 179 "unconnected-(U19-~{FLT}-Pad3)")
			(pinfunction "~{FLT}")
			(pintype "open_collector")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "Net-(U19-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "/Preamp_Control/LNA_5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 133.985 142.875 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP7"
			(at 0 -4.445 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ADC_RF0_3"
			(at 0 -4.445 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 33 "/rf_power_sensor/ADC_RF0_3")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 137.795 139.7 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP11"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Vdd_RF"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 190 "Net-(JP11-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 35 "RF_REV_POW")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 192 "POW_REV")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 100.965 98.425 -90)
		(property "Reference" "R66"
			(at 0 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "Net-(D13-K)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 150.495 98.425 180)
		(property "Reference" "C53"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "Net-(JP6-C)")
			(pintype "passive")
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 149.225 123.825 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D1"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "MBR120"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?123*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "VBUS")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 109.5525 80.01 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q15"
			(at 0.9675 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "LNA_EN")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "~{LNA_EN}")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 102.87 -90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP42"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPIO_G"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical"
		(layer "F.Cu")
		(at 104.775 125.94)
		(descr "Potentiometer, vertical, top-adjust, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
		(tags "Potentiometer vertical Bourns 3314G")
		(property "Reference" "RV2"
			(at 2.54 3.092 180)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 4.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.7 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -2.75)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 198 "Net-(R80-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 2.75)
			(size 2 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 195 "Net-(U25A-+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.15 -2.75)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 2 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 140.335 104.648)
		(property "Reference" "R70"
			(at 0 1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "DIO_SRC_SELECT")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 82.555 -90)
		(property "Reference" "R19"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "USRP_GPIO_4")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 111.76 72.39 180)
		(property "Reference" "C43"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 6.175 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 153 "Net-(U15-BP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:1206"
		(layer "F.Cu")
		(at 95.25 114.935)
		(descr "http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/LTST-C230KFKT_5-24-06.pdf")
		(property "Reference" "FB3"
			(at 4.445 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.8 0)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "PA_28V_RTN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.8 0)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 131.445 97.79 180)
		(property "Reference" "R67"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "Net-(D15-K)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 106.045 108.585 90)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP29"
			(at 0 -2.148 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SP4T1_TTL1"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 83 "/RF Switch Control/SP4T1_TTL1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 78.745 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q8"
			(at 1.5725 -1.41 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 -1.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "USRP_GPIO_5")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "Net-(Q8-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 100.33 128.27 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP44"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "REV"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 195 "Net-(U25A-+)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 120.65 125.73 180)
		(property "Reference" "C58"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 100.584 89.392 -90)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D18"
			(at 2.048 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 124 "Net-(D18-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "unconnected-(D18-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 180)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:MSOP-8_W2.80mm"
		(layer "F.Cu")
		(at 125.984 84.836 -90)
		(property "Reference" "U16"
			(at -1.651 1.524 180)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC1G139"
			(at 0 4.375 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:MSOP-8_W2.80mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g139.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-to-4 line decoder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*5.3x6.2mm*P0.65mm*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "MODE_0")
			(pinfunction "A")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -0.325 1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "MODE_1")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at 0.325 1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "Net-(U16-~{Y3})")
			(pinfunction "~{Y3}")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0.975 1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 0.975 -1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "Net-(U16-~{Y2})")
			(pinfunction "~{Y2}")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 0.325 -1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 174 "Net-(U16-~{Y1})")
			(pinfunction "~{Y1}")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at -0.325 -1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 175 "Net-(U16-~{Y0})")
			(pinfunction "~{Y0}")
			(pintype "output")
			(solder_mask_margin 0.07)
			(solder_paste_margin -0.025)
		)
		(pad "8" smd rect
			(at -0.975 -1.7 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5mm"
		(layer "F.Cu")
		(at 84.622 112.107)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx0162.pdf")
		(property "Reference" "J1"
			(at 2.7 -4.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "+28V_IN"
			(at 2.05 5.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 29 "+28V_IN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 128 "PA_28V_RTN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.665 99.06)
		(property "Reference" "R58"
			(at -2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "Net-(U22A--)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "Net-(U22B--)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 105.68 80.01)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D8"
			(at 1 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(D8-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "~{LNA_EN}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 84.455 97.79 180)
		(property "Reference" "C12"
			(at 0 -1.84 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "Net-(U4-BP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 97.795 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 1.5725 1.275 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "USRP_GPIO_0")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 79.375 128.905)
		(property "Reference" "C35"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.045 88.9 -90)
		(property "Reference" "R52"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "Net-(D10-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "Net-(R52-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 83.82 90.805 90)
		(property "Reference" "C15"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(JP2-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 100.33 125.095)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP43"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FWD"
			(at 0 2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 199 "Net-(U25A--)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 102.87 73.025 -90)
		(property "Reference" "R44"
			(at 0 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "500"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "Net-(Q14-G)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "Net-(Q13-C)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 84.3225 94.615)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U4"
			(at 1.5295 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SPX3819M5-L-3-3"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "+12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "Net-(U4-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "Net-(U4-BP)")
			(pinfunction "BP")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(JP2-A)")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 81.28 79.375 90)
		(property "Reference" "C9"
			(at 0.635 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:1206"
		(layer "F.Cu")
		(at 126.365 113.665 -90)
		(descr "http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/LTST-C230KFKT_5-24-06.pdf")
		(property "Reference" "FB1"
			(at 0 -1.69 90)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:1206"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.8 0 270)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(A1-GND-Pad16)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.8 0 270)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 92.075 130.81)
		(property "Reference" "C27"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "~{PA_FET_PTT}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 75.565 128.905 180)
		(property "Reference" "R14"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "~{PA_CURR_ALERT}")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 81.28 90.805 90)
		(property "Reference" "C7"
			(at 3.175 -0.08 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 115.57 83.185)
		(property "Reference" "R51"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "Net-(D10-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 81.915 70.485 90)
		(property "Reference" "R36"
			(at -2.286 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "Net-(Q12-G)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 86.365 -90)
		(property "Reference" "R18"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "USRP_GPIO_3")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 165.1 139.7)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H3"
			(at 5.08 3.81 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MH"
			(at 0 4.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 100.965 93.98 90)
		(property "Reference" "R68"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "Net-(D10-K)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 158.115 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP1"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPIO7"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 44 "/USRP GPIO Interface/gpio_7")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 125.095 92.71 180)
		(property "Reference" "R60"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "Net-(U22C--)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "Net-(U22D--)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 155.575 134.112 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP47"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "D12"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 204 "D12")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 93.985 180)
		(property "Reference" "R24"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "Net-(R24-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 76.2 124.785)
		(descr "TSSOP, 16 Pin (https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO JEDEC-MO-153-AB TI-PW0016A Microchip-ST Toshiba-TSSOP16-P-0044-0.65A NXP-SOT403-1 Infineon-P-TSSOP-16-800")
		(property "Reference" "U10"
			(at 0 -3.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "INA260"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina260.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Current/power/voltage monitor with Integrated 2mΩ Shunt Resistor, 2.7V - 5.5V, I2C, TSSOP-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/power_amp_interface/PA_28V")
			(pinfunction "IN+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/power_amp_interface/PA_28V")
			(pinfunction "IN+")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/power_amp_interface/PA_28V")
			(pinfunction "IN+")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "~{PA_CURR_ALERT}")
			(pinfunction "ALERT")
			(pintype "open_collector")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/power_amp_interface/PA_28V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "unconnected-(U10-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "PA_28V_SEND")
			(pinfunction "IN-")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "PA_28V_SEND")
			(pinfunction "IN-")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "PA_28V_SEND")
			(pinfunction "IN-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 111.379 64.643)
		(property "Reference" "R83"
			(at -3.937 1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 208 "Net-(D21-K)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 160.02 104.14)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q22"
			(at 1.905 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "PTT")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 205 "Net-(Q22-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 111.125 75.565 -90)
		(property "Reference" "C47"
			(at 0 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "/Preamp_Control/LNA_5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 69.85 69.85)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MH"
			(at 0 4.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 71.755 88.265)
		(property "Reference" "C6"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 92.075 133.985)
		(property "Reference" "C26"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "~{PA_FET_DIS}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 122.555 142.875 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP19"
			(at 0 -4.445 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RF_POW_FWD"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "RF_FWD_POW")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:1206"
		(layer "F.Cu")
		(at 95.25 120.015)
		(descr "http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/LTST-C230KFKT_5-24-06.pdf")
		(property "Reference" "FB5"
			(at 4.445 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.8 0)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "PA_28V_RTN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.8 0)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 109.855 97.155 180)
		(property "Reference" "C52"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 99.695 138.43 -90)
		(property "Reference" "C33"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 149 "/power_amp_interface/TEMP_PA")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:1206"
		(layer "F.Cu")
		(at 95.25 117.475)
		(descr "http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/LTST-C230KFKT_5-24-06.pdf")
		(property "Reference" "FB4"
			(at 4.445 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.8 0)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "PA_28V_RTN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.8 0)
			(size 1.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 83.455 74.676)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D5"
			(at 1.762 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "unconnected-(D5-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "~{XFER_PTT}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 78.105 137.795)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP51"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_GND"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 103.505 138.43 -90)
		(property "Reference" "C31"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "/power_amp_interface/TEMP_COMP")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 85.725 142.875 180)
		(property "Reference" "C29"
			(at 0 -1.27 360)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 360)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 212 "TEMP_PCB")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:TO-252-3"
		(layer "F.Cu")
		(at 72.12 95.505 180)
		(descr "http://www.digikey.com/products/en?keywords=MC7805BDTRKGOSCT-ND")
		(property "Reference" "U2"
			(at 7.35 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "MC7812BDTRKG"
			(at 0 5.1 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:TO-252-3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/onsemi/MC7812BDTRKG/1481271"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC REG LINEAR 12V 1A DPAK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MC7812BDTRKGOSTR-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MC7812BDTRKG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits (ICs)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "PMIC - Voltage Regulators - Linear"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.onsemi.com/pub/Collateral/MC7800-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/MC7805BDTRKG/MC7805BDTRKGOSCT-ND/1139742"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "IC REG LINEAR 5V 1A DPAK"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.03 -0.12 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.08 -2.285)
			(size 3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pinfunction "IN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -4.08 2.285)
			(size 3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd rect
			(at 3.09 0)
			(size 6.2 5.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 119.38 135.89 -90)
		(property "Reference" "C16"
			(at 0 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Vdd_rf")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 131.445 139.065 180)
		(property "Reference" "C19"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/rf_power_sensor/ADC_RF0_2")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 95.25 138.43 -90)
		(property "Reference" "C28"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(JP5-C)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 77.475 180)
		(property "Reference" "R29"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(Q9-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "Net-(R29-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 83.185 104.995 -90)
		(property "Reference" "C2"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 160.655 100.965 180)
		(property "Reference" "R82"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 205 "Net-(Q22-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 206 "Net-(D20-K)")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 81.28 83.82 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.905 90)
			(layer "F.SilkS")
		)
		(property "Value" "5V"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 45 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 25 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 114.935 75.565 -90)
		(property "Reference" "C49"
			(at 3.175 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1000pf"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "/Preamp_Control/LNA_5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:SOT-23-3"
		(layer "F.Cu")
		(at 79.06 68.58 90)
		(property "Reference" "Q11"
			(at 1.27 -1.59 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBTA06LT1G"
			(at 0.025 3.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOT-23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MMBTA05LT1-D.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TRANS NPN 80V 0.5A SOT23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MMBTA06LT1GOSCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MMBTA06LT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Discrete Semiconductor Products"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Transistors - Bipolar (BJT) - Single"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.onsemi.com/pub/Collateral/MMBTA05LT1-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/MMBTA06LT1G/MMBTA06LT1GOSCT-ND/1139832"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "TRANS NPN 80V 0.5A SOT23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.125 0.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "Net-(Q11-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -1.05 0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(D5-A)")
			(pinfunction "E")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at 1.05 0 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "Net-(Q11-C)")
			(pinfunction "C")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 102.87 80.645 90)
		(property "Reference" "R38"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "8k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "Net-(D8-A)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.68 85.09)
		(property "Reference" "R57"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "Net-(U22A--)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 148.59 136.525 180)
		(property "Reference" "C25"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.905 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/rf_power_sensor/ADC_RF1_3")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 119.888 82.804 180)
		(property "Reference" "C46"
			(at 0 -1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.045 133.35)
		(property "Reference" "R74"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 193 "Net-(U5A--)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 120.65 116.205 180)
		(property "Reference" "C56"
			(at 0 1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 86.995 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP38"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPO_4"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 67 "USRP_GPIO_4")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 76.2 76.2 90)
		(property "Reference" "R33"
			(at -0.635 1.27 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "+28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(D4-A)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 82.555 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q7"
			(at 1.5725 -1.41 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 -1.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "USRP_GPIO_4")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "Net-(Q7-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 90.17 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP37"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPO_3"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 69 "USRP_GPIO_3")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 153.035 142.875)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP21"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RF_POW_GND"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 113.665 115.57 180)
		(property "Reference" "U13"
			(at 5.08 -0.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "74HC00"
			(at 0 1.11 180)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOIC-14_W3.9mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc00"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SO14*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "MODE_0")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "MODE_0")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "Net-(U13-Pad3)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "Net-(U13-Pad3)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "Net-(U13-Pad3)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/RF Switch Control/SP4T0_TTL0")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "/RF Switch Control/SP4T0_TTL1")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "Net-(U13-Pad10)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "Net-(U13-Pad10)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "Net-(U13-Pad10)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "MODE_1")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "MODE_1")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 118.745 130.175 180)
		(property "Reference" "C57"
			(at -0.635 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 97.155 84.455 180)
		(property "Reference" "C39"
			(at 0.127 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "~{LNA_PTT}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 97.795 -90)
		(property "Reference" "R15"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "USRP_GPIO_0")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 119.38 95.885)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U22"
			(at -2.54 -5.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM324"
			(at 0 5.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2902-n.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "Net-(R62-Pad1)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 159 "Net-(U22A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U22A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "Net-(U22B-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 160 "Net-(U22B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 139 "Net-(R63-Pad1)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "Net-(R64-Pad1)")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 161 "Net-(U22C--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 157 "Net-(U22C-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 158 "Net-(U22D-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 162 "Net-(U22D--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "Net-(R65-Pad1)")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 104.775 69.435 -90)
		(property "Reference" "C41"
			(at -3.141 0.381 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "LNA_12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 120.65 111.76 180)
		(property "Reference" "C55"
			(at 0 -1.84 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
		(layer "F.Cu")
		(at 145.3275 90.805 180)
		(descr "SOP, 16 Pin (https://www.vishay.com/docs/83513/tcmd1000.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U11"
			(at 3.7225 5.715 0)
			(layer "F.SilkS")
		)
		(property "Value" "LTV-247"
			(at 0 6.15 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2009-0014/LTV-2X7%20sereis%20Mar17.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Quad Optocoupler, Vce 80V, CTR 100-600%, SOP-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOP*4.4x10.4mm*P1.27mm*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.0875 -4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -3.0875 -3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "Net-(R24-Pad2)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.0875 -1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -3.0875 -0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "Net-(R25-Pad2)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -3.0875 0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -3.0875 1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "Net-(R26-Pad2)")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -3.0875 3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -3.0875 4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "Net-(R27-Pad2)")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 3.0875 4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 110 "/USRP GPIO Interface/gpio_3")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 3.0875 3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 3.0875 1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "USRP_PTT")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 3.0875 0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 3.0875 -0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "USRP_MODE_1")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 3.0875 -1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 3.0875 -3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "USRP_MODE_0")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 3.0875 -4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOP-16_4.4x10.4mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 109.22 122.555)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP45"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HI_VSWR"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 209 "Net-(D22-A)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 131.445 95.25 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q19"
			(at -1.905 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.955 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "Net-(D15-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "~{XFER_PTT}")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 106.045 104.775 90)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP28"
			(at 0 -2.148 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SP4T1_TTL0"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 84 "/RF Switch Control/SP4T1_TTL0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.665 97.155)
		(property "Reference" "R54"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "Net-(C51-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "Net-(U22B-+)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 97.4575 98.425 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q18"
			(at 1.905 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "Net-(D13-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "~{PA_FET_PTT}")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 120.396 78.8615 90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U21"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2065CDBV"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "LNA3_VDD")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "unconnected-(U21-~{FLT}-Pad3)")
			(pinfunction "~{FLT}")
			(pintype "open_collector")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 143 "Net-(U21-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "/Preamp_Control/LNA_5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 146.685 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP2"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPIO3"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 110 "/USRP GPIO Interface/gpio_3")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 87.9 135.636)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D2"
			(at 0 1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "unconnected-(D2-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "~{PA_FET_DIS}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 138.43 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP22"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LNA0"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 64 "LNA0_VDD")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 136.525 95.25)
		(property "Reference" "R48"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "PTT")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 126.365 124.875 -90)
		(property "Reference" "R2"
			(at -2.955 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "SDA")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 107.315 137.795 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP14"
			(at 0 -5.715 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_5V"
			(at 0 2.25 180)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 86.36 139.7 90)
		(property "Reference" "R8"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "~{TEMP_ADC_AR}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(JP5-C)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 90.175 -90)
		(property "Reference" "R17"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "USRP_GPIO_2")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 134.62 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP23"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LNA1"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 73 "LNA1_VDD")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 76.835 117.475 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q2"
			(at 2.54 -4.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "FQP27P06"
			(at 2.54 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FQP27P06-D.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-27A Id, -60V Vds, QFET P-Channel MOSFET, TO-220"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?220*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 211 "Net-(Q2-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 55 "/power_amp_interface/PA_28V")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 29 "+28V_IN")
			(pinfunction "S")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 125.095 99.695)
		(property "Reference" "R64"
			(at 0 1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 140 "Net-(R64-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(D16-A)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 145.415 142.875)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP9"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ADC_RF1_1"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 42 "/rf_power_sensor/ADC_RF1_2")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 99.06 68.385 90)
		(property "Reference" "R43"
			(at -0.195 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "Net-(Q14-G)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 111.6275 69.435)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U15"
			(at 2.1645 0.034 90)
			(layer "F.SilkS")
		)
		(property "Value" "SPX3819M5-L-5-0"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.exar.com/content/document.ashx?id=22106&languageid=1033&type=Datasheet&partnumber=SPX3819&filename=SPX3819.pdf&part=SPX3819"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "500mA Low drop-out regulator, Fixed Output 5.0V, SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "LNA_12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 148 "Net-(U15-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(U15-BP)")
			(pinfunction "BP")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 207 "Net-(D21-A)")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 85.36 78.74)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D4"
			(at -0.05 -1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "unconnected-(D4-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "~{XFER_DIS}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 128.905 100.33)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D16"
			(at -0.05 1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(D16-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 123 "unconnected-(D16-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "Net-(D15-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 89.535 82.55)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP52"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~{XFER_PTT}"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 51 "~{XFER_PTT}")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.665 80.645 180)
		(property "Reference" "R46"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 184 "LNA_EN")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 101.915 68.485)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q14"
			(at -0.3325 -2.22 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRLML9301"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irlml9301pbf.pdf?fileId=5546d462533600a401535668e5e42640"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-3.6A Id, -30V Vds, 64mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "Net-(Q14-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "+12V")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "LNA_12V")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 101.6 134.62 180)
		(property "Reference" "R72"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "PA_FET_DIS")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "Net-(Q21-G)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 125.095 97.155 180)
		(property "Reference" "R55"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "Net-(C51-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "Net-(U22C-+)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.045 75.565 90)
		(property "Reference" "R39"
			(at 3.175 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2.5k"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "Net-(D8-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 69.85 104.14)
		(property "Reference" "C34"
			(at -3.175 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -1.27 1.905 360)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 167.64 93.345 90)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP36"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPO_2"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 72 "USRP_GPIO_2")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 126.332 77.724 90)
		(property "Reference" "U17"
			(at 5.08 -0.475 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC00"
			(at 0 5.29 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:SOIC-14_W3.9mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc00"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "quad 2-input NAND gate"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SO14*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 175 "Net-(U16-~{Y0})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 175 "Net-(U16-~{Y0})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 177 "Net-(U18-EN)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 174 "Net-(U16-~{Y1})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 174 "Net-(U16-~{Y1})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 176 "Net-(U19-EN)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 142 "Net-(U20-EN)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "Net-(U16-~{Y2})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "Net-(U16-~{Y2})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "Net-(U21-EN)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "Net-(U16-~{Y3})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "Net-(U16-~{Y3})")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 90)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 158.745 78.745 -90)
		(property "Reference" "R20"
			(at 0 -1.84 90)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "USRP_GPIO_5")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 127 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP25"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LNA3"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 75 "LNA3_VDD")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 87.9 130.81)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D3"
			(at 1.905 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "unconnected-(D3-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "~{PA_FET_PTT}")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 104.14 99.695 180)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D13"
			(at 0.127 -1.89 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "DIO_PA_PTT")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "unconnected-(D13-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "Net-(D13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 119.38 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP46"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LNA12V"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 50 "LNA_12V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 125.095 94.615 180)
		(property "Reference" "R56"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "Net-(C51-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "Net-(U22D-+)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 79.375 79.375 90)
		(property "Reference" "C8"
			(at 0.635 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 94.488 125.73)
		(property "Reference" "R9"
			(at 0 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "+28V_IN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(D2-A)")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 79.375 104.14 90)
		(descr "TSSOP, 16 Pin (https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO JEDEC-MO-153-AB TI-PW0016A Microchip-ST Toshiba-TSSOP16-P-0044-0.65A NXP-SOT403-1 Infineon-P-TSSOP-16-800")
		(property "Reference" "U1"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "INA260"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina260.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "+28V_IN")
			(pinfunction "IN+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "+28V_IN")
			(pinfunction "IN+")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "+28V_IN")
			(pinfunction "IN+")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 164 "unconnected-(U1-ALERT-Pad7)")
			(pinfunction "ALERT")
			(pintype "open_collector")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "+28V_IN")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 163 "unconnected-(U1-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "+28V")
			(pinfunction "IN-")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "+28V")
			(pinfunction "IN-")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "+28V")
			(pinfunction "IN-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 76.2 72.39 90)
		(property "Reference" "R34"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "6k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(D4-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "Net-(Q11-B)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 136.652 102.108)
		(property "Reference" "R86"
			(at 0 -1.84 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "USRP_MODE_1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 131.318 115.316)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP50"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TX/D1"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 203 "TX{slash}D1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 142.875 132.08)
		(property "Reference" "R5"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "~{RF_ADC1_AR}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(JP4-C)")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 93.985 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 1.5725 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "USRP_GPIO_1")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "Net-(Q4-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 141.605 142.875)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP8"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ADC_RF1_0"
			(at 0 4.445 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 41 "/rf_power_sensor/ADC_RF1_1")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 81.28 94.615 -90)
		(property "Reference" "R3"
			(at 3.175 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 154 "Net-(U4-EN)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.665 100.965 180)
		(property "Reference" "R63"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "Net-(R63-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "Net-(D14-A)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 70.993 124.68 -90)
		(property "Reference" "C30"
			(at -0.22 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/power_amp_interface/PA_28V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 148.59 134.62)
		(property "Reference" "C21"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(JP4-C)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:VSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 145.415 98.425)
		(descr "VSSOP, 10 Pin (http://www.ti.com/lit/ds/symlink/ads1115.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "VSSOP SO")
		(property "Reference" "U23"
			(at -5.08 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "TS5A23159DGS"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts5a23159.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual SPDT 1ohm Bidirectional Analog Switch with Off protection, VSSOP-10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VSSOP*3x3mm*P0.5mm*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.2 -1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "DIO_SRC_SELECT")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.2 -0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "DIO_PTT")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.2 0)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.2 0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "unconnected-(U23-Pad4)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -2.2 1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 183 "unconnected-(U23-Pad5)")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.2 1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "unconnected-(U23-Pad6)")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.2 0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 180 "unconnected-(U23-Pad7)")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.2 0)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "Net-(JP6-C)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.2 -0.5)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "USRP_PTT")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 2.2 -1)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "PTT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 113.665 126.365)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U25"
			(at 0 3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "TLC277"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc272.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual LinCMOS Precision Dual Operational Amplifiers, DIP-8/SOIC-8/SSOP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 209 "Net-(D22-A)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "Net-(U25A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 195 "Net-(U25A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 202 "unconnected-(U25B-+-Pad5)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 200 "unconnected-(U25B---Pad6)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "unconnected-(U25-Pad7)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 97.79 133.985 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q21"
			(at 1.27 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "Net-(Q21-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "~{PA_FET_DIS}")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 156.21 104.14 90)
		(property "Reference" "R81"
			(at -0.635 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 90)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "PTT")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 135.128 115.316)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP49"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RX/D0"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 186 "RX{slash}D0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 131.445 92.075)
		(property "Reference" "C37"
			(at -1.27 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RF Switch Control")
		(sheetfile "rf_switch_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "~{XFER_PTT}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 132.588 78.74 -90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U18"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2065CDBV"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2051c.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Current limited power switch, single channel, output discharge, reverse blocking, SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "LNA0_VDD")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "unconnected-(U18-~{FLT}-Pad3)")
			(pinfunction "~{FLT}")
			(pintype "open_collector")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "Net-(U18-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "/Preamp_Control/LNA_5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 154.305 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP4"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPIO5"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 47 "/USRP GPIO Interface/gpio_5")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 155.8725 86.365 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q6"
			(at 1.5725 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG3414U"
			(at 0 2.26 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31739.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4.2A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "USRP_GPIO_3")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(Q6-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical"
		(layer "F.Cu")
		(at 108.375 93.345 90)
		(descr "Potentiometer, vertical, top-adjust, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
		(tags "Potentiometer vertical Bourns 3314G")
		(property "Reference" "RV1"
			(at 3.175 1.48 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 0 4.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.7 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -2.75 90)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 147 "Net-(C51-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 2.75 90)
			(size 2 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 147 "Net-(C51-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.15 -2.75 90)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 137 "Net-(R52-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 88.905 180)
		(property "Reference" "R26"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "Net-(Q5-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 100 "Net-(R26-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 80.01 132.08 180)
		(property "Reference" "R11"
			(at 0 -1.27 360)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.95 360)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 113.665 92.075 180)
		(property "Reference" "R62"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "Net-(R62-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "Net-(D12-A)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 111.379 66.548 180)
		(property "Reference" "C44"
			(at 2.921 0.254 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "Net-(D21-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.68 69.435 -90)
		(property "Reference" "C42"
			(at -3.141 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "LNA_12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-323_SC-70"
		(layer "F.Cu")
		(at 107.95 99.695 180)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "D14"
			(at -0.05 -1.905 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAS16W"
			(at -0.05 2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAS16_SER.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V, 0.175A, High-speed Switching Diode, SOT-323"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?323*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.65 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 120 "unconnected-(D14-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at 1 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "Net-(D13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 81.915 137.795)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP55"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEMP_5V"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 96.52 128.27)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP53"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~{PA_PTT}"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 94 "~{PA_FET_PTT}")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
		(layer "F.Cu")
		(at 145.415 79.375 180)
		(descr "SOP, 16 Pin (https://www.vishay.com/docs/83513/tcmd1000.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U12"
			(at 3.81 5.715 0)
			(layer "F.SilkS")
		)
		(property "Value" "LTV-247"
			(at 0 6.15 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2009-0014/LTV-2X7%20sereis%20Mar17.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Quad Optocoupler, Vce 80V, CTR 100-600%, SOP-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOP*4.4x10.4mm*P1.27mm*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.0875 -4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -3.0875 -3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(R23-Pad2)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.0875 -1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -3.0875 -0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "Net-(R28-Pad2)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -3.0875 0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -3.0875 1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "Net-(R29-Pad2)")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -3.0875 3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -3.0875 4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "Net-(R30-Pad2)")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 3.0875 4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "USRP_GPIO_7")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 3.0875 3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 3.0875 1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "USRP_GPIO_6")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 3.0875 0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 3.0875 -0.635 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/USRP GPIO Interface/gpio_5")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 3.0875 -1.905 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 3.0875 -3.175 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/USRP GPIO Interface/gpio_4")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 3.0875 -4.445 180)
			(size 1.825 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOP-16_4.4x10.4mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 114.935 69.435 -90)
		(property "Reference" "R47"
			(at 0.034 -1.397 90)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "Net-(D21-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 270)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "/Preamp_Control/LNA_5V")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 156.845 100.965 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D20"
			(at -0.889 -1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 206 "Net-(D20-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 91.05 141.105)
		(descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
		(tags "SSOP 0.5")
		(property "Reference" "U8"
			(at 0 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115IDGS"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 -1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.15 -0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "~{TEMP_ADC_AR}")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -2.15 0)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -2.15 0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "/power_amp_interface/TEMP_CASE")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.15 1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 212 "TEMP_PCB")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.15 1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 149 "/power_amp_interface/TEMP_PA")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.15 0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "/power_amp_interface/TEMP_COMP")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.15 0)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(JP5-C)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 2.15 -0.5)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 2.15 -1)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 67.625 100.965)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U9"
			(at -1.905 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "MCP9700Ax-ELT"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001942G.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±2C accuracy, -40C to +125C, in SC-70-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SC?70*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "unconnected-(U9-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "TEMP_PCB")
			(pinfunction "V_{OUT}")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "V_{DD}")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "unconnected-(U9-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 161.925 113.665 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D19"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "MBR120"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?123*")
		(sheetname "power_conditioning")
		(sheetfile "power_conditioning.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 188 "Net-(D19-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "u3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 106.68 83.185)
		(property "Reference" "R50"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "500"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "W6PQL_Sequencer")
		(sheetfile "w6pql_sequencer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "+12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 136 "Net-(Q17-B)")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 132.715 136.525 180)
		(property "Reference" "C20"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/rf_power_sensor/ADC_RF0_3")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 87.884 133.35)
		(property "Reference" "R7"
			(at -2.794 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.5k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 151.76 74.935 180)
		(property "Reference" "R30"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 1.27 -10.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USRP GPIO Interface")
		(sheetfile "usrp_gpio_interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(Q10-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 104 "Net-(R30-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 150.495 67.31)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP3"
			(at 0 -2.148 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USRP_GPIO4"
			(at 0 2.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 46 "/USRP GPIO Interface/gpio_4")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 136.652 99.06)
		(property "Reference" "R85"
			(at 0 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "USRP_MODE_0")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 120.65 107.315)
		(property "Reference" "R87"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Preamp_Control")
		(sheetfile "preamp_control.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "MODE_0")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 122.555 137.16)
		(property "Reference" "C17"
			(at 0 -3.81 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 189 "Net-(JP10-A)")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 106.045 112.395 90)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP26"
			(at 0 -2.148 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SP4T0_TTL0"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "kicad_node_ctrl_v3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0 90)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net 81 "/RF Switch Control/SP4T0_TTL0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 122.555 134.62 180)
		(property "Reference" "R4"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "~{RF_ADC0_AR}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Vdd_rf")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:0805"
		(layer "F.Cu")
		(at 127 139.065 180)
		(property "Reference" "C18"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/rf_power_sensor/ADC_RF0_1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 145.415 89.535 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP7"
			(at 0 -1.905 90)
			(layer "B.SilkS")
		)
		(property "Value" "PTT_SEL"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 106 "USRP_PTT")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 127 "PTT")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 112 "DIO_PTT")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "B.Cu")
		(at 127.635 135.89 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP3"
			(at 0 1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "Vdd_RF"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 5 "Vdd_rf")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 10 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 150.495 103.505 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP8"
			(at 0 1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "MODE0_SEL"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 105 "USRP_MODE_0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 108 "MODE_0")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 8 "DIO_MODE_TTL0")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "B.Cu")
		(at 142.875 135.89 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP4"
			(at 0 1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "Vdd_RF"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "rf_power_sensor")
		(sheetfile "rf_power_sensor.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 34 "Net-(JP4-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 10 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "B.Cu")
		(at 95.885 141.605)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP18"
			(at 0 2.148 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VDD_TEMP"
			(at 0 -2.25 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.5x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "B.Cu" "B.Mask")
			(net 17 "Net-(JP5-C)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "B.Cu")
		(at 91.44 137.795 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP5"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "Vdd_Temp"
			(at 0 -1.9 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "power_amp_interface")
		(sheetfile "power_amp_interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 17 "Net-(JP5-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 10 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(layer "B.Cu")
		(at 145.415 95.25 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP6"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "Src_SEL"
			(at 0 -1.9 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(pad "1" smd custom
			(at -1.3 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 76 "Net-(JP6-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 10 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 145.415 101.6 90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP9"
			(at 0 1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "MODE1_SEL"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Source_Select")
		(sheetfile "ptt_interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 90)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 107 "USRP_MODE_1")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 109 "MODE_1")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 90)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 4 "DIO_MODE_TTL1")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(gr_line
		(start 63.5 139.7)
		(end 63.5 69.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 69.85 146.05)
		(end 63.5 139.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.1 146.05)
		(end 69.85 146.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.45 69.85)
		(end 171.45 139.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 69.85 63.5)
		(end 63.5 69.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.45 139.7)
		(end 165.1 146.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.1 63.5)
		(end 69.85 63.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.1 63.5)
		(end 171.45 69.85)
		(layer "Edge.Cuts")
	)
	(gr_text "Node_Control_V3_RevA, Sept 2025"
		(at 137.795 144.78 0)
		(layer "B.SilkS")
	)
	(gr_text "MODE SELECT\n1 - USRP\n3 - MCU"
		(at 154.94 98.425 90)
		(layer "B.SilkS")
	)
	(gr_text "ADC_TEMP\nVDD"
		(at 94.234 141.605 0)
		(layer "B.SilkS")
	)
	(gr_text "PTT"
		(at 144.145 89.535 90)
		(layer "B.SilkS")
	)
	(gr_text "PTT SELECT\n1 - USRP\n3 - MCU"
		(at 142.24 89.535 0)
		(layer "B.SilkS")
	)
	(gr_text "MODE_0"
		(at 152.146 103.505 90)
		(layer "B.SilkS")
	)
	(gr_text "MODE_1"
		(at 144.145 101.6 90)
		(layer "B.SilkS")
	)
	(gr_text "MODE_SEL\nVDD"
		(at 145.415 98.425 0)
		(layer "B.SilkS")
	)
	(gr_text "ADC_RF0\nVDD"
		(at 130.81 135.89 90)
		(layer "B.SilkS")
	)
	(gr_text "ADC_RF1\nVDD"
		(at 146.05 135.89 90)
		(layer "B.SilkS")
	)
	(gr_text "+5V"
		(at 100.965 104.775 90)
		(layer "F.SilkS")
	)
	(gr_text "LNA Supply"
		(at 128.905 70.485 0)
		(layer "F.SilkS")
	)
	(gr_text "CASE"
		(at 81.915 144.145 0)
		(layer "F.SilkS")
	)
	(gr_text "+24V"
		(at 88.9 68.58 0)
		(layer "F.SilkS")
	)
	(gr_text "INT Temp Monitor"
		(at 80.645 145.796 0)
		(layer "F.SilkS")
	)
	(gr_text "XFER SW"
		(at 90.805 67.31 0)
		(layer "F.SilkS")
	)
	(gr_text "RF1_3"
		(at 149.225 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "2-~{PA_PTT}"
		(at 98.298 128.27 90)
		(layer "F.SilkS")
	)
	(gr_text "+3V3"
		(at 88.265 91.567 90)
		(layer "F.SilkS")
	)
	(gr_text "REV"
		(at 137.795 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 170.18 99.695 90)
		(layer "F.SilkS")
	)
	(gr_text "EXT Temp Monitor"
		(at 104.14 145.796 0)
		(layer "F.SilkS")
	)
	(gr_text "0-~{LNA_PTT}"
		(at 93.98 87.503 90)
		(layer "F.SilkS")
	)
	(gr_text "FWD"
		(at 100.33 123.825 0)
		(layer "F.SilkS")
	)
	(gr_text "GPO3"
		(at 146.685 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 170.18 83.82 90)
		(layer "F.SilkS")
	)
	(gr_text "GPO5"
		(at 154.305 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "D12"
		(at 155.575 136.652 0)
		(layer "F.SilkS")
	)
	(gr_text "D13"
		(at 159.258 136.652 0)
		(layer "F.SilkS")
	)
	(gr_text "SP4T0\nTTL1"
		(at 103.505 116.205 90)
		(layer "F.SilkS")
	)
	(gr_text "SP4T RX\nSWITCHES"
		(at 96.52 106.68 90)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 170.18 80.645 90)
		(layer "F.SilkS")
	)
	(gr_text "USRP GPIO Interface"
		(at 164.465 90.17 90)
		(layer "F.SilkS")
	)
	(gr_text "PA"
		(at 103.505 144.145 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 170.18 77.47 90)
		(layer "F.SilkS")
	)
	(gr_text "SP4T1\nTTL0"
		(at 103.505 104.775 90)
		(layer "F.SilkS")
	)
	(gr_text "~{XFER}"
		(at 95.25 90.17 90)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 154.94 100.965 90)
		(layer "F.SilkS")
	)
	(gr_text "REV"
		(at 100.33 130.175 0)
		(layer "F.SilkS")
	)
	(gr_text "LNA1"
		(at 134.62 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "LNA2"
		(at 130.81 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 142.875 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 170.18 90.17 90)
		(layer "F.SilkS")
	)
	(gr_text "#4x4"
		(at 73.025 66.167 0)
		(layer "F.SilkS")
	)
	(gr_text "TX/D1"
		(at 131.318 117.856 0)
		(layer "F.SilkS")
	)
	(gr_text "SP4T0\nTTL0"
		(at 103.505 112.395 90)
		(layer "F.SilkS")
	)
	(gr_text "RX/D0"
		(at 135.128 117.856 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 116.713 66.04 90)
		(layer "F.SilkS")
	)
	(gr_text "USRP GPIO - DIO"
		(at 147.955 70.485 0)
		(layer "F.SilkS")
	)
	(gr_text "RF0_2"
		(at 130.175 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "+5V"
		(at 81.788 136.144 0)
		(layer "F.SilkS")
	)
	(gr_text "VBUS"
		(at 82.931 83.82 90)
		(layer "F.SilkS")
	)
	(gr_text "RF1_1"
		(at 141.605 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "LNA0"
		(at 138.43 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "GPO4"
		(at 150.495 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 170.18 93.345 90)
		(layer "F.SilkS")
	)
	(gr_text "HIGH \nVSWR"
		(at 109.22 121.285 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 170.18 96.52 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 123.19 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "SP4T1\nTTL1"
		(at 103.505 108.585 90)
		(layer "F.SilkS")
	)
	(gr_text "FWD"
		(at 122.555 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "COMP"
		(at 99.695 144.145 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 100.965 108.585 90)
		(layer "F.SilkS")
	)
	(gr_text "RF1_2"
		(at 145.415 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "+12V"
		(at 119.38 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "RF0_1"
		(at 126.365 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 153.035 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "RF Power\nMonitor"
		(at 154.94 141.224 0)
		(layer "F.SilkS")
	)
	(gr_text "GPI7"
		(at 158.115 65.86 0)
		(layer "F.SilkS")
	)
	(gr_text "+5V"
		(at 109.855 137.795 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 107.315 144.145 0)
		(layer "F.SilkS")
	)
	(gr_text "RF0_3"
		(at 133.985 145.415 0)
		(layer "F.SilkS")
	)
	(gr_text "1-~{XFER_PTT}"
		(at 91.313 82.677 90)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 170.18 86.995 90)
		(layer "F.SilkS")
	)
	(gr_text "NOTIFY"
		(at 162.433 75.565 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 170.18 102.87 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 92.71 68.58 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 78.105 136.144 0)
		(layer "F.SilkS")
	)
	(gr_text "LNA3"
		(at 127 65.86 0)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(layer "B.SilkS")
		(pts
			(xy 165.1 69.85) (xy 69.85 69.85)
		)
		(height -6.35)
		(gr_text "3750.0000 mils"
			(at 117.475 75.1 0)
			(layer "B.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "B.SilkS")
		(pts
			(xy 69.85 63.5) (xy 69.85 146.05)
		)
		(height -8.89)
		(gr_text "3250.0000 mils"
			(at 77.64 104.775 90)
			(layer "B.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "B.SilkS")
		(pts
			(xy 69.85 69.85) (xy 69.85 139.7)
		)
		(height -6.35)
		(gr_text "2750.0000 mils"
			(at 75.1 104.775 90)
			(layer "B.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "B.SilkS")
		(pts
			(xy 171.45 69.85) (xy 63.5 69.85)
		)
		(height -9.305)
		(gr_text "4250.0000 mils"
			(at 117.475 78.055 0)
			(layer "B.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 63.5 69.85) (xy 171.45 69.85)
		)
		(height -13.97)
		(gr_text "4250.0000 mils"
			(at 117.475 54.73 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 165.1 69.85) (xy 69.85 69.85)
		)
		(height 9.525)
		(gr_text "3750.0000 mils"
			(at 117.475 59.175 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 69.85 69.85) (xy 69.85 139.7)
		)
		(height 12.7)
		(gr_text "2750.0000 mils"
			(at 56 104.775 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 69.85 146.05) (xy 69.85 63.5)
		)
		(height -19.05)
		(gr_text "3250.0000 mils"
			(at 49.65 104.775 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 14)
		(net_name "+28V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 74.93 96.52) (xy 78.105 96.52) (xy 78.74 97.155) (xy 78.74 102.87) (xy 74.93 102.87)
			)
		)
	)
	(zone
		(net 43)
		(net_name "PA_28V_SEND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.635)
		)
		(polygon
			(pts
				(xy 82.55 121.285) (xy 85.805 121.285) (xy 85.805 124.265) (xy 78.105 124.265) (xy 78.105 121.92)
				(xy 81.915 121.92)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/power_amp_interface/PA_28V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.635)
		)
		(polygon
			(pts
				(xy 69.85 122.555) (xy 72.39 119.38) (xy 74.295 119.38) (xy 74.295 124.079) (xy 69.85 124.079)
			)
		)
	)
	(zone
		(net 128)
		(net_name "PA_28V_RTN")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.44 121.285) (xy 94.615 121.285) (xy 94.615 113.665) (xy 91.44 113.665) (xy 91.44 110.49)
				(xy 87.63 110.49) (xy 87.63 124.46) (xy 91.44 124.46)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 165.1 63.5) (xy 69.85 63.5) (xy 63.5 69.85) (xy 63.5 139.7) (xy 69.85 146.05) (xy 165.1 146.05)
				(xy 171.45 139.7) (xy 171.45 69.85)
			)
		)
	)
)
