<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="5.588" y1="77.47" x2="32.492" y2="77.47" width="0" layer="20"/>
<wire x1="32.492" y1="77.47" x2="32.492" y2="100" width="0" layer="20"/>
<wire x1="32.492" y1="100" x2="5.588" y2="100" width="0" layer="20"/>
<wire x1="5.588" y1="100" x2="5.588" y2="77.47" width="0" layer="20"/>
<text>Crystal</text>
<text>Element18592</text>
<text>The Mod Shop</text>
<text>4gb NAND Adapter</text>
<text>REV. B</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Wuerth_Elektronik_eiCan_FPC_Connectors__Flat_Flexible_Cable">
<description>&lt;BR&gt;Würth Elektronik -- Electronic Interconnect &amp; Electromechanical Solutions&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com"&gt;http://www.we-online.com&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:pm.hotline@we-online.de"&gt;pm.hotline@we-online.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Version 1.0,   June 16-th 2010
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="68611014422">
<description>&lt;b&gt;WR-FPC 1.00mm SMT ZIF Horizontal Bottom Contact, 10 Pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0603K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="13" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="16" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="4+6" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="2" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="1" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="3" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="11" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="14" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="7" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="K1" library="Wuerth_Elektronik_eiCan_FPC_Connectors__Flat_Flexible_Cable" package="68611014422" value="68611014422"/>
</elements>
<signals>
<signal name="N$2">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$1">
</signal>
<signal name="N$11">
</signal>
<signal name="N$3">
</signal>
<signal name="N$7">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
</signals>
</board>
</drawing>
</eagle>
