(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 40)
    (no_connects 0)
    (area 144.197599 85.034 206.12 114.302402)
    (thickness 1.6)
    (drawings 50)
    (tracks 266)
    (zones 0)
    (modules 13)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 1.2192)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 2.9 2.55)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 VCCIO)
  (net 6 "Net-(P1-Pad4)")
  (net 7 CBUS0)
  (net 8 CBUS1)
  (net 9 CBUS2)
  (net 10 CBUS3)
  (net 11 RESET)
  (net 12 TXD)
  (net 13 RXD)
  (net 14 RTS)
  (net 15 CTS)
  (net 16 DTR)
  (net 17 DSR)
  (net 18 DCD)
  (net 19 "Net-(R2-Pad1)")
  (net 20 "Net-(R3-Pad1)")
  (net 21 RI)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net CBUS0)
    (add_net CBUS1)
    (add_net CBUS2)
    (add_net CBUS3)
    (add_net CTS)
    (add_net DCD)
    (add_net DSR)
    (add_net DTR)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net RESET)
    (add_net RI)
    (add_net RTS)
    (add_net RXD)
    (add_net TXD)
    (add_net VCC)
    (add_net VCCIO)
  )
  (net_class Huge ""
    (clearance 0.1524)
    (trace_width 1.2192)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class Large ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class Larger ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A8541A)
    (at 155.575 111.76 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.025 -0.64 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.675 1.46 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 57A853ED)
    (at 155.575 93.98)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at -4.075 1.27) (layer F.SilkS))
    (fp_text value 4.7µF (at -4.925 -1.18) (layer F.SilkS))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A85475)
    (at 160.02 98.425 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.02 -0.625 180) (layer F.SilkS))
    (fp_text value 47pF (at 1.07 1.475 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A86371)
    (at 160.02 107.315 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 1.67 -1.535 180) (layer F.SilkS))
    (fp_text value 47pF (at 1.02 1.465 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A86422)
    (at 179.1 99.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.7 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.65 1.45 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VCCIO))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_Mini-B (layer F.Cu) (tedit 57A881CF)
    (at 149.225 102.87)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P1 (at -2.975 6.23) (layer F.SilkS))
    (fp_text value "MiniUSB B fem." (at 0.625 -6.17) (layer F.SilkS))
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 57A86383)
    (at 162.56 111.76 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -1.39 -2.46 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 25.4 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 CBUS0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 CBUS1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 CBUS2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 CBUS3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 RESET))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCCIO))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 57A85446)
    (at 162.56 93.98 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -1.37 -2.46 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 25.4 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 TXD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RXD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 RTS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 CTS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 DTR))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 DSR))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 DCD))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 RI))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A85496)
    (at 163.195 101.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.095 -0.65 180) (layer F.SilkS))
    (fp_text value 27R (at 1.395 1.45 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A863AD)
    (at 163.195 104.14 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1.805 -1.51 180) (layer F.SilkS))
    (fp_text value 27R (at 3.445 0.54 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SSOP-20 (layer F.Cu) (tedit 57A86405)
    (at 170.815 102.87 180)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U1 (at -4.385 1.17 270) (layer F.SilkS))
    (fp_text value FT231XS (at 4.315 0.02 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.921 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 DTR))
    (pad 2 smd rect (at -2.286 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 RTS))
    (pad 3 smd rect (at -1.6256 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 VCCIO))
    (pad 4 smd rect (at -0.9652 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 RXD))
    (pad 5 smd rect (at -0.3302 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 RI))
    (pad 6 smd rect (at 0.3302 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.9906 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 DSR))
    (pad 8 smd rect (at 1.6256 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 18 DCD))
    (pad 9 smd rect (at 2.286 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 CTS))
    (pad 10 smd rect (at 2.921 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 CBUS2))
    (pad 11 smd rect (at 2.921 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad1)"))
    (pad 12 smd rect (at 2.286 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R2-Pad1)"))
    (pad 13 smd rect (at 1.6256 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 VCCIO))
    (pad 14 smd rect (at 0.9906 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 RESET))
    (pad 15 smd rect (at 0.3302 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 16 smd rect (at -0.3302 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at -0.9652 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 CBUS1))
    (pad 18 smd rect (at -1.6256 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 CBUS0))
    (pad 19 smd rect (at -2.286 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 CBUS3))
    (pad 20 smd rect (at -2.921 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 TXD))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A8643A)
    (at 179.1 106.3 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.8 -1.5 180) (layer F.SilkS))
    (fp_text value 100K (at 1.05 1.45 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 VCCIO))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 RESET))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Logo:DeuxVis_big (layer B.Cu) (tedit 0)
    (at 166.878 102.616 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text CB0 (at 162.56 109.4105) (layer F.SilkS))
  (gr_text CB1 (at 165.1 109.4105) (layer F.SilkS))
  (gr_text CB2 (at 167.64 109.4105) (layer F.SilkS))
  (gr_text CB3 (at 170.18 109.4105) (layer F.SilkS))
  (gr_text RST (at 172.72 109.4105) (layer F.SilkS))
  (gr_text GND (at 175.26 109.4105) (layer F.SilkS))
  (gr_text 3.3V (at 177.8 109.4105) (layer F.SilkS))
  (gr_text 5V (at 180.4035 109.347) (layer F.SilkS))
  (gr_text RI (at 180.34 96.393) (layer F.SilkS))
  (gr_text DCD (at 177.8 96.393) (layer F.SilkS))
  (gr_text DSR (at 175.26 96.393) (layer F.SilkS))
  (gr_text DTR (at 172.72 96.393) (layer F.SilkS))
  (gr_text CTS (at 170.18 96.393) (layer F.SilkS))
  (gr_text RTS (at 167.64 96.393) (layer F.SilkS))
  (gr_text RXD (at 165.1 96.393) (layer F.SilkS))
  (gr_text TXD (at 162.56 96.393) (layer F.SilkS))
  (gr_text + (at 151.7015 93.98) (layer F.SilkS))
  (gr_text CB3 (at 170.18 109.4105) (layer B.SilkS))
  (gr_text CB2 (at 167.64 109.4105) (layer B.SilkS))
  (gr_text CB1 (at 165.1 109.4105) (layer B.SilkS))
  (gr_text CB0 (at 162.56 109.4105) (layer B.SilkS))
  (gr_text RST (at 172.72 109.4105) (layer B.SilkS))
  (gr_text GND (at 175.26 109.4105) (layer B.SilkS))
  (gr_text 3.3V (at 177.8 109.4105) (layer B.SilkS))
  (gr_text 5V (at 180.4035 109.347) (layer B.SilkS))
  (gr_text RI (at 180.34 96.393) (layer B.SilkS))
  (gr_text DCD (at 177.8 96.393) (layer B.SilkS))
  (gr_text DSR (at 175.26 96.393) (layer B.SilkS))
  (gr_text DTR (at 172.72 96.393) (layer B.SilkS))
  (gr_text CTS (at 170.18 96.393) (layer B.SilkS))
  (gr_text RTS (at 167.64 96.393) (layer B.SilkS))
  (gr_text RXD (at 165.1 96.393) (layer B.SilkS))
  (gr_text TXD (at 162.56 96.393) (layer B.SilkS))
  (gr_text https://github.com/DeuxVis/FT231X_breakout (at 159.639 102.87 90) (layer B.SilkS))
  (gr_text "V1.0 - 2016 - DeuxVis" (at 154.305 102.87 90) (layer B.SilkS))
  (gr_text "FT231X breakout" (at 152.019 102.6795 90) (layer B.SilkS))
  (gr_text "D+ →" (at 156.972 104.14) (layer F.SilkS))
  (gr_text "D- →" (at 156.972 102.5525) (layer F.SilkS))
  (gr_text " ←VCC" (at 156.6545 101.6635) (layer F.SilkS))
  (gr_text "GND →" (at 155.448 105.41) (layer F.SilkS))
  (dimension 37.084 (width 0.3) (layer Cmts.User)
    (gr_text "37,084 mm" (at 163.83 86.534) (layer Cmts.User))
    (feature1 (pts (xy 182.372 91.948) (xy 182.372 85.184)))
    (feature2 (pts (xy 145.288 91.948) (xy 145.288 85.184)))
    (crossbar (pts (xy 145.288 87.884) (xy 182.372 87.884)))
    (arrow1a (pts (xy 182.372 87.884) (xy 181.245496 88.470421)))
    (arrow1b (pts (xy 182.372 87.884) (xy 181.245496 87.297579)))
    (arrow2a (pts (xy 145.288 87.884) (xy 146.414504 88.470421)))
    (arrow2b (pts (xy 145.288 87.884) (xy 146.414504 87.297579)))
  )
  (dimension 37.084 (width 0.3) (layer Cmts.User)
    (gr_text "1,4600 in" (at 163.83 89.582) (layer Cmts.User))
    (feature1 (pts (xy 182.372 91.948) (xy 182.372 88.232)))
    (feature2 (pts (xy 145.288 91.948) (xy 145.288 88.232)))
    (crossbar (pts (xy 145.288 90.932) (xy 182.372 90.932)))
    (arrow1a (pts (xy 182.372 90.932) (xy 181.245496 91.518421)))
    (arrow1b (pts (xy 182.372 90.932) (xy 181.245496 90.345579)))
    (arrow2a (pts (xy 145.288 90.932) (xy 146.414504 91.518421)))
    (arrow2b (pts (xy 145.288 90.932) (xy 146.414504 90.345579)))
  )
  (dimension 21.844 (width 0.3) (layer Cmts.User)
    (gr_text "0,8600 in" (at 196.422 102.87 270) (layer Cmts.User))
    (feature1 (pts (xy 182.372 113.792) (xy 197.772 113.792)))
    (feature2 (pts (xy 182.372 91.948) (xy 197.772 91.948)))
    (crossbar (pts (xy 195.072 91.948) (xy 195.072 113.792)))
    (arrow1a (pts (xy 195.072 113.792) (xy 194.485579 112.665496)))
    (arrow1b (pts (xy 195.072 113.792) (xy 195.658421 112.665496)))
    (arrow2a (pts (xy 195.072 91.948) (xy 194.485579 93.074504)))
    (arrow2b (pts (xy 195.072 91.948) (xy 195.658421 93.074504)))
  )
  (dimension 21.844 (width 0.3) (layer Cmts.User)
    (gr_text "21,844 mm" (at 199.47 102.87 270) (layer Cmts.User))
    (feature1 (pts (xy 182.372 113.792) (xy 200.82 113.792)))
    (feature2 (pts (xy 182.372 91.948) (xy 200.82 91.948)))
    (crossbar (pts (xy 198.12 91.948) (xy 198.12 113.792)))
    (arrow1a (pts (xy 198.12 113.792) (xy 197.533579 112.665496)))
    (arrow1b (pts (xy 198.12 113.792) (xy 198.706421 112.665496)))
    (arrow2a (pts (xy 198.12 91.948) (xy 197.533579 93.074504)))
    (arrow2b (pts (xy 198.12 91.948) (xy 198.706421 93.074504)))
  )
  (dimension 17.78 (width 0.3) (layer Cmts.User)
    (gr_text "17,780 mm" (at 187.96 102.616 270) (layer Cmts.User))
    (feature1 (pts (xy 180.34 111.76) (xy 192.184 111.76)))
    (feature2 (pts (xy 180.34 93.98) (xy 192.184 93.98)))
    (crossbar (pts (xy 189.484 93.98) (xy 189.484 111.76)))
    (arrow1a (pts (xy 189.484 111.76) (xy 188.897579 110.633496)))
    (arrow1b (pts (xy 189.484 111.76) (xy 190.070421 110.633496)))
    (arrow2a (pts (xy 189.484 93.98) (xy 188.897579 95.106504)))
    (arrow2b (pts (xy 189.484 93.98) (xy 190.070421 95.106504)))
  )
  (dimension 17.78 (width 0.3) (layer Cmts.User)
    (gr_text "0,7000 in" (at 184.404 102.108 270) (layer Cmts.User))
    (feature1 (pts (xy 180.34 111.76) (xy 188.628 111.76)))
    (feature2 (pts (xy 180.34 93.98) (xy 188.628 93.98)))
    (crossbar (pts (xy 185.928 93.98) (xy 185.928 111.76)))
    (arrow1a (pts (xy 185.928 111.76) (xy 185.341579 110.633496)))
    (arrow1b (pts (xy 185.928 111.76) (xy 186.514421 110.633496)))
    (arrow2a (pts (xy 185.928 93.98) (xy 185.341579 95.106504)))
    (arrow2b (pts (xy 185.928 93.98) (xy 186.514421 95.106504)))
  )
  (gr_line (start 182.372 91.948) (end 145.288 91.948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 113.792) (end 182.372 91.948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.288 113.792) (end 182.372 113.792) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.288 91.948) (end 145.288 113.792) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 182.372 113.792) (xy 145.288 113.792) (xy 145.288 91.948) (xy 182.372 91.948)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 182.372 113.792) (xy 145.288 113.792) (xy 145.288 91.948) (xy 182.372 91.948)
      )
    )
  )
)
