<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="16.51" y1="33.1058625" x2="16.51" y2="24.65605" width="0" layer="20"/>
<wire x1="16.51" y1="24.65605" x2="18.30605" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="18.30605" y1="22.86" x2="34.82091875" y2="22.86" width="0" layer="20"/>
<wire x1="34.82091875" y1="22.86" x2="36.81" y2="24.84908125" width="0" layer="20" curve="90"/>
<wire x1="36.81" y1="24.84908125" x2="36.81" y2="33.120378125" width="0" layer="20"/>
<wire x1="36.81" y1="33.120378125" x2="35.081378125" y2="34.849" width="0" layer="20" curve="90"/>
<wire x1="35.081378125" y1="34.849" x2="18.2531375" y2="34.849" width="0" layer="20"/>
<wire x1="18.2531375" y1="34.849" x2="16.51" y2="33.1058625" width="0" layer="20" curve="90"/>
<text>Rx</text>
<text>Tx</text>
<text>GP0</text>
<text>GP2</text>
<text>GND</text>
<text>CH</text>
<text>RST</text>
<text>3.3</text>
<text>ESP8266 Breadboard Adapter</text>
<text>C:/Users/Douglas/Desktop/Untitled-1.bmp</text>
<text>C:/Users/Douglas/Desktop/Untitled-1.bmp</text>
<text>C:/Users/Douglas/Desktop/Untitled-1.bmp</text>
<text>Douglas Reilly 
2k17</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="adafruit" package="2X04" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3.3V">
<contactref element="JP1" pad="7"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="CH_PD">
<contactref element="JP1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="GPIO2">
<contactref element="JP1" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GPIO0">
<contactref element="JP1" pad="6"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="JP1" pad="8"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
