(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 29)
    (zones 0)
    (modules 5)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J4-Pad1)")
  (net 9 "Net-(J4-Pad2)")
  (net 10 "Net-(J4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
  )
  (module myDevices:PinHeader_1x03_P5.08mm_Vertical (layer B.Cu) (tedit 5E39C537)
    (at 177.546 131.826 90)
    (fp_text reference J1 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 -12.49 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -5.08) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -5.08 90) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -10.16 90) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myDevices:PinHeader_1x02_P5.08mm_Vertical (layer B.Cu) (tedit 5E39C4C9)
    (at 144.526 131.826 90)
    (fp_text reference J2 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 -7.41 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -2.54) (layer B.Fab) hide)
    (pad 2 thru_hole circle (at 0 -5.08 90) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myDevices:PinHeader_1x02_P5.08mm_Vertical (layer B.Cu) (tedit 5E39C4C9)
    (at 139.446 114.046 270)
    (fp_text reference J3 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 -7.41 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -2.54) (layer B.Fab) hide)
    (pad 2 thru_hole circle (at 0 -5.08 270) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myDevices:PinHeader_1x03_P5.08mm_Vertical (layer B.Cu) (tedit 5E39C537)
    (at 167.386 114.046 270)
    (fp_text reference J4 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 -12.49 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -5.08) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at 0 -5.08 270) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad2)"))
    (pad 3 thru_hole circle (at 0 -10.16 270) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myDevices:Socket_Noval_04 (layer F.Cu) (tedit 5E39D494)
    (at 155.956 122.784)
    (fp_text reference V1 (at 0 -12.045) (layer F.SilkS) hide)
    (fp_text value Noval_Socket_02 (at 0 12.045) (layer F.Fab))
    (pad 10 thru_hole circle (at 0 0) (size 6 6) (drill 3.5) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (pad 3 thru_hole oval (at -5.583959 -7.685661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 4 thru_hole oval (at -9.035036 -2.935661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 5 thru_hole oval (at -9.035036 2.935661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 6 thru_hole oval (at -5.583959 7.685661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 7 thru_hole oval (at 0 9.5) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 8 thru_hole oval (at 5.583959 7.685661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 9 thru_hole oval (at 9.035036 2.935661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 1 thru_hole oval (at 5.583959 -7.685661) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 0 -9.5) (size 3 3) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
  )
  (gr_arc (start 137.414 113.284) (end 137.414 112.014) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.414 132.588) (end 136.144 132.588) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 179.578 113.284) (end 180.848 113.284) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 179.578 132.588) (end 179.578 133.858) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_text 3 (at 144.526 117.094) (layer F.SilkS))
  (gr_text 4 (at 139.446 117.094) (layer F.SilkS))
  (gr_text 5 (at 139.446 128.778) (layer F.SilkS))
  (gr_text 6 (at 144.526 128.778) (layer F.SilkS))
  (gr_text 7 (at 167.513 128.778) (layer F.SilkS))
  (gr_text 8 (at 172.593 128.778) (layer F.SilkS))
  (gr_text 9 (at 177.673 128.778) (layer F.SilkS))
  (gr_text 2 (at 167.386 117.094) (layer F.SilkS))
  (gr_text 1 (at 172.466 117.094) (layer F.SilkS))
  (gr_text C (at 177.546 117.094) (layer F.SilkS))
  (gr_arc (start 155.956 137.414) (end 166.37 112.014) (angle -44.58725832) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.956 108.458) (end 145.542 133.858) (angle -44.58725832) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.414 112.014) (end 145.542 112.014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.144 132.588) (end 136.144 113.284) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.414 133.858) (end 145.542 133.858) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 179.578 112.014) (end 166.37 112.014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.848 132.588) (end 180.848 113.284) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 179.578 133.858) (end 166.37 133.858) (layer Edge.Cuts) (width 0.1))
  (gr_text "Noval breadboard adapter\n20_06_0002\nBjørner Sandom" (at 179.197 121.92) (layer B.SilkS))
)
