(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 51)
    (no_connects 0)
    (area 124.383799 50.323799 209.376201 116.526201)
    (thickness 1.6)
    (drawings 6)
    (tracks 224)
    (zones 0)
    (modules 17)
    (nets 40)
  )
  (page USLetter)
  (title_block
    (company "Released under the CERN Open Hardware License v1.2")
    (comment 1 "jenner@wickerbox.net - http://wickerbox.net")
    (comment 2 "Designed by Jenner at Wickerbox Electronics")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 /~RESET)
  (net 2 /FTDI_RESET)
  (net 3 GND)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 +5V)
  (net 7 /D0)
  (net 8 /D1)
  (net 9 "Net-(J2-Pad5)")
  (net 10 /D11)
  (net 11 /D13)
  (net 12 /D12)
  (net 13 /D2)
  (net 14 /D3)
  (net 15 /D4)
  (net 16 /D5)
  (net 17 /D6)
  (net 18 /D7)
  (net 19 /D8)
  (net 20 /D9)
  (net 21 /D10)
  (net 22 "Net-(LED1-Pad2)")
  (net 23 "Net-(J5-Pad3)")
  (net 24 "Net-(J5-Pad4)")
  (net 25 "Net-(J5-Pad5)")
  (net 26 "Net-(J5-Pad6)")
  (net 27 "Net-(J5-Pad7)")
  (net 28 "Net-(J5-Pad8)")
  (net 29 "Net-(J5-Pad9)")
  (net 30 "Net-(J5-Pad10)")
  (net 31 "Net-(U2-Pad19)")
  (net 32 "Net-(U2-Pad20)")
  (net 33 "Net-(U2-Pad22)")
  (net 34 "Net-(U2-Pad23)")
  (net 35 "Net-(U2-Pad24)")
  (net 36 "Net-(U2-Pad25)")
  (net 37 "Net-(U2-Pad26)")
  (net 38 "Net-(U2-Pad27)")
  (net 39 "Net-(U2-Pad28)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /FTDI_RESET)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
  )
  (module Wickerlib:TQFP-32-7x7MM-P0.8MM (layer F.Cu) (tedit 587459A6)
    (at 166.624 82.296)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 0) (layer F.Fab))
    (fp_text value ATMEGA328 (at 0 6.05) (layer F.Fab) hide)
    (fp_text user %R (at 4.953 -4.386 180) (layer F.SilkS))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /D3))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /D4))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /D5))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /D6))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /D7))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /D8))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /D9))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /D10))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /D12))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /D11))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /D13))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /D0))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /D1))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /D2))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 171.196 65.278 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C1 (at 0.09 0.04 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /FTDI_RESET))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 140.97 71.06 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C3 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 22pF (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 133.97 76.47 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C4 (at 0.09 0.04 90) (layer F.Fab))
    (fp_text value 22pF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 137.55 59.33 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C5 (at 0.09 0.04 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 145.94 59.2 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C7 (at 0.09 0.04 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 133.04 59.27 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C8 (at 0.09 0.04 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 141.42 59.2 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C9 (at 0.09 0.04 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x06 (layer F.Cu) (tedit 58155E08)
    (at 171.21 57.66 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at -0.01 6.35 360) (layer F.Fab))
    (fp_text value FTDI (at -2.63 6.86 360) (layer F.Fab) hide)
    (fp_text user %R (at 0.14 -2.74 450) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /FTDI_RESET))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D0))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 +5V))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-2x03 (layer F.Cu) (tedit 589D56B3)
    (at 194.31 58.928 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 1.27 2.54 90) (layer F.Fab))
    (fp_text value ISP-2560 (at 3.556 2.794 180) (layer F.Fab) hide)
    (fp_text user %R (at -0.254 -2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D11))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D13))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D12))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /~RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x10 (layer F.Cu) (tedit 58155EC8)
    (at 152.05 107.79 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 0.1 11.5 180) (layer F.Fab))
    (fp_text value DIGOUT1 (at -3 11 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /D2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D8))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D9))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D10))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D11))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x10 (layer F.Cu) (tedit 58155EC8)
    (at 201.71 73.96)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J5 (at 0.1 11.5 90) (layer F.Fab))
    (fp_text value DIGOUT2 (at -3 11 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D12))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D13))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J5-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J5-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J5-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J5-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J5-Pad10)"))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 159.38 113.52)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference LED1 (at 0.09 0.04) (layer F.Fab))
    (fp_text value AMBER (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(LED1-Pad2)"))
  )
  (module Wickerlib:RLC-0805-SMD (layer F.Cu) (tedit 57904162)
    (at 181.102 65.024 270)
    (descr "Capacitor SMD RLC-0805-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0805-SMD")
    (attr smd)
    (fp_text reference R1 (at 0 0 450) (layer F.Fab))
    (fp_text value 10K (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 3.048 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 164.09 113.49 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R2 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /D7))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(LED1-Pad2)"))
  )
  (module Wickerlib:SWITCH-OMRON-MOMENTARY-SMD-B3U-1000P (layer F.Cu) (tedit 57904124)
    (at 176.53 62.738 270)
    (descr SW-B3F-10XX)
    (tags "Omron B3F-10xx")
    (fp_text reference S1 (at 1.778 0 270) (layer F.Fab))
    (fp_text value RESET (at 1.524 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.286 270) (layer F.SilkS))
    (pad 2 smd rect (at 3.4 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
    (pad 1 smd rect (at 0 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Wickerlib:CRYSTAL-CTS-4SMD (layer F.Cu) (tedit 58156A29)
    (at 141.49 75.75 180)
    (fp_text reference X1 (at 0 0 180) (layer F.Fab))
    (fp_text value "16MHz 18pF" (at 0 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -3 180) (layer F.SilkS))
    (pad 3 smd rect (at 2.1844 -1.4732 180) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at -2.286 -1.4732 180) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 2.1844 1.016 180) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.286 1.016 180) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (gr_line (start 126.36 50.41) (end 126.36 50.4) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 124.46 50.41) (end 126.36 50.41) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 124.46 116.45) (end 124.46 50.41) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 209.3 116.45) (end 124.46 116.45) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 209.3 50.41) (end 209.3 116.45) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 125.79 50.41) (end 209.3 50.41) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.98 50.8) (xy 208.93 50.67) (xy 208.94 116.06) (xy 208.94 116.24) (xy 126.01 116.01)
      )
    )
  )
  (zone (net 6) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.11 50.86) (xy 208.75 50.67) (xy 208.82 116.12) (xy 125.62 115.73) (xy 126.07 50.89)
      )
    )
  )
)
