(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 228)
    (no_connects 2)
    (area 134.565714 57.3508 188.727715 113.025)
    (thickness 1.6)
    (drawings 5)
    (tracks 1272)
    (zones 0)
    (modules 89)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.4)
    (trace_clearance 0.18)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3)
    (user_via 0.6 0.4)
    (user_via 0.8 0.5)
    (user_via 1 0.7)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /VCCINT)
  (net 4 /VCCO-1)
  (net 5 +5V)
  (net 6 +2V8)
  (net 7 "Net-(C30-Pad1)")
  (net 8 "Net-(C31-Pad1)")
  (net 9 "Net-(C33-Pad1)")
  (net 10 "Net-(C34-Pad1)")
  (net 11 /VBUS)
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(D2-Pad1)")
  (net 14 /S6_M1)
  (net 15 /S6_CSI_B)
  (net 16 /S6_RDWR)
  (net 17 /S6_M0)
  (net 18 "Net-(P1-Pad2)")
  (net 19 "Net-(P1-Pad3)")
  (net 20 /TDI)
  (net 21 /TCK)
  (net 22 /TDO)
  (net 23 /TMS)
  (net 24 /DONE)
  (net 25 /D-)
  (net 26 /D+)
  (net 27 "Net-(R4-Pad1)")
  (net 28 /CS_FLASH)
  (net 29 "Net-(R7-Pad2)")
  (net 30 "Net-(R8-Pad1)")
  (net 31 /AVR_RESET)
  (net 32 "Net-(R10-Pad2)")
  (net 33 "Net-(R3-Pad2)")
  (net 34 /AVR_MISO)
  (net 35 /AVR_MOSI)
  (net 36 /SCK)
  (net 37 /SS)
  (net 38 /D0)
  (net 39 /CCLK)
  (net 40 /AVR_RX)
  (net 41 /AVR_TX)
  (net 42 /INIT_B)
  (net 43 "Net-(U6-Pad25)")
  (net 44 /D3)
  (net 45 /D2)
  (net 46 /D1)
  (net 47 /PROGRAM_B)
  (net 48 "Net-(U6-Pad36)")
  (net 49 "Net-(U6-Pad37)")
  (net 50 "Net-(U6-Pad38)")
  (net 51 "Net-(U6-Pad39)")
  (net 52 "Net-(U6-Pad40)")
  (net 53 "Net-(U6-Pad41)")
  (net 54 "Net-(U7-Pad38)")
  (net 55 /CLK)
  (net 56 "Net-(U7-Pad74)")
  (net 57 "Net-(U7-Pad144)")
  (net 58 /S6_CCLK)
  (net 59 "Net-(P6-Pad2)")
  (net 60 "Net-(P5-Pad2)")
  (net 61 "Net-(J2-Pad2)")
  (net 62 "Net-(J3-Pad2)")
  (net 63 "Net-(J4-Pad2)")
  (net 64 "Net-(J5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.18)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net /AVR_MISO)
    (add_net /AVR_MOSI)
    (add_net /AVR_RESET)
    (add_net /AVR_RX)
    (add_net /AVR_TX)
    (add_net /CCLK)
    (add_net /CLK)
    (add_net /CS_FLASH)
    (add_net /D+)
    (add_net /D-)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /DONE)
    (add_net /INIT_B)
    (add_net /PROGRAM_B)
    (add_net /S6_CCLK)
    (add_net /S6_CSI_B)
    (add_net /S6_M0)
    (add_net /S6_M1)
    (add_net /S6_RDWR)
    (add_net /SCK)
    (add_net /SS)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /VBUS)
    (add_net /VCCINT)
    (add_net /VCCO-1)
    (add_net GND)
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U6-Pad25)")
    (add_net "Net-(U6-Pad36)")
    (add_net "Net-(U6-Pad37)")
    (add_net "Net-(U6-Pad38)")
    (add_net "Net-(U6-Pad39)")
    (add_net "Net-(U6-Pad40)")
    (add_net "Net-(U6-Pad41)")
    (add_net "Net-(U7-Pad144)")
    (add_net "Net-(U7-Pad38)")
    (add_net "Net-(U7-Pad74)")
  )
  (net_class 3V3 ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class PWR ""
    (clearance 0.25)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.7)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F9213F)
    (at 172.76 107.22 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV2 (at 2.97 -0.15 180) (layer F.SilkS))
    (fp_text value CG0603MLC-05E (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F91ECB)
    (at 172.75 108.71)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.57 0.19) (layer F.SilkS))
    (fp_text value 22 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /D+))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 155.24 73.69 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 155.21 71.1 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 138.53 91.55)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module visionFeet:TQFP-44_10x10mm_p0.8mm-HS (layer F.Cu) (tedit 54130A77)
    (at 160.85 100.22 90)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U6 (at -0.39 1.16 180) (layer F.SilkS))
    (fp_text value ATMEGA32U4-A (at 0 7.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.95 -4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -5.95 -3.2 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.95 -2.4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /D-))
    (pad 4 smd rect (at -5.95 -1.6 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /D+))
    (pad 5 smd rect (at -5.95 -0.8 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -5.95 0 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -5.95 0.8 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /VBUS))
    (pad 8 smd rect (at -5.95 1.6 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /SS))
    (pad 9 smd rect (at -5.95 2.4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /SCK))
    (pad 10 smd rect (at -5.95 3.2 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /AVR_MOSI))
    (pad 11 smd rect (at -5.95 4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /AVR_MISO))
    (pad 12 smd rect (at -4 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /D0))
    (pad 13 smd rect (at -3.2 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /AVR_RESET))
    (pad 14 smd rect (at -2.4 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 15 smd rect (at -1.6 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.8 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C33-Pad1)"))
    (pad 17 smd rect (at 0 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C31-Pad1)"))
    (pad 18 smd rect (at 0.8 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /CCLK))
    (pad 19 smd rect (at 1.6 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /CS_FLASH))
    (pad 20 smd rect (at 2.4 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /AVR_RX))
    (pad 21 smd rect (at 3.2 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /AVR_TX))
    (pad 22 smd rect (at 4 5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 /INIT_B))
    (pad 23 smd rect (at 5.95 4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 5.95 3.2 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C30-Pad1)"))
    (pad 25 smd rect (at 5.95 2.4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U6-Pad25)"))
    (pad 26 smd rect (at 5.95 1.6 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(P6-Pad2)"))
    (pad 27 smd rect (at 5.95 0.8 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(P5-Pad2)"))
    (pad 28 smd rect (at 5.95 0 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 /D3))
    (pad 29 smd rect (at 5.95 -0.8 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /D2))
    (pad 30 smd rect (at 5.95 -1.6 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /D1))
    (pad 31 smd rect (at 5.95 -2.4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /DONE))
    (pad 32 smd rect (at 5.95 -3.2 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /PROGRAM_B))
    (pad 33 smd rect (at 5.95 -4 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R10-Pad2)"))
    (pad 34 smd rect (at 4 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 35 smd rect (at 3.2 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 36 smd rect (at 2.4 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U6-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U6-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U6-Pad38)"))
    (pad 39 smd rect (at 0 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U6-Pad39)"))
    (pad 40 smd rect (at -0.8 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U6-Pad40)"))
    (pad 41 smd rect (at -1.6 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U6-Pad41)"))
    (pad 42 smd rect (at -2.4 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C34-Pad1)"))
    (pad 43 smd rect (at -3.2 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -4 -5.95 180) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C30-Pad1)"))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:TQFP-144_20x20mm_0.5mm_HS (layer F.Cu) (tedit 54130A77)
    (at 149.51 72.57)
    (descr "P/PG-TQFP-144-2, -3, -7 (see MAXIM 21-0087.PDF and 90-0144.PDF)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U7 (at 2.33 -5.91) (layer F.SilkS))
    (fp_text value XC6SLX9-TQFP144 (at 0 13.462) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -10.8 -8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -10.8 -8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -10.8 -7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -10.8 -7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -10.8 -6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -10.8 -6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -10.8 -5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -10.8 -5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -10.8 -4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -10.8 -4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -10.8 -3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -10.8 -3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -10.8 -2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -10.8 -2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -10.8 -1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -10.8 -1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -10.8 -0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -10.8 -0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 19 smd rect (at -10.8 0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 20 smd rect (at -10.8 0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 21 smd rect (at -10.8 1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -10.8 1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -10.8 2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -10.8 2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at -10.8 3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at -10.8 3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at -10.8 4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at -10.8 4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 29 smd rect (at -10.8 5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at -10.8 5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at -10.8 6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 32 smd rect (at -10.8 6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at -10.8 7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at -10.8 7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at -10.8 8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at -10.8 8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 37 smd rect (at -8.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 /PROGRAM_B))
    (pad 38 smd rect (at -8.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U7-Pad38)"))
    (pad 39 smd rect (at -7.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /INIT_B))
    (pad 40 smd rect (at -7.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at -6.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at -6.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 43 smd rect (at -5.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 /SCK))
    (pad 44 smd rect (at -5.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 /AVR_MOSI))
    (pad 45 smd rect (at -4.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 /AVR_MISO))
    (pad 46 smd rect (at -4.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 /D3))
    (pad 47 smd rect (at -3.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /S6_RDWR))
    (pad 48 smd rect (at -3.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /SS))
    (pad 49 smd rect (at -2.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 50 smd rect (at -2.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 51 smd rect (at -1.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 52 smd rect (at -1.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 53 smd rect (at -0.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 54 smd rect (at -0.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 55 smd rect (at 0.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 /AVR_TX))
    (pad 56 smd rect (at 0.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 /CLK))
    (pad 57 smd rect (at 1.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 58 smd rect (at 1.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 59 smd rect (at 2.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /AVR_RX))
    (pad 60 smd rect (at 2.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /S6_M1))
    (pad 61 smd rect (at 3.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /D2))
    (pad 62 smd rect (at 3.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 /D1))
    (pad 63 smd rect (at 4.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 64 smd rect (at 4.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /S6_CSI_B))
    (pad 65 smd rect (at 5.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /D0))
    (pad 66 smd rect (at 5.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 67 smd rect (at 6.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 68 smd rect (at 6.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 69 smd rect (at 7.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /S6_M0))
    (pad 70 smd rect (at 7.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 /S6_CCLK))
    (pad 71 smd rect (at 8.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /DONE))
    (pad 72 smd rect (at 8.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 73 smd rect (at 10.8 8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R8-Pad1)"))
    (pad 74 smd rect (at 10.8 8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U7-Pad74)"))
    (pad 75 smd rect (at 10.8 7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 76 smd rect (at 10.8 7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCO-1))
    (pad 77 smd rect (at 10.8 6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 78 smd rect (at 10.8 6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 79 smd rect (at 10.8 5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 80 smd rect (at 10.8 5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 81 smd rect (at 10.8 4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 82 smd rect (at 10.8 4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 83 smd rect (at 10.8 3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 84 smd rect (at 10.8 3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 85 smd rect (at 10.8 2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 86 smd rect (at 10.8 2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCO-1))
    (pad 87 smd rect (at 10.8 1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 88 smd rect (at 10.8 1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 89 smd rect (at 10.8 0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 90 smd rect (at 10.8 0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 91 smd rect (at 10.8 -0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 92 smd rect (at 10.8 -0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 93 smd rect (at 10.8 -1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 94 smd rect (at 10.8 -1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 95 smd rect (at 10.8 -2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 96 smd rect (at 10.8 -2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 97 smd rect (at 10.8 -3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 98 smd rect (at 10.8 -3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at 10.8 -4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 100 smd rect (at 10.8 -4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 101 smd rect (at 10.8 -5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 102 smd rect (at 10.8 -5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 103 smd rect (at 10.8 -6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCO-1))
    (pad 104 smd rect (at 10.8 -6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 105 smd rect (at 10.8 -7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 106 smd rect (at 10.8 -7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /TDO))
    (pad 107 smd rect (at 10.8 -8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /TMS))
    (pad 108 smd rect (at 10.8 -8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 109 smd rect (at 8.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /TCK))
    (pad 110 smd rect (at 8.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /TDI))
    (pad 111 smd rect (at 7.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 112 smd rect (at 7.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 113 smd rect (at 6.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 114 smd rect (at 6.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 115 smd rect (at 5.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 116 smd rect (at 5.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 117 smd rect (at 4.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 118 smd rect (at 4.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 119 smd rect (at 3.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 120 smd rect (at 3.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 121 smd rect (at 2.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 122 smd rect (at 2.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 123 smd rect (at 1.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 124 smd rect (at 1.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 125 smd rect (at 0.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 126 smd rect (at 0.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 127 smd rect (at -0.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 128 smd rect (at -0.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 129 smd rect (at -1.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 130 smd rect (at -1.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 131 smd rect (at -2.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 132 smd rect (at -2.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 133 smd rect (at -3.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 134 smd rect (at -3.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 135 smd rect (at -4.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 136 smd rect (at -4.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 137 smd rect (at -5.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 138 smd rect (at -5.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 139 smd rect (at -6.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 140 smd rect (at -6.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 141 smd rect (at -7.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 142 smd rect (at -7.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 143 smd rect (at -8.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 144 smd rect (at -8.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U7-Pad144)"))
    (model Housings_QFP.3dshapes/TQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 162.6 79.7 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.73 0.08 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 163.65 90.35 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at -3.46 -0.22 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58F47A2F)
    (at 179.214 84.136)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U4 (at 3.106 -3.446) (layer F.SilkS))
    (fp_text value NCP1117ST33T3G (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58F479B5)
    (at 179.166 74.194)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 3.214 -3.194) (layer F.SilkS))
    (fp_text value AP7361-28E-13 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 6 +2V8))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +2V8))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58F47915)
    (at 179.172 93.526)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.218 -3.466) (layer F.SilkS))
    (fp_text value LD1117S12CTR (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 145.88 89.2 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.73 0.03 90) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 155.09 81.28)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.06 1.43) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 143.16 76.1 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 141.75 81.55)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.02 1.43) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 145.288 81.28)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.012 1.58) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 148.336 78.8)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0.004 -1.57) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 144.272 64.008 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -0.028 -1.432 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 143.14 71.09 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0.09 1.84 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 162.5 73.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0.02 1.38 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCO-1))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 147.65 65.2 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -0.04 -1.51 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 157.87 65.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0.01 1.51 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /VCCO-1))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 140.462 74.676 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 1.25 270) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 147.98 64.02 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 2.6 1.69 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 151.93 64.12)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at -0.02 1.51) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 158.242 78.74 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0 1.25 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /VCCO-1))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 179.77 81.39 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 1.25 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 173.468 80.452 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at -3.082 -0.072 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 179.536 69.782)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 1.25) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 171.638 80.042 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at -3.552 -0.092 270) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 140.462 78.486 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 1.25 270) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 149.098 62.738 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at -0.012 1.198 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 140.462 70.866 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at -0.074 -1.532 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 152.908 62.738)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0.002 -1.288) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 178.47 92.252 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C27 (at 0.802 -1.75 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 178.42 75.236 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 +2V8))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 149.28 80.74)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at -0.03 1.44) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 165.862 101.346 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at -0.006 -1.618 270) (layer B.SilkS))
    (fp_text value 22p (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 141.2 64.27 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0.57 -1.42 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 170.13 101.03 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 0.17 1.15 270) (layer F.SilkS))
    (fp_text value 22p (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58F92575)
    (at 158.54 102.18)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0.01 1.43) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:SOD-123FL-HS (layer F.Cu) (tedit 5889E1F2)
    (at 175.42 99.17 270)
    (fp_text reference D1 (at -0.17 -1.85 270) (layer F.SilkS))
    (fp_text value MBRX120-TP (at 0 2.54 270) (layer F.Fab))
    (pad 1 smd rect (at -1.64 0 270) (size 1.2 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1.64 0 270) (size 1.2 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 11 /VBUS))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 165.6 82.05)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -0.33 1.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 169.164 71.882 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 2.354 2.592 180) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +2V8))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCCO-1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 139.69 102.34 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at -0.08 -2.08 90) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 176.91 62.75 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at -2.61 -1.57 180) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 172.974 66.802)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at -0.034 7.358) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_smd_inductors:inductor_smd_1008 (layer F.Cu) (tedit 58F91F11)
    (at 152.05 105.4 90)
    (descr "Inductor SMD, 1008")
    (fp_text reference L1 (at -2.77 -0.56 180) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.49936 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.143 0 90) (size 1.016 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.143 0 90) (size 1.016 2.54) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C30-Pad1)"))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:USB_Micro-B-HS_RHOLE (layer F.Cu) (tedit 5891155B)
    (at 179.48 106.89)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at 3.18 -3.4) (layer F.SilkS))
    (fp_text value USB-Micro-B (at 0 5.01) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /VBUS))
    (pad 2 smd rect (at -0.65 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 0 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35 90) (size 1.1 1.25) (drill 0.95) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.5 -1.35 90) (size 1.1 1.25) (drill 0.95) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.5 1.35 90) (size 1.55 1.55) (drill 1.25) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.5 1.35 90) (size 1.55 1.55) (drill 1.25) (layers *.Cu *.Mask))
  )
  (module w_conn_jst-ph:b2b-ph-kl (layer F.Cu) (tedit 58F920D9)
    (at 179.55124 67.242 180)
    (descr "JST PH series connector, B2B-PH-KL")
    (fp_text reference P2 (at -7.43876 0.122 180) (layer F.SilkS) hide)
    (fp_text value "CON JST 1x2" (at 0.15124 8.422 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.00076 0 180) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.00076 0 180) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (model walter/conn_jst-ph/b2b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 165.608 62.738 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P3 (at 0.458 -2.448 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /TDI))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /TCK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /TDO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /TMS))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 165.55 79.75 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.2 -0.1 360) (layer F.SilkS))
    (fp_text value MOSFET (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /DONE))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 172.77 105.75)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.02 -1.3) (layer F.SilkS))
    (fp_text value 22 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /D-))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 148.2 99.02 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.77 -0.12 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58AAD9E8)
    (at 163.576 98.552)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0.114 -1.452) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 28 /CS_FLASH))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58F92488)
    (at 180.248 92.252 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.028 1.612 90) (layer B.SilkS))
    (fp_text value 120 (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 1.45 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 143.764 96.774 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.046 -1.234 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 167.55 106.42 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.31 -1.41 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /AVR_RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 159.85 89.15 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 2.22 -1.36 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 169.926 79.756 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 3.266 0.024 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /DONE))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58AAD9E8)
    (at 150.57 91.67)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -0.1 -1.63) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(J2-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 /S6_M1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 159.85 87.7 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 2.37 1.28 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /S6_CSI_B))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58F9208A)
    (at 138.43 85.598 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -0.802 1.12 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /S6_RDWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 165.84 85.92 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at -3.28 -0.01 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58AAD9E8)
    (at 171.1 70.612 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 4.028 0 270) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 1.45 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(J5-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 17 /S6_M0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:Crys_Abracon_ABM3B-4pin_5.0x3.2mmHS (layer F.Cu) (tedit 588AD733)
    (at 146.75 88.95)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3B http://www.abracon.com/Resonators/abm3b.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference U1 (at 0 -2.8) (layer F.SilkS))
    (fp_text value ASFLMB-50.000MHZ-LC-T (at 0 3.81) (layer F.Fab))
    (pad 1 smd rect (at -2 1.2) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 1.2) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2 -1.2) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 33 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -2 -1.2) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (model Crystals.3dshapes/Crystal_SMD_Abracon_ABM3B-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:SOIC-8_3.9x4.9mm_p1.27mm_HS (layer F.Cu) (tedit 54130A77)
    (at 149.062 95.662 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at -0.248 0.242 180) (layer F.SilkS))
    (fp_text value M25P40-VMN6TPBCT-ND (at 0 3.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.9 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /CS_FLASH))
    (pad 2 smd rect (at -2.9 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /AVR_MISO))
    (pad 3 smd rect (at -2.9 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad1)"))
    (pad 4 smd rect (at -2.9 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.9 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /AVR_MOSI))
    (pad 6 smd rect (at 2.9 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /SCK))
    (pad 7 smd rect (at 2.9 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R7-Pad2)"))
    (pad 8 smd rect (at 2.9 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm_HandSoldering (layer F.Cu) (tedit 58CD2E9C)
    (at 172.4 98.48 90)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3 http://www.abracon.com/Resonators/abm3.pdf, hand-soldering, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 5.45 0.89 90) (layer F.SilkS))
    (fp_text value 8MHz (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7625 0 90) (size 3.325 2.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 2.7625 0 90) (size 3.325 2.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 152.14 89.69 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at -0.09 -1.52 270) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 /CLK))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 139.7 105.156 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 0 -1.99 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /AVR_MOSI))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /AVR_MISO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SCK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /AVR_RESET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 150.74 88.97 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.08 -1.25 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 /CLK))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58AAD9E8)
    (at 179 98.6)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV1 (at -0.13 1.68) (layer B.SilkS))
    (fp_text value CG0603MLC-05E (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 163.642 89.1 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at -3.448 -0.11 180) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 58 /S6_CCLK))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 163.8 87.7)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 3.28 0.14) (layer F.SilkS))
    (fp_text value 50 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 /S6_CCLK))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /CCLK))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58AAD9E8)
    (at 161.83 85.9)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -0.37 -1.38) (layer F.SilkS))
    (fp_text value 100 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 /S6_CCLK))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 139.67 99.57 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P5 (at -0.03 -2.06 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /S6_RDWR))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P5-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 147.52 101.61 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P6 (at 1.29 -1.74 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /S6_CSI_B))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P6-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module gj_feet:TP-M (layer F.Cu) (tedit 58F7D7A0)
    (at 139.446 61.976 270)
    (fp_text reference W1 (at -0.026 1.426 270) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2 270) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U7-Pad144)"))
  )
  (module gj_feet:TP-M (layer B.Cu) (tedit 58F7D7A0)
    (at 161.75 80.8)
    (fp_text reference W2 (at -0.1 1.8) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(U7-Pad74)"))
  )
  (module gj_feet:TP-M (layer B.Cu) (tedit 58F7D7A0)
    (at 164.1 94.1 270)
    (fp_text reference W3 (at -1.12 -1.3 360) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2 270) (layer B.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U6-Pad25)"))
  )
  (module gj_feet:TP-M (layer B.Cu) (tedit 58F92455)
    (at 162.47 94.33 90)
    (fp_text reference W4 (at -0.51 -1.88 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2 90) (layer B.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(P6-Pad2)"))
  )
  (module gj_feet:TP-M (layer F.Cu) (tedit 58F91F2C)
    (at 152.12 102.76 90)
    (fp_text reference W6 (at -0.86 -2.35 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U6-Pad41)"))
  )
  (module gj_feet:TP-M (layer F.Cu) (tedit 58F91F37)
    (at 152.85 101.21 90)
    (fp_text reference W7 (at -0.52 -1.31 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U6-Pad40)"))
  )
  (module gj_feet:TP-M (layer F.Cu) (tedit 58F91F71)
    (at 151.52 99.92 90)
    (fp_text reference W8 (at 0.08 -1.39 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U6-Pad39)"))
  )
  (module gj_feet:TP-M (layer F.Cu) (tedit 58F91F4A)
    (at 152.96 99.15 90)
    (fp_text reference W9 (at 0.41 -1.46 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U6-Pad38)"))
  )
  (module gj_feet:TP-M (layer B.Cu) (tedit 58F7D7A0)
    (at 158.33 98.99 270)
    (fp_text reference W10 (at 1.04 2.15 360) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2 270) (layer B.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U6-Pad37)"))
  )
  (module gj_feet:TP-M (layer B.Cu) (tedit 58F7D7A0)
    (at 156.87 98.05 270)
    (fp_text reference W11 (at 0.02 2.33 360) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2 270) (layer B.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U6-Pad36)"))
  )
  (module gj_feet:TP-M (layer F.Cu) (tedit 58F9207A)
    (at 138.45 82.85)
    (fp_text reference W12 (at 1.22 0 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U7-Pad38)"))
  )
  (gr_line (start 185.32 109.66) (end 185.32 60.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.749999 109.66) (end 185.330001 109.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.75 60.2) (end 136.75 109.661107) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.320004 60.2) (end 136.75 60.2) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name /VCCINT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.312 89.712) (xy 184.312 98.602) (xy 179.203482 98.602) (xy 179.203347 88.95) (xy 184.312 88.95)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.708 87.948) (xy 184.312 87.948) (xy 184.312 78.804) (xy 177.708 78.804)
      )
    )
  )
  (zone (net 6) (net_name +2V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.79 78.18) (xy 184.31 78.19) (xy 184.362 70.156) (xy 177.758 70.156)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.79 60.24) (xy 136.78 109.63) (xy 185.3 109.6) (xy 185.29 60.23)
      )
    )
  )
)
