(kicad_pcb (version 3) (host pcbnew "(2013-07-07 BZR 4022)-stable")
  (general
    (links 300)
    (no_connects 0)
    (area 24.225999 62.42574 97.300001 120.274001)
    (thickness 1.6)
    (drawings 56)
    (tracks 967)
    (zones 0)
    (modules 145)
    (nets 100)
  )
  (page A4)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal hide)
    (18 B.Paste user hide)
    (19 F.Paste user hide)
    (20 B.SilkS user hide)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (trace_clearance 0.199)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.3)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.2)
    (via_min_drill 0.2)
    (user_via 1 0.5)
    (user_via 2 1)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.15)
    (pad_size 2 1.5)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFD9F)
    (pcbplotparams
      (layerselection 284983297)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 /3V3)
  (net 2 /3V3_AMP)
  (net 3 /3V3_AN)
  (net 4 /3V3_ESP)
  (net 5 /3V3_MCU)
  (net 6 /3V3_MEM1)
  (net 7 /3V3_SD)
  (net 8 /5V)
  (net 9 /5V_BUS)
  (net 10 /BOOT0)
  (net 11 /BOOT1)
  (net 12 /CD)
  (net 13 /D+)
  (net 14 /D-)
  (net 15 /DAC)
  (net 16 /ESP_BOOT)
  (net 17 /ESP_CS)
  (net 18 /ESP_EN)
  (net 19 /ESP_IO1)
  (net 20 /ESP_IO2)
  (net 21 /ESP_MISO)
  (net 22 /ESP_MOSI)
  (net 23 /ESP_RESET)
  (net 24 /ESP_RX)
  (net 25 /ESP_SCK)
  (net 26 /ESP_TX)
  (net 27 /ESP_TX2)
  (net 28 /ESP_WAKE)
  (net 29 /JRST)
  (net 30 /JTDI)
  (net 31 /JTDO)
  (net 32 /MEM_SCL)
  (net 33 /MEM_SDA)
  (net 34 /RESET_MCU)
  (net 35 /SD_CD)
  (net 36 /SD_CK)
  (net 37 /SD_CS1)
  (net 38 /SD_MISO)
  (net 39 /SD_MOSI)
  (net 40 /SWCLK)
  (net 41 /SWDIO)
  (net 42 /UART_RX)
  (net 43 /UART_TX)
  (net 44 /Vbat)
  (net 45 /Vref)
  (net 46 /XIN)
  (net 47 /XIN32)
  (net 48 /XOUT)
  (net 49 /XOUT32)
  (net 50 /an1)
  (net 51 /an2)
  (net 52 /an3)
  (net 53 /an4)
  (net 54 AGND)
  (net 55 N-000001)
  (net 56 N-0000012)
  (net 57 N-0000017)
  (net 58 N-0000019)
  (net 59 N-000002)
  (net 60 N-0000020)
  (net 61 N-0000022)
  (net 62 N-0000023)
  (net 63 N-0000024)
  (net 64 N-0000026)
  (net 65 N-0000028)
  (net 66 N-0000029)
  (net 67 N-000003)
  (net 68 N-0000031)
  (net 69 N-0000032)
  (net 70 N-0000033)
  (net 71 N-0000043)
  (net 72 N-0000046)
  (net 73 N-0000047)
  (net 74 N-0000049)
  (net 75 N-0000050)
  (net 76 N-0000051)
  (net 77 N-0000052)
  (net 78 N-0000054)
  (net 79 N-0000055)
  (net 80 N-0000057)
  (net 81 N-0000058)
  (net 82 N-000006)
  (net 83 N-0000063)
  (net 84 N-0000067)
  (net 85 N-0000069)
  (net 86 N-000007)
  (net 87 N-0000070)
  (net 88 N-0000071)
  (net 89 N-0000072)
  (net 90 N-0000073)
  (net 91 N-0000074)
  (net 92 N-0000075)
  (net 93 N-0000076)
  (net 94 N-0000077)
  (net 95 N-0000078)
  (net 96 N-0000079)
  (net 97 N-000008)
  (net 98 N-0000080)
  (net 99 N-0000081)
  (net_class Default "Esta é a classe de net default."
    (clearance 0.199)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net /3V3)
    (add_net /3V3_AMP)
    (add_net /3V3_AN)
    (add_net /3V3_ESP)
    (add_net /3V3_MCU)
    (add_net /3V3_MEM1)
    (add_net /3V3_SD)
    (add_net /5V)
    (add_net /5V_BUS)
    (add_net /BOOT0)
    (add_net /BOOT1)
    (add_net /CD)
    (add_net /D+)
    (add_net /D-)
    (add_net /DAC)
    (add_net /ESP_BOOT)
    (add_net /ESP_CS)
    (add_net /ESP_EN)
    (add_net /ESP_IO1)
    (add_net /ESP_IO2)
    (add_net /ESP_MISO)
    (add_net /ESP_MOSI)
    (add_net /ESP_RESET)
    (add_net /ESP_RX)
    (add_net /ESP_SCK)
    (add_net /ESP_TX)
    (add_net /ESP_TX2)
    (add_net /ESP_WAKE)
    (add_net /JRST)
    (add_net /JTDI)
    (add_net /JTDO)
    (add_net /MEM_SCL)
    (add_net /MEM_SDA)
    (add_net /RESET_MCU)
    (add_net /SD_CD)
    (add_net /SD_CK)
    (add_net /SD_CS1)
    (add_net /SD_MISO)
    (add_net /SD_MOSI)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net /Vbat)
    (add_net /Vref)
    (add_net /XIN)
    (add_net /XIN32)
    (add_net /XOUT)
    (add_net /XOUT32)
    (add_net /an1)
    (add_net /an2)
    (add_net /an3)
    (add_net /an4)
    (add_net AGND)
    (add_net N-000001)
    (add_net N-0000012)
    (add_net N-0000017)
    (add_net N-0000019)
    (add_net N-000002)
    (add_net N-0000020)
    (add_net N-0000022)
    (add_net N-0000023)
    (add_net N-0000024)
    (add_net N-0000026)
    (add_net N-0000028)
    (add_net N-0000029)
    (add_net N-000003)
    (add_net N-0000031)
    (add_net N-0000032)
    (add_net N-0000033)
    (add_net N-0000043)
    (add_net N-0000046)
    (add_net N-0000047)
    (add_net N-0000049)
    (add_net N-0000050)
    (add_net N-0000051)
    (add_net N-0000052)
    (add_net N-0000054)
    (add_net N-0000055)
    (add_net N-0000057)
    (add_net N-0000058)
    (add_net N-000006)
    (add_net N-0000063)
    (add_net N-0000067)
    (add_net N-0000069)
    (add_net N-000007)
    (add_net N-0000070)
    (add_net N-0000071)
    (add_net N-0000072)
    (add_net N-0000073)
    (add_net N-0000074)
    (add_net N-0000075)
    (add_net N-0000076)
    (add_net N-0000077)
    (add_net N-0000078)
    (add_net N-0000079)
    (add_net N-000008)
    (add_net N-0000080)
    (add_net N-0000081)
  )
  (module furo3 (layer F.Cu) (tedit 55DC7C0A)
    (at 94.5 65.5)
    (attr virtual)
    (fp_text reference H1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FURO (at 0 0.70104) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 3.1)
      (layers *.SilkS *.Mask F.Cu)
      (clearance 0.50038)
    )
  )
  (module furo3 (layer F.Cu) (tedit 55DC7C0A)
    (at 29.5 65.5)
    (attr virtual)
    (fp_text reference H2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FURO (at 0 0.70104) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 3.1)
      (layers *.SilkS *.Mask F.Cu)
      (clearance 0.50038)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 67.7 106.3)
    (attr virtual)
    (fp_text reference V25 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 57 89.6)
    (attr virtual)
    (fp_text reference V29 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 5 /3V3_MCU)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 64.6 94.2)
    (attr virtual)
    (fp_text reference V15 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 66.5 82.6)
    (attr virtual)
    (fp_text reference V27 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 5 /3V3_MCU)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 63.8 106.3)
    (attr virtual)
    (fp_text reference V16 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 39.5 68)
    (attr virtual)
    (fp_text reference V24 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 47.35 92.75)
    (attr virtual)
    (fp_text reference V23 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 47.35 91.75)
    (attr virtual)
    (fp_text reference V22 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 47.35 96)
    (attr virtual)
    (fp_text reference V21 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 67.7 105.3)
    (attr virtual)
    (fp_text reference V20 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 67.6 76.5)
    (attr virtual)
    (fp_text reference V19 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 67.6 73.7)
    (attr virtual)
    (fp_text reference V18 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 46.6 66.2)
    (attr virtual)
    (fp_text reference V12 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 39.5 71.65)
    (attr virtual)
    (fp_text reference V10 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 55.2 88.6)
    (attr virtual)
    (fp_text reference V13 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 56.55 79.55)
    (attr virtual)
    (fp_text reference V9 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 54 65.6)
    (attr virtual)
    (fp_text reference V7 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 64.2 84.3)
    (attr virtual)
    (fp_text reference V6 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 54 64)
    (attr virtual)
    (fp_text reference V4 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module SOIC-8 (layer F.Cu) (tedit 575808F3)
    (at 50.4 94.3 90)
    (attr smd)
    (fp_text reference U4 (at -1.8 -2.7 90) (layer F.SilkS))
    (fp_text value 24LC64 (at 0 2.25 90) (layer F.SilkS) hide)
    (pad 5 smd oval (at 2.9 1.905) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 98 N-0000080)
    )
    (pad 6 smd oval (at 2.9 0.635) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 96 N-0000079)
    )
    (pad 7 smd oval (at 2.9 -0.635) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 8 smd oval (at 2.9 -1.905) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /3V3_MEM1)
    )
    (pad 1 smd oval (at -2.9 -1.905) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at -2.9 -0.635) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 3 smd oval (at -2.9 0.635) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 4 smd oval (at -2.9 1.905) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model Neurotec\smd\cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOD-123 (layer B.Cu) (tedit 575815E1)
    (at 51.4 73)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference D3 (at 2.4 1.05) (layer B.SilkS))
    (fp_text value DIODE (at 0 -0.8001) (layer B.SilkS) hide)
    (fp_text user K (at -2.5 0) (layer B.SilkS))
    (pad 1 smd oval (at -1.6 0) (size 1.2 1.3)
      (layers B.Cu B.Paste B.Mask)
      (net 73 N-0000047)
    )
    (pad 2 smd oval (at 1.6 0) (size 1.2 1.3)
      (layers B.Cu B.Paste B.Mask)
      (net 44 /Vbat)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3216 (layer F.Cu) (tedit 57506054)
    (at 62.4 71.1 270)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C8 (at 0 4.35 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 0.8001 270) (layer F.SilkS) hide)
    (fp_text user + (at -2.4003 1.09982 270) (layer F.SilkS))
    (pad 1 smd oval (at -1.5 0 270) (size 1.4 1.8)
      (layers F.Cu F.Paste F.Mask)
      (net 44 /Vbat)
    )
    (pad 2 smd oval (at 1.5 0 270) (size 1.4 1.8)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd\capacitors\C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3216 (layer F.Cu) (tedit 57506051)
    (at 59.6 71.1 270)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C7 (at 0 2.3 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 0.8001 270) (layer F.SilkS) hide)
    (fp_text user + (at -2.4003 1.09982 270) (layer F.SilkS))
    (pad 1 smd oval (at -1.5 0 270) (size 1.4 1.8)
      (layers F.Cu F.Paste F.Mask)
      (net 76 N-0000051)
    )
    (pad 2 smd oval (at 1.5 0 270) (size 1.4 1.8)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd\capacitors\C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1210 (layer B.Cu) (tedit 57506107)
    (at 50.6 68.3)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference PTC1 (at 0 -2) (layer B.SilkS))
    (fp_text value 500mA (at 0 -1.89992) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.5 0) (size 1.4 2.5)
      (layers B.Cu B.Paste B.Mask)
      (net 9 /5V_BUS)
    )
    (pad 2 smd oval (at 1.5 0) (size 1.4 2.5)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /5V)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.2 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57580B51)
    (at 55.7 64)
    (attr smd)
    (fp_text reference R8 (at 0.825 2.85) (layer F.SilkS))
    (fp_text value "1K 5%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 92 N-0000075)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061C8)
    (at 62.7 87.9)
    (attr smd)
    (fp_text reference C10 (at 2.75 0) (layer B.SilkS))
    (fp_text value "100KpF X7R" (at 0 -0.50038) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 55E48764)
    (at 68 82.6 180)
    (attr smd)
    (fp_text reference R5 (at 0 1.09982 180) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 34 /RESET_MCU)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 5788D7D0)
    (at 59.4 74.5 180)
    (attr smd)
    (fp_text reference R6 (at 1.869 1.221 180) (layer F.SilkS))
    (fp_text value "10K 5%" (at 0 0.50038 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 46 /XIN)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 48 /XOUT)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506156)
    (at 52.3 94.2 270)
    (attr smd)
    (fp_text reference R34 (at 2.2 -0.05 270) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 98 N-0000080)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 6 /3V3_MEM1)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57580B91)
    (at 57.2 100.5 270)
    (attr smd)
    (fp_text reference R24 (at -2.2 0 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 37 /SD_CS1)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-000002)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506162)
    (at 49.9 105.6)
    (attr smd)
    (fp_text reference R29 (at 0.55 -1.1) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /CD)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506125)
    (at 79.1 75.3)
    (attr smd)
    (fp_text reference R38 (at 0 -1.1) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 27 /ESP_TX2)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /3V3_ESP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506120)
    (at 79.1 77.3)
    (attr smd)
    (fp_text reference R37 (at 0 1.25) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 16 /ESP_BOOT)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /3V3_ESP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57506063)
    (at 55.15 79.55 180)
    (attr smd)
    (fp_text reference R12 (at 0.55 -1.25 180) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 50 /an1)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F30)
    (at 69.8 104.8 270)
    (attr smd)
    (fp_text reference R3 (at -1.95 -0.05 270) (layer F.SilkS))
    (fp_text value "0R 1%" (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /D-)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 72 N-0000046)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 575808E6)
    (at 53.4 88.7 270)
    (attr smd)
    (fp_text reference R31 (at -2.2 0 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 32 /MEM_SCL)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 98 N-0000080)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506167)
    (at 55.4 105.6 180)
    (attr smd)
    (fp_text reference R30 (at 2.25 0 180) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 59 N-000002)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F35)
    (at 71.4 104.8 270)
    (attr smd)
    (fp_text reference R4 (at -1.95 0 270) (layer F.SilkS))
    (fp_text value "0R 1%" (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /D+)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 80 N-0000057)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 55E48764)
    (at 54.55 77.3 90)
    (attr smd)
    (fp_text reference R11 (at 0 -1.09982 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 50 /an1)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 44 /Vbat)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061B1)
    (at 65.2 112.7 90)
    (attr smd)
    (fp_text reference R10 (at 0 -1.15 90) (layer B.SilkS))
    (fp_text value "1K 5%" (at 0 -0.50038 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 99 N-0000081)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 95 N-0000078)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F87)
    (at 55.7 94.2 270)
    (attr smd)
    (fp_text reference R13 (at 2.2 0 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /3V3_SD)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 575808E3)
    (at 51.7 88.7 270)
    (attr smd)
    (fp_text reference R32 (at -2.2 0 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 33 /MEM_SDA)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 96 N-0000079)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506152)
    (at 50.5 94.2 270)
    (attr smd)
    (fp_text reference R33 (at 2.2 0 270) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 96 N-0000079)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 6 /3V3_MEM1)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061B3)
    (at 66.8 112.7 90)
    (attr smd)
    (fp_text reference R7 (at 0 1.25 90) (layer B.SilkS))
    (fp_text value "1K 5%" (at 0 -0.50038 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 94 N-0000077)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 91 N-0000074)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 5750616C)
    (at 55.4 107.2)
    (attr smd)
    (fp_text reference C19 (at -2.25 0) (layer B.SilkS))
    (fp_text value "100KpF X7R" (at 0 -0.50038) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061D1)
    (at 62.7 86.3)
    (attr smd)
    (fp_text reference C14 (at 1.95 0 90) (layer B.SilkS))
    (fp_text value "100KpF X7R" (at 0 -0.50038) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /3V3_AN)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061D6)
    (at 60.1 87.1 90)
    (attr smd)
    (fp_text reference BF1 (at -0.45 -1.1 90) (layer B.SilkS))
    (fp_text value BEAD (at 0 -0.50038 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /3V3_AN)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57615354)
    (at 68 82.6)
    (attr smd)
    (fp_text reference C12 (at 2.25 0.4) (layer F.SilkS))
    (fp_text value "100KpF X7R" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F8B)
    (at 64.6 92.3 270)
    (attr smd)
    (fp_text reference C11 (at 0.55 -1.25 270) (layer F.SilkS))
    (fp_text value "100KpF X7R" (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57506024)
    (at 66.7 77.3 90)
    (attr smd)
    (fp_text reference C4 (at 0 1.25 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 0.50038 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 47 /XIN32)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 5750602E)
    (at 56.6 74.5 180)
    (attr smd)
    (fp_text reference C3 (at 2 0 180) (layer F.SilkS))
    (fp_text value 20pF (at 0 0.50038 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 48 /XOUT)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 55E48764)
    (at 68.6 84.8 270)
    (attr smd)
    (fp_text reference C6 (at 0 1.09982 270) (layer B.SilkS))
    (fp_text value "100KpF X7R" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 34 /RESET_MCU)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 5750601F)
    (at 66.7 74.5 90)
    (attr smd)
    (fp_text reference C5 (at 0 1.2 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 0.50038 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 49 /XOUT32)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 5750605F)
    (at 62.2 74.5)
    (attr smd)
    (fp_text reference C2 (at 2.25 0) (layer F.SilkS))
    (fp_text value 20pF (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 46 /XIN)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F3E)
    (at 66.8 107.1 90)
    (attr smd)
    (fp_text reference R1 (at -0.8 1.25 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 97 N-000008)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F46)
    (at 65.2 107.1 90)
    (attr smd)
    (fp_text reference C1 (at -0.85 -1.15 90) (layer F.SilkS))
    (fp_text value "100KpF X7R" (at 0 0.50038 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 97 N-000008)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061B8)
    (at 69.8 104.8 270)
    (attr smd)
    (fp_text reference D2 (at -1.95 0 270) (layer B.SilkS))
    (fp_text value CG0603 (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 72 N-0000046)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061BB)
    (at 71.4 104.8 270)
    (attr smd)
    (fp_text reference D1 (at -1.9 0.05 270) (layer B.SilkS))
    (fp_text value CG0603 (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 80 N-0000057)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506178)
    (at 56.4 111.3 270)
    (attr smd)
    (fp_text reference R18 (at -2.25 -0.05 270) (layer B.SilkS))
    (fp_text value "1K 5%" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 82 N-000006)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F5D)
    (at 49.1 100.5 270)
    (attr smd)
    (fp_text reference R28 (at -1.75 0 360) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 35 /SD_CD)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /CD)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F6C)
    (at 51.2 100.5 270)
    (attr smd)
    (fp_text reference R27 (at 0 -1.15 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 38 /SD_MISO)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 70 N-0000033)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F70)
    (at 53.4 100.5 270)
    (attr smd)
    (fp_text reference R26 (at 0 -1.15 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 36 /SD_CK)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 69 N-0000032)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57580B93)
    (at 55.6 100.5 270)
    (attr smd)
    (fp_text reference R25 (at -2.2 0.3 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 39 /SD_MOSI)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 68 N-0000031)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 5750617D)
    (at 58 111.3 270)
    (attr smd)
    (fp_text reference R19 (at -2.25 0 270) (layer B.SilkS))
    (fp_text value "1K 5%" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 86 N-000007)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506174)
    (at 54.8 111.3 270)
    (attr smd)
    (fp_text reference R17 (at -2.25 0 270) (layer B.SilkS))
    (fp_text value "1K 5%" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 67 N-000003)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F8E)
    (at 54.7 91.9)
    (attr smd)
    (fp_text reference R16 (at 0.55 -1.1) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F82)
    (at 54.1 94.2 270)
    (attr smd)
    (fp_text reference R15 (at 2.2 0 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /3V3_MEM1)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505FF7)
    (at 73.6 90.5)
    (attr smd)
    (fp_text reference R14 (at 0 1.15) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /3V3_ESP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module CRISTAL-ABM3 (layer F.Cu) (tedit 5750606E)
    (at 60.1 77)
    (descr CRYSTAL)
    (tags CRYSTAL)
    (attr smd)
    (fp_text reference X1 (at -0.1 2.2) (layer F.SilkS))
    (fp_text value "CRISTAL ABM3 -8MHZ" (at 0 -1.85) (layer F.SilkS) hide)
    (pad 1 smd oval (at -2.2 0) (size 2 2.5)
      (layers F.Cu F.Paste F.Mask)
      (net 48 /XOUT)
    )
    (pad 2 smd oval (at 2.2 0) (size 2 2.5)
      (layers F.Cu F.Paste F.Mask)
      (net 46 /XIN)
    )
  )
  (module APA3010 (layer B.Cu) (tedit 57506195)
    (at 62 117)
    (attr smd)
    (fp_text reference LD5 (at -0.05 -1.5) (layer B.SilkS))
    (fp_text value APA3010QGC (at -0.05 0) (layer B.SilkS) hide)
    (fp_text user K (at -2.5 -1.1 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 42 /UART_RX)
    )
    (pad 1 smd rect (at 1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 86 N-000007)
    )
    (pad ~ smd rect (at 0 -0.65 180) (size 0.9 0.9)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module APA3010 (layer B.Cu) (tedit 5750618E)
    (at 56 117)
    (attr smd)
    (fp_text reference LD4 (at -0.05 -1.5) (layer B.SilkS))
    (fp_text value APA3010QGC (at -0.05 0) (layer B.SilkS) hide)
    (fp_text user K (at -2.45 -1.1 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 43 /UART_TX)
    )
    (pad 1 smd rect (at 1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 82 N-000006)
    )
    (pad ~ smd rect (at 0 -0.65 180) (size 0.9 0.9)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module APA3010 (layer B.Cu) (tedit 57506186)
    (at 50 117)
    (attr smd)
    (fp_text reference LD3 (at 0 -1.5) (layer B.SilkS))
    (fp_text value APA3010QGC (at -0.05 0) (layer B.SilkS) hide)
    (fp_text user K (at -2.2 -1.15 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (pad 1 smd rect (at 1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 67 N-000003)
    )
    (pad ~ smd rect (at 0 -0.65 180) (size 0.9 0.9)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module APA3010 (layer B.Cu) (tedit 575856DF)
    (at 74 117)
    (attr smd)
    (fp_text reference LD2 (at 0.15 -1.5) (layer B.SilkS))
    (fp_text value APA3010QGC (at -0.05 0) (layer B.SilkS) hide)
    (fp_text user K (at -2.4 -1.15 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 94 N-0000077)
    )
    (pad 1 smd rect (at 1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (pad ~ smd rect (at 0 -0.65 180) (size 0.9 0.9)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module APA3010 (layer B.Cu) (tedit 575061A1)
    (at 68 117)
    (attr smd)
    (fp_text reference LD1 (at 0 -1.5) (layer B.SilkS))
    (fp_text value APA3010QGC (at -0.05 0) (layer B.SilkS) hide)
    (fp_text user K (at -2.3 -1.1 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 99 N-0000081)
    )
    (pad 1 smd rect (at 1.75 0 180) (size 1.5 1.5)
      (layers B.Cu B.Paste B.Mask)
      (net 7 /3V3_SD)
    )
    (pad ~ smd rect (at 0 -0.65 180) (size 0.9 0.9)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AB26TRQ (layer F.Cu) (tedit 5750601B)
    (at 64.8 77.8)
    (descr "Led verticale diam 6mm")
    (tags "LED DEV")
    (fp_text reference X2 (at 1.7 -6.7) (layer F.SilkS))
    (fp_text value "CRISTAL AB26TRQ-32.768kHz" (at -1.25 -3.8 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.45 0) (size 0.6 1.2)
      (layers F.Cu F.Paste F.Mask)
      (net 49 /XOUT32)
    )
    (pad 2 smd oval (at 0.45 0) (size 0.6 1.2)
      (layers F.Cu F.Paste F.Mask)
      (net 47 /XIN32)
    )
    (pad 3 smd oval (at 0 -5.6) (size 1.5 2.4)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model device/crystal_low_profile.wrl
      (at (xyz 0 0.25 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 90))
    )
  )
  (module MAT_8X1_2,54 (layer F.Cu) (tedit 570E54F7)
    (at 95.6 79 90)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P2 (at -10.1 -1.8 90) (layer F.SilkS))
    (fp_text value CONN_8 (at 0 1.1 90) (layer F.SilkS) hide)
    (pad 8 thru_hole circle (at 8.89 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 4 /3V3_ESP)
    )
    (pad 1 thru_hole circle (at -8.89 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 23 /ESP_RESET)
    )
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 83 N-0000063)
    )
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 18 /ESP_EN)
    )
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 28 /ESP_WAKE)
    )
    (pad 5 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 25 /ESP_SCK)
    )
    (pad 6 thru_hole circle (at 3.81 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 21 /ESP_MISO)
    )
    (pad 7 thru_hole circle (at 6.35 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 22 /ESP_MOSI)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_B_MICRO (layer F.Cu) (tedit 57505F4A)
    (at 71 113.5 90)
    (descr "MINI USB-B R/A SMT W/ REAR")
    (tags "MINI USB-B R/A SMT W/ REAR")
    (attr smd)
    (fp_text reference J1 (at -3.05 -5.95 90) (layer F.SilkS))
    (fp_text value USB-MINI-B (at 0 4.59994 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.99974 -1.59766 90) (size 3.0988 0.49784)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /5V_BUS)
    )
    (pad 2 smd rect (at 2.99974 -0.79756 90) (size 3.0988 0.49784)
      (layers F.Cu F.Paste F.Mask)
      (net 72 N-0000046)
    )
    (pad 3 smd rect (at 2.99974 0 90) (size 3.0988 0.49784)
      (layers F.Cu F.Paste F.Mask)
      (net 80 N-0000057)
    )
    (pad 4 smd rect (at 2.99974 0.79756 90) (size 3.0988 0.49784)
      (layers F.Cu F.Paste F.Mask)
      (net 75 N-0000050)
    )
    (pad 5 smd rect (at 2.99974 1.59766 90) (size 3.0988 0.49784)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 6 smd rect (at -2.99974 4.44754 90) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 97 N-000008)
    )
    (pad 6 smd rect (at -2.99974 -4.44754 90) (size 2.49936 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 97 N-000008)
    )
    (pad 6 smd rect (at 2.89814 -4.44754 90) (size 3.29946 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 97 N-000008)
    )
    (pad 6 smd rect (at 2.89814 4.44754 90) (size 3.29946 1.99898)
      (layers F.Cu F.Paste F.Mask)
      (net 97 N-000008)
    )
    (pad ~ thru_hole circle (at 0 -2.19964 90) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Mask F.Cu F.SilkS)
    )
    (pad ~ thru_hole circle (at 0 2.19964 90) (size 0.89916 0.89916) (drill 0.89916)
      (layers *.Mask F.Cu F.SilkS)
    )
  )
  (module MAT_8X1_2,54 (layer F.Cu) (tedit 570E54F7)
    (at 73.6 79 90)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P3 (at -10.1 -1.8 90) (layer F.SilkS))
    (fp_text value CONN_8 (at 0 1.1 90) (layer F.SilkS) hide)
    (pad 8 thru_hole circle (at 8.89 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (pad 1 thru_hole circle (at -8.89 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 26 /ESP_TX)
    )
    (pad 2 thru_hole circle (at -6.35 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 24 /ESP_RX)
    )
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 19 /ESP_IO1)
    )
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 20 /ESP_IO2)
    )
    (pad 5 thru_hole circle (at 1.27 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 16 /ESP_BOOT)
    )
    (pad 6 thru_hole circle (at 3.81 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 27 /ESP_TX2)
    )
    (pad 7 thru_hole circle (at 6.35 0 90) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 17 /ESP_CS)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 64.2 87.9)
    (attr virtual)
    (fp_text reference V3 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module uSD (layer F.Cu) (tedit 57505F55)
    (at 55.6 113.8)
    (fp_text reference J4 (at 8 2.75 90) (layer F.SilkS))
    (fp_text value MICROSD (at 0 0.6) (layer F.SilkS) hide)
    (pad 9 smd rect (at -6.55 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /CD)
    )
    (pad 10 smd rect (at -7.75 -10) (size 1.2 1.4)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 11 smd rect (at -7.75 -0.4) (size 1.2 2)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 12 smd rect (at 7.75 -0.4) (size 1.2 2)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 1 smd rect (at 2.25 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 2 smd rect (at 1.15 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-000002)
    )
    (pad 3 smd rect (at 0.05 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 68 N-0000031)
    )
    (pad 4 smd rect (at -1.05 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /3V3_SD)
    )
    (pad 5 smd rect (at -2.15 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 69 N-0000032)
    )
    (pad 6 smd rect (at -3.25 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 7 smd rect (at -4.35 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
      (net 70 N-0000033)
    )
    (pad 8 smd rect (at -5.45 -10.5) (size 0.7 1.6)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 13 smd rect (at 6.85 -10) (size 1.4 1.6)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad "" thru_hole circle (at -4.95 0) (size 1 1) (drill 1)
      (layers *.Cu F.SilkS)
    )
    (pad "" thru_hole circle (at 3.05 0) (size 1 1) (drill 1)
      (layers *.Cu F.SilkS)
    )
  )
  (module SM3216 (layer B.Cu) (tedit 575061FE)
    (at 89.1 71.3 180)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C22 (at -1.65 1.5 180) (layer B.SilkS))
    (fp_text value 10uf (at 0 -0.8001 180) (layer B.SilkS) hide)
    (fp_text user + (at -2.45 -1 180) (layer B.SilkS))
    (pad 1 smd oval (at -1.5 0 180) (size 1.4 1.8)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /3V3_ESP)
    )
    (pad 2 smd oval (at 1.5 0 180) (size 1.4 1.8)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd\capacitors\C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57580B54)
    (at 55.7 65.6)
    (attr smd)
    (fp_text reference R9 (at 0.825 2.05) (layer F.SilkS))
    (fp_text value "1K 5%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 93 N-0000076)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 55E48764)
    (at 90.1 85.3 180)
    (attr smd)
    (fp_text reference R36 (at 0 1.09982 180) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /ESP_RESET)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /3V3_ESP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 55E48764)
    (at 90.1 81.3 180)
    (attr smd)
    (fp_text reference R35 (at 0 1.09982 180) (layer B.SilkS))
    (fp_text value "10K 5%" (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 18 /ESP_EN)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /3V3_ESP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 5750612F)
    (at 90.2 73.4 180)
    (attr smd)
    (fp_text reference C21 (at -0.55 -1.25 180) (layer B.SilkS))
    (fp_text value "100KpF X7R" (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 4 /3V3_ESP)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 5750615D)
    (at 48.5 94.2 270)
    (attr smd)
    (fp_text reference C20 (at 2.65 0 360) (layer B.SilkS))
    (fp_text value "100KpF X7R" (at 0 -0.50038 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 6 /3V3_MEM1)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3528 (layer F.Cu) (tedit 57614B58)
    (at 42.3 68 180)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C17 (at 3.15 -1.1 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 -1.24968 180) (layer F.SilkS) hide)
    (fp_text user + (at -2.65 1.6 180) (layer F.SilkS))
    (pad 1 smd oval (at -1.75 0 180) (size 1.5 2.8)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 1.75 0 180) (size 1.5 2.8)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3216 (layer B.Cu) (tedit 575061CD)
    (at 61.6 89.9)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C13 (at 3 0 90) (layer B.SilkS))
    (fp_text value 10uf (at 0 -0.8001) (layer B.SilkS) hide)
    (fp_text user + (at -2.4003 -1.09982) (layer B.SilkS))
    (pad 1 smd oval (at -1.5 0) (size 1.4 1.8)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 1.5 0) (size 1.4 1.8)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd\capacitors\C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3528 (layer F.Cu) (tedit 57614B66)
    (at 42.3 71.65 180)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C18 (at 3.2 -1.05 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 -1.24968 180) (layer F.SilkS) hide)
    (fp_text user + (at -2.65 1.65 180) (layer F.SilkS))
    (pad 1 smd oval (at -1.75 0 180) (size 1.5 2.8)
      (layers F.Cu F.Paste F.Mask)
      (net 73 N-0000047)
    )
    (pad 2 smd oval (at 1.75 0 180) (size 1.5 2.8)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3216 (layer B.Cu) (tedit 575061DB)
    (at 61.6 84.3)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C15 (at 1.65 -1.55) (layer B.SilkS))
    (fp_text value 10uf (at 0 -0.8001) (layer B.SilkS) hide)
    (fp_text user + (at -2.4003 -1.09982) (layer B.SilkS))
    (pad 1 smd oval (at -1.5 0) (size 1.4 1.8)
      (layers B.Cu B.Paste B.Mask)
      (net 3 /3V3_AN)
    )
    (pad 2 smd oval (at 1.5 0) (size 1.4 1.8)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd\capacitors\C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP-12E (layer F.Cu) (tedit 575060AB)
    (at 84.6 78.8 180)
    (fp_text reference U5 (at -8.75 -13.6 180) (layer F.SilkS))
    (fp_text value ESP-12E (at 0 2.1 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -8.5 -6.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /ESP_RESET)
    )
    (pad 2 smd oval (at -8.5 -4.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 83 N-0000063)
    )
    (pad 3 smd oval (at -8.5 -2.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 18 /ESP_EN)
    )
    (pad 4 smd oval (at -8.5 -0.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 28 /ESP_WAKE)
    )
    (pad 5 smd oval (at -8.5 1.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 25 /ESP_SCK)
    )
    (pad 6 smd oval (at -8.5 3.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 21 /ESP_MISO)
    )
    (pad 7 smd oval (at -8.5 5.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 22 /ESP_MOSI)
    )
    (pad 8 smd oval (at -8.5 7.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /3V3_ESP)
    )
    (pad 15 smd oval (at 8.5 7.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 16 smd oval (at 8.5 5.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 17 /ESP_CS)
    )
    (pad 17 smd oval (at 8.5 3.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 27 /ESP_TX2)
    )
    (pad 18 smd oval (at 8.5 1.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 16 /ESP_BOOT)
    )
    (pad 19 smd oval (at 8.5 -0.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /ESP_IO2)
    )
    (pad 20 smd oval (at 8.5 -2.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /ESP_IO1)
    )
    (pad 21 smd oval (at 8.5 -4.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 24 /ESP_RX)
    )
    (pad 22 smd oval (at 8.5 -6.5 180) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 26 /ESP_TX)
    )
    (pad 9 smd oval (at -5 10 270) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 90 N-0000073)
    )
    (pad 10 smd oval (at -3 10 270) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 89 N-0000072)
    )
    (pad 11 smd oval (at -1 10 270) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 88 N-0000071)
    )
    (pad 14 smd oval (at 5 10 270) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 84 N-0000067)
    )
    (pad 13 smd oval (at 3 10 270) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 85 N-0000069)
    )
    (pad 12 smd oval (at 1 10 270) (size 2 1)
      (layers F.Cu F.Paste F.Mask)
      (net 87 N-0000070)
    )
  )
  (module SOT-223 (layer F.Cu) (tedit 57580780)
    (at 49.9 69.8 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 4 -2.2 360) (layer F.SilkS))
    (fp_text value LM117MPX (at 0 0.762 270) (layer F.SilkS) hide)
    (pad 4 smd oval (at 0 -3 270) (size 3.8 2)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 0 3.3 270) (size 1.4 2)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 3 smd oval (at 2.3 3.3 270) (size 1.4 2)
      (layers F.Cu F.Paste F.Mask)
      (net 73 N-0000047)
    )
    (pad 1 smd oval (at -2.3 3.3 270) (size 1.4 2)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/SOT223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TQFP-48 (layer F.Cu) (tedit 57333C27)
    (at 61.4 85.8 180)
    (descr "TQFP48 9X9MM 0.5MM PITCH 0.25MM PAD")
    (tags "TQFP48 9X9MM 0.5MM PITCH 0.25MM PAD")
    (attr smd)
    (fp_text reference U2 (at -4.30022 4.50088 180) (layer F.SilkS))
    (fp_text value STM32-48 (at 3.15 0 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -2.75 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at -2.25 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-000001)
    )
    (pad 3 smd oval (at -1.75 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 47 /XIN32)
    )
    (pad 4 smd oval (at -1.25 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 49 /XOUT32)
    )
    (pad 5 smd oval (at -0.75 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 46 /XIN)
    )
    (pad 6 smd oval (at -0.25 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 48 /XOUT)
    )
    (pad 7 smd oval (at 0.25 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 34 /RESET_MCU)
    )
    (pad 8 smd oval (at 0.75 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 56 N-0000012)
    )
    (pad 9 smd oval (at 1.25 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3_AN)
    )
    (pad 10 smd oval (at 1.75 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 50 /an1)
    )
    (pad 11 smd oval (at 2.25 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 63 N-0000024)
    )
    (pad 12 smd oval (at 2.75 4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 62 N-0000023)
    )
    (pad 13 smd oval (at 4.4 2.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 51 /an2)
    )
    (pad 14 smd oval (at 4.4 2.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /DAC)
    )
    (pad 15 smd oval (at 4.4 1.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 52 /an3)
    )
    (pad 16 smd oval (at 4.4 1.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 53 /an4)
    )
    (pad 17 smd oval (at 4.4 0.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 71 N-0000043)
    )
    (pad 18 smd oval (at 4.4 0.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 74 N-0000049)
    )
    (pad 19 smd oval (at 4.4 -0.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 61 N-0000022)
    )
    (pad 20 smd oval (at 4.4 -0.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /BOOT1)
    )
    (pad 21 smd oval (at 4.4 -1.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 32 /MEM_SCL)
    )
    (pad 22 smd oval (at 4.4 -1.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 33 /MEM_SDA)
    )
    (pad 23 smd oval (at 4.4 -2.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 24 smd oval (at 4.4 -2.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 25 smd oval (at 2.75 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 37 /SD_CS1)
    )
    (pad 32 smd oval (at -0.75 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /D-)
    )
    (pad 31 smd oval (at -0.25 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 42 /UART_RX)
    )
    (pad 30 smd oval (at 0.25 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 43 /UART_TX)
    )
    (pad 29 smd oval (at 0.75 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 35 /SD_CD)
    )
    (pad 28 smd oval (at 1.25 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 39 /SD_MOSI)
    )
    (pad 27 smd oval (at 1.75 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 38 /SD_MISO)
    )
    (pad 26 smd oval (at 2.25 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 36 /SD_CK)
    )
    (pad 33 smd oval (at -1.25 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /D+)
    )
    (pad 34 smd oval (at -1.75 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 41 /SWDIO)
    )
    (pad 35 smd oval (at -2.25 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 36 smd oval (at -2.75 -4.4 270) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 37 smd oval (at -4.4 -2.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 40 /SWCLK)
    )
    (pad 38 smd oval (at -4.4 -2.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 30 /JTDI)
    )
    (pad 39 smd oval (at -4.4 -1.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 31 /JTDO)
    )
    (pad 40 smd oval (at -4.4 -1.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 29 /JRST)
    )
    (pad 41 smd oval (at -4.4 -0.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /ESP_RESET)
    )
    (pad 42 smd oval (at -4.4 -0.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 24 /ESP_RX)
    )
    (pad 43 smd oval (at -4.4 0.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 26 /ESP_TX)
    )
    (pad 44 smd oval (at -4.4 0.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /BOOT0)
    )
    (pad 45 smd oval (at -4.4 1.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /ESP_IO1)
    )
    (pad 46 smd oval (at -4.4 1.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /ESP_IO2)
    )
    (pad 47 smd oval (at -4.4 2.25 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 48 smd oval (at -4.4 2.75 180) (size 1.2 0.3)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd\vqfp64.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 5750606A)
    (at 58 79.55)
    (attr smd)
    (fp_text reference BF2 (at 2.2 0.45) (layer F.SilkS))
    (fp_text value BEAD (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 56 N-0000012)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOIC-8 (layer F.Cu) (tedit 57580B71)
    (at 61 65.9)
    (attr smd)
    (fp_text reference U1 (at -4.5 2.5) (layer F.SilkS))
    (fp_text value TP4056 (at 0 2.25) (layer F.SilkS) hide)
    (pad 5 smd oval (at 2.9 1.905 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 44 /Vbat)
    )
    (pad 6 smd oval (at 2.9 0.635 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 95 N-0000078)
    )
    (pad 7 smd oval (at 2.9 -0.635 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 91 N-0000074)
    )
    (pad 8 smd oval (at 2.9 -1.905 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 76 N-0000051)
    )
    (pad 1 smd oval (at -2.9 -1.905 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 92 N-0000075)
    )
    (pad 2 smd oval (at -2.9 -0.635 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 93 N-0000076)
    )
    (pad 3 smd oval (at -2.9 0.635 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 4 smd oval (at -2.9 1.905 270) (size 0.5 1.5)
      (layers F.Cu F.Paste F.Mask)
      (net 76 N-0000051)
    )
    (model Neurotec\smd\cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAT_6X1_2,54 (layer F.Cu) (tedit 57506000)
    (at 83.9 64.5 180)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P4 (at -7.15 -1.9 180) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 1.7 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -6.35 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 90 N-0000073)
    )
    (pad 2 thru_hole circle (at -3.81 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 89 N-0000072)
    )
    (pad 3 thru_hole circle (at -1.27 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 88 N-0000071)
    )
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 87 N-0000070)
    )
    (pad 5 thru_hole circle (at 3.81 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 85 N-0000069)
    )
    (pad 6 thru_hole circle (at 6.35 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 84 N-0000067)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57615352)
    (at 68 81)
    (attr smd)
    (fp_text reference C16 (at 2.25 0.45) (layer F.SilkS))
    (fp_text value "100KpF X7R" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57505F38)
    (at 73 104.8 270)
    (attr smd)
    (fp_text reference R20 (at -2.2 0 270) (layer F.SilkS))
    (fp_text value 1K5 (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3_MCU)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 80 N-0000057)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57506017)
    (at 70.9 69.7 90)
    (attr smd)
    (fp_text reference R39 (at -2.75 -1.85 180) (layer F.SilkS))
    (fp_text value 100K (at 0 0.50038 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /BOOT0)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 78 N-0000054)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57506014)
    (at 69.3 69.7 270)
    (attr smd)
    (fp_text reference R43 (at 2.75 -1.8 360) (layer F.SilkS))
    (fp_text value 100K (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 79 N-0000055)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /BOOT1)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506145)
    (at 69.9 92.9 180)
    (attr smd)
    (fp_text reference R42 (at 2.2 -0.05 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 40 /SWCLK)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506139)
    (at 69.9 97.7 180)
    (attr smd)
    (fp_text reference R41 (at 2.2 0 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 41 /SWDIO)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506140)
    (at 69.9 94.5 180)
    (attr smd)
    (fp_text reference R40 (at 2.2 -0.05 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 29 /JRST)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 5750613D)
    (at 69.9 96.1 180)
    (attr smd)
    (fp_text reference R23 (at 2.2 0 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 31 /JTDO)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 57506135)
    (at 69.9 99.3 180)
    (attr smd)
    (fp_text reference R22 (at 2.25 -0.05 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -0.50038 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 30 /JTDI)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 5 /3V3_MCU)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOD-123 (layer B.Cu) (tedit 575815E5)
    (at 51.4 71)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference D4 (at 2.4 1) (layer B.SilkS))
    (fp_text value DIODE (at 0 -0.8001) (layer B.SilkS) hide)
    (fp_text user K (at -2.5 0) (layer B.SilkS))
    (pad 1 smd oval (at -1.6 0) (size 1.2 1.3)
      (layers B.Cu B.Paste B.Mask)
      (net 73 N-0000047)
    )
    (pad 2 smd oval (at 1.6 0) (size 1.2 1.3)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /5V)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.21 0.3 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 65.2 79.7)
    (attr virtual)
    (fp_text reference V1 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 55 N-000001)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module SM0603 (layer B.Cu) (tedit 575061C0)
    (at 73 104.8 90)
    (attr smd)
    (fp_text reference R2 (at 1.9 0.05 90) (layer B.SilkS))
    (fp_text value "0R 1%" (at 0 -0.50038 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 75 N-0000050)
    )
    (pad 2 smd oval (at 0.8 0 90) (size 0.65 1)
      (layers B.Cu B.Paste B.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAT_5X1_2,54 (layer F.Cu) (tedit 575814FD)
    (at 75.565 99.568 270)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P1 (at 7.182 -0.835 270) (layer F.SilkS))
    (fp_text value CONN_5 (at 0 1.7 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.7 1.7) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 34 /RESET_MCU)
    )
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 40 /SWCLK)
    )
    (pad 3 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 41 /SWDIO)
    )
    (pad 4 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 5 /3V3_MCU)
    )
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAT_6X1_2,54 (layer F.Cu) (tedit 575859C4)
    (at 45.3 64.5 180)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P8 (at 7.15 -1.9 180) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 1.7 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -6.35 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 44 /Vbat)
    )
    (pad 2 thru_hole circle (at -3.81 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 9 /5V_BUS)
    )
    (pad 3 thru_hole circle (at -1.27 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 1 /3V3)
    )
    (pad 5 thru_hole circle (at 3.81 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 51 /an2)
    )
    (pad 6 thru_hole circle (at 6.35 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 57582BC9)
    (at 44.15 79.8 270)
    (descr SOT23-5)
    (attr smd)
    (fp_text reference U6 (at 0 -1.55 540) (layer F.SilkS))
    (fp_text value MCP6001 (at -0.09906 -0.50038 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2 1.9 360) (layer F.SilkS))
    (pad 1 smd oval (at -0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 77 N-0000052)
    )
    (pad 3 smd oval (at 0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 45 /Vref)
    )
    (pad 5 smd oval (at -0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3_AMP)
    )
    (pad 2 smd oval (at 0 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 4 smd oval (at 0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 77 N-0000052)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 57582BC6)
    (at 44.15 83.4 270)
    (descr SOT23-5)
    (attr smd)
    (fp_text reference U7 (at 0 -1.55 540) (layer F.SilkS))
    (fp_text value MCP6001 (at -0.09906 -0.50038 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2 2.1 360) (layer F.SilkS))
    (pad 1 smd oval (at -0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 52 /an3)
    )
    (pad 3 smd oval (at 0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 64 N-0000026)
    )
    (pad 5 smd oval (at -0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3_AMP)
    )
    (pad 2 smd oval (at 0 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 4 smd oval (at 0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 52 /an3)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAT_6X1_2,54 (layer F.Cu) (tedit 575817FE)
    (at 49.2 82.4 270)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P9 (at -7.2 -1.9 270) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 1.7 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 51 /an2)
    )
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 15 /DAC)
    )
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 52 /an3)
    )
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 53 /an4)
    )
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 71 N-0000043)
    )
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 74 N-0000049)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B33)
    (at 46 75.1 270)
    (attr smd)
    (fp_text reference R44 (at 0.5 -1.25 270) (layer F.SilkS))
    (fp_text value 0R (at 0 0.50038 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3)
    )
    (pad 2 smd oval (at 0.8 0 270) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3_AMP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 5758509A)
    (at 43.7 74.5)
    (attr smd)
    (fp_text reference R45 (at 1.25 1.7 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 45 /Vref)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3_AMP)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57580BC5)
    (at 40.9 74.5)
    (attr smd)
    (fp_text reference R46 (at -1.8 0 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 45 /Vref)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 67.7 104.3)
    (attr virtual)
    (fp_text reference V2 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 58.3 73.35)
    (attr virtual)
    (fp_text reference V5 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module SM0805 (layer B.Cu) (tedit 5751EDFA)
    (at 55.6 70.15 180)
    (attr smd)
    (fp_text reference R47 (at 0 -1.45 180) (layer B.SilkS))
    (fp_text value "1K 5%" (at 0 0.70104 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -0.95 0 180) (size 1 1.4)
      (layers B.Cu B.Paste B.Mask)
      (net 76 N-0000051)
    )
    (pad 2 smd oval (at 0.95 0 180) (size 1 1.4)
      (layers B.Cu B.Paste B.Mask)
      (net 8 /5V)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 57582BBF)
    (at 44.15 87.2 270)
    (descr SOT23-5)
    (attr smd)
    (fp_text reference U8 (at 0 -1.55 540) (layer F.SilkS))
    (fp_text value MCP6001 (at -0.09906 -0.50038 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2 2 360) (layer F.SilkS))
    (pad 1 smd oval (at -0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 66 N-0000029)
    )
    (pad 3 smd oval (at 0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 45 /Vref)
    )
    (pad 5 smd oval (at -0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3_AMP)
    )
    (pad 2 smd oval (at 0 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 4 smd oval (at 0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 66 N-0000029)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 57614B01)
    (at 44.15 90.8 270)
    (descr SOT23-5)
    (attr smd)
    (fp_text reference U9 (at 0 -1.6 540) (layer F.SilkS))
    (fp_text value MCP6001 (at -0.09906 -0.50038 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2 2 360) (layer F.SilkS))
    (pad 1 smd oval (at -0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 53 /an4)
    )
    (pad 3 smd oval (at 0.95 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 81 N-0000058)
    )
    (pad 5 smd oval (at -0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3_AMP)
    )
    (pad 2 smd oval (at 0 1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (pad 4 smd oval (at 0.95 -1.45 270) (size 0.55 1)
      (layers F.Cu F.Paste F.Mask)
      (net 53 /an4)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM3216 (layer F.Cu) (tedit 57580BC7)
    (at 42 76.6 180)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C9 (at 2.9 0 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 0.8001 180) (layer F.SilkS) hide)
    (fp_text user + (at -2.3 1.1 180) (layer F.SilkS))
    (pad 1 smd oval (at -1.5 0 180) (size 1.4 1.8)
      (layers F.Cu F.Paste F.Mask)
      (net 45 /Vref)
    )
    (pad 2 smd oval (at 1.5 0 180) (size 1.4 1.8)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd\capacitors\C0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B24)
    (at 40.2 80.75)
    (attr smd)
    (fp_text reference R48 (at -2.4 0 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 60 N-0000020)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000028)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57582C13)
    (at 40.2 78.85)
    (attr smd)
    (fp_text reference R50 (at -2.35 -0.05 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000028)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 77 N-0000052)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B1D)
    (at 40.2 82.45)
    (attr smd)
    (fp_text reference R51 (at -2.35 0 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 60 N-0000020)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 64 N-0000026)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B10)
    (at 40.2 88.15)
    (attr smd)
    (fp_text reference R49 (at -2.4 0 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 58 N-0000019)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 57 N-0000017)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57582BED)
    (at 40.2 86.25)
    (attr smd)
    (fp_text reference R52 (at -2.35 0.05 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 57 N-0000017)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 66 N-0000029)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B13)
    (at 40.2 89.85)
    (attr smd)
    (fp_text reference R53 (at -2.35 0 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 0.50038) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 58 N-0000019)
    )
    (pad 2 smd oval (at 0.8 0) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 81 N-0000058)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module EJA (layer F.Cu) (tedit 57584ED5)
    (at 31 86.8)
    (fp_text reference J3 (at 0.05 -2.25) (layer F.SilkS))
    (fp_text value EJA (at -0.15 2.35) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 57 N-0000017)
    )
    (pad 2 thru_hole oval (at 5 5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 58 N-0000019)
    )
    (pad 3 thru_hole oval (at 5 -5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 58 N-0000019)
    )
    (pad 4 thru_hole oval (at 5 2.5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 58 N-0000019)
    )
    (pad 5 thru_hole oval (at 5 -2.5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 58 N-0000019)
    )
    (pad ~ thru_hole circle (at 0 -5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at -2.5 -5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at 0 5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at -2.5 5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at 5 0) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
  )
  (module EJA (layer F.Cu) (tedit 57584ED5)
    (at 31 74.2)
    (fp_text reference J2 (at 0.05 -2.25) (layer F.SilkS))
    (fp_text value EJA (at -0.15 2.35) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 65 N-0000028)
    )
    (pad 2 thru_hole oval (at 5 5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 60 N-0000020)
    )
    (pad 3 thru_hole oval (at 5 -5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 60 N-0000020)
    )
    (pad 4 thru_hole oval (at 5 2.5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 60 N-0000020)
    )
    (pad 5 thru_hole oval (at 5 -2.5) (size 2 1.5) (drill 1.2)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 60 N-0000020)
    )
    (pad ~ thru_hole circle (at 0 -5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at -2.5 -5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at 0 5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at -2.5 5) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
    (pad ~ thru_hole circle (at 5 0) (size 1.2 1.2) (drill 1.2)
      (layers *.Cu F.Mask)
    )
  )
  (module MAT_3X1_2,54 (layer F.Cu) (tedit 5758520F)
    (at 73.025 97.028 270)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P5 (at -4.628 0.925 270) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 1.7 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 29 /JRST)
    )
    (pad 2 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 31 /JTDO)
    )
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 30 /JTDI)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAT_3X2_2,54 (layer F.Cu) (tedit 5758565C)
    (at 70.9 65.6)
    (descr "Double rangee de contacts 2 x 3 pins")
    (tags CONN)
    (fp_text reference P7 (at -4.7 -1.85) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 3 2.4) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 1.27) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 5 /3V3_MCU)
    )
    (pad 3 thru_hole circle (at 0 1.27) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 78 N-0000054)
    )
    (pad 5 thru_hole circle (at 2.54 1.27) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (pad 2 thru_hole circle (at -2.54 -1.27) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 5 /3V3_MCU)
    )
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 79 N-0000055)
    )
    (pad 6 thru_hole circle (at 2.54 -1.27) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (model pin_array/pins_array_3x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAT_3X1_2,54 (layer F.Cu) (tedit 575851D5)
    (at 62.15 100.5 180)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference P6 (at -3.6 -1.8 180) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 1.7 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 54 AGND)
    )
    (pad 2 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 42 /UART_RX)
    )
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 1)
      (layers *.Cu *.Paste *.Mask F.SilkS)
      (net 43 /UART_TX)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 56.55 82.15)
    (attr virtual)
    (fp_text reference V8 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 63 N-0000024)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 56.55 81.15)
    (attr virtual)
    (fp_text reference V11 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 62 N-0000023)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 55.4 86.3)
    (attr virtual)
    (fp_text reference V14 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 61 N-0000022)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B0A)
    (at 40.2 91.75 180)
    (attr smd)
    (fp_text reference C24 (at 2.4 0 270) (layer F.SilkS))
    (fp_text value "100KpF X7R" (at 0 0.50038 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 81 N-0000058)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 47.35 102.65)
    (attr virtual)
    (fp_text reference V17 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 71.9 80.15)
    (attr virtual)
    (fp_text reference V26 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module SM0603 (layer F.Cu) (tedit 57614B19)
    (at 40.2 84.35 180)
    (attr smd)
    (fp_text reference C25 (at 2.4 0 270) (layer F.SilkS))
    (fp_text value "100KpF X7R" (at 0 0.50038 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 64 N-0000026)
    )
    (pad 2 smd oval (at 0.8 0 180) (size 0.65 1)
      (layers F.Cu F.Paste F.Mask)
      (net 54 AGND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module LOGO_SENO (layer F.Cu) (tedit 57585AAC)
    (at 34.5 65.6)
    (fp_text reference Lg1 (at 0 -1.4) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 1.2) (layer F.SilkS) hide)
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 42.3 66.2)
    (attr virtual)
    (fp_text reference V28 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (module via (layer F.Cu) (tedit 55DEF6C8)
    (at 42.3 73.15)
    (attr virtual)
    (fp_text reference V30 (at 0 -0.35052) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 0.35052) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.55 0.55) (drill 0.4)
      (layers *.Cu *.Paste *.SilkS *.Mask)
      (net 54 AGND)
      (clearance 0.0508)
      (zone_connect 2)
      (thermal_width 0.1)
      (thermal_gap 0.1)
    )
  )
  (gr_text 3V3 (at 93.8 69.3 90) (layer F.SilkS))
  (gr_text GND (at 64.7 98.7) (layer F.SilkS))
  (gr_text "BY HARDLAB\n" (at 34.4 63.85) (layer F.SilkS))
  (gr_text "BISENO V1.0\n" (at 34.35 67.65) (layer F.SilkS))
  (gr_text GND (at 75.5 69.3 90) (layer F.SilkS))
  (gr_text GND (at 74.7 107.1 90) (layer F.SilkS))
  (gr_text RX (at 62.15 98.7) (layer F.SilkS))
  (gr_text TX (at 59.55 98.7) (layer F.SilkS))
  (gr_line (start 28.25 71.95) (end 28.25 76.45) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 28.25 71.95) (end 26.85 71.95) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 26.85 71.95) (end 26.85 62.85) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 26.85 76.45) (end 28.25 76.45) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 26.85 84.55) (end 26.85 76.45) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 26.85 89.05) (end 26.85 93.15) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 28.25 89.05) (end 26.85 89.05) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 28.25 89.05) (end 28.25 84.55) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 28.25 84.55) (end 26.85 84.55) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 26.85 93.15) (end 46.85 93.15) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 46.85 93.15) (end 46.85 118.15) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 77.15 118.15) (end 46.85 118.15) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 77.15 93.15) (end 97.15 93.15) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 97.15 93.15) (end 97.15 62.85) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 97.15 62.85) (end 26.85 62.85) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 77.15 118.15) (end 77.15 93.15) (angle 90) (layer Edge.Cuts) (width 0.3))
  (zone (net 54) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 77 103.6) (xy 77 110) (xy 66.95 110) (xy 66.95 99.85) (xy 59.8 92.7)
        (xy 68.4 92.7) (xy 68.4 99.15) (xy 72.4 103.15) (xy 74.1 103.15) (xy 74.55 103.6)
      )
    )
    (polygon
      (pts        (xy 69 104.9) (xy 69 107.5) (xy 73.8 107.5) (xy 73.8 104.9)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 62.7 82.7) (xy 62.7 88.4) (xy 62.4 89) (xy 62.4 91.1) (xy 70.2 91.1)
        (xy 70.2 85.2) (xy 66.6 85.2) (xy 66.6 82.7)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 53.4 63) (xy 53.4 69) (xy 66.8 69) (xy 66.8 63)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 89.7 75.1) (xy 80.5 75.1) (xy 80.5 74.5) (xy 75 74.5) (xy 75 71.2)
        (xy 72.2 71.2) (xy 72.2 81) (xy 59.8 81) (xy 58.4 82.4) (xy 58.4 89)
        (xy 54.15 89) (xy 54.15 75.55) (xy 57.2 72.5) (xy 64.3 72.5) (xy 67 69.8)
        (xy 67 68.4) (xy 73.4 68.4) (xy 73.4 63.2) (xy 76.1 63.2) (xy 76.1 65.9)
        (xy 89.7 65.9) (xy 89.7 70.1) (xy 89.1 70.1) (xy 89.1 72.3) (xy 89.7 72.3)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 42.6 73.5) (xy 40.9 73.5) (xy 40.9 78.05) (xy 37.6 78.05) (xy 37.6 63.2)
        (xy 40.05 63.2) (xy 40.05 65.9) (xy 42.6 65.9)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 45.5 63.6) (xy 45.5 67.8) (xy 49.3 67.8) (xy 49.3 67.1) (xy 57 67.1)
        (xy 57 66.5) (xy 55.3 66.5) (xy 55.3 63.2) (xy 53.4 63.2) (xy 53.4 65.9)
        (xy 47.6 65.9) (xy 47.6 63.6)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 68 106.55) (xy 63.4 106.55) (xy 63.4 99) (xy 64.35 99) (xy 68 102.65)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 66.1 110) (xy 62.8 110) (xy 62.8 109.7) (xy 55.9 109.7) (xy 55.9 106.8)
        (xy 57.4 106.8) (xy 57.4 103.9) (xy 47 103.9) (xy 47 94.7) (xy 49 94.7)
        (xy 49 99) (xy 58.1 99) (xy 58.1 101.9) (xy 63.4 101.9) (xy 63.4 99)
        (xy 64.4 99) (xy 66.1 100.7)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 37.6 93) (xy 37.6 63.2) (xy 40.05 63.2) (xy 40.05 65.9) (xy 45.5 65.9)
        (xy 45.5 63.6) (xy 47.6 63.6) (xy 47.6 93)
      )
    )
  )
  (zone (net 54) (net_name AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 56.1 75) (xy 56.1 73.6) (xy 62.6 73.6) (xy 62.6 75) (xy 63.8 75)
        (xy 64.7 74.1) (xy 67.5 74.1) (xy 67.5 78.65) (xy 68.05 78.65) (xy 68.05 83.4)
        (xy 69.6 83.4) (xy 72.2 80.8) (xy 72.2 71.4) (xy 57 71.4) (xy 57 67.2)
        (xy 55.5 67.2) (xy 55.5 75)
      )
    )
  )
)
