(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 20)
    (no_connects 0)
    (area 47.676999 40.056999 93.039001 61.543001)
    (thickness 1.6)
    (drawings 55)
    (tracks 121)
    (zones 0)
    (modules 4)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 R1)
  (net 2 G1)
  (net 3 B1)
  (net 4 GND)
  (net 5 R2)
  (net 6 G2)
  (net 7 B2)
  (net 8 ADX0)
  (net 9 ADX1)
  (net 10 ADX2)
  (net 11 ADX3)
  (net 12 CLK)
  (net 13 LATCH)
  (net 14 OE)
  (net 15 "Net-(U1-Pad0)")
  (net 16 "Net-(U1-Pad1)")
  (net 17 "Net-(U1-Pad11)")
  (net 18 "Net-(U1-Pad12)")
  (net 19 "Net-(U1-Pad15)")
  (net 20 "Net-(U1-Pad16)")
  (net 21 "Net-(U1-Pad17)")
  (net 22 "Net-(U1-Pad18)")
  (net 23 "Net-(U1-Pad19)")
  (net 24 "Net-(U1-Pad26)")
  (net 25 "Net-(R1-Pad1)")
  (net 26 "Net-(U1-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ADX0)
    (add_net ADX1)
    (add_net ADX2)
    (add_net ADX3)
    (add_net B1)
    (add_net B2)
    (add_net CLK)
    (add_net G1)
    (add_net G2)
    (add_net GND)
    (add_net LATCH)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad0)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad26)")
    (add_net OE)
    (add_net R1)
    (add_net R2)
  )
  (module Teensy:HUB75 (layer F.Cu) (tedit 57899CEA)
    (at 50.8 50.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -9.6 0.8) (layer F.SilkS) hide)
    (fp_text value CONN_02X08 (at -8.4 3) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -1.27 -8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 R1))
    (pad 2 thru_hole oval (at 1.27 -8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 G1))
    (pad 3 thru_hole oval (at -1.27 -6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 B1))
    (pad 4 thru_hole oval (at 1.27 -6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at -1.27 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 R2))
    (pad 6 thru_hole oval (at 1.27 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 G2))
    (pad 7 thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 B2))
    (pad 8 thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 9 thru_hole oval (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 ADX0))
    (pad 10 thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 ADX1))
    (pad 11 thru_hole oval (at -1.27 3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 ADX2))
    (pad 12 thru_hole oval (at 1.27 3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 ADX3))
    (pad 13 thru_hole oval (at -1.27 6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 CLK))
    (pad 14 thru_hole oval (at 1.27 6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 LATCH))
    (pad 15 thru_hole oval (at -1.27 8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 OE))
    (pad 16 thru_hole oval (at 1.27 8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Teensy:Teensy-3.1_NoSilk (layer F.Cu) (tedit 5789A77B)
    (at 88.9 43.18 180)
    (fp_text reference U1 (at -5.08 -7.62 270) (layer F.SilkS) hide)
    (fp_text value Teensy_3.1 (at 5.08 -10.16 180) (layer F.Fab) hide)
    (pad 0 thru_hole circle (at 0 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U1-Pad0)"))
    (pad 1 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 R1))
    (pad 3 thru_hole circle (at 7.62 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 LATCH))
    (pad 4 thru_hole circle (at 10.16 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 OE))
    (pad 5 thru_hole circle (at 12.7 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 G1))
    (pad 6 thru_hole circle (at 15.24 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 B1))
    (pad 7 thru_hole circle (at 17.78 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 G2))
    (pad 8 thru_hole circle (at 20.32 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 LATCH))
    (pad 9 thru_hole circle (at 22.86 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 ADX0))
    (pad 10 thru_hole circle (at 25.4 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 ADX1))
    (pad 11 thru_hole circle (at 27.94 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 30.48 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 27.94 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 CLK))
    (pad 15 thru_hole circle (at 25.4 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at 22.86 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U1-Pad16)"))
    (pad 17 thru_hole circle (at 20.32 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 17.78 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 15.24 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 12.7 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 B2))
    (pad 21 thru_hole circle (at 10.16 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 R2))
    (pad 22 thru_hole circle (at 7.62 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 ADX2))
    (pad 23 thru_hole circle (at 5.08 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 ADX3))
    (pad 24 thru_hole circle (at 2.54 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R1-Pad1)"))
    (pad 25 thru_hole circle (at 0 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 26 thru_hole circle (at -2.54 -15.24 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at -2.54 0 180) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Logo:logo (layer B.Cu) (tedit 0)
    (at 87.1 51.5 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Discret:R3 (layer B.Cu) (tedit 57A5CA28)
    (at 85.09 45.72 180)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R1 (at 0 -0.127 180) (layer B.SilkS) hide)
    (fp_text value 4.7k (at 0 -0.127 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask B.SilkS)
      (net 14 OE))
  )
  (gr_text "Female Headers\nFor Panel Socket" (at 55.1 50.8 90) (layer B.SilkS))
  (gr_text "Male Headers\nFor Cable" (at 55.1 50.8 90) (layer F.SilkS))
  (gr_text "RED WIRE" (at 55.4 41.4) (layer F.SilkS))
  (gr_text USB (at 91.44 50.8 270) (layer F.SilkS))
  (gr_text "Teensy 3.x\nThis Side" (at 72.136 50.8) (layer F.SilkS))
  (gr_text "Maniacal Labs\nHUB75 \nTeensy Adapter" (at 72.5 51.7) (layer B.SilkS))
  (gr_line (start 48.768 61.468) (end 91.948 61.468) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.964 41.148) (end 92.964 60.452) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 91.948 60.452) (end 92.964 60.452) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.768 40.132) (end 91.948 40.132) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 91.948 41.148) (end 91.948 40.132) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47.752 41.148) (end 47.752 60.452) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 48.768 60.452) (end 48.768 61.468) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 48.768 41.148) (end 47.752 41.148) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.456 60.96) (xy 48.26 60.96) (xy 48.26 40.64) (xy 92.456 40.64) (xy 92.456 60.96)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.456 60.96) (xy 48.26 60.96) (xy 48.26 40.64) (xy 92.456 40.64) (xy 92.456 60.96)
      )
    )
  )
)
